# pcieIrqEOIReg_s Struct Reference
[PCIE LLD Application Register Definitions]

Specification of the End of Interrupt Register. More...

`#include <pcie.h>`

## Data Fields

uint32_t | raw
uint8_t | EOI
| [wo] EOI for interrupts.

## Detailed Description

Specification of the End of Interrupt Register.

## Field Documentation

uint8_t pcieIrqEOIReg_s::EOI

[wo] EOI for interrupts.

Write to indicate end-of-interrupt for the interrupt events. Write 0 to mark EOI for INTA, 1 for INTB and so on.

Field size: 4 bits

uint32_t pcieIrqEOIReg_s::raw

[ro] Raw image of register on read; actual value on write

The documentation for this struct was generated from the following file:

- pcie.h

Copyright 2012, Texas Instruments Incorporated