# hyplnkIntPtrIdxReg_s Struct Reference
[HYPLNK LLD Register Definitions]

Specification of the Interupt Control Index Register. More...

`#include <hyplnk.h>`

## Data Fields

uint32_t | raw
| [ro] Raw image of register on read; actual value on write
uint8_t | intPtrIdx
| [rw] Selects which Interrupt Pointer is used

## Detailed Description

Specification of the Interupt Control Index Register.

The Interrupt Pointer Index Register is used to control which Interrupt Pointer Register is read or written via hyplnkIntPtrIdxReg_s. The Interrupt Pointer Registers typically map to microprocessor interrupt controller set registers which get set to a one to interrupt that processor.

## Field Documentation

uint8_t hyplnkIntPtrIdxReg_s::intPtrIdx

[rw] Selects which Interrupt Pointer is used

Field size: 4 bits

The interrupt pointer specified by intPtrIdx can be read or written via hyplnkIntPtrValReg_s;

The documentation for this struct was generated from the following file:

- hyplnk.h

Copyright 2012, Texas Instruments Incorporated