# Srio_DioBindAddrInfo Struct Reference
[SRIO LLD Data Structures]

SRIO Socket DIO Binding Information. More...

`#include <srio_drv.h>`

## Data Fields

uint8_t | doorbellValid
| Indicates if doorbell information needs to be sent out or not.
uint8_t | intrRequest
| CPU controlled request bit used for interrupt generation.
uint8_t | supInt
| Supress good interrupt.
uint8_t | xambs
| RapidIO xambs field specifying extended address.
uint8_t | priority
| Packet Priority.

## Detailed Description

SRIO Socket DIO Binding Information.

The structure describes the address information required for binding a DIO socket. This includes information which describes the DIO endpoint characteristics and is used to describe the local characteristics of the endpoint.

The documentation for this struct was generated from the following file:

- srio_drv.h

Copyright 2012, Texas Instruments Incorporated