# pcieLegacyIrqEnableClrReg_s Struct Reference
[PCIE LLD Application Register Definitions]

Specification of the Legacy Interrupt Enable Clear Register. More...

`#include <pcie.h>`

## Data Fields

uint32_t | raw
uint8_t | legacyIrqEnClr
| [rw] 0 has no effect; 1 disables the interrupt

## Detailed Description

Specification of the Legacy Interrupt Enable Clear Register.

There are multiple instances (0-7) of this register.

## Field Documentation

uint8_t pcieLegacyIrqEnableClrReg_s::legacyIrqEnClr

[rw] 0 has no effect; 1 disables the interrupt

Field size: 1 bits

uint32_t pcieLegacyIrqEnableClrReg_s::raw

[ro] Raw image of register on read; actual value on write

The documentation for this struct was generated from the following file:

- pcie.h

Copyright 2012, Texas Instruments Incorporated