# pcieLegacyIrqEnableSetReg_s Struct Reference
[PCIE LLD Application Register Definitions]

Specification of the Legacy Interrupt Enable Set Register. More...

`#include <pcie.h>`

## Data Fields

uint32_t | raw
uint8_t | legacyIrqEnSet
| [rw] 0: has no effect; 1: enables the interrupt

## Detailed Description

Specification of the Legacy Interrupt Enable Set Register.

There are multiple instances (0-7) of this register.

## Field Documentation

uint8_t pcieLegacyIrqEnableSetReg_s::legacyIrqEnSet

[rw] 0: has no effect; 1: enables the interrupt

Field size: 1 bits

uint32_t pcieLegacyIrqEnableSetReg_s::raw

[ro] Raw image of register on read; actual value on write

The documentation for this struct was generated from the following file:

- pcie.h

Copyright 2012, Texas Instruments Incorporated