# RM Low Level Driver Enums
[RM LLD Module API]

## Enumerations

enum | Rm_ResourceType { Rm_resource_QMSS_FIRMWARE_PDSP = 0, Rm_resource_QMSS_QUEUE, Rm_resource_QMSS_MEMORY_REGION, Rm_resource_QMSS_LINKING_RAM_CONTROL, Rm_resource_QMSS_LINKING_RAM, Rm_resource_QMSS_ACCUM_CH, Rm_resource_QMSS_QOS_TIMER, Rm_resource_QMSS_QOS_CLUSTER,
Rm_resource_QMSS_QOS_QUEUE, Rm_resource_CPPI_TX_CH, Rm_resource_CPPI_RX_CH, Rm_resource_CPPI_RX_FLOW,
Rm_resource_PA_FIRMWARE, Rm_resource_PA_LUT
}
| LLD resource type. More...

## Enumeration Type Documentation

enum Rm_ResourceType

LLD resource type.

Enumerator:

  Rm_resource_QMSS_FIRMWARE_PDSP | QMSS Firmware Type
  Rm_resource_QMSS_QUEUE | QMSS Queue Type
  Rm_resource_QMSS_MEMORY_REGION | QMSS Memory Region Type
  Rm_resource_QMSS_LINKING_RAM_CONTROL | QMSS Linking RAM Control Type
  Rm_resource_QMSS_LINKING_RAM | QMSS Linking RAM Type
  Rm_resource_QMSS_ACCUM_CH | QMSS Accumulator Channel Type
  Rm_resource_QMSS_QOS_TIMER | QMSS QOS PDSP Timer
  Rm_resource_QMSS_QOS_CLUSTER | QMSS QOS Cluster Type
  Rm_resource_QMSS_QOS_QUEUE | QMSS QOS Queue Type
  Rm_resource_CPPI_TX_CH | CPPI Transmit Channel Type
  Rm_resource_CPPI_RX_CH | CPPI Receive Channel Type
  Rm_resource_CPPI_RX_FLOW | CPPI Receive Flow Type
  Rm_resource_PA_FIRMWARE | PA Firmware Type
  Rm_resource_PA_LUT | PA LUT Type

Copyright 2012, Texas Instruments Incorporated