# pcieErrSrcIDReg_s Struct Reference
[PCIE LLD Extended Capabilities Register Definitions]

Specification of the Error Source Identification register. More...

`#include <pcie.h>`

## Data Fields

uint32_t | raw
uint16_t | fnfSrcID
| [ro] Fatal or Non-Fatal error source identification
uint16_t | corrSrcID
| [ro] Correctable error source identification

## Detailed Description

Specification of the Error Source Identification register.

This register may be used for both endpoint and root complex modes.

## Field Documentation

uint16_t pcieErrSrcIDReg_s::corrSrcID

[ro] Correctable error source identification

Field size: 16 bits

uint16_t pcieErrSrcIDReg_s::fnfSrcID

[ro] Fatal or Non-Fatal error source identification

Field size: 16 bits

uint32_t pcieErrSrcIDReg_s::raw

[ro] Raw image of register on read; actual value on write

The documentation for this struct was generated from the following file:

- pcie.h

Copyright 2012, Texas Instruments Incorporated