# pcieIbStartLoReg_s Struct Reference
[PCIE LLD Application Register Definitions]

Specification of the Inbound Translation Start Address Low Register. More...

`#include <pcie.h>`

## Data Fields

uint32_t | raw
| [ro] Raw image of register on read; actual value on write
uint32_t | ibStartLo
| [rw] Start address bits [31:8] for inbound translation region

## Detailed Description

Specification of the Inbound Translation Start Address Low Register.

There are multiple instances (0-3) of this register.

## Field Documentation

uint32_t pcieIbStartLoReg_s::ibStartLo

[rw] Start address bits [31:8] for inbound translation region

Field size: 24 bits

The documentation for this struct was generated from the following file:

- pcie.h

Copyright 2012, Texas Instruments Incorporated