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1SO776x High-speed, robust EMC, reil

1 Features

+ 100 Mbps data rate
* Robust isolation barrier:
— >30-Year projected lifetime
— Up to 5000 Vrys isolation rating
— Up to 12.8 kV surge capability
— +100 kV/ps Typical CMTI
« Wide supply range: 2.25V to 5.5V
¢ 2.25-Vto 5.5-V Level translation
« Default output high (1ISO776x) and low (ISO776xF)
Options




