#
#Component attribute names
#
@0 .comp_mount_type
@1 .comp_height

# CMP 0
CMP 48 0.7702052 3.2430224 180 N R191 HCJ0805ZT0R00 ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.seielect.com/Catalog/SEI-HCJ.pdf'
PRP Datasheet 'https://www.seielect.com/Catalog/SEI-HCJ.pdf'
PRP Datasheet_Path 'datasheets/Res-HCJ0805ZT0R00.pdf'
PRP Digikey_Description 'RES 0 OHM JUMPER 1/2W 0805'
PRP Digikey_Part_Number 'HCJ0805ZT0R00CT-ND'
PRP helpURL 'https://upverter.com/upn/revision/7e7e8a5f55cb1810/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Stackpole'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0805'
PRP Part_Number 'HCJ0805ZT0R00'
PRP PartNumber 'HCJ0805ZT0R00'
PRP Power '500mW'
PRP Power_W '500mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'HCJ'
PRP SizeZ_mm '0.85mm'
PRP Supplier_1 'Digikey'
PRP Supplier_Part_Number_1 'HCJ0805ZT0R00CT-ND'
PRP Technology 'Metal Foil'
PRP Value '0'
TOP 0 0.8135123 3.2430224 180 N 3 2 1
TOP 1 0.7268981 3.2430224 180 N 138 14 2
#
# CMP 1
CMP 42 1.0069684 3.3486303 90 N R190 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 1.0069684 3.3688074 90 N 4 1 1
TOP 1 1.0069684 3.3284531 90 N 146 2 2
#
# CMP 2
CMP 42 0.985 3.2668117 270 N R95 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 0.985 3.2466346 270 N 14 1 1
TOP 1 0.985 3.2869889 270 N 24 2 2
#
# CMP 3
CMP 31 3.2529932 1.9800011 90 N J3 1909763-1 ;0=1,1=0.0130
PRP AEC_Qualified 'No'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1909763%7FB3%7Fpdf%7FEnglish%7FENG_CD_1909763_B3.pdf%7F1909763-1'
PRP Conn_Orientation 'Vertical'
PRP ContactFinish 'Gold,Nickel'
PRP Datasheet 'https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1909763%7FB3%7Fpdf%7FEnglish%7FENG_CD_1909763_B3.pdf%7F1909763-1'
PRP Datasheet_Path 'datasheets/Conn-1909763-1.pdf'
PRP Dielectric_Material 'Liquid Crystal Polymer'
PRP Digikey_Description 'CONN UMCC JACK STR 50OHM SMD'
PRP Digikey_Part_Number 'A118077CT-ND'
PRP Frequency_Fixed '0-6GHz'
PRP helpURL 'https://upverter.com/upn/revision/11470e095e29653d/'
PRP Impedance '50O'
PRP Lead_Free 'Yes'
PRP Manufacturer 'TE Connectivity'
PRP Mouser_Description 'RF Connectors / Coaxial Connectors 2/2.55MM STD SMT ULTRA MINI RF JACK'
PRP Mouser_Part_Number '571-1909763-1'
PRP Operating_Temperature_Range '-40°C to +90°C'
PRP PackageReference 'SMT_JACK _CONN'
PRP Part_Number '1909763-1'
PRP PartNumber '1909763-1'
PRP PinCount '1'
PRP RoHS 'TRUE'
PRP SizeZ_mm '1.5mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'A118077CT-ND'
PRP Supplier_Part_Number_2 '571-1909763-1'
TOP 0 3.1900011 1.9800011 90 N 16 7 1
TOP 1 3.2500404 2.038072 90 N 424 630 2
TOP 2 3.2500404 1.9219302 90 N 424 631 3
#
# CMP 4
CMP 32 0.8790005 3.5702625 270 N L11 ADL32VHR-3R9M ;0=1,1=0.0130
PRP AEC_Qualified 'No'
PRP Datasheet_Path 'datasheets/Ind-ADL32VHR-3R9M.pdf'
PRP DCR_ohm '0.36'
PRP helpURL 'https://upverter.com/upn/revision/bc70136ade516722/'
PRP Imax_A '540mA'
PRP Ind_H '3.9µH'
PRP Isat '860mA'
PRP Lead_Free 'Yes'
PRP Manufacturer 'TDK'
PRP Operating_Temperature_Range '-40°C to +150°C'
PRP PackageReference 'SMT_3MM2_2MM5'
PRP Part_Number 'ADL32VHR-3R9M'
PRP PartNumber 'ADL32VHR-3R9M'
PRP RoHS 'TRUE'
PRP SizeZ_mm '2.5mm'
PRP Technology 'Wirewound'
PRP Test_Frequency '100kHz'
PRP Tolerance__ '20%'
TOP 0 0.8484887 3.5131759 270 N 70 4 1
TOP 1 0.9095123 3.5131759 270 N 30 0 2
TOP 2 0.9095123 3.6273491 270 N 424 632 3
TOP 3 0.8484887 3.6273491 270 N 71 4 4
#
# CMP 5
CMP 33 1.3130005 3.3883863 90 N FB3 BLM18KG601SH1 ;0=1,1=0.0130
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.murata.com/products/productdata/8796737273886/QNFA9101.pdf?1590156016000'
PRP Datasheet 'https://www.murata.com/products/productdata/8796737273886/QNFA9101.pdf?1590156016000'
PRP Datasheet_Path 'datasheets/FBead-BLM18KG601SH1.pdf'
PRP DCR_ohm '0.15'
PRP Digikey_Description 'FERRITE BEAD 600 OHM 0603 1LN'
PRP Digikey_Part_Number '490-13259-1-ND'
PRP helpURL 'https://upverter.com/upn/revision/22cc867aa2f8f768/'
PRP Imax_A '1.3A'
PRP Impedance_At_Frequency '600O @ 100MHz'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Murata'
PRP Material 'Ferrite'
PRP Mouser_Part_Number '81-BLM18KG601SH1D'
PRP Operating_Temperature_Range '-55°C to +125°C'
PRP PackageReference '0603 (1608 Metric)'
PRP Part_Number 'BLM18KG601SH1'
PRP PartNumber 'BLM18KG601SH1'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.95mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '490-13259-1-ND'
PRP Supplier_Part_Number_2 '81-BLM18KG601SH1D'
PRP Test_Frequency '100MHz'
PRP Tolerance__ '25%'
TOP 0 1.3130005 3.4149611 90 N 109 37 1
TOP 1 1.3130005 3.3618115 90 N 98 5 2
#
# CMP 6
CMP 37 2.0990005 1.9971265 90 N R199 CRCW04020000Z0EDHP ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.vishay.com/docs/20043/crcwhpe3.pdf'
PRP Datasheet 'https://www.vishay.com/docs/20043/crcwhpe3.pdf'
PRP Datasheet_Path 'datasheets/Res-CRCW04020000Z0EDHP.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/5W 0402'
PRP Digikey_Part_Number '541-0.0YBCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/5e0a18f71149352e/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Vishay Dale'
PRP Mouser_Description 'Resistor; Thick Film; 0 Ohms; 0.125 W; 0 Ohms Jumper; SMT; 0402; TCR 0 ppm/DegC'
PRP Mouser_Part_Number '71-CRCW04020000Z0EDH'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'CRCW04020000Z0EDHP'
PRP PartNumber 'CRCW04020000Z0EDHP'
PRP Power_W '200mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'CRCW-HP e3'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '541-0.0YBCT-ND'
PRP Supplier_Part_Number_2 '71-CRCW04020000Z0EDH'
PRP Technology 'Thick Film'
PRP Value '0'
PRP VDC_V '50V'
TOP 0 2.0990005 2.0177958 90 N 308 74 1
TOP 1 2.0990005 1.9764572 90 N 109 38 2
#
# CMP 7
CMP 1 0.4279755 1.4685422 270 N R72 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 0.4279755 1.4575186 180 N 124 1 1
TOP 1 0.4279755 1.4795658 180 N 58 1 2
#
# CMP 8
CMP 1 0.9580236 0.602 0 N R366 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 0.947 0.602 270 N 66 0 1
TOP 1 0.9690472 0.602 270 N 52 1 2
#
# CMP 9
CMP 1 0.9580236 0.63 0 N R365 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 0.947 0.63 270 N 65 0 1
TOP 1 0.9690472 0.63 270 N 51 1 2
#
# CMP 10
CMP 1 0.9580236 0.661055 0 N R364 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 0.947 0.661055 270 N 64 0 1
TOP 1 0.9690472 0.661055 270 N 50 1 2
#
# CMP 11
CMP 1 0.9580236 0.689055 0 N R363 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 0.947 0.689055 270 N 63 0 1
TOP 1 0.9690472 0.689055 270 N 49 1 2
#
# CMP 12
CMP 1 0.9580236 0.734 0 N R361 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 0.947 0.734 270 N 6 1 1
TOP 1 0.9690472 0.734 270 N 10 2 2
#
# CMP 13
CMP 1 0.9580236 0.7619998 0 N R351 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 0.947 0.7619998 270 N 5 1 1
TOP 1 0.9690472 0.7619998 270 N 9 2 2
#
# CMP 14
CMP 1 0.9144388 0.835871 0 N R349 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 0.9034152 0.835871 270 N 8 1 1
TOP 1 0.9254624 0.835871 270 N 48 3 2
#
# CMP 15
CMP 1 0.9144388 0.863871 0 N R345 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 0.9034152 0.863871 270 N 7 1 1
TOP 1 0.9254624 0.863871 270 N 47 3 2
#
# CMP 16
CMP 1 0.9144388 0.929 0 N R341 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 0.9034152 0.929 270 N 60 1 1
TOP 1 0.9254624 0.929 270 N 46 2 2
#
# CMP 17
CMP 1 0.9144388 0.957 0 N R327 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 0.9034152 0.957 270 N 59 1 1
TOP 1 0.9254624 0.957 270 N 45 2 2
#
# CMP 18
CMP 5 1.1617485 3.1874034 180 N R350 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 1.1814335 3.1874034 90 N 90 1 1
TOP 1 1.1420634 3.1874034 90 N 424 542 2
#
# CMP 19
CMP 11 0.634176 3.6154368 0 N R281 ERJ-P06F1001V ;0=1,1=0.0571
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE4.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'ERJ-P06F1001V'
PRP Power_W '250mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '1k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 'P16058CT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-P06F1001V'
PRP Supplier_Part_Number_3 '1750754'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '1.00k'
PRP Value1 '1%'
PRP Value2 '0.25W'
PRP Value_Code '1k00'
PRP ValueDisplayed '1.00k'
PRP VDC_V '400V'
TOP 0 0.6046484 3.6154368 270 N 93 0 1
TOP 1 0.6637035 3.6154368 270 N 71 3 2
#
# CMP 20
CMP 11 0.634176 3.5250877 0 N R275 ERJ-P06F1001V ;0=1,1=0.0571
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000CE4.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'ERJ-P06F1001V'
PRP Power_W '250mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '1k'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 'P16058CT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-P06F1001V'
PRP Supplier_Part_Number_3 '1750754'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '1.00k'
PRP Value1 '1%'
PRP Value2 '0.25W'
PRP Value_Code '1k00'
PRP ValueDisplayed '1.00k'
PRP VDC_V '400V'
TOP 0 0.6046484 3.5250877 270 N 93 1 1
TOP 1 0.6637035 3.5250877 270 N 70 3 2
#
# CMP 21
CMP 85 1.1400005 3.3658115 270 N TP3 TESTPOINT ;0=1,1=0.0000
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ClassName ''
PRP ComponentLink1Description ''
PRP ComponentLink1URL ''
PRP CompType 'Testpoint'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'N/A'
PRP MountType ''
PRP Note ''
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
PRP RoHS ''
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Value ''
TOP 0 1.1400005 3.3658115 270 N 43 3 1
#
# CMP 22
CMP 10 0.4892282 3.6154368 0 N R282 CRCW0805100KJNEA ;0=1,1=0.0571
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'CRCW0805100KJNEA'
PRP Power_W '125mW'
PRP Res_ohm '100k'
PRP RoHS 'E'
PRP SizeArea_mm2 '2.5'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-100KACT-ND'
PRP Supplier_Part_Number_2 '59M6850'
PRP Supplier_Part_Number_3 '71-CRCW0805J-100K-E3'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP Value '100k'
PRP Value1 '5%'
PRP Value2 '0.125W'
PRP Value_Code '100k'
PRP ValueDisplayed '100k'
PRP VDC_V '150V'
TOP 0 0.4492283 3.6154368 0 N 424 620 1
TOP 1 0.5292283 3.6154368 0 N 93 2 2
#
# CMP 23
CMP 5 1.6300675 3.2369922 0 N R258 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 1.6103825 3.2369922 270 N 35 1 1
TOP 1 1.6497526 3.2369922 270 N 69 15 2
#
# CMP 24
CMP 5 1.6300203 3.1519707 0 N R257 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 1.6103353 3.1519707 270 N 79 1 1
TOP 1 1.6497054 3.1519707 270 N 69 16 2
#
# CMP 25
CMP 5 1.6300203 3.1039445 0 N R256 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 1.6103353 3.1039445 270 N 80 1 1
TOP 1 1.6497054 3.1039445 270 N 69 17 2
#
# CMP 26
CMP 5 1.6300203 3.0560566 0 N R255 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 1.6103353 3.0560566 270 N 81 1 1
TOP 1 1.6497054 3.0560566 270 N 69 18 2
#
# CMP 27
CMP 5 1.4747464 3.3600489 270 N R254 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 1.4747464 3.3403639 180 N 108 1 1
TOP 1 1.4747464 3.379734 180 N 69 19 2
#
# CMP 28
CMP 5 1.4012914 3.3600489 270 N R252 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 1.4012914 3.3403639 180 N 77 1 1
TOP 1 1.4012914 3.379734 180 N 69 20 2
#
# CMP 29
CMP 5 1.1900005 3.3824965 270 N R251 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 1.1900005 3.3628115 180 N 43 2 1
TOP 1 1.1900005 3.4021816 180 N 424 543 2
#
# CMP 30
CMP 5 1.116036 2.280804 90 N R249 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 1.116036 2.300489 0 N 404 1 1
TOP 1 1.116036 2.2611189 0 N 82 1 2
#
# CMP 31
CMP 5 1.1714942 2.280804 90 N R247 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 1.1714942 2.300489 0 N 403 3 1
TOP 1 1.1714942 2.2611189 0 N 83 1 2
#
# CMP 32
CMP 5 1.47338 2.860812 0 N R245 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 1.453695 2.860812 270 N 401 1 1
TOP 1 1.4930651 2.860812 270 N 77 2 2
#
# CMP 33
CMP 5 1.4733801 2.7730898 0 N R240 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 1.4536951 2.7730898 270 N 397 1 1
TOP 1 1.4930652 2.7730898 270 N 78 1 2
#
# CMP 34
CMP 5 1.4731156 2.7248875 0 N R239 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 1.4534306 2.7248875 270 N 398 1 1
TOP 1 1.4928007 2.7248875 270 N 79 2 2
#
# CMP 35
CMP 5 1.4716736 2.6765989 0 N R238 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 1.4519886 2.6765989 270 N 399 1 1
TOP 1 1.4913587 2.6765989 270 N 80 2 2
#
# CMP 36
CMP 5 1.472398 2.6313103 0 N R237 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 1.452713 2.6313103 270 N 400 1 1
TOP 1 1.4920831 2.6313103 270 N 81 2 2
#
# CMP 37
CMP 5 1.4720913 2.5770217 0 N R234 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 1.4524063 2.5770217 270 N 402 1 1
TOP 1 1.4917764 2.5770217 270 N 42 1 2
#
# CMP 38
CMP 5 1.2605111 3.1422048 180 N R93 ERJ-2RKF4700X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/lecs/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF4700X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '470'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 'P470LCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2RKF4700X'
PRP Supplier_Part_Number_3 '2397145'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '470'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '470R'
PRP ValueDisplayed '470'
PRP VDC_V '50V'
TOP 0 1.2801961 3.1422048 90 N 91 0 1
TOP 1 1.240826 3.1422048 90 N 34 1 2
#
# CMP 39
CMP 5 1.162885 3.0889941 0 N R46 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 1.1432 3.0889941 270 N 69 21 1
TOP 1 1.1825701 3.0889941 270 N 106 2 2
#
# CMP 40
CMP 56 1.3019126 3.091949 180 N D14 SML-P12DTT86R ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP Color 'Orange'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://fscdn.rohm.com/en/products/databook/datasheet/opto/led/chip_mono/sml-p12dtt86(r)-e.pdf'
PRP Datasheet 'https://fscdn.rohm.com/en/products/databook/datasheet/opto/led/chip_mono/sml-p12dtt86(r)-e.pdf'
PRP Datasheet_Path 'datasheets/Diode-SML-P12DTT86R.pdf'
PRP Digikey_Description 'LED ORANGE CLEAR 1006 SMD'
PRP Digikey_Part_Number '846-1200-1-ND'
PRP Forward_Current '20mA'
PRP helpURL 'https://upverter.com/upn/revision/731415a088c17ee2/'
PRP LambdaD '605nm'
PRP Lead_Free 'Yes'
PRP Led_Orientation 'Top View'
PRP Luminous_Intensity '100mcd'
PRP Manufacturer 'Rohm Semiconductor'
PRP Mouser_Description 'SML-P1 Series Orange 0402 Clear 100 mcd 2.1V Surface Mount PICOLED? LED'
PRP Mouser_Part_Number '755-SML-P12DTT86R'
PRP Operating_Temperature_Range '-40°C to +85°C'
PRP PackageReference '0402'
PRP Part_Number 'SML-P12DTT86R'
PRP PartNumber 'SML-P12DTT86R'
PRP Power_TotalModule '52mW'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.25mm'
PRP TJmax_C '110°C'
PRP Vf_V '2.1V'
PRP Vr_V '5V'
TOP 0 1.3196291 3.091949 180 N 424 666 1
TOP 1 1.2841961 3.091949 180 N 91 1 2
#
# CMP 41
CMP 57 1.4568398 2.9906679 270 N D10 SML-P12YTT86R ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP Color 'Yellow'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://fscdn.rohm.com/en/products/databook/datasheet/opto/led/chip_mono/sml-p12ytt86(r)-e.pdf'
PRP Datasheet 'https://fscdn.rohm.com/en/products/databook/datasheet/opto/led/chip_mono/sml-p12ytt86(r)-e.pdf'
PRP Datasheet_Path 'datasheets/Diode-SML-P12YTT86R.pdf'
PRP Digikey_Description 'LED YELLOW CLEAR 1006 SMD'
PRP Digikey_Part_Number '846-1204-1-ND'
PRP Forward_Current '20mA'
PRP helpURL 'https://upverter.com/upn/revision/614bdbe763342bb9/'
PRP LambdaD '590nm'
PRP Lead_Free 'Yes'
PRP Led_Orientation 'Top View'
PRP Luminous_Intensity '100mcd'
PRP Manufacturer 'Rohm Semiconductor'
PRP Mouser_Description 'SML-P1 Series Yellow 0402 Clear 100 mcd 2.1V Surface Mount PICOLED? LED'
PRP Mouser_Part_Number '755-SML-P12YTT86R'
PRP Operating_Temperature_Range '-40°C to +85°C'
PRP PackageReference '0402'
PRP Part_Number 'SML-P12YTT86R'
PRP PartNumber 'SML-P12YTT86R'
PRP Power_TotalModule '52mW'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.25mm'
PRP TJmax_C '110°C'
PRP Vf_V '2.1V'
PRP Vr_V '5V'
TOP 0 1.4568398 2.9729514 270 N 424 667 1
TOP 1 1.4568398 3.0083844 270 N 92 1 2
#
# CMP 42
CMP 31 3.2529932 1.6500011 90 N J5 1909763-1 ;0=1,1=0.0461
PRP AEC_Qualified 'No'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1909763%7FB3%7Fpdf%7FEnglish%7FENG_CD_1909763_B3.pdf%7F1909763-1'
PRP Conn_Orientation 'Vertical'
PRP ContactFinish 'Gold,Nickel'
PRP Datasheet 'https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1909763%7FB3%7Fpdf%7FEnglish%7FENG_CD_1909763_B3.pdf%7F1909763-1'
PRP Datasheet_Path 'datasheets/Conn-1909763-1.pdf'
PRP Dielectric_Material 'Liquid Crystal Polymer'
PRP Digikey_Description 'CONN UMCC JACK STR 50OHM SMD'
PRP Digikey_Part_Number 'A118077CT-ND'
PRP Frequency_Fixed '0-6GHz'
PRP helpURL 'https://upverter.com/upn/revision/11470e095e29653d/'
PRP Impedance '50O'
PRP Lead_Free 'Yes'
PRP Manufacturer 'TE Connectivity'
PRP Mouser_Description 'RF Connectors / Coaxial Connectors 2/2.55MM STD SMT ULTRA MINI RF JACK'
PRP Mouser_Part_Number '571-1909763-1'
PRP Operating_Temperature_Range '-40°C to +90°C'
PRP PackageReference 'SMT_JACK _CONN'
PRP Part_Number '1909763-1'
PRP PartNumber '1909763-1'
PRP PinCount '1'
PRP RoHS 'TRUE'
PRP SizeZ_mm '1.5mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'A118077CT-ND'
PRP Supplier_Part_Number_2 '571-1909763-1'
TOP 0 3.1900011 1.6500011 90 N 56 7 1
TOP 1 3.2500404 1.708072 90 N 424 544 2
TOP 2 3.2500404 1.5919302 90 N 424 545 3
#
# CMP 43
CMP 31 1.5900011 2.117009 180 N J1 1909763-1 ;0=1,1=0.0461
PRP AEC_Qualified 'No'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1909763%7FB3%7Fpdf%7FEnglish%7FENG_CD_1909763_B3.pdf%7F1909763-1'
PRP Conn_Orientation 'Vertical'
PRP ContactFinish 'Gold,Nickel'
PRP Datasheet 'https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1909763%7FB3%7Fpdf%7FEnglish%7FENG_CD_1909763_B3.pdf%7F1909763-1'
PRP Datasheet_Path 'datasheets/Conn-1909763-1.pdf'
PRP Dielectric_Material 'Liquid Crystal Polymer'
PRP Digikey_Description 'CONN UMCC JACK STR 50OHM SMD'
PRP Digikey_Part_Number 'A118077CT-ND'
PRP Frequency_Fixed '0-6GHz'
PRP helpURL 'https://upverter.com/upn/revision/11470e095e29653d/'
PRP Impedance '50O'
PRP Lead_Free 'Yes'
PRP Manufacturer 'TE Connectivity'
PRP Mouser_Description 'RF Connectors / Coaxial Connectors 2/2.55MM STD SMT ULTRA MINI RF JACK'
PRP Mouser_Part_Number '571-1909763-1'
PRP Operating_Temperature_Range '-40°C to +90°C'
PRP PackageReference 'SMT_JACK _CONN'
PRP Part_Number '1909763-1'
PRP PartNumber '1909763-1'
PRP PinCount '1'
PRP RoHS 'TRUE'
PRP SizeZ_mm '1.5mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'A118077CT-ND'
PRP Supplier_Part_Number_2 '571-1909763-1'
TOP 0 1.5900011 2.1800011 180 N 57 8 1
TOP 1 1.648072 2.1199618 180 N 424 547 2
TOP 2 1.5319302 2.1199618 180 N 424 546 3
#
# CMP 44
CMP 85 1.336 3.251 0 N TP2 TESTPOINT ;0=1,1=0.0000
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ClassName ''
PRP ComponentLink1Description ''
PRP ComponentLink1URL ''
PRP CompType 'Testpoint'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'N/A'
PRP MountType ''
PRP Note ''
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
PRP RoHS ''
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Value ''
TOP 0 1.336 3.251 0 N 108 2 1
#
# CMP 45
CMP 5 0.2220005 1.2271264 270 N R36 CRCW040210R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '10.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '541-10.2LCT-ND'
PRP Supplier_Part_Number_2 '71-CRCW0402-10.2-E3'
PRP Supplier_Part_Number_3 '1158303'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10R2'
PRP ValueDisplayed '10.2'
PRP VDC_V '50V'
TOP 0 0.2220005 1.2074414 180 N 111 1 1
TOP 1 0.2220005 1.2468115 180 N 110 0 2
#
# CMP 46
CMP 77 0.1870005 1.3005714 270 N D2 SMS3923-040LF ;0=1,1=0.0197
PRP AEC_Category 'Q101'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.skyworksinc.com/uploads/documents/SMS392x_Series_200042AC.pdf'
PRP CompType 'Diode'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Io_A '10mA'
PRP Manufacturer 'Skyworks Solutions'
PRP MountType 'SMT'
PRP PackageReference 'SOD-882'
PRP PartNumber 'SMS3923-040LF'
PRP RJC_CperW ''
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.6'
PRP SizeAreaWB_mm2 '3.2'
PRP SizeX_mm '1'
PRP SizeY_mm '0.6'
PRP SizeZ_mm '0.5'
PRP TJmax_C '150°C'
PRP Type 'Schottky'
PRP Value 'V'
PRP Value1 '0.01A'
PRP Value2 '0.34V'
PRP Vf_V '340mV'
PRP Vr_V ''
TOP 0 0.1870005 1.2843313 270 N 110 1 1
TOP 1 0.1870005 1.3168115 270 N 272 8 2
#
# CMP 47
CMP 86 1.1126254 4.1028582 0 N U19 93LC46B-I/ST ;0=1,1=0.0472
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://ww1.microchip.com/downloads/en/DeviceDoc/20001749K.pdf'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Microchip'
PRP MountType 'SMT'
PRP PackageReference 'TSSOP-8'
PRP PartNumber '93LC46B-I/ST'
PRP RoHS 'Y'
PRP SizeArea_mm2 '19.2'
PRP SizeAreaWB_mm2 '42'
PRP SizeX_mm '6.4'
PRP SizeY_mm '3'
PRP SizeZ_mm '1.2'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '93LC46B-I/ST-ND'
PRP Supplier_Part_Number_2 '92C7658'
PRP Supplier_Part_Number_3 '579-93LC46B-I/ST'
TOP 0 1.0004207 4.141244 270 N 452 2 1
TOP 1 1.0004207 4.1156535 270 N 453 2 2
TOP 2 1.0004207 4.0900629 270 N 324 1 3
TOP 3 1.0004207 4.0644724 270 N 451 3 4
TOP 4 1.2248301 4.0644724 270 N 424 660 5
TOP 5 1.2248301 4.0900629 270 N 0 185 6
TOP 6 1.2248301 4.1156535 270 N 0 186 7
TOP 7 1.2248301 4.141244 270 N 373 1 8
#
# CMP 48
CMP 1 0.4729808 1.4574172 0 N R226 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 0.4619572 1.4574172 270 N 124 2 1
TOP 1 0.4840044 1.4574172 270 N 414 2 2
#
# CMP 49
CMP 8 2.4819797 0.8553635 180 N C10 GCM188R71C105KA64D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM188R71C105KA64%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM188R71C105KA64D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5241-6-ND'
PRP Supplier_Part_Number_2 '81-GCM188R71C105K64D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '1uF'
PRP VDC_V '16V'
TOP 0 2.5095388 0.8553635 90 N 170 0 1
TOP 1 2.4544207 0.8553635 90 N 424 548 2
#
# CMP 50
CMP 8 1.144559 3.292 180 N C11 GCM188R70J225KE22D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '2.2µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM188R70J225KE22%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM188R70J225KE22D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5316-1-ND'
PRP Supplier_Part_Number_2 '81-GCM188R70J225KE2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '2.2uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '2.2uF'
PRP VDC_V '6.3V'
TOP 0 1.1721181 3.292 90 N 424 549 1
TOP 1 1.117 3.292 90 N 18 9 2
#
# CMP 51
CMP 5 1.2660493 1.6237056 90 N C18 C0402C104K8RACTU ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://content.kemet.com/datasheets/KEM_C1002_X7R_SMD.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'Kemet'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'C0402C104K8RACTU'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '399-3520-1-ND'
PRP Supplier_Part_Number_2 '68X2393'
PRP Supplier_Part_Number_3 '80-C0402C104K8R'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.1uF'
PRP Value1 ''
PRP Value2 '10V'
PRP ValueDisplayed '0.1µF'
PRP VDC_V '10V'
TOP 0 1.2660493 1.6433906 0 N 424 550 1
TOP 1 1.2660493 1.6040205 0 N 308 53 2
#
# CMP 52
CMP 5 2.4750005 0.9207355 270 N C21 GCM155R71C224KE02D ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM155R71C224KE02%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71C224KE02D'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-10671-1-ND'
PRP Supplier_Part_Number_2 '81-GCM155R71C224KE2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.22uF'
PRP Value1 ''
PRP Value2 '16V'
PRP ValueDisplayed '0.22µF'
PRP VDC_V '16V'
TOP 0 2.4750005 0.9010505 180 N 161 0 1
TOP 1 2.4750005 0.9404206 180 N 160 1 2
#
# CMP 53
CMP 5 2.6082024 1.1766951 270 N C22 GCM155R71C224KE02D ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM155R71C224KE02%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71C224KE02D'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-10671-1-ND'
PRP Supplier_Part_Number_2 '81-GCM155R71C224KE2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.22uF'
PRP Value1 ''
PRP Value2 '16V'
PRP ValueDisplayed '0.22µF'
PRP VDC_V '16V'
TOP 0 2.6082024 1.1570101 180 N 424 551 1
TOP 1 2.6082024 1.1963802 180 N 308 54 2
#
# CMP 54
CMP 12 2.9520004 1.1766951 90 N C23 GCM31CR71A226KE02L ;0=1,1=0.0709
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '1206'
PRP Cap_F '22µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM31CR71A226KE02%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '1206'
PRP PartNumber 'GCM31CR71A226KE02L'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '5.12'
PRP SizeAreaWB_mm2 '10.92'
PRP SizeX_mm '3.2'
PRP SizeY_mm '1.6'
PRP SizeZ_mm '1.8'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '22uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '22uF'
PRP VDC_V '10V'
TOP 0 2.9520004 1.2298447 0 N 308 66 1
TOP 1 2.9520004 1.1235455 0 N 424 621 2
#
# CMP 55
CMP 8 1.2540005 3.3912524 90 N C24 GCM188R70J225KE22D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '2.2µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM188R70J225KE22%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM188R70J225KE22D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5316-1-ND'
PRP Supplier_Part_Number_2 '81-GCM188R70J225KE2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '2.2uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '2.2uF'
PRP VDC_V '6.3V'
TOP 0 1.2540005 3.4188115 0 N 424 552 1
TOP 1 1.2540005 3.3636934 0 N 98 4 2
#
# CMP 56
CMP 12 2.7708332 1.1766951 90 N C25 GCM31CR71A226KE02L ;0=1,1=0.0709
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '1206'
PRP Cap_F '22µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM31CR71A226KE02%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '1206'
PRP PartNumber 'GCM31CR71A226KE02L'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '5.12'
PRP SizeAreaWB_mm2 '10.92'
PRP SizeX_mm '3.2'
PRP SizeY_mm '1.6'
PRP SizeZ_mm '1.8'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '22uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '22uF'
PRP VDC_V '10V'
TOP 0 2.7708332 1.2298447 0 N 308 55 1
TOP 1 2.7708332 1.1235455 0 N 424 553 2
#
# CMP 57
CMP 12 2.8614168 1.1766951 90 N C26 GCM31CR71A226KE02L ;0=1,1=0.0709
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '1206'
PRP Cap_F '22µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM31CR71A226KE02%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '1206'
PRP PartNumber 'GCM31CR71A226KE02L'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '5.12'
PRP SizeAreaWB_mm2 '10.92'
PRP SizeX_mm '3.2'
PRP SizeY_mm '1.6'
PRP SizeZ_mm '1.8'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '22uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '22uF'
PRP VDC_V '10V'
TOP 0 2.8614168 1.2298447 0 N 308 56 1
TOP 1 2.8614168 1.1235455 0 N 424 554 2
#
# CMP 58
CMP 12 2.6802496 1.1766951 90 N C29 GCM31CR71A226KE02L ;0=1,1=0.0709
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '1206'
PRP Cap_F '22µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM31CR71A226KE02%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '1206'
PRP PartNumber 'GCM31CR71A226KE02L'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '5.12'
PRP SizeAreaWB_mm2 '10.92'
PRP SizeX_mm '3.2'
PRP SizeY_mm '1.6'
PRP SizeZ_mm '1.8'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '22uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '22uF'
PRP VDC_V '10V'
TOP 0 2.6802496 1.2298447 0 N 308 57 1
TOP 1 2.6802496 1.1235455 0 N 424 555 2
#
# CMP 59
CMP 5 1.0864203 2.1923874 0 N C30 GCM1555C1H270JA16D ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '27pF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GCM1555C1H270JA16-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM1555C1H270JA16D'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'C0G/NP0'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '27pF'
PRP Value1 ''
PRP Value2 '50V'
PRP ValueDisplayed '27pF'
PRP VDC_V '50V'
TOP 0 1.0667353 2.1923874 270 N 377 0 1
TOP 1 1.1061054 2.1923874 270 N 424 556 2
#
# CMP 60
CMP 8 1.3643934 2.976154 180 N C32 GCM188R70J225KE22D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '2.2µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM188R70J225KE22%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM188R70J225KE22D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5316-1-ND'
PRP Supplier_Part_Number_2 '81-GCM188R70J225KE2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '2.2uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '2.2uF'
PRP VDC_V '6.3V'
TOP 0 1.3919525 2.976154 90 N 424 557 1
TOP 1 1.3368344 2.976154 90 N 69 22 2
#
# CMP 61
CMP 5 0.9804352 2.1923874 180 N C33 GCM1555C1H270JA16D ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '27pF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GCM1555C1H270JA16-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM1555C1H270JA16D'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'C0G/NP0'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '27pF'
PRP Value1 ''
PRP Value2 '50V'
PRP ValueDisplayed '27pF'
PRP VDC_V '50V'
TOP 0 1.0001202 2.1923874 90 N 376 0 1
TOP 1 0.9607501 2.1923874 90 N 424 558 2
#
# CMP 62
CMP 5 0.798296 2.9115228 270 N C34 GCM155R71H102KA37D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '1nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM155R71H102KA37%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71H102KA37D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-4761-1-ND'
PRP Supplier_Part_Number_2 '45Y5158'
PRP Supplier_Part_Number_3 '81-GCM155R71H102KA7D'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '1000pF'
PRP Value1 'Unknown'
PRP Value2 '50V'
PRP ValueDisplayed '1000pF'
PRP VDC_V '50V'
TOP 0 0.798296 2.8918378 180 N 456 4 1
TOP 1 0.798296 2.9312079 180 N 375 0 2
#
# CMP 63
CMP 11 0.6870227 2.9271024 180 N C38 CGA4J3X7R1H225K125AB ;0=1,1=0.0571
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0805'
PRP Cap_F '2.2µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=CGA4J3X7R1H225K125AB'
PRP CompType 'Capacitor'
PRP ESR_ohm '3.288m'
PRP IRMS_A '3.60029A'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'CGA4J3X7R1H225K125AB'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '445-174216-1-ND'
PRP Supplier_Part_Number_2 '810-CGA4J3X7R1H225K125AB'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '2.2uF'
PRP Value1 '0.003288 ohm'
PRP Value2 '50V'
PRP ValueDisplayed '2.2uF'
PRP VDC_V '50V'
TOP 0 0.7165503 2.9271024 90 N 456 5 1
TOP 1 0.6574952 2.9271024 90 N 424 559 2
#
# CMP 64
CMP 5 0.9490076 4.5229074 270 N C47 C0402C104K8RACTU ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://content.kemet.com/datasheets/KEM_C1002_X7R_SMD.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'Kemet'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'C0402C104K8RACTU'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '399-3520-1-ND'
PRP Supplier_Part_Number_2 '68X2393'
PRP Supplier_Part_Number_3 '80-C0402C104K8R'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.1uF'
PRP Value1 ''
PRP Value2 '10V'
PRP ValueDisplayed '0.1µF'
PRP VDC_V '10V'
TOP 0 0.9490076 4.5032224 180 N 424 560 1
TOP 1 0.9490076 4.5425925 180 N 308 58 2
#
# CMP 65
CMP 8 0.6870227 3.0598431 90 N C48 GCM188R71C105KA64D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM188R71C105KA64%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM188R71C105KA64D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5241-6-ND'
PRP Supplier_Part_Number_2 '81-GCM188R71C105K64D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '1uF'
PRP VDC_V '16V'
TOP 0 0.6870227 3.0874022 0 N 308 59 1
TOP 1 0.6870227 3.0322841 0 N 424 561 2
#
# CMP 66
CMP 8 2.3966541 2.0423076 180 N C51 GCM188R70J225KE22D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '2.2µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM188R70J225KE22%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM188R70J225KE22D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5316-1-ND'
PRP Supplier_Part_Number_2 '81-GCM188R70J225KE2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '2.2uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '2.2uF'
PRP VDC_V '6.3V'
TOP 0 2.4242132 2.0423076 90 N 424 562 1
TOP 1 2.3690951 2.0423076 90 N 23 5 2
#
# CMP 67
CMP 8 1.3730101 2.0120195 270 N C60 GCM188R71C105KA64D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM188R71C105KA64%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM188R71C105KA64D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5241-6-ND'
PRP Supplier_Part_Number_2 '81-GCM188R71C105K64D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '1uF'
PRP VDC_V '16V'
TOP 0 1.3730101 1.9844604 180 N 309 12 1
TOP 1 1.3730101 2.0395785 180 N 424 563 2
#
# CMP 68
CMP 4 1.1290052 0.7206248 180 N C61 GCM155C71A105KE38D ;0=1,1=0.0276
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM155C71A105KE38%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155C71A105KE38D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GCM155C71A105KE8D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7S'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '1uF'
PRP VDC_V '10V'
TOP 0 1.1490052 0.7206248 90 N 308 60 1
TOP 1 1.1090052 0.7206248 90 N 424 564 2
#
# CMP 69
CMP 4 1.6000424 1.1679297 270 N C62 GCM155C71A105KE38D ;0=1,1=0.0276
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM155C71A105KE38%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155C71A105KE38D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GCM155C71A105KE8D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7S'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '1uF'
PRP VDC_V '10V'
TOP 0 1.6000424 1.1479297 180 N 262 4 1
TOP 1 1.6000424 1.1879297 180 N 424 565 2
#
# CMP 70
CMP 8 1.2900122 2.1224324 180 N C65 GCM188R71C105KA64D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM188R71C105KA64%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM188R71C105KA64D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5241-6-ND'
PRP Supplier_Part_Number_2 '81-GCM188R71C105K64D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '1uF'
PRP VDC_V '16V'
TOP 0 1.3175713 2.1224324 90 N 459 8 1
TOP 1 1.2624532 2.1224324 90 N 424 566 2
#
# CMP 71
CMP 8 0.7414445 4.2211046 180 N C68 C1608X7S1A475K080AC ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '4.7µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://product.tdk.com/en/catalog/datasheets/mlcc_commercial_general_en.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'C1608X7S1A475K080AC'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '445-14258-1-ND'
PRP Supplier_Part_Number_2 '29X4799'
PRP Supplier_Part_Number_3 '810-C1608X7S1A475KAC'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7S'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '4.7uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '4.7uF'
PRP VDC_V '10V'
TOP 0 0.7690036 4.2211046 90 N 259 3 1
TOP 1 0.7138855 4.2211046 90 N 424 567 2
#
# CMP 72
CMP 8 0.7414445 4.3195298 180 N C72 C1608X7S1A475K080AC ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '4.7µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://product.tdk.com/en/catalog/datasheets/mlcc_commercial_general_en.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'C1608X7S1A475K080AC'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '445-14258-1-ND'
PRP Supplier_Part_Number_2 '29X4799'
PRP Supplier_Part_Number_3 '810-C1608X7S1A475KAC'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7S'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '4.7uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '4.7uF'
PRP VDC_V '10V'
TOP 0 0.7690036 4.3195298 90 N 258 3 1
TOP 1 0.7138855 4.3195298 90 N 424 568 2
#
# CMP 73
CMP 3 1.1215784 0.8232444 0 N C74 C1005X7S1A225K050BC ;0=1,1=0.0256
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402_065'
PRP Cap_F '2.2µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=C1005X7S1A225K050BC'
PRP CompType 'Capacitor'
PRP ESR_ohm '5.925m'
PRP IRMS_A '2.05591A'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'C1005X7S1A225K050BC'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.65'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '445-9097-1-ND'
PRP Supplier_Part_Number_2 '810-C1005X7S1A225K'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7S'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '2.2uF'
PRP Value1 '0.005925 ohm'
PRP Value2 '10V'
PRP ValueDisplayed '2.2uF'
PRP VDC_V '10V'
TOP 0 1.1018934 0.8232444 270 N 424 619 1
TOP 1 1.1412635 0.8232444 270 N 262 5 2
#
# CMP 74
CMP 5 1.3449987 4.0144116 0 N C78 C0402C104K8RACTU ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://content.kemet.com/datasheets/KEM_C1002_X7R_SMD.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'Kemet'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'C0402C104K8RACTU'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '399-3520-1-ND'
PRP Supplier_Part_Number_2 '68X2393'
PRP Supplier_Part_Number_3 '80-C0402C104K8R'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.1uF'
PRP Value1 ''
PRP Value2 '10V'
PRP ValueDisplayed '0.1µF'
PRP VDC_V '10V'
TOP 0 1.3253137 4.0144116 270 N 425 8 1
TOP 1 1.3646838 4.0144116 270 N 424 569 2
#
# CMP 75
CMP 43 2.3031501 2.0147486 270 N C80 GCJ188C70J475KE02J ;0=1,1=0.0000
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP Cap_F '4.7µF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.murata.com/en-us/products/productdetail?partno=GCJ188C70J475KE02%23'
PRP Datasheet 'https://www.murata.com/en-us/products/productdetail?partno=GCJ188C70J475KE02%23'
PRP Datasheet_Path 'datasheets/Cap-GCJ188C70J475KE02J.pdf'
PRP helpURL 'https://upverter.com/upn/revision/50667d1a23a19155/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Murata'
PRP Operating_Temperature_Range '-55°C to +125°C'
PRP PackageReference '0603'
PRP Part_Number 'GCJ188C70J475KE02J'
PRP PartNumber 'GCJ188C70J475KE02J'
PRP RoHS 'TRUE'
PRP SizeZ_mm '1mm'
PRP TempCo '22%'
PRP Temperature_Characteristic 'X7S'
PRP Tolerance__ '10%'
PRP Value '4.7µF'
PRP ValueDisplayed '4.7uF'
PRP VDC_V '6.3V'
TOP 0 2.3031501 1.9842368 270 N 424 570 1
TOP 1 2.3031501 2.0452604 270 N 23 6 2
#
# CMP 76
CMP 5 1.2051451 4.2027166 180 N C86 C0402C104K8RACTU ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://content.kemet.com/datasheets/KEM_C1002_X7R_SMD.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'Kemet'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'C0402C104K8RACTU'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '399-3520-1-ND'
PRP Supplier_Part_Number_2 '68X2393'
PRP Supplier_Part_Number_3 '80-C0402C104K8R'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.1uF'
PRP Value1 ''
PRP Value2 '10V'
PRP ValueDisplayed '0.1µF'
PRP VDC_V '10V'
TOP 0 1.2248301 4.2027166 90 N 373 0 1
TOP 1 1.18546 4.2027166 90 N 424 571 2
#
# CMP 77
CMP 8 1.2687642 3.9265673 90 N C90 GCM188R71C105KA64D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM188R71C105KA64%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM188R71C105KA64D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5241-6-ND'
PRP Supplier_Part_Number_2 '81-GCM188R71C105K64D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '1uF'
PRP VDC_V '16V'
TOP 0 1.2687642 3.9541264 0 N 436 16 1
TOP 1 1.2687642 3.8990083 0 N 424 572 2
#
# CMP 78
CMP 5 1.6313549 0.7695142 90 N C98 C0402C104K8RACTU ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://content.kemet.com/datasheets/KEM_C1002_X7R_SMD.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'Kemet'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'C0402C104K8RACTU'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '399-3520-1-ND'
PRP Supplier_Part_Number_2 '68X2393'
PRP Supplier_Part_Number_3 '80-C0402C104K8R'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.1uF'
PRP Value1 ''
PRP Value2 '10V'
PRP ValueDisplayed '0.1µF'
PRP VDC_V '10V'
TOP 0 1.6313549 0.7891992 0 N 424 573 1
TOP 1 1.6313549 0.7498291 0 N 308 61 2
#
# CMP 79
CMP 71 3.0829392 0.7887975 0 N C99 EEHZC1V680XP ;0=1,1=0.3150
PRP AC_Derating ''
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case ''
PRP Cap_F '68µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/www-data/pdf/ABA0000/ABA0000CE138.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm '35'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A '1.4A'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '6.3x7.7'
PRP PartNumber 'EEHZC1V680XP'
PRP Polarized 'Y'
PRP RoHS 'Y'
PRP Series 'ZC'
PRP SizeArea_mm2 '48.18'
PRP SizeAreaWB_mm2 '79.98'
PRP SizeX_mm '7.3'
PRP SizeY_mm '6.6'
PRP SizeZ_mm '7.7'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'P15474CT-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Polymer Hybrid'
PRP Tolerance__ '20%'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '68uF'
PRP Value1 '35 ohm'
PRP Value2 '35V'
PRP ValueDisplayed '68uF'
PRP VDC_V '35V'
TOP 0 2.97664 0.7887975 180 N 138 13 1
TOP 1 3.1892384 0.7887975 180 N 424 650 2
#
# CMP 80
CMP 12 2.442 0.621 270 N C100 C3216X7R1H475K160AC ;0=1,1=0.0709
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '1206_180'
PRP Cap_F '4.7µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=C3216X7R1H475K160AC'
PRP CompType 'Capacitor'
PRP ESR_ohm '3.158m'
PRP IRMS_A '4.08379A'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '1206'
PRP PartNumber 'C3216X7R1H475K160AC'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '5.12'
PRP SizeAreaWB_mm2 '10.92'
PRP SizeX_mm '3.2'
PRP SizeY_mm '1.6'
PRP SizeZ_mm '1.8'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '445-8032-1-ND'
PRP Supplier_Part_Number_2 '810-C3216X7R1H475K160AC'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '4.7uF'
PRP Value1 '0.003158 ohm'
PRP Value2 '50V'
PRP ValueDisplayed '4.7uF'
PRP VDC_V '50V'
TOP 0 2.442 0.5678504 180 N 371 1 1
TOP 1 2.442 0.6741496 180 N 424 574 2
#
# CMP 81
CMP 8 2.7050545 0.2480515 90 N C104 CGA3E3X8R1H104K080AB ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://product.tdk.com/info/en/catalog/datasheets/mlcc_automotive_hightemp_en.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'CGA3E3X8R1H104K080AB'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '445-12606-1-ND'
PRP Supplier_Part_Number_2 '51X6942'
PRP Supplier_Part_Number_3 '810-CGA3E3X8R1H104KB'
PRP TaMax_C '150°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X8R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '50V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '50V'
TOP 0 2.7050545 0.2756106 0 N 370 2 1
TOP 1 2.7050545 0.2204925 0 N 424 575 2
#
# CMP 82
CMP 5 0.1059644 1.2966457 270 N C105 GCM155R71C104KA55D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.murata.com/capacitor/product/GCM155R71C104KA55%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71C104KA55D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-4759-2-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '16V'
TOP 0 0.1059644 1.2769607 180 N 424 576 1
TOP 1 0.1059644 1.3163308 180 N 272 2 2
#
# CMP 83
CMP 36 2.7860702 1.0015763 90 N C118 CGA4J1X7R1H475K125AC ;0=1,1=0.0010
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP Cap_F '4.7µF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://product.tdk.com/info/en/catalog/spec/mlccspec_automotive_general_en.pdf'
PRP Datasheet 'https://product.tdk.com/info/en/catalog/spec/mlccspec_automotive_general_en.pdf'
PRP Datasheet_Path 'datasheets/Cap-CGA4J1X7R1H475K125AC.pdf'
PRP helpURL 'https://upverter.com/upn/revision/c0dd355a50af42c5/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'TDK Corporation'
PRP Operating_Temperature_Range '-55°C to +125°C'
PRP PackageReference '0805'
PRP Part_Number 'CGA4J1X7R1H475K125AC'
PRP PartNumber 'CGA4J1X7R1H475K125AC'
PRP RoHS 'TRUE'
PRP SizeZ_mm '1.45mm'
PRP TempCo '15%'
PRP Temperature_Characteristic 'X7R'
PRP Tolerance__ '0.1%'
PRP Value '4.7µF'
PRP ValueDisplayed '4.7uF'
PRP VDC_V '50V'
TOP 0 2.7860702 1.0379936 90 N 424 633 1
TOP 1 2.7860702 0.965159 90 N 138 11 2
#
# CMP 84
CMP 8 2.6359525 0.2484355 90 N C126 CGA3E3X8R1H104K080AB ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://product.tdk.com/info/en/catalog/datasheets/mlcc_automotive_hightemp_en.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'CGA3E3X8R1H104K080AB'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '445-12606-1-ND'
PRP Supplier_Part_Number_2 '51X6942'
PRP Supplier_Part_Number_3 '810-CGA3E3X8R1H104KB'
PRP TaMax_C '150°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X8R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '50V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '50V'
TOP 0 2.6359525 0.2759946 0 N 370 3 1
TOP 1 2.6359525 0.2208765 0 N 424 577 2
#
# CMP 85
CMP 5 2.747 4.012 180 N C138 GCM155R71C224KE02D ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM155R71C224KE02%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71C224KE02D'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-10671-1-ND'
PRP Supplier_Part_Number_2 '81-GCM155R71C224KE2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.22uF'
PRP Value1 ''
PRP Value2 '16V'
PRP ValueDisplayed '0.22µF'
PRP VDC_V '16V'
TOP 0 2.766685 4.012 90 N 424 578 1
TOP 1 2.7273149 4.012 90 N 458 32 2
#
# CMP 86
CMP 5 2.747 4.0608704 180 N C142 GCM155R71C224KE02D ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM155R71C224KE02%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71C224KE02D'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-10671-1-ND'
PRP Supplier_Part_Number_2 '81-GCM155R71C224KE2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.22uF'
PRP Value1 ''
PRP Value2 '16V'
PRP ValueDisplayed '0.22µF'
PRP VDC_V '16V'
TOP 0 2.766685 4.0608704 90 N 424 579 1
TOP 1 2.7273149 4.0608704 90 N 458 33 2
#
# CMP 87
CMP 8 0.4084448 4.7298246 270 N C145 GCM188R71C105KA64D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM188R71C105KA64%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM188R71C105KA64D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5241-6-ND'
PRP Supplier_Part_Number_2 '81-GCM188R71C105K64D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '1uF'
PRP VDC_V '16V'
TOP 0 0.4084448 4.7022655 180 N 308 62 1
TOP 1 0.4084448 4.7573836 180 N 424 580 2
#
# CMP 88
CMP 8 0.4661196 4.55969 90 N C149 GCM188R70J225KE22D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '2.2µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM188R70J225KE22%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM188R70J225KE22D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5316-1-ND'
PRP Supplier_Part_Number_2 '81-GCM188R70J225KE2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '2.2uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '2.2uF'
PRP VDC_V '6.3V'
TOP 0 0.4661196 4.5872491 0 N 424 581 1
TOP 1 0.4661196 4.532131 0 N 67 2 2
#
# CMP 89
CMP 5 1.4326855 2.5220466 0 N C158 GCM155R71A104KA55D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GCM155R71A104KA55-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71A104KA55D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GCM155R71A104K5D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '10V'
TOP 0 1.4130005 2.5220466 270 N 261 8 1
TOP 1 1.4523706 2.5220466 270 N 424 582 2
#
# CMP 90
CMP 5 1.1569094 2.8241525 270 N C160 GCM155R71A104KA55D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GCM155R71A104KA55-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71A104KA55D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GCM155R71A104K5D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '10V'
TOP 0 1.1569094 2.8044675 180 N 459 9 1
TOP 1 1.1569094 2.8438376 180 N 424 583 2
#
# CMP 91
CMP 35 0.4884998 3.5250877 180 N C167 CC1206KKX7RCBB472 ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP Cap_F '4.7nF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.yageo.com/upload/media/product/productsearch/datasheet/mlcc/UPY-NP0X7R_HV_500V-to-3KV_16.pdf'
PRP Datasheet 'https://www.yageo.com/upload/media/product/productsearch/datasheet/mlcc/UPY-NP0X7R_HV_500V-to-3KV_16.pdf'
PRP Datasheet_Path 'datasheets/Cap-CC1206KKX7RCBB472.pdf'
PRP Digikey_Description 'CAP CER 4700PF 1KV X7R 1206'
PRP Digikey_Part_Number '311-1971-1-ND'
PRP helpURL 'https://upverter.com/upn/revision/9150da02aa68dabd/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'YAGEO'
PRP Mouser_Description 'Multilayer Ceramic Capacitors MLCC - SMD/SMT 4.7nF 1K V X7R 10%'
PRP Mouser_Part_Number '603-CC126KKX7RCBB472'
PRP Operating_Temperature_Range '-55°C to +125°C'
PRP PackageReference '1206'
PRP Part_Number 'CC1206KKX7RCBB472'
PRP PartNumber 'CC1206KKX7RCBB472'
PRP RoHS 'TRUE'
PRP SizeZ_mm '1.45mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '311-1971-1-ND'
PRP Supplier_Part_Number_2 '603-CC126KKX7RCBB472'
PRP TempCo '15%'
PRP Temperature_Characteristic 'X7R'
PRP Tolerance__ '10%'
PRP Value '4.7nF'
PRP ValueDisplayed '4.7nF'
PRP VDC_V '1kV'
TOP 0 0.5475549 3.5250877 180 N 93 3 1
TOP 1 0.4294447 3.5250877 180 N 424 665 2
#
# CMP 92
CMP 36 2.8590005 1.0017248 90 N C173 CGA4J1X7R1H475K125AC ;0=1,1=0.0010
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP Cap_F '4.7µF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://product.tdk.com/info/en/catalog/spec/mlccspec_automotive_general_en.pdf'
PRP Datasheet 'https://product.tdk.com/info/en/catalog/spec/mlccspec_automotive_general_en.pdf'
PRP Datasheet_Path 'datasheets/Cap-CGA4J1X7R1H475K125AC.pdf'
PRP helpURL 'https://upverter.com/upn/revision/c0dd355a50af42c5/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'TDK Corporation'
PRP Operating_Temperature_Range '-55°C to +125°C'
PRP PackageReference '0805'
PRP Part_Number 'CGA4J1X7R1H475K125AC'
PRP PartNumber 'CGA4J1X7R1H475K125AC'
PRP RoHS 'TRUE'
PRP SizeZ_mm '1.45mm'
PRP TempCo '15%'
PRP Temperature_Characteristic 'X7R'
PRP Tolerance__ '0.1%'
PRP Value '4.7µF'
PRP ValueDisplayed '4.7uF'
PRP VDC_V '50V'
TOP 0 2.8590005 1.0381421 90 N 424 584 1
TOP 1 2.8590005 0.9653075 90 N 138 6 2
#
# CMP 93
CMP 5 1.2209187 2.3131495 90 N C184 GCM155R71A104KA55D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GCM155R71A104KA55-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71A104KA55D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GCM155R71A104K5D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '10V'
TOP 0 1.2209187 2.3328345 0 N 261 9 1
TOP 1 1.2209187 2.2934644 0 N 424 585 2
#
# CMP 94
CMP 5 1.223155 2.8241524 270 N C185 GCM155R71A104KA55D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GCM155R71A104KA55-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71A104KA55D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GCM155R71A104K5D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '10V'
TOP 0 1.223155 2.8044674 180 N 261 10 1
TOP 1 1.223155 2.8438375 180 N 424 586 2
#
# CMP 95
CMP 5 0.9250349 2.5163298 180 N C188 GCM155R71A104KA55D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GCM155R71A104KA55-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71A104KA55D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GCM155R71A104K5D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '10V'
TOP 0 0.9447199 2.5163298 90 N 456 6 1
TOP 1 0.9053498 2.5163298 90 N 424 587 2
#
# CMP 96
CMP 5 0.9250349 2.6451464 180 N C189 GCM155R71A104KA55D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GCM155R71A104KA55-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71A104KA55D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GCM155R71A104K5D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '10V'
TOP 0 0.9447199 2.6451464 90 N 456 7 1
TOP 1 0.9053498 2.6451464 90 N 424 588 2
#
# CMP 97
CMP 5 1.284196 2.3153188 90 N C191 GCM155R71A104KA55D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GCM155R71A104KA55-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71A104KA55D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GCM155R71A104K5D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '10V'
TOP 0 1.284196 2.3350038 0 N 459 10 1
TOP 1 1.284196 2.2956337 0 N 424 589 2
#
# CMP 98
CMP 8 2.687595 0.9687219 180 N C195 CGA3E3X7R1H224K080AB ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=CGA3E3X7R1H224K080AB'
PRP CompType 'Capacitor'
PRP ESR_ohm '0.021699'
PRP IRMS_A '1.12496A'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'CGA3E3X7R1H224K080AB'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '445-6926-1-ND'
PRP Supplier_Part_Number_2 '810-CGA3E3X7R1H224K080AB'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.22uF'
PRP Value1 '0.021699 ohm'
PRP Value2 '50V'
PRP ValueDisplayed '0.22uF'
PRP VDC_V '50V'
TOP 0 2.7151541 0.9687219 90 N 138 7 1
TOP 1 2.660036 0.9687219 90 N 424 590 2
#
# CMP 99
CMP 84 1.2691749 4.5275562 90 N D1 TLMY1000-GS08 ;0=1,1=0.0256
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Angle '160'
PRP Color 'yellow'
PRP ColorTemperature ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/83172/tlmo1000.pdf'
PRP CompType 'LED'
PRP DynamicResistance ''
PRP Family_Io ''
PRP FamilyName ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Io_A '2mA'
PRP Ir_A '10µA'
PRP LambdaD ''
PRP LambdaP ''
PRP Luminance_Lv ''
PRP LuminousFlux_PhiV ''
PRP LuminousIntensity_IV ''
PRP Manufacturer 'Vishay-Semiconductor'
PRP MountType 'SMT'
PRP NumParallelLEDs ''
PRP NumSeriesLEDs ''
PRP PackageReference '1.6x0.8mm'
PRP PartNumber 'TLMY1000-GS08'
PRP Power_TotalModule '40mW'
PRP RJC_CperW ''
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '0.65'
PRP TJmax_C '120°C'
PRP Type 'AlInGaP'
PRP Value 'Yellow'
PRP Value1 '.04W'
PRP Value2 '1.8V'
PRP Vf_V '1.8V'
PRP Vr_V '6V'
TOP 0 1.2691749 4.5560994 90 N 369 1 1
TOP 1 1.2691749 4.4990128 90 N 424 659 2
#
# CMP 100
CMP 74 2.7874635 0.2376365 270 N D3 ATV02W280B-HF ;0=1,1=0.0531
PRP AEC_Category 'Q101'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.comchiptech.com/cms/UserFiles/ATV02W-HF%20series%20RevA.pdf'
PRP CompType 'TVS'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Ipp '4.41A'
PRP Manufacturer 'Comchip Technology'
PRP MountType 'SMT'
PRP PackageReference 'SOD-123'
PRP PartNumber 'ATV02W280B-HF'
PRP Ppk '200W'
PRP RJA_CperW ''
PRP RoHS 'Y'
PRP SizeArea_mm2 '6.545'
PRP SizeAreaWB_mm2 '13.095'
PRP SizeX_mm '3.85'
PRP SizeY_mm '1.7'
PRP SizeZ_mm '1.35'
PRP Value '28V'
PRP Value1 '200W'
PRP Vbr_Max '34.4V'
PRP Vbr_Min '31.1V'
PRP Vc '45.4V'
PRP VRWM '28V'
TOP 0 2.7874635 0.173168 90 N 424 651 1
TOP 1 2.7874635 0.302105 90 N 370 4 2
#
# CMP 101
CMP 77 0.0649764 1.3000909 270 N D4 SMS3923-040LF ;0=1,1=0.0197
PRP AEC_Category 'Q101'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.skyworksinc.com/uploads/documents/SMS392x_Series_200042AC.pdf'
PRP CompType 'Diode'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Io_A '10mA'
PRP Manufacturer 'Skyworks Solutions'
PRP MountType 'SMT'
PRP PackageReference 'SOD-882'
PRP PartNumber 'SMS3923-040LF'
PRP RJC_CperW ''
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.6'
PRP SizeAreaWB_mm2 '3.2'
PRP SizeX_mm '1'
PRP SizeY_mm '0.6'
PRP SizeZ_mm '0.5'
PRP TJmax_C '150°C'
PRP Type 'Schottky'
PRP Value 'V'
PRP Value1 '0.01A'
PRP Value2 '0.34V'
PRP Vf_V '340mV'
PRP Vr_V ''
TOP 0 0.0649764 1.2838508 270 N 368 0 1
TOP 1 0.0649764 1.316331 270 N 272 3 2
#
# CMP 102
CMP 62 0.5226399 3.1563294 180 N D7 LS_L29K-G1J2-1-Z ;0=1,1=0.0264
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Angle '160'
PRP Color 'Red'
PRP ColorTemperature ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.osram-os.com/Graphics/XPic2/00077099_0.pdf'
PRP CompType 'LED'
PRP DynamicResistance ''
PRP Family_Io ''
PRP FamilyName ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Io_A '20mA'
PRP Ir_A ''
PRP LambdaD ''
PRP LambdaP ''
PRP Luminance_Lv ''
PRP LuminousFlux_PhiV ''
PRP LuminousIntensity_IV ''
PRP Manufacturer 'OSRAM'
PRP MountType 'SMT'
PRP NumParallelLEDs ''
PRP NumSeriesLEDs ''
PRP PackageReference 'SMD, 2-Leads, Body 1.3x0.8mm'
PRP PartNumber 'LS L29K-G1J2-1-Z'
PRP Power_TotalModule ''
PRP RJC_CperW ''
PRP RoHS 'Y'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm ''
PRP TJmax_C '110°C'
PRP Type '?'
PRP Value 'Red'
PRP Value1 'W'
PRP Value2 '1.8V'
PRP Vf_V '1.8V'
PRP Vr_V '12V'
TOP 0 0.5521674 3.1563294 180 N 366 1 1
TOP 1 0.4931123 3.1563294 180 N 365 0 2
#
# CMP 103
CMP 62 0.268015 2.1114259 180 N D8 LS_L29K-G1J2-1-Z ;0=1,1=0.0264
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Angle '160'
PRP Color 'Red'
PRP ColorTemperature ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.osram-os.com/Graphics/XPic2/00077099_0.pdf'
PRP CompType 'LED'
PRP DynamicResistance ''
PRP Family_Io ''
PRP FamilyName ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Io_A '20mA'
PRP Ir_A ''
PRP LambdaD ''
PRP LambdaP ''
PRP Luminance_Lv ''
PRP LuminousFlux_PhiV ''
PRP LuminousIntensity_IV ''
PRP Manufacturer 'OSRAM'
PRP MountType 'SMT'
PRP NumParallelLEDs ''
PRP NumSeriesLEDs ''
PRP PackageReference 'SMD, 2-Leads, Body 1.3x0.8mm'
PRP PartNumber 'LS L29K-G1J2-1-Z'
PRP Power_TotalModule ''
PRP RJC_CperW ''
PRP RoHS 'Y'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm ''
PRP TJmax_C '110°C'
PRP Type '?'
PRP Value 'Red'
PRP Value1 'W'
PRP Value2 '1.8V'
PRP Vf_V '1.8V'
PRP Vr_V '12V'
TOP 0 0.2975425 2.1114259 180 N 364 0 1
TOP 1 0.2384874 2.1114259 180 N 424 591 2
#
# CMP 104
CMP 73 1.4290085 4.1031285 270 N D9 SML-E12Y8WT86 ;0=1,1=0.0181
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Angle ''
PRP Color 'yellow'
PRP ColorTemperature ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://rohmfs.rohm.com/en/products/databook/datasheet/opto/led/chip_mono/sml-e1.pdf'
PRP CompType 'LED'
PRP DynamicResistance ''
PRP Family_Io ''
PRP FamilyName ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Io_A '20mA'
PRP Ir_A '10µA'
PRP LambdaD ''
PRP LambdaP ''
PRP Luminance_Lv ''
PRP LuminousFlux_PhiV ''
PRP LuminousIntensity_IV '63'
PRP Manufacturer 'Rohm'
PRP MountType 'SMT'
PRP NumParallelLEDs ''
PRP NumSeriesLEDs ''
PRP PackageReference '1.6x0.8mm'
PRP PartNumber 'SML-E12Y8WT86'
PRP Power_TotalModule '54mW'
PRP RJC_CperW ''
PRP RoHS 'Y'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm ''
PRP TJmax_C '85°C'
PRP Type '?'
PRP Value 'Yellow'
PRP Value1 '0.054W'
PRP Value2 '2.2V'
PRP Vf_V '2.2V'
PRP Vr_V '5V'
TOP 0 1.4290085 4.1356088 270 N 190 1 1
TOP 1 1.4290085 4.0706482 270 N 267 5 2
#
# CMP 105
CMP 76 2.6298036 0.3878115 0 N D11 PMEG3050EP,115 ;0=1,1=0.0433
PRP AEC_Category 'Q101'
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.nexperia.com/documents/data_sheet/PMEG3050EP.pdf'
PRP CompType 'Diode'
PRP Green_EU_RoHS 'Incomplete'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Not Set'
PRP Green_REACh 'Incomplete'
PRP Io_A '5A'
PRP Manufacturer 'Nexperia'
PRP MountType 'SMT'
PRP PackageReference 'SOD-128'
PRP PartNumber 'PMEG3050EP,115'
PRP RJC_CperW ''
PRP RoHS 'Y'
PRP SizeArea_mm2 '11.5'
PRP SizeAreaWB_mm2 '19.6'
PRP SizeX_mm '4.6'
PRP SizeY_mm '2.5'
PRP SizeZ_mm '1.1'
PRP TJmax_C '150°C'
PRP Type 'Schottky'
PRP Value '30V'
PRP Value1 '5A'
PRP Value2 '0.36V'
PRP Vf_V '360mV'
PRP Vr_V '30V'
TOP 0 2.5431894 0.3878115 0 N 371 3 1
TOP 1 2.7164178 0.3878115 0 N 370 5 2
#
# CMP 106
CMP 72 3.1733391 1.0178115 0 N D12 SML-LXT0805GW-TR ;0=1,1=0.0315
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Angle '140'
PRP Color 'Green'
PRP ColorTemperature ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.lumex.com/content/files/ProductAttachment/SML-LXT0805GW-TR.pdf'
PRP CompType 'LED'
PRP DynamicResistance ''
PRP Family_Io ''
PRP FamilyName ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Io_A '20mA'
PRP Ir_A '100µA'
PRP LambdaD ''
PRP LambdaP ''
PRP Luminance_Lv ''
PRP LuminousFlux_PhiV ''
PRP LuminousIntensity_IV ''
PRP Manufacturer 'Lumex'
PRP MountType 'SMT'
PRP NumParallelLEDs ''
PRP NumSeriesLEDs ''
PRP PackageReference '0805'
PRP PartNumber 'SML-LXT0805GW-TR'
PRP Power_TotalModule '50mW'
PRP RJC_CperW ''
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '0.8'
PRP TJmax_C '80°C'
PRP Type '?'
PRP Value 'Green'
PRP Value1 '0.05W'
PRP Value2 '2V'
PRP Vf_V '2V'
PRP Vr_V '5V'
TOP 0 3.1320005 1.0178115 0 N 363 0 1
TOP 1 3.2146777 1.0178115 0 N 424 592 2
#
# CMP 107
CMP 73 0.2624728 1.75171 270 N D13 SML-E12Y8WT86 ;0=1,1=0.0181
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Angle ''
PRP Color 'yellow'
PRP ColorTemperature ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://rohmfs.rohm.com/en/products/databook/datasheet/opto/led/chip_mono/sml-e1.pdf'
PRP CompType 'LED'
PRP DynamicResistance ''
PRP Family_Io ''
PRP FamilyName ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Io_A '20mA'
PRP Ir_A '10µA'
PRP LambdaD ''
PRP LambdaP ''
PRP Luminance_Lv ''
PRP LuminousFlux_PhiV ''
PRP LuminousIntensity_IV '63'
PRP Manufacturer 'Rohm'
PRP MountType 'SMT'
PRP NumParallelLEDs ''
PRP NumSeriesLEDs ''
PRP PackageReference '1.6x0.8mm'
PRP PartNumber 'SML-E12Y8WT86'
PRP Power_TotalModule '54mW'
PRP RJC_CperW ''
PRP RoHS 'Y'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm ''
PRP TJmax_C '85°C'
PRP Type '?'
PRP Value 'Yellow'
PRP Value1 '0.054W'
PRP Value2 '2.2V'
PRP Vf_V '2.2V'
PRP Vr_V '5V'
TOP 0 0.2624728 1.7841903 270 N 362 0 1
TOP 1 0.2624728 1.7192297 270 N 361 0 2
#
# CMP 108
CMP 75 0.9005123 3.3664571 270 N D16 PMEG6020ER,115 ;0=1,1=0.0433
PRP AEC_Category 'Q101'
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.nexperia.com/documents/data_sheet/PMEG6020ER.pdf'
PRP CompType 'Diode'
PRP Green_EU_RoHS 'Incomplete'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Not Set'
PRP Green_REACh 'Incomplete'
PRP Io_A '2A'
PRP Manufacturer 'Nexperia'
PRP MountType 'SMT'
PRP PackageReference 'SOD-123W'
PRP PartNumber 'PMEG6020ER,115'
PRP RJC_CperW ''
PRP RoHS 'Y'
PRP SizeArea_mm2 '5.95'
PRP SizeAreaWB_mm2 '12.15'
PRP SizeX_mm '3.5'
PRP SizeY_mm '1.7'
PRP SizeZ_mm '1.0'
PRP TJmax_C '150°C'
PRP Type 'Schottky'
PRP Value '60V'
PRP Value1 '2A'
PRP Value2 '0.53V'
PRP Vf_V '530mV'
PRP Vr_V '60V'
TOP 0 0.9005123 3.311339 90 N 3 1 1
TOP 1 0.9005123 3.4215752 90 N 30 1 2
#
# CMP 109
CMP 62 2.0116892 2.1224323 270 N DS2 LS_L29K-G1J2-1-Z ;0=1,1=0.0264
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Angle '160'
PRP Color 'Red'
PRP ColorTemperature ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.osram-os.com/Graphics/XPic2/00077099_0.pdf'
PRP CompType 'LED'
PRP DynamicResistance ''
PRP Family_Io ''
PRP FamilyName ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Io_A '20mA'
PRP Ir_A ''
PRP LambdaD ''
PRP LambdaP ''
PRP Luminance_Lv ''
PRP LuminousFlux_PhiV ''
PRP LuminousIntensity_IV ''
PRP Manufacturer 'OSRAM'
PRP MountType 'SMT'
PRP NumParallelLEDs ''
PRP NumSeriesLEDs ''
PRP PackageReference 'SMD, 2-Leads, Body 1.3x0.8mm'
PRP PartNumber 'LS L29K-G1J2-1-Z'
PRP Power_TotalModule ''
PRP RJC_CperW ''
PRP RoHS 'Y'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm ''
PRP TJmax_C '110°C'
PRP Type '?'
PRP Value 'Red'
PRP Value1 'W'
PRP Value2 '1.8V'
PRP Vf_V '1.8V'
PRP Vr_V '12V'
TOP 0 2.0116892 2.0929048 270 N 360 0 1
TOP 1 2.0116892 2.1519599 270 N 274 2 2
#
# CMP 110
CMP 30 0.3610005 0.1118115 270 N FID3 Fiducial ;0=1,1=0.0010
PRP ClassName 'FiducialMark'
PRP CompType 'Fiducial'
PRP Manufacturer 'N/A'
PRP MountType 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 0.3610005 0.1118115 270 N 0 154 1
#
# CMP 111
CMP 30 2.1950005 0.1218115 270 N FID6 Fiducial ;0=1,1=0.0010
PRP ClassName 'FiducialMark'
PRP CompType 'Fiducial'
PRP Manufacturer 'N/A'
PRP MountType 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 2.1950005 0.1218115 270 N 0 155 1
#
# CMP 112
CMP 30 0.2499996 5.0968424 270 N FID8 Fiducial ;0=1,1=0.0010
PRP ClassName 'FiducialMark'
PRP CompType 'Fiducial'
PRP Manufacturer 'N/A'
PRP MountType 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 0.2499996 5.0968424 270 N 0 156 1
#
# CMP 113
CMP 30 0.1565493 4.7729139 270 N FID10 Fiducial ;0=1,1=0.0010
PRP ClassName 'FiducialMark'
PRP CompType 'Fiducial'
PRP Manufacturer 'N/A'
PRP MountType 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 0.1565493 4.7729139 270 N 0 157 1
#
# CMP 114
CMP 30 0.250001 -0.1755887 270 N FID12 Fiducial ;0=1,1=0.0010
PRP ClassName 'FiducialMark'
PRP CompType 'Fiducial'
PRP Manufacturer 'N/A'
PRP MountType 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 0.250001 -0.1755887 270 N 0 158 1
#
# CMP 115
CMP 30 3.0964499 5.0968421 270 N FID14 Fiducial ;0=1,1=0.0010
PRP ClassName 'FiducialMark'
PRP CompType 'Fiducial'
PRP Manufacturer 'N/A'
PRP MountType 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 3.0964499 5.0968421 270 N 0 159 1
#
# CMP 116
CMP 30 3.0964513 -0.175589 270 N FID16 Fiducial ;0=1,1=0.0010
PRP ClassName 'FiducialMark'
PRP CompType 'Fiducial'
PRP Manufacturer 'N/A'
PRP MountType 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 3.0964513 -0.175589 270 N 0 160 1
#
# CMP 117
CMP 59 1.046 3.52 180 N J2 128-0711-201 ;0=1,1=0.0492
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'FALSE'
PRP Color ''
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'https://cinchconnectivity.com/OA_MEDIA/catalog/pdf_UMCCatalogcatalog.pdf'
PRP CompType 'Jack'
PRP ContactFinish 'Gold'
PRP CT 'FALSE'
PRP Current_A ''
PRP Gender 'Female'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Cinch Connectivity'
PRP MountType 'SMT'
PRP Note ''
PRP Orientation 'Vertical'
PRP PackageReference 'UMC Straight Jack Receptacle, SMT'
PRP PartNumber '128-0711-201'
PRP PinCount '3'
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'J983CT-ND'
PRP Supplier_Part_Number_2 '99M0460'
PRP Supplier_Part_Number_3 '530-1280711201'
PRP Voltage_V ''
TOP 0 1.046 3.4599606 180 N 4 0 1
TOP 1 1.1040709 3.52 180 N 424 662 2
TOP 2 0.9879291 3.52 180 N 424 661 3
#
# CMP 118
CMP 70 0.5102892 0.9286112 0 N J7 QSH-030-01-L-D-A ;0=1,1=0.1310
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'False'
PRP Color 'Black'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.samtec.com/ftppub/cpdf/QSH-XXX-01-X-D-XX-MKT.pdf'
PRP CompType 'Receptacle'
PRP ContactFinish 'Gold'
PRP CT 'False'
PRP Current_A ''
PRP Gender 'Female'
PRP Green_EU_RoHS 'Passed with Exemption'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '2017-07-12'
PRP Manufacturer 'Samtec'
PRP MountType 'SMT'
PRP Note ''
PRP Orientation 'Vertical'
PRP PackageReference 'Receptacle, 0.5 mm, 30x2, TH'
PRP PartNumber 'QSH-030-01-L-D-A'
PRP PinCount '60'
PRP Pitch_mm '0.5'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count '2'
PRP RowSpacing_mm '5.73'
PRP Shrouded 'N'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 'SAM8180-ND'
PRP Supplier_Part_Number_2 '19M9181'
PRP Supplier_Part_Number_3 '1667876'
PRP Voltage_V ''
TOP 0 0.3974939 1.2140443 90 N 0 182 1
TOP 1 0.6230845 1.2140443 90 N 0 175 2
TOP 2 0.3974939 1.1943593 90 N 0 181 3
TOP 3 0.6230845 1.1943593 90 N 357 1 4
TOP 4 0.3974939 1.1746742 90 N 424 640 5
TOP 5 0.6230845 1.1746742 90 N 359 1 6
TOP 6 0.3974939 1.1549892 90 N 233 1 7
TOP 7 0.6230845 1.1549892 90 N 424 641 8
TOP 8 0.3974939 1.1353041 90 N 234 1 9
TOP 9 0.6230845 1.1353041 90 N 157 1 10
TOP 10 0.3974939 1.1156191 90 N 231 1 11
TOP 11 0.6230845 1.1156191 90 N 232 1 12
TOP 12 0.3974939 1.0959341 90 N 183 1 13
TOP 13 0.6230845 1.0959341 90 N 358 1 14
TOP 14 0.3974939 1.076249 90 N 181 1 15
TOP 15 0.6230845 1.076249 90 N 136 1 16
TOP 16 0.3974939 1.056564 90 N 180 1 17
TOP 17 0.6230845 1.056564 90 N 424 642 18
TOP 18 0.3974939 1.0368789 90 N 356 1 19
TOP 19 0.6230845 1.0368789 90 N 179 1 20
TOP 20 0.3974939 1.0171939 90 N 355 1 21
TOP 21 0.6230845 1.0171939 90 N 178 1 22
TOP 22 0.3974939 0.9975089 90 N 0 180 23
TOP 23 0.6230845 0.9975089 90 N 424 643 24
TOP 24 0.3974939 0.9778238 90 N 0 179 25
TOP 25 0.6230845 0.9778238 90 N 61 1 26
TOP 26 0.3974939 0.9581388 90 N 354 1 27
TOP 27 0.6230845 0.9581388 90 N 62 1 28
TOP 28 0.3974939 0.9384537 90 N 353 1 29
TOP 29 0.6230845 0.9384537 90 N 424 644 30
TOP 30 0.3974939 0.9187687 90 N 0 178 31
TOP 31 0.6230845 0.9187687 90 N 59 2 32
TOP 32 0.3974939 0.8990837 90 N 29 1 33
TOP 33 0.6230845 0.8990837 90 N 60 2 34
TOP 34 0.3974939 0.8793986 90 N 0 177 35
TOP 35 0.6230845 0.8793986 90 N 424 645 36
TOP 36 0.3974939 0.8597136 90 N 352 1 37
TOP 37 0.6230845 0.8597136 90 N 7 2 38
TOP 38 0.3974939 0.8400285 90 N 351 1 39
TOP 39 0.6230845 0.8400285 90 N 8 2 40
TOP 40 0.3974939 0.8203435 90 N 350 1 41
TOP 41 0.6230845 0.8203435 90 N 424 646 42
TOP 42 0.3974939 0.8006585 90 N 349 1 43
TOP 43 0.6230845 0.8006585 90 N 5 2 44
TOP 44 0.3974939 0.7809735 90 N 229 1 45
TOP 45 0.6230845 0.7809735 90 N 6 2 46
TOP 46 0.3974939 0.7612884 90 N 0 176 47
TOP 47 0.6230845 0.7612884 90 N 424 647 48
TOP 48 0.3974939 0.7416033 90 N 230 1 49
TOP 49 0.6230845 0.7416033 90 N 63 1 50
TOP 50 0.3974939 0.7219183 90 N 236 1 51
TOP 51 0.6230845 0.7219183 90 N 64 1 52
TOP 52 0.3974939 0.7022333 90 N 235 1 53
TOP 53 0.6230845 0.7022333 90 N 424 648 54
TOP 54 0.3974939 0.6825483 90 N 156 1 55
TOP 55 0.6230845 0.6825483 90 N 65 1 56
TOP 56 0.3974939 0.6628632 90 N 155 1 57
TOP 57 0.6230845 0.6628632 90 N 66 1 58
TOP 58 0.3974939 0.6431781 90 N 135 1 59
TOP 59 0.6230845 0.6431781 90 N 424 649 60
TOP 60 0.6154073 1.324871 90 N 0 151 MH1
TOP 61 0.6154073 0.5323514 90 N 0 150 MH2
TOP 62 0.5102892 1.2461309 90 N 424 639 MP1
TOP 63 0.5102892 1.0536111 90 N 424 638 MP2
TOP 64 0.5102892 0.8036113 270 N 424 637 MP3
TOP 65 0.5102892 0.6110915 270 N 424 636 MP4
#
# CMP 119
CMP 59 0.985 3.1362382 0 N J14 128-0711-201 ;0=1,1=0.0492
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'FALSE'
PRP Color ''
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'https://cinchconnectivity.com/OA_MEDIA/catalog/pdf_UMCCatalogcatalog.pdf'
PRP CompType 'Jack'
PRP ContactFinish 'Gold'
PRP CT 'FALSE'
PRP Current_A ''
PRP Gender 'Female'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Cinch Connectivity'
PRP MountType 'SMT'
PRP Note ''
PRP Orientation 'Vertical'
PRP PackageReference 'UMC Straight Jack Receptacle, SMT'
PRP PartNumber '128-0711-201'
PRP PinCount '3'
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'J983CT-ND'
PRP Supplier_Part_Number_2 '99M0460'
PRP Supplier_Part_Number_3 '530-1280711201'
PRP Voltage_V ''
TOP 0 0.985 3.1962776 0 N 14 0 1
TOP 1 0.9269291 3.1362382 0 N 424 664 2
TOP 2 1.0430709 3.1362382 0 N 424 663 3
#
# CMP 120
CMP 87 2.2595253 0.3679127 0 N J17 TSW-102-07-G-S ;0=2,1=0.3300
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA 'Y'
PRP Cert_CULUS 'N'
PRP Cert_UL 'Y'
PRP Cert_VDE 'N'
PRP ClassName 'Header'
PRP Color 'Black'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://samtec.com/ftppub/pdf/TSW_TH.PDF'
PRP CompType 'Header'
PRP ContactFinish 'Gold'
PRP Current_A '6.3A'
PRP Gender 'Male'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP Manufacturer 'Samtec'
PRP MountType 'TH'
PRP Note ''
PRP Orientation 'Vertical'
PRP PackageReference '2x1 Header'
PRP PartNumber 'TSW-102-07-G-S'
PRP PinCount '2'
PRP Pitch_mm '2.54'
PRP RoHS 'Y'
PRP Row_Count '1'
PRP RowSpacing_mm ''
PRP Shrouded 'N'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'SAM1029-02-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Voltage_V '550V'
TOP 0 2.2095253 0.3679127 0 N 198 0 1
TOP 1 2.3095253 0.3679127 0 N 109 24 2
#
# CMP 121
CMP 87 2.2595253 0.5891704 0 N J18 TSW-102-07-G-S ;0=2,1=0.3300
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA 'Y'
PRP Cert_CULUS 'N'
PRP Cert_UL 'Y'
PRP Cert_VDE 'N'
PRP ClassName 'Header'
PRP Color 'Black'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://samtec.com/ftppub/pdf/TSW_TH.PDF'
PRP CompType 'Header'
PRP ContactFinish 'Gold'
PRP Current_A '6.3A'
PRP Gender 'Male'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP Manufacturer 'Samtec'
PRP MountType 'TH'
PRP Note ''
PRP Orientation 'Vertical'
PRP PackageReference '2x1 Header'
PRP PartNumber 'TSW-102-07-G-S'
PRP PinCount '2'
PRP Pitch_mm '2.54'
PRP RoHS 'Y'
PRP Row_Count '1'
PRP RowSpacing_mm ''
PRP Shrouded 'N'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'SAM1029-02-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Voltage_V '550V'
TOP 0 2.2095253 0.5891704 0 N 197 0 1
TOP 1 2.3095253 0.5891704 0 N 109 22 2
#
# CMP 122
CMP 87 2.2597792 0.8189797 0 N J20 TSW-102-07-G-S ;0=2,1=0.3300
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA 'Y'
PRP Cert_CULUS 'N'
PRP Cert_UL 'Y'
PRP Cert_VDE 'N'
PRP ClassName 'Header'
PRP Color 'Black'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://samtec.com/ftppub/pdf/TSW_TH.PDF'
PRP CompType 'Header'
PRP ContactFinish 'Gold'
PRP Current_A '6.3A'
PRP Gender 'Male'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP Manufacturer 'Samtec'
PRP MountType 'TH'
PRP Note ''
PRP Orientation 'Vertical'
PRP PackageReference '2x1 Header'
PRP PartNumber 'TSW-102-07-G-S'
PRP PinCount '2'
PRP Pitch_mm '2.54'
PRP RoHS 'Y'
PRP Row_Count '1'
PRP RowSpacing_mm ''
PRP Shrouded 'N'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'SAM1029-02-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Voltage_V '550V'
TOP 0 2.2097792 0.8189797 0 N 196 0 1
TOP 1 2.3097792 0.8189797 0 N 109 23 2
#
# CMP 123
CMP 80 0.7830005 0.1398115 270 N J22 GBC01SFBN-M30 ;0=1,1=0.4925
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL 'Y'
PRP Cert_VDE ''
PRP ClassName 'Header'
PRP Color 'Black'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'https://drawings-pdf.s3.amazonaws.com/C10058.pdf'
PRP CompType 'Header'
PRP ContactFinish 'Gold'
PRP Current_A '3A'
PRP Gender 'Male'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Sullins Connector Solutions'
PRP MountType 'SMT'
PRP Note ''
PRP Orientation 'Vertical'
PRP PackageReference 'Header, 1x1, SMT'
PRP PartNumber 'GBC01SFBN-M30'
PRP PinCount '1'
PRP Pitch_mm ''
PRP RoHS 'Y'
PRP Row_Count '1'
PRP RowSpacing_mm ''
PRP Shrouded 'N'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Voltage_V ''
TOP 0 0.6830005 0.1398115 270 N 424 593 1
#
# CMP 124
CMP 80 1.769 1.438 180 N J23 GBC01SFBN-M30 ;0=1,1=0.4925
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL 'Y'
PRP Cert_VDE ''
PRP ClassName 'Header'
PRP Color 'Black'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'https://drawings-pdf.s3.amazonaws.com/C10058.pdf'
PRP CompType 'Header'
PRP ContactFinish 'Gold'
PRP Current_A '3A'
PRP Gender 'Male'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Sullins Connector Solutions'
PRP MountType 'SMT'
PRP Note ''
PRP Orientation 'Vertical'
PRP PackageReference 'Header, 1x1, SMT'
PRP PartNumber 'GBC01SFBN-M30'
PRP PinCount '1'
PRP Pitch_mm ''
PRP RoHS 'Y'
PRP Row_Count '1'
PRP RowSpacing_mm ''
PRP Shrouded 'N'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Voltage_V ''
TOP 0 1.769 1.338 180 N 424 594 1
#
# CMP 125
CMP 58 2.597654 0.5558115 0 N L5 XAL4030-472MEC ;0=1,1=0.0010
PRP AEC_Category ''
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.coilcraft.com/pdfs/xal4000.pdf'
PRP CompType ''
PRP Datasheet 'https://www.coilcraft.com/pdfs/xal4000.pdf'
PRP Datasheet_Path 'datasheets/Ind-XAL4030-472MEC.pdf'
PRP DCR_ohm '0.0441'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP helpURL 'https://upverter.com/upn/revision/10feddbc79c167e6/'
PRP Imax_A ''
PRP Ind_H '4.7µH'
PRP Irms '5.1A'
PRP Isat '4.5A'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Coilcraft'
PRP Material 'Composite'
PRP MountType ''
PRP Mouser_Description 'Power inductor, shielded, 20% tol, SMT, RoHS, halogen f'
PRP Mouser_Part_Number '994-XAL4030-472MEC'
PRP Operating_Temperature_Range 'to +165°C'
PRP PackageReference 'SMD2'
PRP Part_Number 'XAL4030-472MEC'
PRP PartNumber 'XAL4030-472MEC'
PRP RoHS 'TRUE'
PRP Self_Resonant_Frequency '36MHz'
PRP Shrouded 'true'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm '3.1mm'
PRP Standoff_Height '0.08mm'
PRP Supplier_1 ''
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 '994-XAL4030-472MEC'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '+125°C'
PRP TaMin_C '-40°C'
PRP Technology 'Wirewound'
PRP Test_Frequency '1MHz'
PRP Tolerance__ '20%'
PRP Value '4.7µH'
PRP Value1 ''
PRP Value2 ''
PRP ValueDisplayed ''
TOP 0 2.5510005 0.5558115 0 N 371 2 1
TOP 1 2.6443075 0.5558115 0 N 138 12 2
#
# CMP 126
CMP 89 2.4750005 1.051583 270 N L6 XEL4030-222MEB ;0=1,1=0.1220
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.coilcraft.com/pdfs/xel4030.pdf'
PRP CompType 'Inductor'
PRP DCR_ohm '0.0201'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Imax_A '6.1A'
PRP Ind_H '2.2µH'
PRP Irms '7.8A @ 40C rise'
PRP Isat '6.1A @ 30% inductance drop'
PRP LatestRevisionDate '2017-06-02'
PRP Manufacturer 'Coilcraft'
PRP Material 'Composite'
PRP MountType 'SMT'
PRP PackageReference '4x4mm'
PRP PartNumber 'XEL4030-222MEB'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '16'
PRP SizeAreaWB_mm2 '25'
PRP SizeX_mm '4'
PRP SizeY_mm '4'
PRP SizeZ_mm '3.1'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Shielded'
PRP Value '2.2uH'
PRP Value1 '0.0201 ohm'
PRP Value2 '6.1A'
PRP ValueDisplayed '2.2uH'
TOP 0 2.4750005 1.0049295 270 N 160 3 1
TOP 1 2.4750005 1.0982365 270 N 308 73 2
#
# CMP 127
CMP 87 0.5521674 4.5823277 90 N P1 TSW-102-07-G-S ;0=2,1=0.3300
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA 'Y'
PRP Cert_CULUS 'N'
PRP Cert_UL 'Y'
PRP Cert_VDE 'N'
PRP ClassName 'Header'
PRP Color 'Black'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://samtec.com/ftppub/pdf/TSW_TH.PDF'
PRP CompType 'Header'
PRP ContactFinish 'Gold'
PRP Current_A '6.3A'
PRP Gender 'Male'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP Manufacturer 'Samtec'
PRP MountType 'TH'
PRP Note ''
PRP Orientation 'Vertical'
PRP PackageReference '2x1 Header'
PRP PartNumber 'TSW-102-07-G-S'
PRP PinCount '2'
PRP Pitch_mm '2.54'
PRP RoHS 'Y'
PRP Row_Count '1'
PRP RowSpacing_mm ''
PRP Shrouded 'N'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'SAM1029-02-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Voltage_V '550V'
TOP 0 0.5521674 4.6323277 90 N 194 3 1
TOP 1 0.5521674 4.5323277 90 N 67 1 2
#
# CMP 128
CMP 79 0.1462534 1.7192279 0 N Q1 BSS123 ;0=1,1=0.0433
PRP AEC_Category 'Q101'
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer 'None'
PRP Alternate_PartNumber ''
PRP ChType 'N'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.fairchildsemi.com/ds/BS/BSS123.pdf'
PRP CompType 'MOSFET'
PRP IdsMax_A '1.7dA'
PRP LatestRevisionDate '2017-03-09'
PRP LatestRevisionNote 'Added parts.'
PRP Manufacturer 'Fairchild Semiconductor'
PRP MountType 'SMT'
PRP PackageReference 'SOT-23'
PRP PartNumber 'BSS123'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP QgTyp_nC '1.8'
PRP Rdson45_ohm '10'
PRP RoHS 'Y'
PRP SizeArea_mm2 '7.5'
PRP SizeAreaWB_mm2 '14'
PRP SizeX_mm '2.5'
PRP SizeY_mm '3'
PRP SizeZ_mm '1.1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'BSS123NCT-ND'
PRP Supplier_Part_Number_2 '58K8768'
PRP Supplier_Part_Number_3 '512-BSS123'
PRP U/M 'EA'
PRP Value '100V'
PRP Value1 '1'
PRP Value2 '1.8 nC'
PRP Vault_Folder ''
PRP VdsMax_V '100V'
PRP Vgs_V '20V'
TOP 0 0.0990093 1.7566295 270 N 344 1 1
TOP 1 0.0990093 1.6818264 270 N 424 656 2
TOP 2 0.1934975 1.7192279 270 N 361 1 3
#
# CMP 129
CMP 42 2.4949797 0.7777575 180 N R1 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 2.5151568 0.7777575 180 N 154 1 1
TOP 1 2.4748025 0.7777575 180 N 424 668 2
#
# CMP 130
CMP 42 2.7866856 0.7928115 180 N R4 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 2.8068627 0.7928115 180 N 145 5 1
TOP 1 2.7665084 0.7928115 180 N 114 1 2
#
# CMP 131
CMP 5 2.7866856 0.8743075 180 N R7 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 2.8063706 0.8743075 90 N 138 8 1
TOP 1 2.7670005 0.8743075 90 N 172 0 2
#
# CMP 132
CMP 5 2.7866855 0.8335595 0 N R8 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 2.7670005 0.8335595 270 N 172 1 1
TOP 1 2.8063706 0.8335595 270 N 424 595 2
#
# CMP 133
CMP 5 2.6153213 0.7225769 0 N R9 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 2.5956363 0.7225769 270 N 171 0 1
TOP 1 2.6350064 0.7225769 270 N 170 1 2
#
# CMP 134
CMP 5 2.6153213 0.7594381 180 N R10 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 2.6350063 0.7594381 90 N 424 596 1
TOP 1 2.5956362 0.7594381 90 N 171 1 2
#
# CMP 135
CMP 5 1.1628851 3.1422048 180 N R13 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 1.1825701 3.1422048 90 N 34 2 1
TOP 1 1.1432 3.1422048 90 N 69 23 2
#
# CMP 136
CMP 5 1.3565195 3.0383929 180 N R15 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 1.3762045 3.0383929 90 N 42 2 1
TOP 1 1.3368344 3.0383929 90 N 69 24 2
#
# CMP 137
CMP 5 1.6300203 3.1968115 0 N R16 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 1.6103353 3.1968115 270 N 78 2 1
TOP 1 1.6497054 3.1968115 270 N 69 25 2
#
# CMP 138
CMP 5 2.7234855 4.6746468 90 N R38 CRCW040247K5FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040247K5FKED'
PRP Power_W '63mW'
PRP Res_ohm '47.5k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-47.5KLCT-ND'
PRP Supplier_Part_Number_2 '52K7100'
PRP Supplier_Part_Number_3 '71-CRCW0402-47.5K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '47.5k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '47k5'
PRP ValueDisplayed '47.5k'
PRP VDC_V '50V'
TOP 0 2.7234855 4.6943318 0 N 307 2 1
TOP 1 2.7234855 4.6549617 0 N 109 25 2
#
# CMP 139
CMP 5 2.4230949 4.6443318 0 N R41 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 2.4034099 4.6443318 270 N 303 2 1
TOP 1 2.44278 4.6443318 270 N 109 26 2
#
# CMP 140
CMP 5 2.7885789 4.5940275 180 N R43 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 2.8082639 4.5940275 90 N 304 2 1
TOP 1 2.7688938 4.5940275 90 N 109 27 2
#
# CMP 141
CMP 5 2.7885789 4.6443317 180 N R49 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 2.8082639 4.6443317 90 N 305 2 1
TOP 1 2.7688938 4.6443317 90 N 109 28 2
#
# CMP 142
CMP 42 1.1617485 3.2222836 180 N R50 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 1.1819256 3.2222836 180 N 90 2 1
TOP 1 1.1415713 3.2222836 180 N 308 75 2
#
# CMP 143
CMP 37 2.622413 2.2996168 180 N R52 CRCW04020000Z0EDHP ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.vishay.com/docs/20043/crcwhpe3.pdf'
PRP Datasheet 'https://www.vishay.com/docs/20043/crcwhpe3.pdf'
PRP Datasheet_Path 'datasheets/Res-CRCW04020000Z0EDHP.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/5W 0402'
PRP Digikey_Part_Number '541-0.0YBCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/5e0a18f71149352e/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Vishay Dale'
PRP Mouser_Description 'Resistor; Thick Film; 0 Ohms; 0.125 W; 0 Ohms Jumper; SMT; 0402; TCR 0 ppm/DegC'
PRP Mouser_Part_Number '71-CRCW04020000Z0EDH'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'CRCW04020000Z0EDHP'
PRP PartNumber 'CRCW04020000Z0EDHP'
PRP Power_W '200mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'CRCW-HP e3'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '541-0.0YBCT-ND'
PRP Supplier_Part_Number_2 '71-CRCW04020000Z0EDH'
PRP Technology 'Thick Film'
PRP Value '0'
PRP VDC_V '50V'
TOP 0 2.6430823 2.2996168 180 N 406 10 1
TOP 1 2.6017437 2.2996168 180 N 27 3 2
#
# CMP 144
CMP 42 2.1330004 2.3878115 0 N R54 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 2.1128233 2.3878115 0 N 274 4 1
TOP 1 2.1531776 2.3878115 0 N 162 4 2
#
# CMP 145
CMP 1 1.6214061 3.2668115 0 N R61 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 1.6103825 3.2668115 270 N 35 2 1
TOP 1 1.6324297 3.2668115 270 N 53 3 2
#
# CMP 146
CMP 5 1.5501549 2.9919959 0 N R77 ERJ-2RKF4700X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/lecs/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF4700X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '470'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 'P470LCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2RKF4700X'
PRP Supplier_Part_Number_3 '2397145'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '470'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '470R'
PRP ValueDisplayed '470'
PRP VDC_V '50V'
TOP 0 1.5304699 2.9919959 270 N 92 0 1
TOP 1 1.56984 2.9919959 270 N 35 3 2
#
# CMP 147
CMP 1 0.7492194 1.2140442 180 N R81 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 0.760243 1.2140442 90 N 408 1 1
TOP 1 0.7381958 1.2140442 90 N 359 0 2
#
# CMP 148
CMP 1 0.7472509 1.2534143 180 N R84 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 0.7582745 1.2534143 90 N 238 1 1
TOP 1 0.7362273 1.2534143 90 N 357 0 2
#
# CMP 149
CMP 1 0.7472509 1.1353041 180 N R90 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 0.7582745 1.1353041 90 N 237 1 1
TOP 1 0.7362273 1.1353041 90 N 358 0 2
#
# CMP 150
CMP 5 0.9724987 2.9555979 270 N R92 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 0.9724987 2.9359129 180 N 442 1 1
TOP 1 0.9724987 2.975283 180 N 261 11 2
#
# CMP 151
CMP 5 0.9814987 2.8229142 270 N R97 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 0.9814987 2.8032292 180 N 424 597 1
TOP 1 0.9814987 2.8425993 180 N 442 2 2
#
# CMP 152
CMP 5 2.622413 2.2269581 180 N R99 CRCW04021K00FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04021K00FKED'
PRP Power_W '63mW'
PRP Res_ohm '1k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-1.00KLCT-ND'
PRP Supplier_Part_Number_2 '52K6545'
PRP Supplier_Part_Number_3 '71-CRCW0402-1.0K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '1.00k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '1k00'
PRP ValueDisplayed '1.00k'
PRP VDC_V '50V'
TOP 0 2.642098 2.2269581 90 N 272 4 1
TOP 1 2.6027279 2.2269581 90 N 147 1 2
#
# CMP 153
CMP 5 2.6224129 2.2628428 0 N R102 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 2.6027279 2.2628428 270 N 147 2 1
TOP 1 2.642098 2.2628428 270 N 424 598 2
#
# CMP 154
CMP 5 0.5521674 3.0668315 90 N R108 ERJ-2RKF4700X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/lecs/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF4700X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '470'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 'P470LCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2RKF4700X'
PRP Supplier_Part_Number_3 '2397145'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '470'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '470R'
PRP ValueDisplayed '470'
PRP VDC_V '50V'
TOP 0 0.5521674 3.0865165 0 N 366 0 1
TOP 1 0.5521674 3.0471464 0 N 261 12 2
#
# CMP 155
CMP 38 2.1333153 2.3478115 0 N R111 CRCW04024K22FKED ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP Datasheet 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP Datasheet_Path 'datasheets/Res-CRCW04024K22FKED.pdf'
PRP helpURL 'https://upverter.com/upn/revision/12ad28d0305e9d35/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Vishay'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'CRCW04024K22FKED'
PRP PartNumber 'CRCW04024K22FKED'
PRP Power_W '63mW'
PRP Res_ohm '4.22k'
PRP RoHS 'TRUE'
PRP Series 'D/CRCW e3'
PRP SizeZ_mm '0.4mm'
PRP Technology 'Thick Film'
PRP TempCo '100ppm/°C'
PRP Tolerance__ '1%'
PRP Value '4.22k'
PRP VDC_V '50V'
TOP 0 2.112646 2.3478115 0 N 54 30 1
TOP 1 2.1539846 2.3478115 0 N 162 3 2
#
# CMP 156
CMP 5 0.5187029 2.9835951 0 N R112 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 0.4990179 2.9835951 270 N 441 0 1
TOP 1 0.538388 2.9835951 270 N 261 13 2
#
# CMP 157
CMP 42 0.4931123 3.0668314 270 N R113 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 0.4931123 3.0466543 270 N 441 3 1
TOP 1 0.4931123 3.0870086 270 N 365 1 2
#
# CMP 158
CMP 1 0.436 0.45 270 N R114 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 0.436 0.4389764 180 N 163 1 1
TOP 1 0.436 0.4610236 180 N 135 0 2
#
# CMP 159
CMP 1 0.7492194 1.0963648 180 N R115 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 0.760243 1.0963648 90 N 53 4 1
TOP 1 0.7381958 1.0963648 90 N 136 0 2
#
# CMP 160
CMP 42 0.6033485 2.1379388 270 N R117 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 0.6033485 2.1177617 270 N 332 1 1
TOP 1 0.6033485 2.158116 270 N 441 4 2
#
# CMP 161
CMP 5 0.6614321 2.1379388 270 N R118 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 0.6614321 2.1182538 180 N 424 599 1
TOP 1 0.6614321 2.1576239 180 N 441 1 2
#
# CMP 162
CMP 5 0.5442938 2.1379388 270 N R120 ERJ-2RKF4700X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/lecs/www-data/pdf/AOA0000/AOA0000CE2.pdf'
PRP CompType 'Resistor'
PRP EIA_Code ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2RKF4700X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '470'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 'P470LCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2RKF4700X'
PRP Supplier_Part_Number_3 '2397145'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '470'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '470R'
PRP ValueDisplayed '470'
PRP VDC_V '50V'
TOP 0 0.5442938 2.1182538 180 N 332 0 1
TOP 1 0.5442938 2.1576239 180 N 364 1 2
#
# CMP 163
CMP 5 2.4580003 1.9198741 90 N R125 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 2.4580003 1.9395591 0 N 145 4 1
TOP 1 2.4580003 1.900189 0 N 54 29 2
#
# CMP 164
CMP 5 1.0306483 2.9555979 270 N R132 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 1.0306483 2.9359129 180 N 440 1 1
TOP 1 1.0306483 2.975283 180 N 261 14 2
#
# CMP 165
CMP 5 1.0306483 2.8229142 270 N R137 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 1.0306483 2.8032292 180 N 424 600 1
TOP 1 1.0306483 2.8425993 180 N 440 2 2
#
# CMP 166
CMP 5 1.1770005 2.9558115 270 N R141 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 1.1770005 2.9361265 180 N 444 0 1
TOP 1 1.1770005 2.9754966 180 N 261 15 2
#
# CMP 167
CMP 5 1.2777193 2.8242524 270 N R142 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 1.2777193 2.8045674 180 N 424 601 1
TOP 1 1.2777193 2.8439375 180 N 444 1 2
#
# CMP 168
CMP 5 0.3239573 4.7180136 90 N R159 CRCW04021K00FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04021K00FKED'
PRP Power_W '63mW'
PRP Res_ohm '1k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-1.00KLCT-ND'
PRP Supplier_Part_Number_2 '52K6545'
PRP Supplier_Part_Number_3 '71-CRCW0402-1.0K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '1.00k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '1k00'
PRP ValueDisplayed '1.00k'
PRP VDC_V '50V'
TOP 0 0.3239573 4.7376986 0 N 132 1 1
TOP 1 0.3239573 4.6983285 0 N 112 0 2
#
# CMP 169
CMP 5 1.3321765 4.4218919 270 N R179 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 1.3321765 4.4022069 180 N 327 1 1
TOP 1 1.3321765 4.441577 180 N 430 0 2
#
# CMP 170
CMP 5 1.3321765 4.5304348 90 N R180 ERJ-2GEJ511X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/DMA0000COL9.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP LatestRevisionDate ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GEJ511X'
PRP Power_W '100mW'
PRP Published ''
PRP Publisher ''
PRP Res_ohm '510'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P510JCT-ND'
PRP Supplier_Part_Number_2 '65T8293'
PRP Supplier_Part_Number_3 '667-ERJ-2GEJ511X'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '510'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '510R'
PRP ValueDisplayed '510'
PRP VDC_V '50V'
TOP 0 1.3321765 4.5501198 0 N 369 0 1
TOP 1 1.3321765 4.5107497 0 N 430 1 2
#
# CMP 171
CMP 42 1.3221478 4.1772309 90 N R181 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 1.3221478 4.197408 90 N 373 2 1
TOP 1 1.3221478 4.1570537 90 N 436 20 2
#
# CMP 172
CMP 5 0.894355 4.1105356 180 N R184 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 0.91404 4.1105356 90 N 453 1 1
TOP 1 0.8746699 4.1105356 90 N 436 17 2
#
# CMP 173
CMP 5 0.894355 4.164299 180 N R187 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 0.91404 4.164299 90 N 452 1 1
TOP 1 0.8746699 4.164299 90 N 436 18 2
#
# CMP 174
CMP 1 1.2819297 1.3820377 90 N R188 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 1.2819297 1.3930613 0 N 223 0 1
TOP 1 1.2819297 1.3710141 0 N 231 0 2
#
# CMP 175
CMP 5 1.43401 2.860812 180 N R195 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 1.453695 2.860812 90 N 401 2 1
TOP 1 1.4143249 2.860812 90 N 187 0 2
#
# CMP 176
CMP 1 0.3706864 0.45 270 N R197 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 0.3706864 0.4389764 180 N 166 1 1
TOP 1 0.3706864 0.4610236 180 N 156 0 2
#
# CMP 177
CMP 1 0.4033432 0.45 270 N R198 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 0.4033432 0.4389764 180 N 167 1 1
TOP 1 0.4033432 0.4610236 180 N 155 0 2
#
# CMP 178
CMP 5 0.894355 4.0067462 0 N R201 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 0.87467 4.0067462 270 N 451 1 1
TOP 1 0.9140401 4.0067462 270 N 436 19 2
#
# CMP 179
CMP 5 0.894355 4.0635546 0 N R205 CRCW04022K20JNED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K20JNED'
PRP Power_W '63mW'
PRP Res_ohm '2.2k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.2KJCT-ND'
PRP Supplier_Part_Number_2 '59M6710'
PRP Supplier_Part_Number_3 '71-CRCW0402J-2.2K-E3'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP Value '2.2k'
PRP Value1 '5%'
PRP Value2 '0.063W'
PRP Value_Code '2k20'
PRP ValueDisplayed '2.2k'
PRP VDC_V '50V'
TOP 0 0.87467 4.0635546 270 N 451 2 1
TOP 1 0.9140401 4.0635546 270 N 324 0 2
#
# CMP 180
CMP 42 0.1042547 4.1428329 270 N R209 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 0.1042547 4.1226558 270 N 424 669 1
TOP 1 0.1042547 4.1630101 270 N 345 10 2
#
# CMP 181
CMP 5 1.39464 2.903812 180 N R211 CRCW04025K76FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04025K76FKED'
PRP Power_W '63mW'
PRP Res_ohm '5.76k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-5.76KLCT-ND'
PRP Supplier_Part_Number_2 '52K7127'
PRP Supplier_Part_Number_3 '71-CRCW0402-5.76K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '5.76k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '5k76'
PRP ValueDisplayed '5.76k'
PRP VDC_V '50V'
TOP 0 1.414325 2.903812 90 N 187 1 1
TOP 1 1.3749549 2.903812 90 N 261 16 2
#
# CMP 182
CMP 1 0.2620005 0.9008115 0 N R215 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 0.2509769 0.9008115 270 N 386 1 1
TOP 1 0.2730241 0.9008115 270 N 352 0 2
#
# CMP 183
CMP 1 1.3524543 1.4903076 0 N R223 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 1.3414307 1.4903076 270 N 222 0 1
TOP 1 1.3634779 1.4903076 270 N 233 0 2
#
# CMP 184
CMP 5 1.7296917 4.1147267 90 N R261 ERJ-2GEJ511X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/DMA0000COL9.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP LatestRevisionDate ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GEJ511X'
PRP Power_W '100mW'
PRP Published ''
PRP Publisher ''
PRP Res_ohm '510'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P510JCT-ND'
PRP Supplier_Part_Number_2 '65T8293'
PRP Supplier_Part_Number_3 '667-ERJ-2GEJ511X'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '510'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '510R'
PRP ValueDisplayed '510'
PRP VDC_V '50V'
TOP 0 1.7296917 4.1344117 0 N 190 0 1
TOP 1 1.7296917 4.0950416 0 N 109 29 2
#
# CMP 185
CMP 5 2.0763794 2.1194138 90 N R262 ERJ-2GEJ511X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/DMA0000COL9.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP LatestRevisionDate ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GEJ511X'
PRP Power_W '100mW'
PRP Published ''
PRP Publisher ''
PRP Res_ohm '510'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P510JCT-ND'
PRP Supplier_Part_Number_2 '65T8293'
PRP Supplier_Part_Number_3 '667-ERJ-2GEJ511X'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '510'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '510R'
PRP ValueDisplayed '510'
PRP VDC_V '50V'
TOP 0 2.0763794 2.1390988 0 N 360 1 1
TOP 1 2.0763794 2.0997287 0 N 109 30 2
#
# CMP 186
CMP 5 0.2427878 1.8228586 180 N R263 ERJ-2GEJ511X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/DMA0000COL9.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP LatestRevisionDate ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GEJ511X'
PRP Power_W '100mW'
PRP Published ''
PRP Publisher ''
PRP Res_ohm '510'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P510JCT-ND'
PRP Supplier_Part_Number_2 '65T8293'
PRP Supplier_Part_Number_3 '667-ERJ-2GEJ511X'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '510'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '510R'
PRP ValueDisplayed '510'
PRP VDC_V '50V'
TOP 0 0.2624728 1.8228586 90 N 362 1 1
TOP 1 0.2231027 1.8228586 90 N 109 31 2
#
# CMP 187
CMP 5 0.144454 1.2966458 90 N R264 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 0.144454 1.3163308 0 N 272 5 1
TOP 1 0.144454 1.2769607 0 N 109 32 2
#
# CMP 188
CMP 5 0.0494598 1.7369444 270 N R266 ERJ-2GEJ511X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/DMA0000COL9.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP LatestRevisionDate ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GEJ511X'
PRP Power_W '100mW'
PRP Published ''
PRP Publisher ''
PRP Res_ohm '510'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P510JCT-ND'
PRP Supplier_Part_Number_2 '65T8293'
PRP Supplier_Part_Number_3 '667-ERJ-2GEJ511X'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '510'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '510R'
PRP ValueDisplayed '510'
PRP VDC_V '50V'
TOP 0 0.0494598 1.7172594 180 N 272 6 1
TOP 1 0.0494598 1.7566295 180 N 344 0 2
#
# CMP 189
CMP 5 0.1851588 1.3859748 90 N R267 CRCW040210R0JNED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210R0JNED'
PRP Power_W '63mW'
PRP Res_ohm '10'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10JCT-ND'
PRP Supplier_Part_Number_2 '59M6698'
PRP Supplier_Part_Number_3 '71-CRCW0402J-10-E3'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP Value '10'
PRP Value1 '5%'
PRP Value2 '0.063W'
PRP Value_Code '10R0'
PRP ValueDisplayed '10'
PRP VDC_V '50V'
TOP 0 0.1851588 1.4056598 0 N 424 602 1
TOP 1 0.1851588 1.3662897 0 N 321 0 2
#
# CMP 190
CMP 5 0.0649767 1.2073116 270 N R268 CRCW040210R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '10.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '541-10.2LCT-ND'
PRP Supplier_Part_Number_2 '71-CRCW0402-10.2-E3'
PRP Supplier_Part_Number_3 '1158303'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10R2'
PRP ValueDisplayed '10.2'
PRP VDC_V '50V'
TOP 0 0.0649767 1.1876266 180 N 273 1 1
TOP 1 0.0649767 1.2269967 180 N 368 1 2
#
# CMP 191
CMP 5 2.001315 1.212 180 N R276 CRCW04022K94FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K94FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.94k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.94KLCT-ND'
PRP Supplier_Part_Number_2 '52K6814'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.94K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.94k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k94'
PRP ValueDisplayed '2.94k'
PRP VDC_V '50V'
TOP 0 2.021 1.212 90 N 406 7 1
TOP 1 1.9816299 1.212 90 N 109 33 2
#
# CMP 192
CMP 5 2.001315 1.291 180 N R277 CRCW04022K94FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K94FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.94k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.94KLCT-ND'
PRP Supplier_Part_Number_2 '52K6814'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.94K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.94k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k94'
PRP ValueDisplayed '2.94k'
PRP VDC_V '50V'
TOP 0 2.021 1.291 90 N 405 9 1
TOP 1 1.9816299 1.291 90 N 109 34 2
#
# CMP 193
CMP 5 1.3006305 1.6237055 270 N R283 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 1.3006305 1.6040205 180 N 221 0 1
TOP 1 1.3006305 1.6433906 180 N 424 603 2
#
# CMP 194
CMP 5 1.4856856 2.903812 180 N R289 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 1.5053706 2.903812 90 N 424 604 1
TOP 1 1.4660005 2.903812 90 N 187 2 2
#
# CMP 195
CMP 5 1.4327213 2.5770217 180 N R290 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 1.4524063 2.5770217 90 N 402 2 1
TOP 1 1.4130362 2.5770217 90 N 188 0 2
#
# CMP 196
CMP 8 0.8704231 2.9047692 90 N R293 CRCW060348K7FKEA ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'CRCW060348K7FKEA'
PRP Power_W '100mW'
PRP Res_ohm '48.7k'
PRP RoHS 'E'
PRP SizeArea_mm2 '1.28'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-48.7KHCT-ND'
PRP Supplier_Part_Number_2 '52K8559'
PRP Supplier_Part_Number_3 '71-CRCW0603-48.7K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '48.7k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '48k7'
PRP ValueDisplayed '48.7k'
PRP VDC_V '75V'
TOP 0 0.8704231 2.9323283 0 N 375 1 1
TOP 1 0.8704231 2.8772102 0 N 456 8 2
#
# CMP 197
CMP 8 0.9278348 2.9047693 270 N R294 CRCW060345K3FKEA ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'CRCW060345K3FKEA'
PRP Power_W '100mW'
PRP Res_ohm '45.3k'
PRP RoHS 'E'
PRP SizeArea_mm2 '1.28'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-45.3KHCT-ND'
PRP Supplier_Part_Number_2 '52K8537'
PRP Supplier_Part_Number_3 '71-CRCW0603-45.3K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '45.3k'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '45k3'
PRP ValueDisplayed '45.3k'
PRP VDC_V '75V'
TOP 0 0.9278348 2.8772102 180 N 424 605 1
TOP 1 0.9278348 2.9323283 180 N 375 2 2
#
# CMP 198
CMP 42 0.9071779 3.0190291 270 N R295 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 0.9071779 2.998852 270 N 261 23 1
TOP 1 0.9071779 3.0392063 270 N 109 39 2
#
# CMP 199
CMP 5 1.7442082 0.7252227 0 N R296 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 1.7245232 0.7252227 270 N 320 0 1
TOP 1 1.7638933 0.7252227 270 N 424 606 2
#
# CMP 200
CMP 5 2.1738018 0.4734074 90 N R298 CRCW0402750RFKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW0402750RFKED'
PRP Power_W '63mW'
PRP Res_ohm '750'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-750LCT-ND'
PRP Supplier_Part_Number_2 '52K7270'
PRP Supplier_Part_Number_3 '71-CRCW0402-750-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '750'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '750R'
PRP ValueDisplayed '750'
PRP VDC_V '50V'
TOP 0 2.1738018 0.4930924 0 N 319 0 1
TOP 1 2.1738018 0.4537223 0 N 269 1 2
#
# CMP 201
CMP 5 2.2916288 0.4734073 270 N R299 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 2.2916288 0.4537223 180 N 286 1 1
TOP 1 2.2916288 0.4930924 180 N 319 1 2
#
# CMP 202
CMP 5 2.2095253 0.4734074 90 N R300 CRCW04027K87FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04027K87FKED'
PRP Power_W '63mW'
PRP Res_ohm '7.87k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-7.87KLCT-ND'
PRP Supplier_Part_Number_2 '52K7249'
PRP Supplier_Part_Number_3 '71-CRCW0402-7.87K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '7.87k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '7k87'
PRP ValueDisplayed '7.87k'
PRP VDC_V '50V'
TOP 0 2.2095253 0.4930924 0 N 319 2 1
TOP 1 2.2095253 0.4537223 0 N 198 1 2
#
# CMP 203
CMP 5 2.2522587 0.4734073 270 N R302 CRCW040282K5FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040282K5FKED'
PRP Power_W '63mW'
PRP Res_ohm '82.5k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-82.5KLCT-ND'
PRP Supplier_Part_Number_2 '52K7304'
PRP Supplier_Part_Number_3 '71-CRCW0402-82.5K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '82.5k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '82k5'
PRP ValueDisplayed '82.5k'
PRP VDC_V '50V'
TOP 0 2.2522587 0.4537223 180 N 424 607 1
TOP 1 2.2522587 0.4930924 180 N 319 3 2
#
# CMP 204
CMP 5 2.1715998 0.6932276 90 N R304 CRCW0402750RFKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW0402750RFKED'
PRP Power_W '63mW'
PRP Res_ohm '750'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-750LCT-ND'
PRP Supplier_Part_Number_2 '52K7270'
PRP Supplier_Part_Number_3 '71-CRCW0402-750-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '750'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '750R'
PRP ValueDisplayed '750'
PRP VDC_V '50V'
TOP 0 2.1715998 0.7129126 0 N 318 0 1
TOP 1 2.1715998 0.6735425 0 N 270 1 2
#
# CMP 205
CMP 5 2.1346186 0.6932274 270 N R305 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 2.1346186 0.6735424 180 N 288 1 1
TOP 1 2.1346186 0.7129125 180 N 318 1 2
#
# CMP 206
CMP 5 2.2095253 0.6932276 90 N R306 CRCW04027K87FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04027K87FKED'
PRP Power_W '63mW'
PRP Res_ohm '7.87k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-7.87KLCT-ND'
PRP Supplier_Part_Number_2 '52K7249'
PRP Supplier_Part_Number_3 '71-CRCW0402-7.87K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '7.87k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '7k87'
PRP ValueDisplayed '7.87k'
PRP VDC_V '50V'
TOP 0 2.2095253 0.7129126 0 N 318 2 1
TOP 1 2.2095253 0.6735425 0 N 197 1 2
#
# CMP 207
CMP 5 2.246926 0.6932275 270 N R307 CRCW040282K5FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040282K5FKED'
PRP Power_W '63mW'
PRP Res_ohm '82.5k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-82.5KLCT-ND'
PRP Supplier_Part_Number_2 '52K7304'
PRP Supplier_Part_Number_3 '71-CRCW0402-82.5K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '82.5k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '82k5'
PRP ValueDisplayed '82.5k'
PRP VDC_V '50V'
TOP 0 2.246926 0.6735425 180 N 424 608 1
TOP 1 2.246926 0.7129126 180 N 318 3 2
#
# CMP 208
CMP 5 2.1725441 0.919852 90 N R308 CRCW0402750RFKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW0402750RFKED'
PRP Power_W '63mW'
PRP Res_ohm '750'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-750LCT-ND'
PRP Supplier_Part_Number_2 '52K7270'
PRP Supplier_Part_Number_3 '71-CRCW0402-750-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '750'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '750R'
PRP ValueDisplayed '750'
PRP VDC_V '50V'
TOP 0 2.1725441 0.939537 0 N 317 0 1
TOP 1 2.1725441 0.9001669 0 N 271 1 2
#
# CMP 209
CMP 5 2.1355629 0.9198519 270 N R310 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 2.1355629 0.9001669 180 N 290 1 1
TOP 1 2.1355629 0.939537 180 N 317 1 2
#
# CMP 210
CMP 5 2.2095253 0.919852 90 N R311 CRCW04027K87FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04027K87FKED'
PRP Power_W '63mW'
PRP Res_ohm '7.87k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-7.87KLCT-ND'
PRP Supplier_Part_Number_2 '52K7249'
PRP Supplier_Part_Number_3 '71-CRCW0402-7.87K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '7.87k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '7k87'
PRP ValueDisplayed '7.87k'
PRP VDC_V '50V'
TOP 0 2.2095253 0.939537 0 N 317 2 1
TOP 1 2.2095253 0.9001669 0 N 196 1 2
#
# CMP 211
CMP 5 2.2456353 0.9198519 270 N R313 CRCW040282K5FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040282K5FKED'
PRP Power_W '63mW'
PRP Res_ohm '82.5k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-82.5KLCT-ND'
PRP Supplier_Part_Number_2 '52K7304'
PRP Supplier_Part_Number_3 '71-CRCW0402-82.5K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '82.5k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '82k5'
PRP ValueDisplayed '82.5k'
PRP VDC_V '50V'
TOP 0 2.2456353 0.9001669 180 N 424 609 1
TOP 1 2.2456353 0.939537 180 N 317 3 2
#
# CMP 212
CMP 1 0.7492194 1.1746741 180 N R320 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 0.760243 1.1746741 90 N 388 4 1
TOP 1 0.7381958 1.1746741 90 N 157 0 2
#
# CMP 213
CMP 1 0.2620005 0.8698115 0 N R324 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 0.2509769 0.8698115 270 N 288 2 1
TOP 1 0.2730241 0.8698115 270 N 351 0 2
#
# CMP 214
CMP 5 1.433028 2.6313103 180 N R325 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 1.452713 2.6313103 90 N 400 2 1
TOP 1 1.4133429 2.6313103 90 N 300 2 2
#
# CMP 215
CMP 1 0.262361 0.8388821 0 N R328 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 0.2513374 0.8388821 270 N 165 1 1
TOP 1 0.2733846 0.8388821 270 N 350 0 2
#
# CMP 216
CMP 1 0.2623592 0.8006586 0 N R329 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 0.2513356 0.8006586 270 N 164 1 1
TOP 1 0.2733828 0.8006586 270 N 349 0 2
#
# CMP 217
CMP 5 3.0356951 0.9933283 90 N R331 CRCW04021K00FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04021K00FKED'
PRP Power_W '63mW'
PRP Res_ohm '1k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-1.00KLCT-ND'
PRP Supplier_Part_Number_2 '52K6545'
PRP Supplier_Part_Number_3 '71-CRCW0402-1.0K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '1.00k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '1k00'
PRP ValueDisplayed '1.00k'
PRP VDC_V '50V'
TOP 0 3.0356951 1.0130133 0 N 363 1 1
TOP 1 3.0356951 0.9736432 0 N 138 9 2
#
# CMP 218
CMP 5 0.0788355 1.8071262 0 N R333 ERJ-2GEJ101X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C84.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GEJ101X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '100'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 'P100JCT-ND'
PRP Supplier_Part_Number_2 '65T8246'
PRP Supplier_Part_Number_3 '2059210'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '100'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '100R'
PRP ValueDisplayed '100'
PRP VDC_V ''
TOP 0 0.0591505 1.8071262 270 N 313 0 1
TOP 1 0.0985206 1.8071262 270 N 109 35 2
#
# CMP 219
CMP 1 0.2159465 1.8674474 270 N R334 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 0.2159465 1.8564238 180 N 312 0 1
TOP 1 0.2159465 1.878471 180 N 33 1 2
#
# CMP 220
CMP 5 0.1793868 1.871756 90 N R335 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 0.1793868 1.891441 0 N 424 610 1
TOP 1 0.1793868 1.8520709 0 N 312 1 2
#
# CMP 221
CMP 5 1.4323036 2.6765989 180 N R336 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 1.4519886 2.6765989 90 N 399 2 1
TOP 1 1.4126185 2.6765989 90 N 299 0 2
#
# CMP 222
CMP 5 0.9250349 2.4188889 180 N R337 CRCW040211K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040211K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '11k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-11.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6621'
PRP Supplier_Part_Number_3 '71-CRCW0402-11K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '11.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '11k0'
PRP ValueDisplayed '11.0k'
PRP VDC_V '50V'
TOP 0 0.9447199 2.4188889 90 N 192 0 1
TOP 1 0.9053498 2.4188889 90 N 424 611 2
#
# CMP 223
CMP 5 1.4337456 2.7248875 180 N R338 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 1.4534306 2.7248875 90 N 398 2 1
TOP 1 1.4140605 2.7248875 90 N 298 2 2
#
# CMP 224
CMP 5 1.4340101 2.7730898 180 N R339 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 1.4536951 2.7730898 90 N 397 2 1
TOP 1 1.414325 2.7730898 90 N 297 0 2
#
# CMP 225
CMP 5 1.0877221 2.9555293 270 N R340 CRCW04022K20JNED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K20JNED'
PRP Power_W '63mW'
PRP Res_ohm '2.2k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.2KJCT-ND'
PRP Supplier_Part_Number_2 '59M6710'
PRP Supplier_Part_Number_3 '71-CRCW0402J-2.2K-E3'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP Value '2.2k'
PRP Value1 '5%'
PRP Value2 '0.063W'
PRP Value_Code '2k20'
PRP ValueDisplayed '2.2k'
PRP VDC_V '50V'
TOP 0 1.0877221 2.9358443 180 N 443 1 1
TOP 1 1.0877221 2.9752144 180 N 261 17 2
#
# CMP 226
CMP 5 1.1432001 2.9555293 270 N R342 CRCW04022K20JNED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K20JNED'
PRP Power_W '63mW'
PRP Res_ohm '2.2k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.2KJCT-ND'
PRP Supplier_Part_Number_2 '59M6710'
PRP Supplier_Part_Number_3 '71-CRCW0402J-2.2K-E3'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP Value '2.2k'
PRP Value1 '5%'
PRP Value2 '0.063W'
PRP Value_Code '2k20'
PRP ValueDisplayed '2.2k'
PRP VDC_V '50V'
TOP 0 1.1432001 2.9358443 180 N 439 1 1
TOP 1 1.1432001 2.9752144 180 N 261 18 2
#
# CMP 227
CMP 1 1.0527522 2.3231707 270 N R344 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 1.0527522 2.3121471 180 N 377 1 1
TOP 1 1.0527522 2.3341943 180 N 438 0 2
#
# CMP 228
CMP 42 1.5532267 0.7682126 90 N R353 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 1.5532267 0.7883897 90 N 256 1 1
TOP 1 1.5532267 0.7480354 90 N 220 1 2
#
# CMP 229
CMP 42 1.4771627 0.6685795 0 N R354 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 1.4569856 0.6685795 0 N 450 3 1
TOP 1 1.4973399 0.6685795 0 N 219 1 2
#
# CMP 230
CMP 42 1.4771627 0.6273705 0 N R355 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 1.4569856 0.6273705 0 N 255 1 1
TOP 1 1.4973399 0.6273705 0 N 218 1 2
#
# CMP 231
CMP 42 1.4771627 0.5865795 0 N R356 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 1.4569856 0.5865795 0 N 449 2 1
TOP 1 1.4973399 0.5865795 0 N 217 1 2
#
# CMP 232
CMP 42 1.7442083 0.5829903 180 N R357 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 1.7643854 0.5829903 180 N 253 1 1
TOP 1 1.7240311 0.5829903 180 N 216 1 2
#
# CMP 233
CMP 42 1.7442083 0.5355795 180 N R358 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 1.7643854 0.5355795 180 N 447 2 1
TOP 1 1.7240311 0.5355795 180 N 215 1 2
#
# CMP 234
CMP 42 1.7442083 0.6778119 180 N R359 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 1.7643854 0.6778119 180 N 254 1 1
TOP 1 1.7240311 0.6778119 180 N 214 1 2
#
# CMP 235
CMP 42 1.7442083 0.6304011 180 N R360 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 1.7643854 0.6304011 180 N 448 2 1
TOP 1 1.7240311 0.6304011 180 N 213 1 2
#
# CMP 236
CMP 5 1.116036 2.3201741 90 N R369 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 1.116036 2.3398591 0 N 228 0 1
TOP 1 1.116036 2.300489 0 N 404 2 2
#
# CMP 237
CMP 1 1.0160202 2.3231707 270 N R370 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 1.0160202 2.3121471 180 N 376 1 1
TOP 1 1.0160202 2.3341943 180 N 437 0 2
#
# CMP 238
CMP 41 1.1573026 1.4302681 0 N R377 ERJ-1GNF33R2C ;0=1,1=0.0000
PRP AEC_Category ''
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP CompType ''
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-1GNF33R2C.pdf'
PRP Digikey_Description 'RES SMD 33.2 OHM 1% 1/20W 0201'
PRP Digikey_Part_Number 'P122945CT-ND'
PRP EIA_Code ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP helpURL 'https://upverter.com/upn/revision/804e6f7ea13c6b2c/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP MountType ''
PRP Mouser_Description 'Thick Film Resistors - SMD 0201 33.2ohm 1% HalogenFree AEC-Q200'
PRP Mouser_Part_Number '667-ERJ-1GNF33R2C'
PRP Operating_Temperature_Range '-55°C to +125°C'
PRP PackageReference '0201'
PRP Part_Number 'ERJ-1GNF33R2C'
PRP PartNumber 'ERJ-1GNF33R2C'
PRP Power_W '50mW'
PRP Res_ohm '33.2'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm '0.26mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'P122945CT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-1GNF33R2C'
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo '200ppm/°C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 ''
PRP Value2 ''
PRP Value_Code ''
PRP ValueDisplayed ''
PRP VDC_V '25V'
TOP 0 1.1454916 1.4302681 0 N 232 0 1
TOP 1 1.1691136 1.4302681 0 N 212 0 2
#
# CMP 239
CMP 1 0.2623592 0.7645455 0 N R379 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 0.2513356 0.7645455 270 N 274 3 1
TOP 1 0.2733828 0.7645455 270 N 230 0 2
#
# CMP 240
CMP 1 0.2636247 0.7324324 0 N R390 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 0.2526011 0.7324324 270 N 406 8 1
TOP 1 0.2746483 0.7324324 270 N 236 0 2
#
# CMP 241
CMP 1 0.2623392 0.6909477 0 N R391 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 0.2513156 0.6909477 270 N 405 10 1
TOP 1 0.2733628 0.6909477 270 N 235 0 2
#
# CMP 242
CMP 1 1.1573026 1.5190201 180 N R399 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 1.1683262 1.5190201 90 N 210 0 1
TOP 1 1.146279 1.5190201 90 N 234 0 2
#
# CMP 243
CMP 5 0.3613588 4.7180136 270 N R409 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 0.3613588 4.6983286 180 N 112 1 1
TOP 1 0.3613588 4.7376987 180 N 109 36 2
#
# CMP 244
CMP 5 1.1714942 2.3201741 90 N R413 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 1.1714942 2.3398591 0 N 193 0 1
TOP 1 1.1714942 2.300489 0 N 403 2 2
#
# CMP 245
CMP 39 1.0341952 2.2492661 180 N R414 CRCW06031M00FKEAC ;0=1,1=0.0000
PRP AEC_Category ''
PRP AEC_Grade 'NA'
PRP AEC_Qualified 'No'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.vishay.com/docs/28773/crcwce3.pdf'
PRP CompType ''
PRP Datasheet 'https://www.vishay.com/docs/28773/crcwce3.pdf'
PRP Datasheet_Path 'datasheets/Res-CRCW06031M00FKEAC.pdf'
PRP Digikey_Description 'RES 1M OHM 1% 1/10W 0603'
PRP Digikey_Part_Number '541-5248-1-ND'
PRP EIA_Code ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP helpURL 'https://upverter.com/upn/revision/a11350b05941555d/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Vishay'
PRP MountType ''
PRP Mouser_Description 'Res Thick Film 0603 1M Ohm 1% 1/10W ±100ppm/°C Molded SMD Paper T/R'
PRP Mouser_Part_Number '71-CRCW06031M00FKEAC'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0603'
PRP Part_Number 'CRCW06031M00FKEAC'
PRP PartNumber 'CRCW06031M00FKEAC'
PRP Power_W '100mW'
PRP Res_ohm '1M'
PRP RoHS 'TRUE'
PRP Series 'CRCW-C'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm '0.55mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '541-5248-1-ND'
PRP Supplier_Part_Number_2 '71-CRCW06031M00FKEAC'
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo '100ppm/°C'
PRP Tolerance__ '1%'
PRP Value '1M'
PRP Value1 ''
PRP Value2 ''
PRP Value_Code ''
PRP ValueDisplayed ''
PRP VDC_V '75V'
TOP 0 1.0637224 2.2492661 180 N 377 2 1
TOP 1 1.0046679 2.2492661 180 N 376 2 2
#
# CMP 246
CMP 5 1.032204 4.6209575 180 N R416 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP INSTALLATION 'DNP'
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 1.051889 4.6209575 90 N 185 0 1
TOP 1 1.0125189 4.6209575 90 N 308 63 2
#
# CMP 247
CMP 5 1.032204 4.672691 0 N R417 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP INSTALLATION 'DNP'
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 1.012519 4.672691 270 N 424 612 1
TOP 1 1.0518891 4.672691 270 N 185 1 2
#
# CMP 248
CMP 5 0.268015 1.1195561 180 N R418 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 0.2877 1.1195561 90 N 183 0 1
TOP 1 0.2483299 1.1195561 90 N 308 64 2
#
# CMP 249
CMP 1 0.2659044 1.0820296 0 N R422 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 0.2548808 1.0820296 270 N 450 2 1
TOP 1 0.276928 1.0820296 270 N 181 0 2
#
# CMP 250
CMP 1 0.2659044 1.0505336 0 N R423 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 0.2548808 1.0505336 270 N 449 1 1
TOP 1 0.276928 1.0505336 270 N 180 0 2
#
# CMP 251
CMP 1 0.7472509 1.0559976 0 N R424 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 0.7362273 1.0559976 270 N 179 0 1
TOP 1 0.7582745 1.0559976 270 N 447 1 2
#
# CMP 252
CMP 1 0.7472509 1.0171938 0 N R425 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 0.7362273 1.0171938 270 N 178 0 1
TOP 1 0.7582745 1.0171938 270 N 448 1 2
#
# CMP 253
CMP 81 1.6028115 0.9039807 180 N S1 CJS-1201TA ;0=1,1=0.0984
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Circuit 'SPDT'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://copal-electronics.info/en/0008e/02461.pdf'
PRP CompType 'Switch'
PRP CurrentRating_mA '100A'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Copal Electronics'
PRP MountType 'SMT'
PRP Orientation 'Side Actuated'
PRP PackageReference 'SW, 3.1x2.5x6 mm'
PRP PartNumber 'CJS-1201TA'
PRP PositionCount '1'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '563-1023-1-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP SwitchFunction 'On-Off-On'
PRP VDC_V '50V'
TOP 0 1.6717091 0.9492563 180 N 308 72 1
TOP 1 1.6028115 0.8587051 180 N 311 1 2
TOP 2 1.5339139 0.9492563 180 N 424 657 3
#
# CMP 254
CMP 82 0.0964721 1.5469985 90 N SW1 KMR243GLFG ;0=1,1=0.0748
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Circuit 'SPST-NO'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.ckswitches.com/media/1479/kmr2.pdf'
PRP CompType 'Switch'
PRP CurrentRating_mA '10A'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'C&K Components'
PRP MountType 'SMT'
PRP Orientation 'Top Actuated'
PRP PackageReference '4.2x2.8mm'
PRP PartNumber 'KMR243GLFG'
PRP PositionCount '1'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '12.88'
PRP SizeAreaWB_mm2 '21.28'
PRP SizeX_mm '4.6'
PRP SizeY_mm '2.8'
PRP SizeZ_mm '1.9'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '401-1432-2-ND'
PRP Supplier_Part_Number_2 '611-KMR243GLFG'
PRP Supplier_Part_Number_3 ''
PRP SwitchFunction 'Off-Mom'
PRP VDC_V '32V'
TOP 0 0.1279682 1.6277072 90 N 0 184 1
TOP 1 0.1279682 1.4662898 90 N 321 1 2
TOP 2 0.064976 1.6277072 90 N 0 183 3
TOP 3 0.064976 1.4662898 90 N 272 9 4
TOP 4 0.1525745 1.5469985 270 N 424 658 5
#
# CMP 255
CMP 82 0.0906468 1.9327798 90 N SW2 KMR243GLFG ;0=1,1=0.0748
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Circuit 'SPST-NO'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.ckswitches.com/media/1479/kmr2.pdf'
PRP CompType 'Switch'
PRP CurrentRating_mA '10A'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'C&K Components'
PRP MountType 'SMT'
PRP Orientation 'Top Actuated'
PRP PackageReference '4.2x2.8mm'
PRP PartNumber 'KMR243GLFG'
PRP PositionCount '1'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '12.88'
PRP SizeAreaWB_mm2 '21.28'
PRP SizeX_mm '4.6'
PRP SizeY_mm '2.8'
PRP SizeZ_mm '1.9'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '401-1432-2-ND'
PRP Supplier_Part_Number_2 '611-KMR243GLFG'
PRP Supplier_Part_Number_3 ''
PRP SwitchFunction 'Off-Mom'
PRP VDC_V '32V'
TOP 0 0.1221429 2.0134885 90 N 0 161 1
TOP 1 0.1221429 1.8520711 90 N 312 2 2
TOP 2 0.0591507 2.0134885 90 N 0 162 3
TOP 3 0.0591507 1.8520711 90 N 313 1 4
TOP 4 0.1467492 1.9327798 270 N 424 613 5
#
# CMP 256
CMP 85 1.429 4.003 0 N TP1 TESTPOINT ;0=1,1=0.0000
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ClassName ''
PRP ComponentLink1Description ''
PRP ComponentLink1URL ''
PRP CompType 'Testpoint'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'N/A'
PRP MountType ''
PRP Note ''
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
PRP RoHS ''
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Value ''
TOP 0 1.429 4.003 0 N 267 4 1
#
# CMP 257
CMP 85 0.2214926 1.6165651 180 N TP4 TESTPOINT ;0=1,1=0.0000
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ClassName ''
PRP ComponentLink1Description ''
PRP ComponentLink1URL ''
PRP CompType 'Testpoint'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'N/A'
PRP MountType ''
PRP Note ''
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
PRP RoHS ''
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Value ''
TOP 0 0.2214926 1.6165651 180 N 272 7 1
#
# CMP 258
CMP 85 1.2674317 2.2140935 270 N TP5 TESTPOINT ;0=1,1=0.0000
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ClassName ''
PRP ComponentLink1Description ''
PRP ComponentLink1URL ''
PRP CompType 'Testpoint'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'N/A'
PRP MountType ''
PRP Note ''
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
PRP RoHS ''
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Value ''
TOP 0 1.2674317 2.2140935 270 N 177 0 1
#
# CMP 259
CMP 85 0.7860336 2.2673188 270 N TP6 TESTPOINT ;0=1,1=0.0000
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ClassName ''
PRP ComponentLink1Description ''
PRP ComponentLink1URL ''
PRP CompType 'Testpoint'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'N/A'
PRP MountType ''
PRP Note ''
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
PRP RoHS ''
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Value ''
TOP 0 0.7860336 2.2673188 270 N 204 1 1
#
# CMP 260
CMP 60 1.03 0.345 270 N TP9 5001 ;0=2,1=0.1811
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'FALSE'
PRP Color 'Black'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.keyelco.com/userAssets/file/M60-2p60.pdf'
PRP CompType 'Test Point'
PRP ContactFinish 'Silver'
PRP CT 'TRUE'
PRP Current_A ''
PRP Gender ''
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Keystone Electronics'
PRP MountType 'TH'
PRP Note ''
PRP Orientation ''
PRP PackageReference 'Black Miniature Testpoint'
PRP PartNumber '5001'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '36-5001-ND'
PRP Supplier_Part_Number_2 '534-5001'
PRP Supplier_Part_Number_3 ''
PRP Voltage_V ''
TOP 0 1.03 0.345 270 N 424 525 1
#
# CMP 261
CMP 27 2.6503606 0.8715229 0 N U2 LM63635DQDRRRQ1 ;0=1,1=0.0010
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP Datasheet_Path 'datasheets/IC_LM63635DQDRRRQ1.pdf'
PRP helpURL 'https://upverter.com/upn/revision/97d64d7c679a76d8/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Texas Instruments'
PRP Max_Duty_Cycle '98%'
PRP Max_Supply_Voltage '32V'
PRP Min_Supply_Voltage '3.5V'
PRP Nominal_Supply_Current '23uA'
PRP Number_Of_Outputs '1'
PRP Operating_Temperature_Range '-40°C to +125°C'
PRP Output_Type 'Fixed,AdjustableProgrammable'
PRP Output_Voltage '3.3/5/1-20V'
PRP PackageReference 'WSON12'
PRP PartNumber 'LM63635DQDRRRQ1'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.8mm'
PRP Standoff_Height '0mm'
PRP Switching_Frequency '400/2100/250-2200kHz'
PRP Switching_Topology 'Buck'
PRP TaMax_C '+125°C'
PRP TaMin_C '-40°C'
PRP TJmax_C '+150°C'
TOP 0 2.5956362 0.9207355 0 N 160 2 1
TOP 1 2.5956362 0.9010505 0 N 161 1 2
TOP 2 2.5956362 0.8813654 0 N 170 2 3
TOP 3 2.5956362 0.8616804 0 N 153 1 4
TOP 4 2.5956362 0.8419953 0 N 154 0 5
TOP 5 2.5956362 0.8223103 0 N 171 2 6
TOP 6 2.705085 0.8223103 0 N 114 0 7
TOP 7 2.705085 0.8419953 0 N 308 68 8
TOP 8 2.705085 0.8616804 0 N 424 627 9
TOP 9 2.705085 0.8813654 0 N 172 2 10
TOP 10 2.705085 0.9010505 0 N 0 167 11
TOP 11 2.705085 0.9207355 0 N 138 10 12
TOP 12 2.6503606 0.8715229 0 N 424 626 13
#
# CMP 262
CMP 20 1.9574353 0.8083828 270 N U7 LM4040C25QDBZR ;0=1,1=0.0441
PRP Code_JEDEC 'TO-236'
PRP ComponentLink1Description 'Manufacturer URL'
PRP ComponentLink1URL 'http://www.ti.com/'
PRP ComponentLink2Description 'Datasheet'
PRP ComponentLink2URL 'http://www.ti.com/general/docs/lit/getliterature.tsp?genericPartNumber=LM4040C25&fileType=pdf'
PRP ComponentLink3Description 'Package Specification'
PRP ComponentLink3URL 'http://www.ti.com/litv/pdf/mpds108a'
PRP DatasheetVersion 'SLOS456K'
PRP Eco-Plan 'Green (RoHS & no Sb/Br)'
PRP Initial_Accuracy_@_25/deg_C(_) '0.5'
PRP Iout/Iz(Max)(mA) '15'
PRP Manufacturer 'Texas Instruments'
PRP Min_Iz_for_Regulation(uA) '75'
PRP Mounting_Technology 'Surface Mount'
PRP PackageDescription '3-Pin Plastic Small Outline, Body 2.92 x 1.3 mm, Pitch 0.95 mm'
PRP PackageReference 'DBZ0003A'
PRP PackageVersion '4203227/B'
PRP PartNumber 'LM4040C25QDBZR'
PRP Rating 'Catalog'
PRP SubFamily 'Shunt Voltage Reference'
PRP Temp_Coeff(Max)(ppm/_degree_C) '100'
PRP Temp_Coeff(Typ)(ppm/_degree_C) '15'
PRP VO(V) '2.5'
TOP 0 1.9200337 0.7611387 180 N 241 4 1
TOP 1 1.9948368 0.7611387 180 N 424 623 2
TOP 2 1.9574353 0.8556269 180 N 0 166 3
#
# CMP 263
CMP 24 0.7420709 2.6681079 0 N U13 TPD4E05U06DQAR ;0=1,1=0.0217
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer 'Texas Instruments'
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/tpd4e05u06.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/tpd4e05u06'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/tpd4e05u06/datasheet'
PRP CompType 'IC'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP PackageDescription 'USON-10'
PRP PackageReference 'DQA0010A'
PRP PartNumber 'TPD4E05U06DQAR'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '7.0'
PRP SizeX_mm '1.0'
PRP SizeY_mm '2.5'
PRP SizeZ_mm '0.55'
TOP 0 0.7256339 2.707478 270 N 282 1 1
TOP 1 0.7256339 2.687793 270 N 283 1 2
TOP 2 0.7256339 2.668108 270 N 424 625 3
TOP 3 0.7256339 2.6484229 270 N 280 2 4
TOP 4 0.7256339 2.6287379 270 N 281 2 5
TOP 5 0.7585079 2.6287379 270 N 281 1 6
TOP 6 0.7585079 2.6484229 270 N 280 1 7
TOP 7 0.7585079 2.668108 270 N 424 624 8
TOP 8 0.7585079 2.687793 270 N 283 2 9
TOP 9 0.7585079 2.707478 270 N 282 2 10
#
# CMP 264
CMP 24 0.7420708 2.4620345 0 N U14 TPD4E05U06DQAR ;0=1,1=0.0217
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer 'Texas Instruments'
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/tpd4e05u06.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/tpd4e05u06'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/tpd4e05u06/datasheet'
PRP CompType 'IC'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP PackageDescription 'USON-10'
PRP PackageReference 'DQA0010A'
PRP PartNumber 'TPD4E05U06DQAR'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '7.0'
PRP SizeX_mm '1.0'
PRP SizeY_mm '2.5'
PRP SizeZ_mm '0.55'
TOP 0 0.7256338 2.5014046 270 N 278 1 1
TOP 1 0.7256338 2.4817196 270 N 279 1 2
TOP 2 0.7256338 2.4620346 270 N 424 614 3
TOP 3 0.7256338 2.4423495 270 N 276 2 4
TOP 4 0.7256338 2.4226645 270 N 277 2 5
TOP 5 0.7585078 2.4226645 270 N 277 1 6
TOP 6 0.7585078 2.4423495 270 N 276 1 7
TOP 7 0.7585078 2.4620346 270 N 424 615 8
TOP 8 0.7585078 2.4817196 270 N 279 2 9
TOP 9 0.7585078 2.5014046 270 N 278 2 10
#
# CMP 265
CMP 67 1.1759283 2.5655424 0 N U15 DP83867ERGZR ;0=1,1=0.0394
PRP Alternate_Manufacturer 'Texas Instruments'
PRP Alternate_PartNumber 'DP83867ERGZT'
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/dp83867e.pdf'
PRP CompType 'IC'
PRP LatestRevisionDate '2017-06-09'
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP PackageDescription 'VQFN-48'
PRP PackageReference 'RGZ0048B'
PRP PartNumber 'DP83867ERGZR'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '49'
PRP SizeAreaWB_mm2 '81'
PRP SizeX_mm '7'
PRP SizeY_mm '7'
PRP SizeZ_mm '1'
PRP U/M 'EA'
TOP 0 1.04207 2.6738101 270 N 282 3 1
TOP 1 1.04207 2.6541251 270 N 283 3 2
TOP 2 1.04207 2.63444 270 N 456 10 3
TOP 3 1.04207 2.614755 270 N 280 3 4
TOP 4 1.04207 2.5950699 270 N 281 3 5
TOP 5 1.04207 2.5753849 270 N 459 12 6
TOP 6 1.04207 2.5556999 270 N 278 3 7
TOP 7 1.04207 2.5360148 270 N 279 3 8
TOP 8 1.04207 2.5163298 270 N 456 11 9
TOP 9 1.04207 2.4966447 270 N 276 3 10
TOP 10 1.04207 2.4769597 270 N 277 3 11
TOP 11 1.04207 2.4572747 270 N 192 1 12
TOP 12 1.0676606 2.4316841 0 N 0 174 13
TOP 13 1.0873456 2.4316841 0 N 437 1 14
TOP 14 1.1070307 2.4316841 0 N 438 1 15
TOP 15 1.1267157 2.4316841 0 N 228 1 16
TOP 16 1.1464008 2.4316841 0 N 193 1 17
TOP 17 1.1660858 2.4316841 0 N 177 1 18
TOP 18 1.1857708 2.4316841 0 N 261 20 19
TOP 19 1.2054559 2.4316841 0 N 0 173 20
TOP 20 1.2251409 2.4316841 0 N 0 172 21
TOP 21 1.244826 2.4316841 0 N 0 171 22
TOP 22 1.264511 2.4316841 0 N 0 170 23
TOP 23 1.284196 2.4316841 0 N 459 13 24
TOP 24 1.3097866 2.4572747 270 N 292 1 25
TOP 25 1.3097866 2.4769597 270 N 293 1 26
TOP 26 1.3097866 2.4966447 270 N 294 1 27
TOP 27 1.3097866 2.5163298 270 N 295 1 28
TOP 28 1.3097866 2.5360148 270 N 296 1 29
TOP 29 1.3097866 2.5556999 270 N 261 21 30
TOP 30 1.3097866 2.5753849 270 N 459 14 31
TOP 31 1.3097866 2.5950699 270 N 188 1 32
TOP 32 1.3097866 2.614755 270 N 300 3 33
TOP 33 1.3097866 2.63444 270 N 299 1 34
TOP 34 1.3097866 2.6541251 270 N 298 3 35
TOP 35 1.3097866 2.6738101 270 N 297 1 36
TOP 36 1.284196 2.6994007 0 N 186 1 37
TOP 37 1.264511 2.6994007 0 N 187 3 38
TOP 38 1.244826 2.6994007 0 N 445 2 39
TOP 39 1.2251409 2.6994007 0 N 444 2 40
TOP 40 1.2054559 2.6994007 0 N 261 22 41
TOP 41 1.1857708 2.6994007 0 N 459 15 42
TOP 42 1.1660858 2.6994007 0 N 439 2 43
TOP 43 1.1464008 2.6994007 0 N 443 2 44
TOP 44 1.1267157 2.6994007 0 N 440 3 45
TOP 45 1.1070307 2.6994007 0 N 441 2 46
TOP 46 1.0873456 2.6994007 0 N 442 3 47
TOP 47 1.0676606 2.6994007 0 N 0 169 48
TOP 48 1.1759283 2.5655424 0 N 424 634 49
#
# CMP 266
CMP 28 0.7805795 3.028347 270 N U16 TPS73501DRVR ;0=1,1=0.0315
PRP Accuracy(_) '2'
PRP ComponentLink1Description 'Manufacturer URL'
PRP ComponentLink1URL 'http://www.ti.com/'
PRP ComponentLink2Description 'Datasheet'
PRP ComponentLink2URL 'http://www.ti.com/general/docs/lit/getliterature.tsp?genericPartNumber=TPS73501&fileType=pdf'
PRP ComponentLink3Description 'Package Specification'
PRP ComponentLink3URL 'http://www.ti.com/litv/pdf/mpds216d'
PRP CompType 'IC'
PRP DatasheetVersion 'SBVS087J'
PRP Eco-Plan 'Green (RoHS & no Sb/Br)'
PRP Iout(Max)(A) '0.5'
PRP Iq(Typ)(mA) '0.04'
PRP Manufacturer 'Texas Instruments'
PRP Mounting_Technology 'Surface Mount'
PRP MountType 'SMT'
PRP PackageDescription 'WSON-6'
PRP PackageReference 'DRV0006A'
PRP PackageVersion '4206925/E'
PRP PartNumber 'TPS73501DRVR'
PRP SizeArea_mm2 '4'
PRP SizeAreaWB_mm2 '9'
PRP SizeX_mm '2'
PRP SizeY_mm '2'
PRP SizeZ_mm '0.8'
PRP SubFamily 'Single Channel LDO'
PRP Vdo(Typ)(mV) '280'
PRP Vin(Max)(V) '6.5'
PRP Vin(Min)(V) '2.7'
PRP Vout_Adj(Max)(V) '6'
PRP Vout_Adj(Min)(V) '1.25'
TOP 0 0.7549889 2.9899612 180 N 456 9 1
TOP 1 0.7805795 2.9899612 180 N 375 3 2
TOP 2 0.80617 2.9899612 180 N 424 628 3
TOP 3 0.80617 3.0667328 180 N 261 19 4
TOP 4 0.7805795 3.0667328 180 N 0 168 5
TOP 5 0.7549889 3.0667328 180 N 308 69 6
TOP 6 0.7805795 3.028347 270 N 424 629 7
#
# CMP 267
CMP 28 1.2839401 2.0186616 90 N U17 TLV73310PQDRVRQ1 ;0=1,1=0.0315
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer 'Texas Instruments'
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/tlv733p-q1.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/tlv733p-q1'
PRP CompType 'IC'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP PackageDescription 'WSON-6'
PRP PackageReference 'DRV0006A'
PRP PartNumber 'TLV73310PQDRVRQ1'
PRP RoHS 'Y'
PRP SizeArea_mm2 '4'
PRP SizeAreaWB_mm2 '9'
PRP SizeX_mm '2'
PRP SizeY_mm '2'
PRP SizeZ_mm '0.8'
TOP 0 1.3095307 2.0570474 0 N 459 11 1
TOP 1 1.2839401 2.0570474 0 N 0 164 2
TOP 2 1.2583496 2.0570474 0 N 424 616 3
TOP 3 1.2583496 1.9802758 0 N 309 14 4
TOP 4 1.2839401 1.9802758 0 N 0 163 5
TOP 5 1.3095307 1.9802758 0 N 309 13 6
TOP 6 1.2839401 2.0186616 90 N 424 617 7
#
# CMP 268
CMP 69 1.6106855 0.6352446 0 N U23 TS3A5018RSVR ;0=1,1=0.0217
PRP Alternate_Manufacturer 'Texas Instruments'
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/ts3a5018.pdf'
PRP CompType 'IC'
PRP Footprint_Path_6 'C:\AltiumLibraries\Footprints\TI\.PcbLib'
PRP LatestRevisionDate '2017-06-09'
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP PackageDescription 'UQFN-16'
PRP PackageReference 'RSV0016A'
PRP PartNumber 'TS3A5018RSVR'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '4.68'
PRP SizeAreaWB_mm2 '10.08'
PRP SizeX_mm '1.8'
PRP SizeY_mm '2.6'
PRP SizeZ_mm '0.55'
PRP U/M 'EA'
TOP 0 1.5811579 0.6588667 270 N 219 0 1
TOP 1 1.5791894 0.6431187 270 N 141 1 2
TOP 2 1.5791894 0.6273706 270 N 218 0 3
TOP 3 1.5791894 0.6116226 270 N 217 0 4
TOP 4 1.5870635 0.5880005 0 N 140 1 5
TOP 5 1.6028115 0.5880005 0 N 424 635 6
TOP 6 1.6185595 0.5880005 0 N 139 1 7
TOP 7 1.6343076 0.5880005 0 N 215 0 8
TOP 8 1.6421816 0.6116226 270 N 216 0 9
TOP 9 1.6421816 0.6273706 270 N 290 2 10
TOP 10 1.6421816 0.6431187 270 N 213 0 11
TOP 11 1.6421816 0.6588667 270 N 214 0 12
TOP 12 1.6343076 0.6824887 0 N 320 1 13
TOP 13 1.6185595 0.6824887 0 N 308 70 14
TOP 14 1.6028115 0.6824887 0 N 311 0 15
TOP 15 1.5870635 0.6824887 0 N 220 0 16
#
# CMP 269
CMP 69 1.2583076 1.4824335 0 N U26 TS3A5018RSVR ;0=1,1=0.0217
PRP Alternate_Manufacturer 'Texas Instruments'
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/ts3a5018.pdf'
PRP CompType 'IC'
PRP Footprint_Path_6 'C:\AltiumLibraries\Footprints\TI\.PcbLib'
PRP LatestRevisionDate '2017-06-09'
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP PackageDescription 'UQFN-16'
PRP PackageReference 'RSV0016A'
PRP PartNumber 'TS3A5018RSVR'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '4.68'
PRP SizeAreaWB_mm2 '10.08'
PRP SizeX_mm '1.8'
PRP SizeY_mm '2.6'
PRP SizeZ_mm '0.55'
PRP U/M 'EA'
TOP 0 1.22878 1.5060556 270 N 210 1 1
TOP 1 1.2268115 1.4903076 270 N 387 1 2
TOP 2 1.2268115 1.4745595 270 N 39 1 3
TOP 3 1.2268115 1.4588115 270 N 212 1 4
TOP 4 1.2346856 1.4351894 0 N 385 1 5
TOP 5 1.2504336 1.4351894 0 N 424 618 6
TOP 6 1.2661816 1.4351894 0 N 384 1 7
TOP 7 1.2819297 1.4351894 0 N 223 1 8
TOP 8 1.2898037 1.4588115 270 N 38 1 9
TOP 9 1.2898037 1.4745595 270 N 225 2 10
TOP 10 1.2898037 1.4903076 270 N 222 1 11
TOP 11 1.2898037 1.5060556 270 N 40 1 12
TOP 12 1.2819297 1.5296776 0 N 221 1 13
TOP 13 1.2661816 1.5296776 0 N 308 65 14
TOP 14 1.2504336 1.5296776 0 N 209 1 15
TOP 15 1.2346856 1.5296776 0 N 41 1 16
#
# CMP 270
CMP 19 0.3613588 4.5884053 90 N U27 TPS78417QDBVRQ1 ;0=1,1=0.0000
PRP Accuracy_Percentage '0.5%'
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.ti.com/lit/ds/symlink/tps784-q1.pdf'
PRP Datasheet 'https://www.ti.com/lit/ds/symlink/tps784-q1.pdf'
PRP Datasheet_Path 'datasheets/IC-TPS78417QDBVRQ1.pdf'
PRP Digikey_Description 'IC REG LINEAR 1.7V 300MA SOT23-5'
PRP Digikey_Part_Number '296-TPS78417QDBVRQ1CT-ND'
PRP Dropout_Voltage '900mV'
PRP helpURL 'https://upverter.com/upn/revision/5a05bdb494de8c30/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Texas Instruments'
PRP Max_Supply_Voltage '6V'
PRP Min_Supply_Voltage '1.65V'
PRP Mouser_Part_Number '595-TPS78417QDBVRQ1'
PRP Nominal_Supply_Current '0.033mA'
PRP Number_Of_Outputs '1'
PRP Operating_Temperature_Range '-40°C to +150°C'
PRP Output_Type 'Fixed'
PRP Output_Voltage '1.7V'
PRP PackageReference 'SOT23-5'
PRP Part_Number 'TPS78417QDBVRQ1'
PRP PartNumber 'TPS78417QDBVRQ1'
PRP RoHS 'TRUE'
PRP SizeZ_mm '1.45mm'
PRP Standoff_Height '0mm'
PRP TaMax_C '+125°C'
PRP TaMin_C '-40°C'
PRP TJmax_C '+150°C'
TOP 0 0.3987604 4.6395864 90 N 308 67 1
TOP 1 0.3613588 4.6395864 90 N 424 622 2
TOP 2 0.3239572 4.6395864 90 N 112 2 3
TOP 3 0.3239572 4.5372242 90 N 0 165 4
TOP 4 0.3987604 4.5372242 90 N 67 3 5
#
# CMP 271
CMP 78 1.080826 4.4358496 270 N U28 CAV24C02WE-GT3 ;0=1,1=0.0689
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.onsemi.com/pub_link/Collateral/CAV24C02-D.PDF'
PRP LatestRevisionDate '09/03/2017'
PRP Manufacturer 'ON Semiconductor'
PRP MountType 'SMT'
PRP PackageReference 'SOIC-8'
PRP PartNumber 'CAV24C02WE-GT3'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '29.351'
PRP SizeAreaWB_mm2 '55.131'
PRP SizeX_mm '5.99'
PRP SizeY_mm '4.9'
PRP SizeZ_mm '1.75'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'CAV24C02WE-GT3OSCT-ND'
PRP Supplier_Part_Number_2 '58T9030'
PRP Supplier_Part_Number_3 '863-CAV24C02WE-GT3'
TOP 0 1.005826 4.3285661 180 N 424 655 1
TOP 1 1.055826 4.3285661 180 N 424 654 2
TOP 2 1.105826 4.3285661 180 N 424 653 3
TOP 3 1.155826 4.3285661 180 N 424 652 4
TOP 4 1.155826 4.543133 180 N 405 11 5
TOP 5 1.105826 4.543133 180 N 406 9 6
TOP 6 1.055826 4.543133 180 N 185 2 7
TOP 7 1.005826 4.543133 180 N 308 71 8
#
# CMP 272
CMP 90 1.0302694 2.0939035 0 N Y4 ABM3-25.000MHZ-D2Y-T ;0=1,1=0.0512
PRP AEC_Category ''
PRP AEC_Grade ''
PRP AEC_Qualified ''
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.abracon.com/Resonators/abm3.pdf'
PRP CompType 'Crystal'
PRP Frequency_Stability '+/-30ppm'
PRP Frequency_Tolerance ''
PRP Frequency_Fixed '25MHz'
PRP Frequency_Max ''
PRP Frequency_Min ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Load_Capacitance ''
PRP Manufacturer 'Abracon Corporation'
PRP MountType 'SMT'
PRP PackageReference 'ABM3'
PRP PartNumber 'ABM3-25.000MHZ-D2Y-T'
PRP REACh 'Y'
PRP RoHS 'E'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '535-10645-1-ND'
PRP Supplier_Part_Number_2 '77R1477'
PRP Supplier_Part_Number_3 '815-ABM3-25-D2Y-T'
PRP TaMax_C '85°C'
PRP TaMin_C '-40°C'
TOP 0 0.9495608 2.0939035 0 N 376 3 1
TOP 1 1.1109781 2.0939035 0 N 377 3 2
#
