#
#Component attribute names
#
@0 .comp_mount_type
@1 .comp_height

# CMP 0
CMP 37 1.416179 3.5541238 0 N R270 CRCW04020000Z0EDHP ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.vishay.com/docs/20043/crcwhpe3.pdf'
PRP Datasheet 'https://www.vishay.com/docs/20043/crcwhpe3.pdf'
PRP Datasheet_Path 'datasheets/Res-CRCW04020000Z0EDHP.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/5W 0402'
PRP Digikey_Part_Number '541-0.0YBCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/5e0a18f71149352e/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Vishay Dale'
PRP Mouser_Description 'Resistor; Thick Film; 0 Ohms; 0.125 W; 0 Ohms Jumper; SMT; 0402; TCR 0 ppm/DegC'
PRP Mouser_Part_Number '71-CRCW04020000Z0EDH'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'CRCW04020000Z0EDHP'
PRP PartNumber 'CRCW04020000Z0EDHP'
PRP Power_W '200mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'CRCW-HP e3'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '541-0.0YBCT-ND'
PRP Supplier_Part_Number_2 '71-CRCW04020000Z0EDH'
PRP Technology 'Thick Film'
PRP Value '0'
PRP VDC_V '50V'
TOP 0 1.4368483 3.5541238 180 N 102 2 1
TOP 1 1.3955097 3.5541238 180 N 74 3 2
#
# CMP 1
CMP 5 2.2294633 4.447 180 N R212 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 2.2097783 4.447 90 N 385 0 1
TOP 1 2.2491484 4.447 90 N 1 1 2
#
# CMP 2
CMP 5 0.748951 1.441 180 N R210 CRCW040210R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '10.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '541-10.2LCT-ND'
PRP Supplier_Part_Number_2 '71-CRCW0402-10.2-E3'
PRP Supplier_Part_Number_3 '1158303'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10R2'
PRP ValueDisplayed '10.2'
PRP VDC_V '50V'
TOP 0 0.729266 1.441 90 N 412 2 1
TOP 1 0.7686361 1.441 90 N 2 0 2
#
# CMP 3
CMP 77 0.832 1.441 180 N D20 SMS3923-040LF ;0=1,1=0.0197
PRP AEC_Category 'Q101'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.skyworksinc.com/uploads/documents/SMS392x_Series_200042AC.pdf'
PRP CompType 'Diode'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Io_A '10mA'
PRP Manufacturer 'Skyworks Solutions'
PRP MountType 'SMT'
PRP PackageReference 'SOD-882'
PRP PartNumber 'SMS3923-040LF'
PRP RJC_CperW ''
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.6'
PRP SizeAreaWB_mm2 '3.2'
PRP SizeX_mm '1'
PRP SizeY_mm '0.6'
PRP SizeZ_mm '0.5'
PRP TJmax_C '150°C'
PRP Type 'Schottky'
PRP Value 'V'
PRP Value1 '0.01A'
PRP Value2 '0.34V'
PRP Vf_V '340mV'
PRP Vr_V ''
TOP 0 0.8157599 1.441 0 N 2 1 1
TOP 1 0.8482401 1.441 0 N 272 1 2
#
# CMP 4
CMP 47 2.0035044 2.472 0 N R193 HCJ0603ZT0R00 ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.seielect.com/Catalog/SEI-HCJ.pdf'
PRP Datasheet 'https://www.seielect.com/Catalog/SEI-HCJ.pdf'
PRP Datasheet_Path 'datasheets/Res-HCJ0603ZT0R00.pdf'
PRP Digikey_Description 'RES 0 OHM JUMPER 1/4W 0603'
PRP Digikey_Part_Number 'HCJ0603ZT0R00CT-ND'
PRP helpURL 'https://upverter.com/upn/revision/19d0386aede22bbe/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Stackpole Electronics'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0603'
PRP Part_Number 'HCJ0603ZT0R00'
PRP PartNumber 'HCJ0603ZT0R00'
PRP Power_W '250mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'HCJ'
PRP SizeZ_mm '0.7mm'
PRP Supplier_1 'Digikey'
PRP Supplier_Part_Number_1 'HCJ0603ZT0R00CT-ND'
PRP Technology 'Metal'
PRP Value '0'
TOP 0 2.040906 2.472 180 N 144 8 1
TOP 1 1.9661028 2.472 180 N 57 6 2
#
# CMP 5
CMP 47 2.0035044 2.4078115 0 N R192 HCJ0603ZT0R00 ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.seielect.com/Catalog/SEI-HCJ.pdf'
PRP Datasheet 'https://www.seielect.com/Catalog/SEI-HCJ.pdf'
PRP Datasheet_Path 'datasheets/Res-HCJ0603ZT0R00.pdf'
PRP Digikey_Description 'RES 0 OHM JUMPER 1/4W 0603'
PRP Digikey_Part_Number 'HCJ0603ZT0R00CT-ND'
PRP helpURL 'https://upverter.com/upn/revision/19d0386aede22bbe/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Stackpole Electronics'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0603'
PRP Part_Number 'HCJ0603ZT0R00'
PRP PartNumber 'HCJ0603ZT0R00'
PRP Power_W '250mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'HCJ'
PRP SizeZ_mm '0.7mm'
PRP Supplier_1 'Digikey'
PRP Supplier_Part_Number_1 'HCJ0603ZT0R00CT-ND'
PRP Technology 'Metal'
PRP Value '0'
TOP 0 2.040906 2.4078115 180 N 144 9 1
TOP 1 1.9661028 2.4078115 180 N 57 7 2
#
# CMP 6
CMP 5 2.0977164 3.807084 180 N C55 GCM155R71C224KE02D ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM155R71C224KE02%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71C224KE02D'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-10671-1-ND'
PRP Supplier_Part_Number_2 '81-GCM155R71C224KE2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.22uF'
PRP Value1 ''
PRP Value2 '16V'
PRP ValueDisplayed '0.22µF'
PRP VDC_V '16V'
TOP 0 2.0780314 3.807084 90 N 424 367 1
TOP 1 2.1174015 3.807084 90 N 174 1 2
#
# CMP 7
CMP 5 2.1636862 4.3710011 0 N R273 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP INSTALLATION 'DNP'
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 2.1833712 4.3710011 270 N 225 0 1
TOP 1 2.1440011 4.3710011 270 N 109 17 2
#
# CMP 8
CMP 47 2.1148561 3.6655067 270 N R189 HCJ0603ZT0R00 ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.seielect.com/Catalog/SEI-HCJ.pdf'
PRP Datasheet 'https://www.seielect.com/Catalog/SEI-HCJ.pdf'
PRP Datasheet_Path 'datasheets/Res-HCJ0603ZT0R00.pdf'
PRP Digikey_Description 'RES 0 OHM JUMPER 1/4W 0603'
PRP Digikey_Part_Number 'HCJ0603ZT0R00CT-ND'
PRP helpURL 'https://upverter.com/upn/revision/19d0386aede22bbe/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Stackpole Electronics'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0603'
PRP Part_Number 'HCJ0603ZT0R00'
PRP PartNumber 'HCJ0603ZT0R00'
PRP Power_W '250mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'HCJ'
PRP SizeZ_mm '0.7mm'
PRP Supplier_1 'Digikey'
PRP Supplier_Part_Number_1 'HCJ0603ZT0R00CT-ND'
PRP Technology 'Metal'
PRP Value '0'
TOP 0 2.1148561 3.6281051 270 N 17 1 1
TOP 1 2.1148561 3.7029083 270 N 266 1 2
#
# CMP 9
CMP 42 1.1690005 3.1488115 90 N R186 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 1.1690005 3.1689886 90 N 105 2 1
TOP 1 1.1690005 3.1286343 90 N 97 4 2
#
# CMP 10
CMP 5 0.8580005 3.2654965 270 N R185 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 0.8580005 3.2458115 0 N 96 0 1
TOP 1 0.8580005 3.2851816 0 N 424 145 2
#
# CMP 11
CMP 5 0.9006671 3.2654966 90 N R177 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 0.9006671 3.2851816 180 N 109 5 1
TOP 1 0.9006671 3.2458115 180 N 96 1 2
#
# CMP 12
CMP 47 1.8610005 3.2468115 180 N R176 HCJ0603ZT0R00 ;0=1,1=0.0130
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.seielect.com/Catalog/SEI-HCJ.pdf'
PRP Datasheet 'https://www.seielect.com/Catalog/SEI-HCJ.pdf'
PRP Datasheet_Path 'datasheets/Res-HCJ0603ZT0R00.pdf'
PRP Digikey_Description 'RES 0 OHM JUMPER 1/4W 0603'
PRP Digikey_Part_Number 'HCJ0603ZT0R00CT-ND'
PRP helpURL 'https://upverter.com/upn/revision/19d0386aede22bbe/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Stackpole Electronics'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0603'
PRP Part_Number 'HCJ0603ZT0R00'
PRP PartNumber 'HCJ0603ZT0R00'
PRP Power_W '250mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'HCJ'
PRP SizeZ_mm '0.7mm'
PRP Supplier_1 'Digikey'
PRP Supplier_Part_Number_1 'HCJ0603ZT0R00CT-ND'
PRP Technology 'Metal'
PRP Value '0'
TOP 0 1.8235989 3.2468115 0 N 15 1 1
TOP 1 1.8984021 3.2468115 0 N 144 2 2
#
# CMP 13
CMP 42 0.9433337 3.2664966 90 N R168 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 0.9433337 3.2866737 90 N 146 1 1
TOP 1 0.9433337 3.2463194 90 N 96 7 2
#
# CMP 14
CMP 1 0.9144388 0.929 180 N R167 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 0.9034152 0.929 90 N 8 0 1
TOP 1 0.9254624 0.929 90 N 46 0 2
#
# CMP 15
CMP 1 0.9144388 0.957 180 N R164 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 0.9034152 0.957 90 N 7 0 1
TOP 1 0.9254624 0.957 90 N 45 0 2
#
# CMP 16
CMP 1 0.9254624 0.8248474 270 N R160 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 0.9254624 0.8138238 0 N 6 0 1
TOP 1 0.9254624 0.835871 0 N 48 0 2
#
# CMP 17
CMP 1 0.9254624 0.8748946 90 N R138 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 0.9254624 0.8859182 180 N 5 0 1
TOP 1 0.9254624 0.863871 180 N 47 0 2
#
# CMP 18
CMP 1 0.9580236 0.734 180 N R135 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 0.947 0.734 90 N 60 0 1
TOP 1 0.9690472 0.734 90 N 10 0 2
#
# CMP 19
CMP 1 0.9580236 0.7619998 180 N R51 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 0.947 0.7619998 90 N 59 0 1
TOP 1 0.9690472 0.7619998 90 N 9 0 2
#
# CMP 20
CMP 8 2.2308916 2.1634184 180 N C148 GCM188R70J225KE22D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '2.2µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM188R70J225KE22%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM188R70J225KE22D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5316-1-ND'
PRP Supplier_Part_Number_2 '81-GCM188R70J225KE2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '2.2uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '2.2uF'
PRP VDC_V '6.3V'
TOP 0 2.2033325 2.1634184 90 N 424 315 1
TOP 1 2.2584506 2.1634184 90 N 54 18 2
#
# CMP 21
CMP 47 2.8842604 1.9118115 180 N R110 HCJ0603ZT0R00 ;0=1,1=0.0130
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.seielect.com/Catalog/SEI-HCJ.pdf'
PRP Datasheet 'https://www.seielect.com/Catalog/SEI-HCJ.pdf'
PRP Datasheet_Path 'datasheets/Res-HCJ0603ZT0R00.pdf'
PRP Digikey_Description 'RES 0 OHM JUMPER 1/4W 0603'
PRP Digikey_Part_Number 'HCJ0603ZT0R00CT-ND'
PRP helpURL 'https://upverter.com/upn/revision/19d0386aede22bbe/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Stackpole Electronics'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0603'
PRP Part_Number 'HCJ0603ZT0R00'
PRP PartNumber 'HCJ0603ZT0R00'
PRP Power_W '250mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'HCJ'
PRP SizeZ_mm '0.7mm'
PRP Supplier_1 'Digikey'
PRP Supplier_Part_Number_1 'HCJ0603ZT0R00CT-ND'
PRP Technology 'Metal'
PRP Value '0'
TOP 0 2.8468588 1.9118115 0 N 454 5 1
TOP 1 2.921662 1.9118115 0 N 16 1 2
#
# CMP 22
CMP 47 2.1693564 1.9703775 270 N R109 HCJ0603ZT0R00 ;0=1,1=0.0130
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.seielect.com/Catalog/SEI-HCJ.pdf'
PRP Datasheet 'https://www.seielect.com/Catalog/SEI-HCJ.pdf'
PRP Datasheet_Path 'datasheets/Res-HCJ0603ZT0R00.pdf'
PRP Digikey_Description 'RES 0 OHM JUMPER 1/4W 0603'
PRP Digikey_Part_Number 'HCJ0603ZT0R00CT-ND'
PRP helpURL 'https://upverter.com/upn/revision/19d0386aede22bbe/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Stackpole Electronics'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0603'
PRP Part_Number 'HCJ0603ZT0R00'
PRP PartNumber 'HCJ0603ZT0R00'
PRP Power_W '250mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'HCJ'
PRP SizeZ_mm '0.7mm'
PRP Supplier_1 'Digikey'
PRP Supplier_Part_Number_1 'HCJ0603ZT0R00CT-ND'
PRP Technology 'Metal'
PRP Value '0'
TOP 0 2.1693564 1.9329759 270 N 454 6 1
TOP 1 2.1693564 2.0077791 270 N 13 1 2
#
# CMP 23
CMP 47 2.2343564 1.9703775 270 N R107 HCJ0603ZT0R00 ;0=1,1=0.0130
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.seielect.com/Catalog/SEI-HCJ.pdf'
PRP Datasheet 'https://www.seielect.com/Catalog/SEI-HCJ.pdf'
PRP Datasheet_Path 'datasheets/Res-HCJ0603ZT0R00.pdf'
PRP Digikey_Description 'RES 0 OHM JUMPER 1/4W 0603'
PRP Digikey_Part_Number 'HCJ0603ZT0R00CT-ND'
PRP helpURL 'https://upverter.com/upn/revision/19d0386aede22bbe/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Stackpole Electronics'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0603'
PRP Part_Number 'HCJ0603ZT0R00'
PRP PartNumber 'HCJ0603ZT0R00'
PRP Power_W '250mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'HCJ'
PRP SizeZ_mm '0.7mm'
PRP Supplier_1 'Digikey'
PRP Supplier_Part_Number_1 'HCJ0603ZT0R00CT-ND'
PRP Technology 'Metal'
PRP Value '0'
TOP 0 2.2343564 1.9329759 270 N 309 4 1
TOP 1 2.2343564 2.0077791 270 N 13 2 2
#
# CMP 24
CMP 37 2.0990005 2.0850634 90 N R106 CRCW04020000Z0EDHP ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.vishay.com/docs/20043/crcwhpe3.pdf'
PRP Datasheet 'https://www.vishay.com/docs/20043/crcwhpe3.pdf'
PRP Datasheet_Path 'datasheets/Res-CRCW04020000Z0EDHP.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/5W 0402'
PRP Digikey_Part_Number '541-0.0YBCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/5e0a18f71149352e/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Vishay Dale'
PRP Mouser_Description 'Resistor; Thick Film; 0 Ohms; 0.125 W; 0 Ohms Jumper; SMT; 0402; TCR 0 ppm/DegC'
PRP Mouser_Part_Number '71-CRCW04020000Z0EDH'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'CRCW04020000Z0EDHP'
PRP PartNumber 'CRCW04020000Z0EDHP'
PRP Power_W '200mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'CRCW-HP e3'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '541-0.0YBCT-ND'
PRP Supplier_Part_Number_2 '71-CRCW04020000Z0EDH'
PRP Technology 'Thick Film'
PRP Value '0'
PRP VDC_V '50V'
TOP 0 2.0990005 2.1057327 90 N 12 4 1
TOP 1 2.0990005 2.0643941 90 N 55 1 2
#
# CMP 25
CMP 47 1.8610005 3.3938115 180 N R89 HCJ0603ZT0R00 ;0=1,1=0.0130
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.seielect.com/Catalog/SEI-HCJ.pdf'
PRP Datasheet 'https://www.seielect.com/Catalog/SEI-HCJ.pdf'
PRP Datasheet_Path 'datasheets/Res-HCJ0603ZT0R00.pdf'
PRP Digikey_Description 'RES 0 OHM JUMPER 1/4W 0603'
PRP Digikey_Part_Number 'HCJ0603ZT0R00CT-ND'
PRP helpURL 'https://upverter.com/upn/revision/19d0386aede22bbe/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Stackpole Electronics'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0603'
PRP Part_Number 'HCJ0603ZT0R00'
PRP PartNumber 'HCJ0603ZT0R00'
PRP Power_W '250mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'HCJ'
PRP SizeZ_mm '0.7mm'
PRP Supplier_1 'Digikey'
PRP Supplier_Part_Number_1 'HCJ0603ZT0R00CT-ND'
PRP Technology 'Metal'
PRP Value '0'
TOP 0 1.8235989 3.3938115 0 N 15 2 1
TOP 1 1.8984021 3.3938115 0 N 23 3 2
#
# CMP 26
CMP 47 1.8610005 3.3203115 180 N R88 HCJ0603ZT0R00 ;0=1,1=0.0130
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.seielect.com/Catalog/SEI-HCJ.pdf'
PRP Datasheet 'https://www.seielect.com/Catalog/SEI-HCJ.pdf'
PRP Datasheet_Path 'datasheets/Res-HCJ0603ZT0R00.pdf'
PRP Digikey_Description 'RES 0 OHM JUMPER 1/4W 0603'
PRP Digikey_Part_Number 'HCJ0603ZT0R00CT-ND'
PRP helpURL 'https://upverter.com/upn/revision/19d0386aede22bbe/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Stackpole Electronics'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0603'
PRP Part_Number 'HCJ0603ZT0R00'
PRP PartNumber 'HCJ0603ZT0R00'
PRP Power_W '250mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'HCJ'
PRP SizeZ_mm '0.7mm'
PRP Supplier_1 'Digikey'
PRP Supplier_Part_Number_1 'HCJ0603ZT0R00CT-ND'
PRP Technology 'Metal'
PRP Value '0'
TOP 0 1.8235989 3.3203115 0 N 15 3 1
TOP 1 1.8984021 3.3203115 0 N 454 7 2
#
# CMP 27
CMP 52 2.7460005 2.4392525 180 N L12 MPZ2012S101ATD25 ;0=1,1=0.0000
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://product.tdk.com/info/en/catalog/datasheets/beads_automotive_power_mpz2012_en.pdf'
PRP Datasheet 'https://product.tdk.com/info/en/catalog/datasheets/beads_automotive_power_mpz2012_en.pdf'
PRP Datasheet_Path 'datasheets/FBead-MPZ2012S101ATD25.pdf'
PRP DCR_ohm '20m'
PRP Digikey_Description 'FERRITE BEAD 100 OHM 0805 1LN'
PRP Digikey_Part_Number '445-172903-1-ND'
PRP helpURL 'https://upverter.com/upn/revision/572b4800072287ce/'
PRP Imax_A '4A'
PRP Impedance_At_Frequency '100O @ 100MHz'
PRP Lead_Free 'Yes'
PRP Manufacturer 'TDK'
PRP Material 'Ferrite'
PRP Mouser_Description 'Ferrite Beads 0805 100ohms@100MHz 4.0A AEC-Q200'
PRP Mouser_Part_Number '810-MPZ2012S101ATD25'
PRP Operating_Temperature_Range '-55°C to +125°C'
PRP PackageReference '0805'
PRP Part_Number 'MPZ2012S101ATD25'
PRP PartNumber 'MPZ2012S101ATD25'
PRP RoHS 'TRUE'
PRP SizeZ_mm '1.05mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '445-172903-1-ND'
PRP Supplier_Part_Number_2 '810-MPZ2012S101ATD25'
PRP Test_Frequency '100MHz'
PRP Tolerance__ '25%'
TOP 0 2.7105674 2.4392525 0 N 309 9 1
TOP 1 2.7814336 2.4392525 0 N 56 6 2
#
# CMP 28
CMP 11 3.1854459 1.8742839 90 N C182 C0805C106J8RACAUTO ;0=1,1=0.0571
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0805'
PRP Cap_F '10µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://content.kemet.com/datasheets/KEM_C1023_X7R_AUTO_SMD.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'Kemet'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'C0805C106J8RACAUTO'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '399-15693-1-ND'
PRP Supplier_Part_Number_2 '80-C0805C106J8RAUTO'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '10uF'
PRP Value1 ''
PRP Value2 '10V'
PRP ValueDisplayed '10µF'
PRP VDC_V '10V'
TOP 0 3.1854459 1.9038115 180 N 16 6 1
TOP 1 3.1854459 1.8447564 180 N 424 317 2
#
# CMP 29
CMP 22 1.9748878 3.6342032 90 N Y7 CDC6CE05000CDLE ;0=1,1=0.0130
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'No'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/GPN.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/GPN'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/GPN/datasheet'
PRP CompType 'IC'
PRP Datasheet_Path 'datasheets/Crys-CDC6CE05000CDLE.pdf'
PRP Frequency_Stability '20ppm'
PRP Frequency_Fixed '50MHz'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP helpURL 'https://upverter.com/upn/revision/8af5cfc5dd9b045e/'
PRP Load_Capacitance '15pF'
PRP Manufacturer 'Texas Instruments'
PRP Max_Supply_Current '4mA'
PRP Max_Supply_Voltage '3.465V'
PRP Min_Supply_Voltage '2.375V'
PRP MountType ''
PRP Operating_Temperature_Range 'to +135°C'
PRP PackageDescription ''
PRP PackageReference 'VSON4'
PRP Part_Number 'CDC6CE05000CDLE'
PRP PartNumber 'CDC6CE05000CDLE'
PRP Rating ''
PRP RoHS 'UNKNOWN'
PRP Series 'CDC6'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm '1mm'
PRP Standoff_Height '0mm'
PRP TaMax_C '+105°C'
PRP TaMin_C '-40°C'
PRP TJmax_C '+135°C'
TOP 0 1.9335492 3.6656993 90 N 32 1 1
TOP 1 2.0162264 3.6656993 90 N 424 326 2
TOP 2 2.0162264 3.6027071 90 N 17 0 3
TOP 3 1.9335492 3.6027071 90 N 20 1 4
#
# CMP 30
CMP 22 0.9020005 3.1528115 90 N Y6 CDC6CE02500CDLE ;0=1,1=0.0000
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP Datasheet_Path 'datasheets/Crys-CDC6CE02500CDLE.pdf'
PRP Frequency_Stability '20ppm'
PRP Frequency_Fixed '25MHz'
PRP helpURL 'https://upverter.com/upn/revision/0402d7ca26a69d69/'
PRP Manufacturer 'Texas Instruments'
PRP Max_Supply_Current '5mA'
PRP Max_Supply_Voltage '3.63V'
PRP Min_Supply_Voltage '1.62V'
PRP Operating_Temperature_Range '-40°C to +125°C'
PRP PackageReference 'VSON4'
PRP Part_Number 'CDC6CE02500CDLE'
PRP PartNumber 'CDC6CE02500CDLE'
PRP RoHS 'UNKNOWN'
PRP Series 'CDC6C'
PRP SizeZ_mm '1mm'
PRP Standoff_Height '0mm'
TOP 0 0.8606619 3.1843076 90 N 96 2 1
TOP 1 0.9433391 3.1843076 90 N 424 146 2
TOP 2 0.9433391 3.1213154 90 N 97 0 3
TOP 3 0.8606619 3.1213154 90 N 19 0 4
#
# CMP 31
CMP 47 2.5482289 1.5510635 0 N R200 HCJ0603ZT0R00 ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.seielect.com/Catalog/SEI-HCJ.pdf'
PRP Datasheet 'https://www.seielect.com/Catalog/SEI-HCJ.pdf'
PRP Datasheet_Path 'datasheets/Res-HCJ0603ZT0R00.pdf'
PRP Digikey_Description 'RES 0 OHM JUMPER 1/4W 0603'
PRP Digikey_Part_Number 'HCJ0603ZT0R00CT-ND'
PRP helpURL 'https://upverter.com/upn/revision/19d0386aede22bbe/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Stackpole Electronics'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0603'
PRP Part_Number 'HCJ0603ZT0R00'
PRP PartNumber 'HCJ0603ZT0R00'
PRP Power_W '250mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'HCJ'
PRP SizeZ_mm '0.7mm'
PRP Supplier_1 'Digikey'
PRP Supplier_Part_Number_1 'HCJ0603ZT0R00CT-ND'
PRP Technology 'Metal'
PRP Value '0'
TOP 0 2.5856305 1.5510635 180 N 308 11 1
TOP 1 2.5108273 1.5510635 180 N 54 8 2
#
# CMP 32
CMP 6 2.4094813 1.9452525 180 N C200 GCM155R71C104KA55D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.murata.com/capacitor/product/GCM155R71C104KA55%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71C104KA55D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-4759-2-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '16V'
TOP 0 2.3894813 1.9452525 90 N 424 314 1
TOP 1 2.4294813 1.9452525 90 N 54 17 2
#
# CMP 33
CMP 2 2.3949538 1.8791129 0 N C199 GCM155R71C224KE02D ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM155R71C224KE02%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71C224KE02D'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-10671-1-ND'
PRP Supplier_Part_Number_2 '81-GCM155R71C224KE2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.22uF'
PRP Value1 ''
PRP Value2 '16V'
PRP ValueDisplayed '0.22µF'
PRP VDC_V '16V'
TOP 0 2.4185758 1.8791129 270 N 54 16 1
TOP 1 2.3713317 1.8791129 270 N 424 312 2
#
# CMP 34
CMP 9 2.552658 1.6920635 180 N C143 CGA4J1X7T0J226M ;0=1,1=0.0610
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0805'
PRP Cap_F '22µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://sps16.itg.ti.com/sites/KMS/crossdivteams/altium/docs/ComponentDatasheets/TDK datasheet_CGA4J1X7T0J226M (preliminary)_TI 03122019.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'CGA4J1X7T0J226M'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.55'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7T'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '22uF'
PRP Value1 ''
PRP Value2 '6.3V'
PRP ValueDisplayed '22µF'
PRP VDC_V '6.3V'
TOP 0 2.5182092 1.6920635 90 N 54 19 1
TOP 1 2.5871068 1.6920635 90 N 424 316 2
#
# CMP 35
CMP 7 1.6938745 3.0138115 0 N FB1 BLM18HE102SN1D ;0=1,1=0.0394
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/PDF/ENG/L0110S0101BLM18H.pdf'
PRP CompType 'Ferrite Bead'
PRP DCR_ohm '3.5d'
PRP Imax_A '6dA'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'BLM18HE102SN1D'
PRP Published '2014-04-30'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-5215-1-ND'
PRP Supplier_Part_Number_2 '87X8573'
PRP Supplier_Part_Number_3 '81-BLM18HE102SN1D'
PRP Value '1000 ohm'
PRP Value1 '0.35 ohm'
PRP Value2 '0.6A'
PRP ValueDisplayed '1000 ohm'
PRP Ztyp@1GHz_Ohm '1k'
PRP ZTyp@100MHz_Ohm '1k'
TOP 0 1.7253706 3.0138115 270 N 109 6 1
TOP 1 1.6623785 3.0138115 270 N 69 5 2
#
# CMP 36
CMP 37 2.0990005 1.9971265 90 N R116 CRCW04020000Z0EDHP ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.vishay.com/docs/20043/crcwhpe3.pdf'
PRP Datasheet 'https://www.vishay.com/docs/20043/crcwhpe3.pdf'
PRP Datasheet_Path 'datasheets/Res-CRCW04020000Z0EDHP.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/5W 0402'
PRP Digikey_Part_Number '541-0.0YBCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/5e0a18f71149352e/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Vishay Dale'
PRP Mouser_Description 'Resistor; Thick Film; 0 Ohms; 0.125 W; 0 Ohms Jumper; SMT; 0402; TCR 0 ppm/DegC'
PRP Mouser_Part_Number '71-CRCW04020000Z0EDH'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'CRCW04020000Z0EDHP'
PRP PartNumber 'CRCW04020000Z0EDHP'
PRP Power_W '200mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'CRCW-HP e3'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '541-0.0YBCT-ND'
PRP Supplier_Part_Number_2 '71-CRCW04020000Z0EDH'
PRP Technology 'Thick Film'
PRP Value '0'
PRP VDC_V '50V'
TOP 0 2.0990005 2.0177958 90 N 55 2 1
TOP 1 2.0990005 1.9764572 90 N 109 19 2
#
# CMP 37
CMP 53 2.356316 3.5381274 0 N C181 NFM18HC105C1C3D ;0=1,1=0.0461
PRP AC_Safety ''
PRP AEC_Category ''
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case ''
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://psearch.en.murata.com/capacitor/product/NFM18HC105C1C3%23.html'
PRP CompType ''
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'Murata'
PRP MountType ''
PRP PackageReference '0603'
PRP PartNumber 'NFM18HC105C1C3D'
PRP Polarized ''
PRP RoHS 'TRUE'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm '0.7mm'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C ''
PRP TaMin_C ''
PRP Technology ''
PRP TempCo ''
PRP Tolerance__ '20%'
PRP U/M ''
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value ''
PRP Value1 ''
PRP Value2 ''
PRP ValueDisplayed '1uF'
PRP VDC_V '16V'
TOP 0 2.3878121 3.5381274 180 N 175 13 1
TOP 1 2.356316 3.5223794 180 N 424 337 2
TOP 2 2.356316 3.5538754 180 N 424 338 2
TOP 3 2.3248199 3.5381274 180 N 175 12 3
#
# CMP 38
CMP 5 1.7800005 4.3728115 180 N R73 CRCW0402100KFKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP INSTALLATION 'DNP'
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW0402100KFKED'
PRP Power_W '63mW'
PRP Res_ohm '100k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-100KLCT-ND'
PRP Supplier_Part_Number_2 '52K6607'
PRP Supplier_Part_Number_3 '71-CRCW0402-100K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '100k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '100k'
PRP ValueDisplayed '100k'
PRP VDC_V '50V'
TOP 0 1.7603155 4.3728115 90 N 435 0 1
TOP 1 1.7996856 4.3728115 90 N 109 7 2
#
# CMP 39
CMP 33 1.6955753 3.3268115 0 N FB2 BLM18KG601SH1 ;0=1,1=0.0010
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.murata.com/products/productdata/8796737273886/QNFA9101.pdf?1590156016000'
PRP Datasheet 'https://www.murata.com/products/productdata/8796737273886/QNFA9101.pdf?1590156016000'
PRP Datasheet_Path 'datasheets/FBead-BLM18KG601SH1.pdf'
PRP DCR_ohm '0.15'
PRP Digikey_Description 'FERRITE BEAD 600 OHM 0603 1LN'
PRP Digikey_Part_Number '490-13259-1-ND'
PRP helpURL 'https://upverter.com/upn/revision/22cc867aa2f8f768/'
PRP Imax_A '1.3A'
PRP Impedance_At_Frequency '600O @ 100MHz'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Murata'
PRP Material 'Ferrite'
PRP Mouser_Part_Number '81-BLM18KG601SH1D'
PRP Operating_Temperature_Range '-55°C to +125°C'
PRP PackageReference '0603 (1608 Metric)'
PRP Part_Number 'BLM18KG601SH1'
PRP PartNumber 'BLM18KG601SH1'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.95mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '490-13259-1-ND'
PRP Supplier_Part_Number_2 '81-BLM18KG601SH1D'
PRP Test_Frequency '100MHz'
PRP Tolerance__ '25%'
TOP 0 1.7221501 3.3268115 180 N 15 4 1
TOP 1 1.6690005 3.3268115 180 N 18 1 2
#
# CMP 40
CMP 11 3.0753375 2.5728115 270 N C198 C0805C106J8RACAUTO ;0=1,1=0.0571
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0805'
PRP Cap_F '10µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://content.kemet.com/datasheets/KEM_C1023_X7R_AUTO_SMD.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'Kemet'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'C0805C106J8RACAUTO'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '399-15693-1-ND'
PRP Supplier_Part_Number_2 '80-C0805C106J8RAUTO'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '10uF'
PRP Value1 ''
PRP Value2 '10V'
PRP ValueDisplayed '10µF'
PRP VDC_V '10V'
TOP 0 3.0753375 2.5432839 0 N 56 1 1
TOP 1 3.0753375 2.602339 0 N 424 147 2
#
# CMP 41
CMP 11 2.9924005 2.5728115 270 N C194 C0805C106J8RACAUTO ;0=1,1=0.0571
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0805'
PRP Cap_F '10µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://content.kemet.com/datasheets/KEM_C1023_X7R_AUTO_SMD.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'Kemet'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'C0805C106J8RACAUTO'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '399-15693-1-ND'
PRP Supplier_Part_Number_2 '80-C0805C106J8RAUTO'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '10uF'
PRP Value1 ''
PRP Value2 '10V'
PRP ValueDisplayed '10µF'
PRP VDC_V '10V'
TOP 0 2.9924005 2.5432839 0 N 56 2 1
TOP 1 2.9924005 2.602339 0 N 424 148 2
#
# CMP 42
CMP 66 2.4094813 2.2583139 0 N U8 LP87725101RAGRQ1 ;0=1,1=0.0000
PRP AEC_Category 'Q200'
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/GPN.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/GPN'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/GPN/datasheet'
PRP CompType 'IC'
PRP Datasheet_Path 'datasheets/IC-LP87725101RAGRQ1.pdf'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP helpURL 'https://upverter.com/upn/revision/9d0aa6ba45dd87e2/'
PRP Manufacturer 'Texas Instruments'
PRP Max_Supply_Voltage '4/4/4/4/3.4V'
PRP Min_Supply_Voltage '3/3/3/1.2/1.6V'
PRP MountType ''
PRP Number_Of_Outputs '5'
PRP Operating_Temperature_Range '-40°C to +150°C'
PRP Output_Voltage '0.9-1.9/0.9-1.9/0.9-1.9/0.6-3.4V'
PRP PackageDescription ''
PRP PackageReference 'VQFN-HR24'
PRP Part_Number 'LP87725101RAGRQ1'
PRP PartNumber 'LP87725101RAGRQ1'
PRP Rating ''
PRP RoHS 'UNKNOWN'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm '1mm'
PRP Standoff_Height '0mm'
PRP TaMax_C '+125°C'
PRP TaMin_C '-40°C'
PRP TJmax_C '+150°C'
TOP 0 2.4697052 2.3185378 180 N 27 2 1
TOP 1 2.4823159 2.297684 180 N 101 2 2
TOP 2 2.4803474 2.2779989 180 N 151 1 3
TOP 3 2.4823159 2.2583139 180 N 68 17 4
TOP 4 2.4803474 2.2386289 180 N 147 0 5
TOP 5 2.4823159 2.2189438 180 N 99 2 6
TOP 6 2.4697052 2.19809 180 N 145 3 7
TOP 7 2.4488514 2.1886289 180 N 142 2 8
TOP 8 2.4291663 2.1958139 180 N 54 26 9
TOP 9 2.4094813 2.2022115 180 N 424 519 10
TOP 10 2.3897963 2.1958139 180 N 23 4 11
TOP 11 2.3701112 2.1886289 180 N 13 4 12
TOP 12 2.3492575 2.19809 180 N 12 5 13
TOP 13 2.3366467 2.2189438 180 N 54 25 14
TOP 14 2.3386152 2.2386289 180 N 158 1 15
TOP 15 2.3366467 2.2583139 180 N 68 18 16
TOP 16 2.3386152 2.2779989 180 N 31 2 17
TOP 17 2.3366467 2.297684 180 N 100 0 18
TOP 18 2.3492575 2.3185378 180 N 162 2 19
TOP 19 2.3701112 2.3279989 180 N 143 2 20
TOP 20 2.3897963 2.3208139 180 N 54 27 21
TOP 21 2.4094813 2.3144163 180 N 424 520 22
TOP 22 2.4291663 2.3208139 180 N 54 28 23
TOP 23 2.4488514 2.3279989 180 N 76 2 24
TOP 24 2.4094813 2.2583139 180 N 68 16 empty-1
#
# CMP 43
CMP 1 0.9144388 0.835871 180 N R323 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 0.9034152 0.835871 90 N 62 0 1
TOP 1 0.9254624 0.835871 90 N 48 1 2
#
# CMP 44
CMP 1 0.9144388 0.863871 180 N R322 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 0.9034152 0.863871 90 N 61 0 1
TOP 1 0.9254624 0.863871 90 N 47 1 2
#
# CMP 45
CMP 23 1.3222864 3.5389825 90 N D19 TPD1E05U06QDPYRQ1 ;0=1,1=0.0177
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer 'Texas Instruments'
PRP Alternate_PartNumber 'TPD1E05U06QDPYTQ1'
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/tpd1e05u06-q1.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/tpd1e05u06-q1'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/tpd1e05u06-q1/datasheet'
PRP CompType 'IC'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP Operating_Temperature_Range '-40 to 125 C'
PRP PackageDescription 'X1SON-2'
PRP PackageReference 'DPY0002A'
PRP PartNumber 'TPD1E05U06QDPYRQ1'
PRP Rating 'Automotive'
PRP RoHS ''
PRP SizeArea_mm2 '0.6'
PRP SizeAreaWB_mm2 '3.2'
PRP SizeX_mm '1.0'
PRP SizeY_mm '0.6'
PRP SizeZ_mm '0.45'
TOP 0 1.3222864 3.5517778 90 N 74 1 1
TOP 1 1.3222864 3.5261872 90 N 424 327 2
#
# CMP 46
CMP 23 1.3222864 3.6015424 270 N D18 TPD1E05U06QDPYRQ1 ;0=1,1=0.0177
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer 'Texas Instruments'
PRP Alternate_PartNumber 'TPD1E05U06QDPYTQ1'
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/tpd1e05u06-q1.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/tpd1e05u06-q1'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/tpd1e05u06-q1/datasheet'
PRP CompType 'IC'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP Operating_Temperature_Range '-40 to 125 C'
PRP PackageDescription 'X1SON-2'
PRP PackageReference 'DPY0002A'
PRP PartNumber 'TPD1E05U06QDPYRQ1'
PRP Rating 'Automotive'
PRP RoHS ''
PRP SizeArea_mm2 '0.6'
PRP SizeAreaWB_mm2 '3.2'
PRP SizeX_mm '1.0'
PRP SizeY_mm '0.6'
PRP SizeZ_mm '0.45'
TOP 0 1.3222864 3.5887471 270 N 75 0 1
TOP 1 1.3222864 3.6143377 270 N 424 149 2
#
# CMP 47
CMP 5 1.8802737 3.5826362 270 N C178 GCM155R71C104KA55D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.murata.com/capacitor/product/GCM155R71C104KA55%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71C104KA55D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-4759-2-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '16V'
TOP 0 1.8802737 3.5629512 0 N 424 150 1
TOP 1 1.8802737 3.6023213 0 N 20 0 2
#
# CMP 48
CMP 8 2.23 2.088 180 N C171 GCM188R70J225KE22D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '2.2µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM188R70J225KE22%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM188R70J225KE22D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5316-1-ND'
PRP Supplier_Part_Number_2 '81-GCM188R70J225KE2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '2.2uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '2.2uF'
PRP VDC_V '6.3V'
TOP 0 2.2024409 2.088 90 N 424 151 1
TOP 1 2.257559 2.088 90 N 12 2 2
#
# CMP 49
CMP 42 2.6226855 2.2248115 180 N R291 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 2.6025084 2.2248115 0 N 99 1 1
TOP 1 2.6428627 2.2248115 0 N 454 12 2
#
# CMP 50
CMP 42 2.6224129 2.3372141 180 N R67 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 2.6022358 2.3372141 0 N 101 1 1
TOP 1 2.6425901 2.3372141 0 N 457 27 2
#
# CMP 51
CMP 43 2.3556713 2.5504344 90 N C153 GCJ188C70J475KE02J ;0=1,1=0.0461
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP Cap_F '4.7µF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.murata.com/en-us/products/productdetail?partno=GCJ188C70J475KE02%23'
PRP Datasheet 'https://www.murata.com/en-us/products/productdetail?partno=GCJ188C70J475KE02%23'
PRP Datasheet_Path 'datasheets/Cap-GCJ188C70J475KE02J.pdf'
PRP helpURL 'https://upverter.com/upn/revision/50667d1a23a19155/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Murata'
PRP Operating_Temperature_Range '-55°C to +125°C'
PRP PackageReference '0603'
PRP Part_Number 'GCJ188C70J475KE02J'
PRP PartNumber 'GCJ188C70J475KE02J'
PRP RoHS 'TRUE'
PRP SizeZ_mm '1mm'
PRP TempCo '22%'
PRP Temperature_Characteristic 'X7S'
PRP Tolerance__ '10%'
PRP Value '4.7µF'
PRP ValueDisplayed '4.7uF'
PRP VDC_V '6.3V'
TOP 0 2.3556713 2.5809462 90 N 424 333 1
TOP 1 2.3556713 2.5199226 90 N 54 20 2
#
# CMP 52
CMP 42 2.8357441 3.2412467 270 N R23 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 2.8357441 3.2210696 270 N 106 1 1
TOP 1 2.8357441 3.2614239 270 N 129 3 2
#
# CMP 53
CMP 15 0.9010524 3.1528406 90 N Y5 ABM8AIG-25.000MHZ-12-2Z-T3 ;0=1,1=0.0315
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.abracon.com/AIGcrystals/ABM8AIG.pdf'
PRP CompType 'Crystal'
PRP Frequency_Stability '50 ppm'
PRP Frequency_Tolerance ''
PRP Frequency_Fixed '25MHz'
PRP Frequency_Max ''
PRP Frequency_Min ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Load_Capacitance '12 pF'
PRP Manufacturer 'Abracon Corporation'
PRP MountType 'SMT'
PRP PackageReference '3.2x2.5mm'
PRP PartNumber 'ABM8AIG-25.000MHZ-12-2Z-T3'
PRP REACh 'Y'
PRP RoHS 'Y'
PRP SizeArea_mm2 '8'
PRP SizeAreaWB_mm2 '14.7'
PRP SizeX_mm '2.5'
PRP SizeY_mm '3.2'
PRP SizeZ_mm '0.8'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-40°C'
TOP 0 0.8557768 3.1902422 0 N 96 6 1
TOP 1 0.946328 3.1902422 0 N 424 322 2
TOP 2 0.946328 3.115439 0 N 97 3 3
TOP 3 0.8557768 3.115439 0 N 19 1 4
#
# CMP 54
CMP 5 1.3779776 3.5220162 0 N R274 CRCW040226R7FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040226R7FKED'
PRP Power_W '63mW'
PRP Res_ohm '26.7'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '541-26.7LCT-ND'
PRP Supplier_Part_Number_2 '71-CRCW040226R7FKED'
PRP Supplier_Part_Number_3 '1151086'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '26.7'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '26R7'
PRP ValueDisplayed '26.7'
PRP VDC_V '50V'
TOP 0 1.3976626 3.5220162 270 N 94 0 1
TOP 1 1.3582925 3.5220162 270 N 74 0 2
#
# CMP 55
CMP 37 1.416179 3.5864018 0 N R265 CRCW04020000Z0EDHP ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.vishay.com/docs/20043/crcwhpe3.pdf'
PRP Datasheet 'https://www.vishay.com/docs/20043/crcwhpe3.pdf'
PRP Datasheet_Path 'datasheets/Res-CRCW04020000Z0EDHP.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/5W 0402'
PRP Digikey_Part_Number '541-0.0YBCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/5e0a18f71149352e/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Vishay Dale'
PRP Mouser_Description 'Resistor; Thick Film; 0 Ohms; 0.125 W; 0 Ohms Jumper; SMT; 0402; TCR 0 ppm/DegC'
PRP Mouser_Part_Number '71-CRCW04020000Z0EDH'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'CRCW04020000Z0EDHP'
PRP PartNumber 'CRCW04020000Z0EDHP'
PRP Power_W '200mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'CRCW-HP e3'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '541-0.0YBCT-ND'
PRP Supplier_Part_Number_2 '71-CRCW04020000Z0EDH'
PRP Technology 'Thick Film'
PRP Value '0'
PRP VDC_V '50V'
TOP 0 1.4368483 3.5864018 180 N 103 2 1
TOP 1 1.3955097 3.5864018 180 N 75 3 2
#
# CMP 56
CMP 5 1.3779775 3.6185094 180 N R260 CRCW040226R7FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040226R7FKED'
PRP Power_W '63mW'
PRP Res_ohm '26.7'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '541-26.7LCT-ND'
PRP Supplier_Part_Number_2 '71-CRCW040226R7FKED'
PRP Supplier_Part_Number_3 '1151086'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '26.7'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '26R7'
PRP ValueDisplayed '26.7'
PRP VDC_V '50V'
TOP 0 1.3582925 3.6185094 90 N 75 1 1
TOP 1 1.3976626 3.6185094 90 N 95 0 2
#
# CMP 57
CMP 5 1.4070215 3.3609678 270 N R253 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 1.4070215 3.3412828 0 N 21 0 1
TOP 1 1.4070215 3.3806529 0 N 69 6 2
#
# CMP 58
CMP 8 1.0086641 3.1491315 90 N R248 CRCW06031M00FKEA ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'CRCW06031M00FKEA'
PRP Power_W '100mW'
PRP Res_ohm '1M'
PRP RoHS 'E'
PRP SizeArea_mm2 '1.28'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-1.00MHCT-ND'
PRP Supplier_Part_Number_2 '52K8053'
PRP Supplier_Part_Number_3 '71-CRCW0603-1.0M-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '1.00Meg'
PRP Value1 '1%'
PRP Value2 '0.1W'
PRP Value_Code '1M00'
PRP ValueDisplayed '1.00M'
PRP VDC_V '75V'
TOP 0 1.0086641 3.1766906 180 N 96 3 1
TOP 1 1.0086641 3.1215725 180 N 97 1 2
#
# CMP 59
CMP 42 1.1893618 3.128268 180 N R246 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 1.1691847 3.128268 0 N 97 5 1
TOP 1 1.209539 3.128268 0 N 104 1 2
#
# CMP 60
CMP 5 1.1489918 3.1706381 0 N R242 ERJ-2GEJ101X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C84.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GEJ101X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '100'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 'P100JCT-ND'
PRP Supplier_Part_Number_2 '65T8246'
PRP Supplier_Part_Number_3 '2059210'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '100'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '100R'
PRP ValueDisplayed '100'
PRP VDC_V ''
TOP 0 1.1686768 3.1706381 270 N 105 0 1
TOP 1 1.1293067 3.1706381 270 N 96 4 2
#
# CMP 61
CMP 42 0.9860003 3.2668115 90 N R241 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 0.9860003 3.2869886 90 N 24 1 1
TOP 1 0.9860003 3.2466343 90 N 96 8 2
#
# CMP 62
CMP 5 3.1783149 4.0769685 180 N R230 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 3.1586299 4.0769685 90 N 395 0 1
TOP 1 3.198 4.0769685 90 N 84 0 2
#
# CMP 63
CMP 5 3.1783149 4.1929055 180 N R178 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 3.1586299 4.1929055 90 N 392 0 1
TOP 1 3.198 4.1929055 90 N 86 0 2
#
# CMP 64
CMP 5 3.1783149 4.019 180 N R74 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 3.1586299 4.019 90 N 396 0 1
TOP 1 3.198 4.019 90 N 89 0 2
#
# CMP 65
CMP 23 0.8737656 3.5379446 90 N D17 TPD1E05U06QDPYRQ1 ;0=1,1=0.0177
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer 'Texas Instruments'
PRP Alternate_PartNumber 'TPD1E05U06QDPYTQ1'
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/tpd1e05u06-q1.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/tpd1e05u06-q1'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/tpd1e05u06-q1/datasheet'
PRP CompType 'IC'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP Operating_Temperature_Range '-40 to 125 C'
PRP PackageDescription 'X1SON-2'
PRP PackageReference 'DPY0002A'
PRP PartNumber 'TPD1E05U06QDPYRQ1'
PRP Rating 'Automotive'
PRP RoHS ''
PRP SizeArea_mm2 '0.6'
PRP SizeAreaWB_mm2 '3.2'
PRP SizeX_mm '1.0'
PRP SizeY_mm '0.6'
PRP SizeZ_mm '0.45'
TOP 0 0.8737656 3.5507399 90 N 70 0 1
TOP 1 0.8737656 3.5251493 90 N 424 152 2
#
# CMP 66
CMP 23 0.8737656 3.6025796 270 N D15 TPD1E05U06QDPYRQ1 ;0=1,1=0.0177
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer 'Texas Instruments'
PRP Alternate_PartNumber 'TPD1E05U06QDPYTQ1'
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/tpd1e05u06-q1.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/tpd1e05u06-q1'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/tpd1e05u06-q1/datasheet'
PRP CompType 'IC'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP Operating_Temperature_Range '-40 to 125 C'
PRP PackageDescription 'X1SON-2'
PRP PackageReference 'DPY0002A'
PRP PartNumber 'TPD1E05U06QDPYRQ1'
PRP Rating 'Automotive'
PRP RoHS ''
PRP SizeArea_mm2 '0.6'
PRP SizeAreaWB_mm2 '3.2'
PRP SizeX_mm '1.0'
PRP SizeY_mm '0.6'
PRP SizeZ_mm '0.45'
TOP 0 0.8737656 3.5897843 270 N 71 0 1
TOP 1 0.8737656 3.6153749 270 N 424 153 2
#
# CMP 67
CMP 49 1.4543805 3.6185094 180 N C156 KGM05ACG1H220FH ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP Cap_F '22pF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://spicat.kyocera-avx.com/product/mlcc/chartview/KGM05ACG1H220FH'
PRP Datasheet 'https://spicat.kyocera-avx.com/product/mlcc/chartview/KGM05ACG1H220FH'
PRP Datasheet_Path 'datasheets/Cap-KGM05ACG1H220FH.pdf'
PRP Digikey_Description 'CAP CER 22PF 50V C0G/NP0 0402'
PRP Digikey_Part_Number '478-KGM05ACG1H220FHCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/b1505dfd3a8c3c16/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'KYOCERA AVX'
PRP Mouser_Part_Number '581-KGM05ACG1H220FH'
PRP Operating_Temperature_Range '-55°C to +125°C'
PRP PackageReference '0402'
PRP Part_Number 'KGM05ACG1H220FH'
PRP PartNumber 'KGM05ACG1H220FH'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.56mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '478-KGM05ACG1H220FHCT-ND'
PRP Supplier_Part_Number_2 '581-KGM05ACG1H220FH'
PRP TempCo '30ppm/°C'
PRP Temperature_Characteristic 'C0G'
PRP Tolerance__ '1%'
PRP Value '22pF'
PRP ValueDisplayed '22pF'
PRP VDC_V '50V'
TOP 0 1.432727 3.6185094 0 N 95 1 1
TOP 1 1.476034 3.6185094 0 N 103 1 2
#
# CMP 68
CMP 7 1.0720005 3.0848115 90 N C95 CGA3E2C0G1H220J080AA ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '22pF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://product.tdk.com/en/catalog/datasheets/mlcc_automotive_general_en.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'CGA3E2C0G1H220J080AA'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '445-5632-1-ND'
PRP Supplier_Part_Number_2 '12T1569'
PRP Supplier_Part_Number_3 '810-CGA3E2C0G1H220J'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'C0G/NP0'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '22pF'
PRP Value1 'Unknown'
PRP Value2 '50V'
PRP ValueDisplayed '22pF'
PRP VDC_V '50V'
TOP 0 1.0720005 3.1163076 180 N 97 2 1
TOP 1 1.0720005 3.0533155 180 N 424 154 2
#
# CMP 69
CMP 11 2.2860011 2.5750011 270 N C15 GCM21BR71A106KE22L ;0=1,1=0.0571
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0805'
PRP Cap_F '10µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.murata.com/products/catalog/pdf/c03e.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'GCM21BR71A106KE22L'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10674-1-ND'
PRP Supplier_Part_Number_2 '06AC6014'
PRP Supplier_Part_Number_3 '81-GCM21BR71A106KE2L'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '10uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '10uF'
PRP VDC_V '10V'
TOP 0 2.2860011 2.5454735 0 N 54 9 1
TOP 1 2.2860011 2.6045286 0 N 424 155 2
#
# CMP 70
CMP 52 2.5561029 1.6170635 0 N L1 MPZ2012S101ATD25 ;0=1,1=0.0000
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://product.tdk.com/info/en/catalog/datasheets/beads_automotive_power_mpz2012_en.pdf'
PRP Datasheet 'https://product.tdk.com/info/en/catalog/datasheets/beads_automotive_power_mpz2012_en.pdf'
PRP Datasheet_Path 'datasheets/FBead-MPZ2012S101ATD25.pdf'
PRP DCR_ohm '20m'
PRP Digikey_Description 'FERRITE BEAD 100 OHM 0805 1LN'
PRP Digikey_Part_Number '445-172903-1-ND'
PRP helpURL 'https://upverter.com/upn/revision/572b4800072287ce/'
PRP Imax_A '4A'
PRP Impedance_At_Frequency '100O @ 100MHz'
PRP Lead_Free 'Yes'
PRP Manufacturer 'TDK'
PRP Material 'Ferrite'
PRP Mouser_Description 'Ferrite Beads 0805 100ohms@100MHz 4.0A AEC-Q200'
PRP Mouser_Part_Number '810-MPZ2012S101ATD25'
PRP Operating_Temperature_Range '-55°C to +125°C'
PRP PackageReference '0805'
PRP Part_Number 'MPZ2012S101ATD25'
PRP PartNumber 'MPZ2012S101ATD25'
PRP RoHS 'TRUE'
PRP SizeZ_mm '1.05mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '445-172903-1-ND'
PRP Supplier_Part_Number_2 '810-MPZ2012S101ATD25'
PRP Test_Frequency '100MHz'
PRP Tolerance__ '25%'
TOP 0 2.591536 1.6170635 180 N 308 37 1
TOP 1 2.5206698 1.6170635 180 N 54 21 2
#
# CMP 71
CMP 83 0.2070701 3.5702624 270 N J4 9-2304372-9 ;0=2,1=0.5315
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP Color 'Blue'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F2304372%7FA2%7Fpdf%7FEnglish%7FENG_CD_2304372_A2.pdf%7F9-2304372-9'
PRP CompType 'Connector'
PRP ContactFinish ''
PRP Current_A ''
PRP Gender 'Male'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'TE Connectivity'
PRP MountType 'TH'
PRP Note ''
PRP Orientation 'R/A'
PRP PackageReference '1 Port Header Assembly'
PRP PartNumber '9-2304372-9'
PRP PinCount '8'
PRP Pitch_mm ''
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded 'Y'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Voltage_V ''
TOP 0 0.7582512 3.5348293 270 N 70 2 1
TOP 1 0.7582512 3.6056955 270 N 71 2 2
TOP 2 0.2070701 3.5702624 270 N 0 153 ALIGN1
TOP 3 0.2070701 3.8301049 270 N 0 152 ALIGN2
TOP 4 0.7582512 3.4167191 270 N 424 537 S1
TOP 5 0.4826607 3.4167191 270 N 424 539 S2
TOP 6 0.2070701 3.4167191 270 N 424 541 S3
TOP 7 0.7582512 3.7238057 270 N 424 536 S4
TOP 8 0.4826607 3.7238057 270 N 424 538 S5
TOP 9 0.2070701 3.7238057 270 N 424 540 S6
#
# CMP 72
CMP 1 1.559701 1.653965 180 N R318 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 1.5486774 1.653965 90 N 406 0 1
TOP 1 1.5707246 1.653965 90 N 315 0 2
#
# CMP 73
CMP 42 2.5700011 4.3586862 90 N R31 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 2.5700011 4.3788633 90 N 405 3 1
TOP 1 2.5700011 4.338509 90 N 113 1 2
#
# CMP 74
CMP 5 2.1490011 4.0928437 90 N C5 GCM155R71C224KE02D ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM155R71C224KE02%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71C224KE02D'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-10671-1-ND'
PRP Supplier_Part_Number_2 '81-GCM155R71C224KE2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.22uF'
PRP Value1 ''
PRP Value2 '16V'
PRP ValueDisplayed '0.22µF'
PRP VDC_V '16V'
TOP 0 2.1490011 4.1125287 0 N 424 156 1
TOP 1 2.1490011 4.0731586 0 N 457 5 2
#
# CMP 75
CMP 5 2.7766677 3.3983262 270 N R236 CRCW040210R0JNED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210R0JNED'
PRP Power_W '63mW'
PRP Res_ohm '10'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10JCT-ND'
PRP Supplier_Part_Number_2 '59M6698'
PRP Supplier_Part_Number_3 '71-CRCW0402J-10-E3'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP Value '10'
PRP Value1 '5%'
PRP Value2 '0.063W'
PRP Value_Code '10R0'
PRP ValueDisplayed '10'
PRP VDC_V '50V'
TOP 0 2.7766677 3.3786412 0 N 115 1 1
TOP 1 2.7766677 3.4180113 0 N 126 1 2
#
# CMP 76
CMP 5 2.6360011 3.2422309 270 N R235 CRCW040210R0JNED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210R0JNED'
PRP Power_W '63mW'
PRP Res_ohm '10'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10JCT-ND'
PRP Supplier_Part_Number_2 '59M6698'
PRP Supplier_Part_Number_3 '71-CRCW0402J-10-E3'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP Value '10'
PRP Value1 '5%'
PRP Value2 '0.063W'
PRP Value_Code '10R0'
PRP ValueDisplayed '10'
PRP VDC_V '50V'
TOP 0 2.6360011 3.2225459 0 N 120 1 1
TOP 1 2.6360011 3.261916 0 N 131 1 2
#
# CMP 77
CMP 42 2.7110011 3.2417389 90 N R233 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 2.7110011 3.261916 90 N 131 3 1
TOP 1 2.7110011 3.2215617 90 N 33 0 2
#
# CMP 78
CMP 5 2.9120011 3.3983262 270 N R232 CRCW040210R0JNED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210R0JNED'
PRP Power_W '63mW'
PRP Res_ohm '10'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10JCT-ND'
PRP Supplier_Part_Number_2 '59M6698'
PRP Supplier_Part_Number_3 '71-CRCW0402J-10-E3'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP Value '10'
PRP Value1 '5%'
PRP Value2 '0.063W'
PRP Value_Code '10R0'
PRP ValueDisplayed '10'
PRP VDC_V '50V'
TOP 0 2.9120011 3.3786412 0 N 116 1 1
TOP 1 2.9120011 3.4180113 0 N 169 1 2
#
# CMP 79
CMP 5 2.7493946 3.2417388 270 N R231 CRCW040210R0JNED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210R0JNED'
PRP Power_W '63mW'
PRP Res_ohm '10'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10JCT-ND'
PRP Supplier_Part_Number_2 '59M6698'
PRP Supplier_Part_Number_3 '71-CRCW0402J-10-E3'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP Value '10'
PRP Value1 '5%'
PRP Value2 '0.063W'
PRP Value_Code '10R0'
PRP ValueDisplayed '10'
PRP VDC_V '50V'
TOP 0 2.7493946 3.2220538 0 N 121 1 1
TOP 1 2.7493946 3.2614239 0 N 129 1 2
#
# CMP 80
CMP 42 2.7940958 3.2412468 90 N R229 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 2.7940958 3.2614239 90 N 129 2 1
TOP 1 2.7940958 3.2210696 90 N 439 0 2
#
# CMP 81
CMP 5 2.48 3.224 270 N R228 CRCW040210R0JNED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210R0JNED'
PRP Power_W '63mW'
PRP Res_ohm '10'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10JCT-ND'
PRP Supplier_Part_Number_2 '59M6698'
PRP Supplier_Part_Number_3 '71-CRCW0402J-10-E3'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP Value '10'
PRP Value1 '5%'
PRP Value2 '0.063W'
PRP Value_Code '10R0'
PRP ValueDisplayed '10'
PRP VDC_V '50V'
TOP 0 2.48 3.204315 0 N 117 1 1
TOP 1 2.48 3.2436851 0 N 36 1 2
#
# CMP 82
CMP 5 2.1250011 3.2768081 270 N R227 CRCW040210R0JNED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210R0JNED'
PRP Power_W '63mW'
PRP Res_ohm '10'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10JCT-ND'
PRP Supplier_Part_Number_2 '59M6698'
PRP Supplier_Part_Number_3 '71-CRCW0402J-10-E3'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP Value '10'
PRP Value1 '5%'
PRP Value2 '0.063W'
PRP Value_Code '10R0'
PRP ValueDisplayed '10'
PRP VDC_V '50V'
TOP 0 2.1250011 3.2571231 0 N 122 1 1
TOP 1 2.1250011 3.2964932 0 N 128 1 2
#
# CMP 83
CMP 5 3.1783149 4.134937 180 N R225 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 3.1586299 4.134937 90 N 391 0 1
TOP 1 3.198 4.134937 90 N 85 0 2
#
# CMP 84
CMP 42 2.08657 3.2763161 90 N R224 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 2.08657 3.2964932 90 N 128 2 1
TOP 1 2.08657 3.2561389 90 N 443 0 2
#
# CMP 85
CMP 5 2.2618614 3.2282468 270 N R221 CRCW040210R0JNED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210R0JNED'
PRP Power_W '63mW'
PRP Res_ohm '10'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10JCT-ND'
PRP Supplier_Part_Number_2 '59M6698'
PRP Supplier_Part_Number_3 '71-CRCW0402J-10-E3'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP Value '10'
PRP Value1 '5%'
PRP Value2 '0.063W'
PRP Value_Code '10R0'
PRP ValueDisplayed '10'
PRP VDC_V '50V'
TOP 0 2.2618614 3.2085618 0 N 118 1 1
TOP 1 2.2618614 3.2479319 0 N 37 1 2
#
# CMP 86
CMP 42 2.8773922 3.2412468 90 N R220 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 2.8773922 3.2614239 90 N 125 3 1
TOP 1 2.8773922 3.2210696 90 N 123 1 2
#
# CMP 87
CMP 42 2.3042364 3.2277548 90 N R219 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 2.3042364 3.2479319 90 N 37 4 1
TOP 1 2.3042364 3.2075776 90 N 163 0 2
#
# CMP 88
CMP 42 2.9606886 3.2412468 90 N R218 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 2.9606886 3.2614239 90 N 125 2 1
TOP 1 2.9606886 3.2210696 90 N 286 0 2
#
# CMP 89
CMP 5 2.6139384 3.3983262 270 N R217 CRCW040210R0JNED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210R0JNED'
PRP Power_W '63mW'
PRP Res_ohm '10'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10JCT-ND'
PRP Supplier_Part_Number_2 '59M6698'
PRP Supplier_Part_Number_3 '71-CRCW0402J-10-E3'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP Value '10'
PRP Value1 '5%'
PRP Value2 '0.063W'
PRP Value_Code '10R0'
PRP ValueDisplayed '10'
PRP VDC_V '50V'
TOP 0 2.6139384 3.3786412 0 N 119 1 1
TOP 1 2.6139384 3.4180113 0 N 130 1 2
#
# CMP 90
CMP 42 2.5548996 3.2402468 90 N R216 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 2.5548996 3.2604239 90 N 127 2 1
TOP 1 2.5548996 3.2200696 90 N 124 0 2
#
# CMP 91
CMP 42 2.5936008 3.2402468 90 N R165 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 2.5936008 3.2604239 90 N 127 1 1
TOP 1 2.5936008 3.2200696 90 N 168 1 2
#
# CMP 92
CMP 8 2.5445601 4.7690011 0 N C1 GCM188R71C105KA64D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM188R71C105KA64%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM188R71C105KA64D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5241-6-ND'
PRP Supplier_Part_Number_2 '81-GCM188R71C105K64D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '1uF'
PRP VDC_V '16V'
TOP 0 2.5721192 4.7690011 270 N 424 157 1
TOP 1 2.5170011 4.7690011 270 N 382 1 2
#
# CMP 93
CMP 5 2.413316 4.7410011 180 N C2 CGA2B3X7R1H104K050BB ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=CGA2B3X7R1H104K050BB'
PRP CompType 'Capacitor'
PRP ESR_ohm '0.039064'
PRP IRMS_A '8.14669dA'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CGA2B3X7R1H104K050BB'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '445-6899-1-ND'
PRP Supplier_Part_Number_2 '04X3148'
PRP Supplier_Part_Number_3 '810-CGA2B3X7R1H104K'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 '0.039064 ohm'
PRP Value2 '50V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '50V'
TOP 0 2.393631 4.7410011 90 N 424 158 1
TOP 1 2.4330011 4.7410011 90 N 382 2 2
#
# CMP 94
CMP 8 2.2305747 2.2734714 180 N C3 GCM188R70J225KE22D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '2.2µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM188R70J225KE22%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM188R70J225KE22D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5316-1-ND'
PRP Supplier_Part_Number_2 '81-GCM188R70J225KE2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '2.2uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '2.2uF'
PRP VDC_V '6.3V'
TOP 0 2.2030156 2.2734714 90 N 68 14 1
TOP 1 2.2581337 2.2734714 90 N 31 0 2
#
# CMP 95
CMP 11 1.8401265 2.5693391 270 N C4 C0805C106J8RACAUTO ;0=1,1=0.0571
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0805'
PRP Cap_F '10µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://content.kemet.com/datasheets/KEM_C1023_X7R_AUTO_SMD.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'Kemet'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'C0805C106J8RACAUTO'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '399-15693-1-ND'
PRP Supplier_Part_Number_2 '80-C0805C106J8RAUTO'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '10uF'
PRP Value1 ''
PRP Value2 '10V'
PRP ValueDisplayed '10µF'
PRP VDC_V '10V'
TOP 0 1.8401265 2.5398115 0 N 57 1 1
TOP 1 1.8401265 2.5988666 0 N 424 159 2
#
# CMP 96
CMP 43 2.3851113 1.8161129 180 N C6 GCJ188C70J475KE02J ;0=1,1=0.0000
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP Cap_F '4.7µF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.murata.com/en-us/products/productdetail?partno=GCJ188C70J475KE02%23'
PRP Datasheet 'https://www.murata.com/en-us/products/productdetail?partno=GCJ188C70J475KE02%23'
PRP Datasheet_Path 'datasheets/Cap-GCJ188C70J475KE02J.pdf'
PRP helpURL 'https://upverter.com/upn/revision/50667d1a23a19155/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Murata'
PRP Operating_Temperature_Range '-55°C to +125°C'
PRP PackageReference '0603'
PRP Part_Number 'GCJ188C70J475KE02J'
PRP PartNumber 'GCJ188C70J475KE02J'
PRP RoHS 'TRUE'
PRP SizeZ_mm '1mm'
PRP TempCo '22%'
PRP Temperature_Characteristic 'X7S'
PRP Tolerance__ '10%'
PRP Value '4.7µF'
PRP ValueDisplayed '4.7uF'
PRP VDC_V '6.3V'
TOP 0 2.3545995 1.8161129 0 N 424 160 1
TOP 1 2.4156231 1.8161129 0 N 54 10 2
#
# CMP 97
CMP 11 2.5400011 2.5750011 270 N C7 GCM21BR71A106KE22L ;0=1,1=0.0571
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0805'
PRP Cap_F '10µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.murata.com/products/catalog/pdf/c03e.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'GCM21BR71A106KE22L'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10674-1-ND'
PRP Supplier_Part_Number_2 '06AC6014'
PRP Supplier_Part_Number_3 '81-GCM21BR71A106KE2L'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '10uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '10uF'
PRP VDC_V '10V'
TOP 0 2.5400011 2.5454735 0 N 54 11 1
TOP 1 2.5400011 2.6045286 0 N 424 161 2
#
# CMP 98
CMP 8 1.6945595 3.2618115 0 N C8 GCM188R70J225KE22D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '2.2µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM188R70J225KE22%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM188R70J225KE22D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5316-1-ND'
PRP Supplier_Part_Number_2 '81-GCM188R70J225KE2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '2.2uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '2.2uF'
PRP VDC_V '6.3V'
TOP 0 1.7221186 3.2618115 270 N 424 162 1
TOP 1 1.6670005 3.2618115 270 N 18 2 2
#
# CMP 99
CMP 53 2.4094813 2.0406091 0 N C9 NFM18HC105C1C3D ;0=1,1=0.0010
PRP AC_Safety ''
PRP AEC_Category ''
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case ''
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://psearch.en.murata.com/capacitor/product/NFM18HC105C1C3%23.html'
PRP CompType ''
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'Murata'
PRP MountType ''
PRP PackageReference '0603'
PRP PartNumber 'NFM18HC105C1C3D'
PRP Polarized ''
PRP RoHS 'TRUE'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm '0.7mm'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C ''
PRP TaMin_C ''
PRP Technology ''
PRP TempCo ''
PRP Tolerance__ '20%'
PRP U/M ''
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value ''
PRP Value1 ''
PRP Value2 ''
PRP ValueDisplayed '1uF'
PRP VDC_V '16V'
TOP 0 2.4409774 2.0406091 180 N 54 12 1
TOP 1 2.4094813 2.0248611 180 N 424 163 2
TOP 2 2.4094813 2.0563571 180 N 424 164 2
TOP 3 2.3779852 2.0406091 180 N 54 13 3
#
# CMP 100
CMP 5 1.0233154 3.3808115 180 N C12 GCM155R71C104KA55D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.murata.com/capacitor/product/GCM155R71C104KA55%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71C104KA55D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-4759-2-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '16V'
TOP 0 1.0036304 3.3808115 90 N 424 165 1
TOP 1 1.0430005 3.3808115 90 N 18 3 2
#
# CMP 101
CMP 5 1.6300005 3.3348116 90 N C13 GCM155R71C104KA55D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.murata.com/capacitor/product/GCM155R71C104KA55%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71C104KA55D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-4759-2-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '16V'
TOP 0 1.6300005 3.3544966 180 N 424 166 1
TOP 1 1.6300005 3.3151265 180 N 18 4 2
#
# CMP 102
CMP 5 3.0952096 2.0482296 270 N C14 GCM155R71A104KA55D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GCM155R71A104KA55-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71A104KA55D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GCM155R71A104K5D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '10V'
TOP 0 3.0952096 2.0285446 0 N 381 0 1
TOP 1 3.0952096 2.0679147 0 N 380 0 2
#
# CMP 103
CMP 5 1.0233155 3.3318115 0 N C16 CGA2B3X7R1H103K050BB ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '10nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=CGA2B3X7R1H103K050BB'
PRP CompType 'Capacitor'
PRP ESR_ohm '0.333065'
PRP IRMS_A '323.373mA'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CGA2B3X7R1H103K050BB'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '445-6893-1-ND'
PRP Supplier_Part_Number_2 '52W9617'
PRP Supplier_Part_Number_3 '2210821'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.01uF'
PRP Value1 '0.333065 ohm'
PRP Value2 '50V'
PRP ValueDisplayed '0.01uF'
PRP VDC_V '50V'
TOP 0 1.0430005 3.3318115 270 N 18 5 1
TOP 1 1.0036304 3.3318115 270 N 424 167 2
#
# CMP 104
CMP 5 2.9190351 2.3054414 90 N C17 GCM155R71A104KA55D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GCM155R71A104KA55-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71A104KA55D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GCM155R71A104K5D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '10V'
TOP 0 2.9190351 2.3251264 180 N 379 0 1
TOP 1 2.9190351 2.2857563 180 N 378 0 2
#
# CMP 105
CMP 5 2.1136226 1.6289859 0 N C19 GCM155R71A104KA55D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GCM155R71A104KA55-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71A104KA55D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GCM155R71A104K5D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '10V'
TOP 0 2.1333076 1.6289859 270 N 201 0 1
TOP 1 2.0939375 1.6289859 270 N 200 0 2
#
# CMP 106
CMP 5 1.5920005 3.3348115 270 N C20 CGA2B3X7R1H103K050BB ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '10nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=CGA2B3X7R1H103K050BB'
PRP CompType 'Capacitor'
PRP ESR_ohm '0.333065'
PRP IRMS_A '323.373mA'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CGA2B3X7R1H103K050BB'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '445-6893-1-ND'
PRP Supplier_Part_Number_2 '52W9617'
PRP Supplier_Part_Number_3 '2210821'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.01uF'
PRP Value1 '0.333065 ohm'
PRP Value2 '50V'
PRP ValueDisplayed '0.01uF'
PRP VDC_V '50V'
TOP 0 1.5920005 3.3151265 0 N 18 6 1
TOP 1 1.5920005 3.3544966 0 N 424 168 2
#
# CMP 107
CMP 34 0.2430184 2.1199049 180 N C27 C0603C104K4RACAUTO ;0=1,1=0.0000
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://api.kemet.com/component-edge/download/datasheet/C0603C100J5GACAUTO.pdf'
PRP Datasheet 'https://api.kemet.com/component-edge/download/datasheet/C0603C100J5GACAUTO.pdf'
PRP Datasheet_Path 'datasheets/Cap-C0603C104K4RACAUTO.pdf'
PRP Digikey_Description 'CAP CER 0.1UF 16V X7R 0603'
PRP Digikey_Part_Number '399-6855-2-ND'
PRP helpURL 'https://upverter.com/upn/revision/a6ffabf7c6033b11/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'KEMET'
PRP Mouser_Description 'Multilayer Ceramic Capacitors MLCC - SMD/SMT 0.1uF 16volts 10% X7R AUTO'
PRP Mouser_Part_Number '80-C0603C104K4RAUTO'
PRP Operating_Temperature_Range '-55°C to +125°C'
PRP PackageReference '0603'
PRP Part_Number 'C0603C104K4RACAUTO'
PRP PartNumber 'C0603C104K4RACAUTO'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.87mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '399-6855-2-ND'
PRP Supplier_Part_Number_2 '80-C0603C104K4RAUTO'
PRP TempCo '30ppm/°C'
PRP Temperature_Characteristic 'X7R'
PRP Tolerance__ '0.1%'
PRP ValueDisplayed '0.10 µF'
PRP VDC_V '16V'
TOP 0 0.2193964 2.1199049 0 N 424 332 1
TOP 1 0.2666404 2.1199049 0 N 446 8 2
#
# CMP 108
CMP 34 0.3437145 3.037465 180 N C28 C0603C104K4RACAUTO ;0=1,1=0.0000
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://api.kemet.com/component-edge/download/datasheet/C0603C100J5GACAUTO.pdf'
PRP Datasheet 'https://api.kemet.com/component-edge/download/datasheet/C0603C100J5GACAUTO.pdf'
PRP Datasheet_Path 'datasheets/Cap-C0603C104K4RACAUTO.pdf'
PRP Digikey_Description 'CAP CER 0.1UF 16V X7R 0603'
PRP Digikey_Part_Number '399-6855-2-ND'
PRP helpURL 'https://upverter.com/upn/revision/a6ffabf7c6033b11/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'KEMET'
PRP Mouser_Description 'Multilayer Ceramic Capacitors MLCC - SMD/SMT 0.1uF 16volts 10% X7R AUTO'
PRP Mouser_Part_Number '80-C0603C104K4RAUTO'
PRP Operating_Temperature_Range '-55°C to +125°C'
PRP PackageReference '0603'
PRP Part_Number 'C0603C104K4RACAUTO'
PRP PartNumber 'C0603C104K4RACAUTO'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.87mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '399-6855-2-ND'
PRP Supplier_Part_Number_2 '80-C0603C104K4RAUTO'
PRP TempCo '30ppm/°C'
PRP Temperature_Characteristic 'X7R'
PRP Tolerance__ '0.1%'
PRP ValueDisplayed '0.10 µF'
PRP VDC_V '16V'
TOP 0 0.3200925 3.037465 0 N 424 169 1
TOP 1 0.3673365 3.037465 0 N 446 5 2
#
# CMP 109
CMP 11 2.5531502 1.7694493 180 N C31 GCM21BR71A106KE22L ;0=1,1=0.0571
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0805'
PRP Cap_F '10µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.murata.com/products/catalog/pdf/c03e.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'GCM21BR71A106KE22L'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10674-1-ND'
PRP Supplier_Part_Number_2 '06AC6014'
PRP Supplier_Part_Number_3 '81-GCM21BR71A106KE2L'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '10uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '10uF'
PRP VDC_V '10V'
TOP 0 2.5236226 1.7694493 90 N 54 14 1
TOP 1 2.5826777 1.7694493 90 N 424 170 2
#
# CMP 110
CMP 8 1.7007879 3.1259847 0 N C35 GCM188R70J225KE22D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '2.2µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM188R70J225KE22%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM188R70J225KE22D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5316-1-ND'
PRP Supplier_Part_Number_2 '81-GCM188R70J225KE2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '2.2uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '2.2uF'
PRP VDC_V '6.3V'
TOP 0 1.728347 3.1259847 270 N 424 171 1
TOP 1 1.6732289 3.1259847 270 N 69 7 2
#
# CMP 111
CMP 5 1.6944966 3.1710556 0 N C36 GCM155R71C104KA55D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.murata.com/capacitor/product/GCM155R71C104KA55%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71C104KA55D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-4759-2-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '16V'
TOP 0 1.7141816 3.1710556 270 N 424 172 1
TOP 1 1.6748115 3.1710556 270 N 69 8 2
#
# CMP 112
CMP 5 1.3110241 2.9527564 0 N C37 CGA2B3X7R1H103K050BB ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '10nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=CGA2B3X7R1H103K050BB'
PRP CompType 'Capacitor'
PRP ESR_ohm '0.333065'
PRP IRMS_A '323.373mA'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CGA2B3X7R1H103K050BB'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '445-6893-1-ND'
PRP Supplier_Part_Number_2 '52W9617'
PRP Supplier_Part_Number_3 '2210821'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.01uF'
PRP Value1 '0.333065 ohm'
PRP Value2 '50V'
PRP ValueDisplayed '0.01uF'
PRP VDC_V '50V'
TOP 0 1.3307091 2.9527564 270 N 69 9 1
TOP 1 1.291339 2.9527564 270 N 424 173 2
#
# CMP 113
CMP 11 0.3332419 4.0911833 0 N C39 CL21B106KOQNNNE ;0=1,1=0.0571
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0805'
PRP Cap_F '10µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.samsungsem.com/servlet/FileDownload?type=spec&file=CL21B106KOQNNNE.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Samsung Electro-Mechanics'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'CL21B106KOQNNNE'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '10uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '10uF'
PRP VDC_V '16V'
TOP 0 0.3627695 4.0911833 270 N 426 4 1
TOP 1 0.3037144 4.0911833 270 N 424 174 2
#
# CMP 114
CMP 2 1.1463785 3.2818115 0 N C40 GRM155R71E473KA88D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '47nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/PnsearchViewAction.do?HnOFG=ON&HnNFG=ON&SEL_CNT=50&sLang=en&sKey=GRM155R71E473KA88D&x=9&y=9&search=startwith'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GRM155R71E473KA88D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-3254-1-ND'
PRP Supplier_Part_Number_2 '14T3282'
PRP Supplier_Part_Number_3 '81-GRM155R71E473KA88'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.047uF'
PRP Value1 'Unknown'
PRP Value2 '25V'
PRP ValueDisplayed '0.047uF'
PRP VDC_V '25V'
TOP 0 1.1700005 3.2818115 270 N 44 0 1
TOP 1 1.1227564 3.2818115 270 N 424 175 2
#
# CMP 115
CMP 4 1.9510005 0.5208115 180 N C41 GCM155C71A105KE38D ;0=1,1=0.0276
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM155C71A105KE38%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155C71A105KE38D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.7'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GCM155C71A105KE8D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7S'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '1uF'
PRP VDC_V '10V'
TOP 0 1.9310005 0.5208115 90 N 308 34 1
TOP 1 1.9710005 0.5208115 90 N 424 313 2
#
# CMP 116
CMP 5 1.1286902 0.7220248 180 N C42 C0402C104K8RACTU ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://content.kemet.com/datasheets/KEM_C1002_X7R_SMD.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'Kemet'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'C0402C104K8RACTU'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '399-3520-1-ND'
PRP Supplier_Part_Number_2 '68X2393'
PRP Supplier_Part_Number_3 '80-C0402C104K8R'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.1uF'
PRP Value1 ''
PRP Value2 '10V'
PRP ValueDisplayed '0.1µF'
PRP VDC_V '10V'
TOP 0 1.1090052 0.7220248 90 N 424 176 1
TOP 1 1.1483753 0.7220248 90 N 308 12 2
#
# CMP 117
CMP 5 1.5516566 1.1676148 90 N C43 C0402C104K8RACTU ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://content.kemet.com/datasheets/KEM_C1002_X7R_SMD.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'Kemet'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'C0402C104K8RACTU'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '399-3520-1-ND'
PRP Supplier_Part_Number_2 '68X2393'
PRP Supplier_Part_Number_3 '80-C0402C104K8R'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.1uF'
PRP Value1 ''
PRP Value2 '10V'
PRP ValueDisplayed '0.1µF'
PRP VDC_V '10V'
TOP 0 1.5516566 1.1872998 180 N 424 177 1
TOP 1 1.5516566 1.1479297 180 N 308 13 2
#
# CMP 118
CMP 5 1.6944965 3.2127485 180 N C44 CGA2B3X7R1H103K050BB ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '10nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=CGA2B3X7R1H103K050BB'
PRP CompType 'Capacitor'
PRP ESR_ohm '0.333065'
PRP IRMS_A '323.373mA'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CGA2B3X7R1H103K050BB'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '445-6893-1-ND'
PRP Supplier_Part_Number_2 '52W9617'
PRP Supplier_Part_Number_3 '2210821'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.01uF'
PRP Value1 '0.333065 ohm'
PRP Value2 '50V'
PRP ValueDisplayed '0.01uF'
PRP VDC_V '50V'
TOP 0 1.6748115 3.2127485 90 N 69 10 1
TOP 1 1.7141816 3.2127485 90 N 424 178 2
#
# CMP 119
CMP 11 3.0629246 1.4653505 180 N C45 CL21B106KOQNNNE ;0=1,1=0.0571
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0805'
PRP Cap_F '10µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.samsungsem.com/servlet/FileDownload?type=spec&file=CL21B106KOQNNNE.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Samsung Electro-Mechanics'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'CL21B106KOQNNNE'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '10uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '10uF'
PRP VDC_V '16V'
TOP 0 3.033397 1.4653505 90 N 246 1 1
TOP 1 3.0924521 1.4653505 90 N 424 179 2
#
# CMP 120
CMP 5 1.311024 2.9141823 180 N C46 GCM155R71C104KA55D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.murata.com/capacitor/product/GCM155R71C104KA55%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71C104KA55D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-4759-2-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '16V'
TOP 0 1.291339 2.9141823 90 N 424 180 1
TOP 1 1.3307091 2.9141823 90 N 69 11 2
#
# CMP 121
CMP 5 1.123527 0.5485438 0 N C49 C0402C104K8RACTU ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://content.kemet.com/datasheets/KEM_C1002_X7R_SMD.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'Kemet'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'C0402C104K8RACTU'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '399-3520-1-ND'
PRP Supplier_Part_Number_2 '68X2393'
PRP Supplier_Part_Number_3 '80-C0402C104K8R'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.1uF'
PRP Value1 ''
PRP Value2 '10V'
PRP ValueDisplayed '0.1µF'
PRP VDC_V '10V'
TOP 0 1.143212 0.5485438 270 N 242 0 1
TOP 1 1.1038419 0.5485438 270 N 424 181 2
#
# CMP 122
CMP 5 1.5664525 0.3491591 0 N C50 C0402C103K4RACTU ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '10nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://content.kemet.com/datasheets/KEM_C1002_X7R_SMD.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP IRMS_A ''
PRP Manufacturer 'Kemet'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'C0402C103K4RACTU'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '399-1038-1-ND'
PRP Supplier_Part_Number_2 '66W8706'
PRP Supplier_Part_Number_3 '80-C0402C103K4R'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.01uF'
PRP Value1 ''
PRP Value2 '16V'
PRP ValueDisplayed '0.01µF'
PRP VDC_V '16V'
TOP 0 1.5861375 0.3491591 270 N 308 14 1
TOP 1 1.5467674 0.3491591 270 N 424 182 2
#
# CMP 123
CMP 5 1.2846838 3.3807862 270 N C52 CGA2B3X7R1H103K050BB ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '10nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=CGA2B3X7R1H103K050BB'
PRP CompType 'Capacitor'
PRP ESR_ohm '0.333065'
PRP IRMS_A '323.373mA'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CGA2B3X7R1H103K050BB'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '445-6893-1-ND'
PRP Supplier_Part_Number_2 '52W9617'
PRP Supplier_Part_Number_3 '2210821'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.01uF'
PRP Value1 '0.333065 ohm'
PRP Value2 '50V'
PRP ValueDisplayed '0.01uF'
PRP VDC_V '50V'
TOP 0 1.2846838 3.3611012 0 N 98 1 1
TOP 1 1.2846838 3.4004713 0 N 424 183 2
#
# CMP 124
CMP 8 1.229155 2.8241525 270 N C53 GCM188R71C105KA64D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM188R71C105KA64%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM188R71C105KA64D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5241-6-ND'
PRP Supplier_Part_Number_2 '81-GCM188R71C105K64D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '1uF'
PRP VDC_V '16V'
TOP 0 1.229155 2.7965934 0 N 261 2 1
TOP 1 1.229155 2.8517115 0 N 424 184 2
#
# CMP 125
CMP 5 1.2480979 3.3807862 90 N C54 GCM155R71C104KA55D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.murata.com/capacitor/product/GCM155R71C104KA55%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71C104KA55D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-4759-2-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '16V'
TOP 0 1.2480979 3.4004712 180 N 424 185 1
TOP 1 1.2480979 3.3611011 180 N 98 2 2
#
# CMP 126
CMP 8 0.9250349 2.5801858 0 N C56 GCM188R71C105KA64D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM188R71C105KA64%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM188R71C105KA64D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5241-6-ND'
PRP Supplier_Part_Number_2 '81-GCM188R71C105K64D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '1uF'
PRP VDC_V '16V'
TOP 0 0.952594 2.5801858 270 N 459 2 1
TOP 1 0.8974759 2.5801858 270 N 424 186 2
#
# CMP 127
CMP 5 1.030826 2.5510953 90 N C57 GCM155R71A104KA55D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GCM155R71A104KA55-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71A104KA55D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GCM155R71A104K5D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '10V'
TOP 0 1.030826 2.5707803 180 N 459 3 1
TOP 1 1.030826 2.5314102 180 N 424 187 2
#
# CMP 128
CMP 54 2.4094811 2.4306305 0 N C58 NFM18HC105C1C3D ;0=1,1=0.0010
PRP AC_Safety ''
PRP AEC_Category ''
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case ''
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://psearch.en.murata.com/capacitor/product/NFM18HC105C1C3%23.html'
PRP CompType ''
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'Murata'
PRP MountType ''
PRP PackageReference '0603'
PRP PartNumber 'NFM18HC105C1C3D'
PRP Polarized ''
PRP RoHS 'TRUE'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm '0.7mm'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C ''
PRP TaMin_C ''
PRP Technology ''
PRP TempCo ''
PRP Tolerance__ '20%'
PRP U/M ''
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value ''
PRP Value1 ''
PRP Value2 ''
PRP ValueDisplayed '1uF'
PRP VDC_V '16V'
TOP 0 2.4409772 2.4306305 180 N 54 23 1
TOP 1 2.4094811 2.4463785 180 N 424 339 2
TOP 2 2.4094811 2.4148825 180 N 424 340 2
TOP 3 2.377985 2.4306305 180 N 54 22 3
#
# CMP 129
CMP 8 0.9250349 2.5163298 0 N C59 GCM188R71C105KA64D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM188R71C105KA64%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM188R71C105KA64D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5241-6-ND'
PRP Supplier_Part_Number_2 '81-GCM188R71C105K64D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '1uF'
PRP VDC_V '16V'
TOP 0 0.952594 2.5163298 270 N 456 2 1
TOP 1 0.8974759 2.5163298 270 N 424 188 2
#
# CMP 130
CMP 5 1.1573066 0.9973627 90 N C63 GCM1555C1H8R0DA16D ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category ''
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case ''
PRP Cap_F '8pF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GCM1555C1H8R0DA16-01.pdf'
PRP CompType ''
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'Murata Electronics North America'
PRP MountType ''
PRP PackageReference '0402'
PRP PartNumber 'GCM1555C1H8R0DA16D'
PRP Polarized ''
PRP RoHS 'TRUE'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm '0.55mm'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C ''
PRP TaMin_C ''
PRP Technology ''
PRP TempCo '30ppm/°C'
PRP Tolerance__ ''
PRP U/M ''
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value ''
PRP Value1 ''
PRP Value2 ''
PRP ValueDisplayed ''
PRP VDC_V ''
TOP 0 1.1573066 1.0170477 180 N 424 189 1
TOP 1 1.1573066 0.9776776 180 N 243 0 2
#
# CMP 131
CMP 5 1.6004424 1.1676148 90 N C64 C0402C104K8RACTU ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://content.kemet.com/datasheets/KEM_C1002_X7R_SMD.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'Kemet'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'C0402C104K8RACTU'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '399-3520-1-ND'
PRP Supplier_Part_Number_2 '68X2393'
PRP Supplier_Part_Number_3 '80-C0402C104K8R'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.1uF'
PRP Value1 ''
PRP Value2 '10V'
PRP ValueDisplayed '0.1µF'
PRP VDC_V '10V'
TOP 0 1.6004424 1.1872998 180 N 424 190 1
TOP 1 1.6004424 1.1479297 180 N 262 0 2
#
# CMP 132
CMP 5 1.9505791 0.8481046 0 N C66 C0402C103K4RACTU ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '10nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://content.kemet.com/datasheets/KEM_C1002_X7R_SMD.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP IRMS_A ''
PRP Manufacturer 'Kemet'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'C0402C103K4RACTU'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '399-1038-1-ND'
PRP Supplier_Part_Number_2 '66W8706'
PRP Supplier_Part_Number_3 '80-C0402C103K4R'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.01uF'
PRP Value1 ''
PRP Value2 '16V'
PRP ValueDisplayed '0.01µF'
PRP VDC_V '16V'
TOP 0 1.9702641 0.8481046 270 N 424 191 1
TOP 1 1.930894 0.8481046 270 N 241 0 2
#
# CMP 133
CMP 5 1.9505791 0.8087679 0 N C67 C0402C104K8RACTU ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://content.kemet.com/datasheets/KEM_C1002_X7R_SMD.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'Kemet'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'C0402C104K8RACTU'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '399-3520-1-ND'
PRP Supplier_Part_Number_2 '68X2393'
PRP Supplier_Part_Number_3 '80-C0402C104K8R'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.1uF'
PRP Value1 ''
PRP Value2 '10V'
PRP ValueDisplayed '0.1µF'
PRP VDC_V '10V'
TOP 0 1.9702641 0.8087679 270 N 424 192 1
TOP 1 1.930894 0.8087679 270 N 241 1 2
#
# CMP 134
CMP 5 0.7414445 4.2211046 180 N C69 C0402C104K8RACTU ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://content.kemet.com/datasheets/KEM_C1002_X7R_SMD.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'Kemet'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'C0402C104K8RACTU'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '399-3520-1-ND'
PRP Supplier_Part_Number_2 '68X2393'
PRP Supplier_Part_Number_3 '80-C0402C104K8R'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.1uF'
PRP Value1 ''
PRP Value2 '10V'
PRP ValueDisplayed '0.1µF'
PRP VDC_V '10V'
TOP 0 0.7217595 4.2211046 90 N 424 193 1
TOP 1 0.7611296 4.2211046 90 N 259 0 2
#
# CMP 135
CMP 5 1.1573066 0.893556 90 N C70 GCM1555C1H8R0DA16D ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category ''
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case ''
PRP Cap_F '8pF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GCM1555C1H8R0DA16-01.pdf'
PRP CompType ''
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'Murata Electronics North America'
PRP MountType ''
PRP PackageReference '0402'
PRP PartNumber 'GCM1555C1H8R0DA16D'
PRP Polarized ''
PRP RoHS 'TRUE'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm '0.55mm'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C ''
PRP TaMin_C ''
PRP Technology ''
PRP TempCo '30ppm/°C'
PRP Tolerance__ ''
PRP U/M ''
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value ''
PRP Value1 ''
PRP Value2 ''
PRP ValueDisplayed ''
PRP VDC_V ''
TOP 0 1.1573066 0.913241 180 N 244 0 1
TOP 1 1.1573066 0.8738709 180 N 424 194 2
#
# CMP 136
CMP 5 1.2406328 1.1725153 90 N C71 C0402C104K8RACTU ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://content.kemet.com/datasheets/KEM_C1002_X7R_SMD.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'Kemet'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'C0402C104K8RACTU'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '399-3520-1-ND'
PRP Supplier_Part_Number_2 '68X2393'
PRP Supplier_Part_Number_3 '80-C0402C104K8R'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.1uF'
PRP Value1 ''
PRP Value2 '10V'
PRP ValueDisplayed '0.1µF'
PRP VDC_V '10V'
TOP 0 1.2406328 1.1922003 180 N 424 195 1
TOP 1 1.2406328 1.1528302 180 N 374 0 2
#
# CMP 137
CMP 5 0.7414445 4.3195298 180 N C73 C0402C104K8RACTU ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://content.kemet.com/datasheets/KEM_C1002_X7R_SMD.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'Kemet'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'C0402C104K8RACTU'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '399-3520-1-ND'
PRP Supplier_Part_Number_2 '68X2393'
PRP Supplier_Part_Number_3 '80-C0402C104K8R'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.1uF'
PRP Value1 ''
PRP Value2 '10V'
PRP ValueDisplayed '0.1µF'
PRP VDC_V '10V'
TOP 0 0.7217595 4.3195298 90 N 424 196 1
TOP 1 0.7611296 4.3195298 90 N 258 0 2
#
# CMP 138
CMP 5 1.1215784 0.8232444 180 N C75 C0402C104K8RACTU ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://content.kemet.com/datasheets/KEM_C1002_X7R_SMD.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'Kemet'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'C0402C104K8RACTU'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '399-3520-1-ND'
PRP Supplier_Part_Number_2 '68X2393'
PRP Supplier_Part_Number_3 '80-C0402C104K8R'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.1uF'
PRP Value1 ''
PRP Value2 '10V'
PRP ValueDisplayed '0.1µF'
PRP VDC_V '10V'
TOP 0 1.1018934 0.8232444 90 N 424 197 1
TOP 1 1.1412635 0.8232444 90 N 262 1 2
#
# CMP 139
CMP 5 1.9509402 0.5648115 0 N C76 C0402C104K8RACTU ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://content.kemet.com/datasheets/KEM_C1002_X7R_SMD.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'Kemet'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'C0402C104K8RACTU'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '399-3520-1-ND'
PRP Supplier_Part_Number_2 '68X2393'
PRP Supplier_Part_Number_3 '80-C0402C104K8R'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.1uF'
PRP Value1 ''
PRP Value2 '10V'
PRP ValueDisplayed '0.1µF'
PRP VDC_V '10V'
TOP 0 1.9706252 0.5648115 270 N 424 198 1
TOP 1 1.9312551 0.5648115 270 N 308 15 2
#
# CMP 140
CMP 5 1.3449987 4.0144116 180 N C77 C0402C104K8RACTU ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://content.kemet.com/datasheets/KEM_C1002_X7R_SMD.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'Kemet'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'C0402C104K8RACTU'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '399-3520-1-ND'
PRP Supplier_Part_Number_2 '68X2393'
PRP Supplier_Part_Number_3 '80-C0402C104K8R'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.1uF'
PRP Value1 ''
PRP Value2 '10V'
PRP ValueDisplayed '0.1µF'
PRP VDC_V '10V'
TOP 0 1.3253137 4.0144116 90 N 425 1 1
TOP 1 1.3646838 4.0144116 90 N 424 199 2
#
# CMP 141
CMP 8 0.9659662 3.9324727 90 N C79 C1608X7S1A475K080AC ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '4.7µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://product.tdk.com/en/catalog/datasheets/mlcc_commercial_general_en.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'C1608X7S1A475K080AC'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '445-14258-1-ND'
PRP Supplier_Part_Number_2 '29X4799'
PRP Supplier_Part_Number_3 '810-C1608X7S1A475KAC'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7S'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '4.7uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '4.7uF'
PRP VDC_V '10V'
TOP 0 0.9659662 3.9600318 180 N 425 2 1
TOP 1 0.9659662 3.9049137 180 N 424 200 2
#
# CMP 142
CMP 5 1.9625869 2.1664637 0 N C81 GCM155R71A104KA55D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GCM155R71A104KA55-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71A104KA55D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GCM155R71A104K5D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '10V'
TOP 0 1.9822719 2.1664637 270 N 159 0 1
TOP 1 1.9429018 2.1664637 270 N 199 0 2
#
# CMP 143
CMP 5 1.480115 4.4006926 180 N C82 C0402C104K8RACTU ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://content.kemet.com/datasheets/KEM_C1002_X7R_SMD.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'Kemet'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'C0402C104K8RACTU'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '399-3520-1-ND'
PRP Supplier_Part_Number_2 '68X2393'
PRP Supplier_Part_Number_3 '80-C0402C104K8R'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.1uF'
PRP Value1 ''
PRP Value2 '10V'
PRP ValueDisplayed '0.1µF'
PRP VDC_V '10V'
TOP 0 1.46043 4.4006926 90 N 425 3 1
TOP 1 1.4998001 4.4006926 90 N 424 201 2
#
# CMP 144
CMP 3 1.6143989 4.4045641 180 N C85 C1005X7S1A225K050BC ;0=1,1=0.0256
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402_065'
PRP Cap_F '2.2µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=C1005X7S1A225K050BC'
PRP CompType 'Capacitor'
PRP ESR_ohm '5.925m'
PRP IRMS_A '2.05591A'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'C1005X7S1A225K050BC'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.65'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '445-9097-1-ND'
PRP Supplier_Part_Number_2 '810-C1005X7S1A225K'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7S'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '2.2uF'
PRP Value1 '0.005925 ohm'
PRP Value2 '10V'
PRP ValueDisplayed '2.2uF'
PRP VDC_V '10V'
TOP 0 1.5947139 4.4045641 90 N 426 5 1
TOP 1 1.634084 4.4045641 90 N 424 202 2
#
# CMP 145
CMP 8 1.3321765 4.6740353 270 N C87 GCM188R71C105KA64D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM188R71C105KA64%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM188R71C105KA64D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5241-6-ND'
PRP Supplier_Part_Number_2 '81-GCM188R71C105K64D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '1uF'
PRP VDC_V '16V'
TOP 0 1.3321765 4.6464762 0 N 436 3 1
TOP 1 1.3321765 4.7015943 0 N 424 203 2
#
# CMP 146
CMP 5 1.2691749 4.6770149 270 N C88 C0402C104K8RACTU ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://content.kemet.com/datasheets/KEM_C1002_X7R_SMD.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'Kemet'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'C0402C104K8RACTU'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '399-3520-1-ND'
PRP Supplier_Part_Number_2 '68X2393'
PRP Supplier_Part_Number_3 '80-C0402C104K8R'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.1uF'
PRP Value1 ''
PRP Value2 '10V'
PRP ValueDisplayed '0.1µF'
PRP VDC_V '10V'
TOP 0 1.2691749 4.6573299 0 N 436 4 1
TOP 1 1.2691749 4.6967 0 N 424 204 2
#
# CMP 147
CMP 5 1.480115 4.2503858 180 N C89 C0402C104K8RACTU ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://content.kemet.com/datasheets/KEM_C1002_X7R_SMD.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'Kemet'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'C0402C104K8RACTU'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '399-3520-1-ND'
PRP Supplier_Part_Number_2 '68X2393'
PRP Supplier_Part_Number_3 '80-C0402C104K8R'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.1uF'
PRP Value1 ''
PRP Value2 '10V'
PRP ValueDisplayed '0.1µF'
PRP VDC_V '10V'
TOP 0 1.46043 4.2503858 90 N 436 5 1
TOP 1 1.4998001 4.2503858 90 N 424 205 2
#
# CMP 148
CMP 5 1.2687642 3.9265673 90 N C91 C0402C104K8RACTU ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://content.kemet.com/datasheets/KEM_C1002_X7R_SMD.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'Kemet'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'C0402C104K8RACTU'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '399-3520-1-ND'
PRP Supplier_Part_Number_2 '68X2393'
PRP Supplier_Part_Number_3 '80-C0402C104K8R'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.1uF'
PRP Value1 ''
PRP Value2 '10V'
PRP ValueDisplayed '0.1µF'
PRP VDC_V '10V'
TOP 0 1.2687642 3.9462523 180 N 436 6 1
TOP 1 1.2687642 3.9068822 180 N 424 206 2
#
# CMP 149
CMP 5 2.5928175 4.2101918 90 N C92 GCM155R71C224KE02D ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM155R71C224KE02%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71C224KE02D'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-10671-1-ND'
PRP Supplier_Part_Number_2 '81-GCM155R71C224KE2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.22uF'
PRP Value1 ''
PRP Value2 '16V'
PRP ValueDisplayed '0.22µF'
PRP VDC_V '16V'
TOP 0 2.5928175 4.2298768 180 N 424 207 1
TOP 1 2.5928175 4.1905067 180 N 458 7 2
#
# CMP 150
CMP 5 1.6143989 4.6170065 180 N C93 04025A150FAT2A ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '15pF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://datasheets.avx.com/C0GNP0-Dielectric.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS 'Incomplete'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Not Set'
PRP Green_REACh 'Incomplete'
PRP IRMS_A ''
PRP Manufacturer 'AVX'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber '04025A150FAT2A'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '478-5126-1-ND'
PRP Supplier_Part_Number_2 '581-04025A150F'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'C0G/NP0'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '15pF'
PRP Value1 ''
PRP Value2 '50V'
PRP ValueDisplayed '15pF'
PRP VDC_V '50V'
TOP 0 1.5947139 4.6170065 90 N 260 1 1
TOP 1 1.634084 4.6170065 90 N 424 208 2
#
# CMP 151
CMP 3 1.6143989 4.6688617 180 N C94 C1005X7S1A225K050BC ;0=1,1=0.0256
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402_065'
PRP Cap_F '2.2µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=C1005X7S1A225K050BC'
PRP CompType 'Capacitor'
PRP ESR_ohm '5.925m'
PRP IRMS_A '2.05591A'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'C1005X7S1A225K050BC'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.65'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '445-9097-1-ND'
PRP Supplier_Part_Number_2 '810-C1005X7S1A225K'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7S'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '2.2uF'
PRP Value1 '0.005925 ohm'
PRP Value2 '10V'
PRP ValueDisplayed '2.2uF'
PRP VDC_V '10V'
TOP 0 1.5947139 4.6688617 90 N 260 2 1
TOP 1 1.634084 4.6688617 90 N 424 209 2
#
# CMP 152
CMP 5 2.7890011 3.6900011 270 N C96 GCM155R71C224KE02D ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM155R71C224KE02%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71C224KE02D'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-10671-1-ND'
PRP Supplier_Part_Number_2 '81-GCM155R71C224KE2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.22uF'
PRP Value1 ''
PRP Value2 '16V'
PRP ValueDisplayed '0.22µF'
PRP VDC_V '16V'
TOP 0 2.7890011 3.6703161 0 N 424 210 1
TOP 1 2.7890011 3.7096862 0 N 458 8 2
#
# CMP 153
CMP 5 0.3782532 4.3308203 180 N C97 C0402C104K8RACTU ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://content.kemet.com/datasheets/KEM_C1002_X7R_SMD.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'Kemet'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'C0402C104K8RACTU'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '399-3520-1-ND'
PRP Supplier_Part_Number_2 '68X2393'
PRP Supplier_Part_Number_3 '80-C0402C104K8R'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.1uF'
PRP Value1 ''
PRP Value2 '10V'
PRP ValueDisplayed '0.1µF'
PRP VDC_V '10V'
TOP 0 0.3585682 4.3308203 90 N 372 1 1
TOP 1 0.3979383 4.3308203 90 N 424 211 2
#
# CMP 154
CMP 12 3.0829392 0.7887975 180 N C101 C3216X7R1H475K160AC ;0=1,1=0.0709
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '1206_180'
PRP Cap_F '4.7µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=C3216X7R1H475K160AC'
PRP CompType 'Capacitor'
PRP ESR_ohm '3.158m'
PRP IRMS_A '4.08379A'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '1206'
PRP PartNumber 'C3216X7R1H475K160AC'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '5.12'
PRP SizeAreaWB_mm2 '10.92'
PRP SizeX_mm '3.2'
PRP SizeY_mm '1.6'
PRP SizeZ_mm '1.8'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '445-8032-1-ND'
PRP Supplier_Part_Number_2 '810-C3216X7R1H475K160AC'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '4.7uF'
PRP Value1 '0.003158 ohm'
PRP Value2 '50V'
PRP ValueDisplayed '4.7uF'
PRP VDC_V '50V'
TOP 0 3.0297896 0.7887975 90 N 138 5 1
TOP 1 3.1360888 0.7887975 90 N 424 212 2
#
# CMP 155
CMP 46 2.101655 3.8661896 0 N C102 GRT155R70J105KE01D ;0=1,1=0.0000
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRT155R70J105KE01-01.pdf'
PRP Datasheet 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRT155R70J105KE01-01.pdf'
PRP Datasheet_Path 'datasheets/Cap_GRT155R70J105KE01D.pdf'
PRP Digikey_Description 'CAP CERAMIC 1UF 6.3V X7R 10% PAD'
PRP Digikey_Part_Number '490-18216-1-ND'
PRP helpURL 'https://upverter.com/upn/revision/e7058e337ffa2e70/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Murata'
PRP Mouser_Description 'Cap Ceramic 1uF 6.3V X7R 10% Pad SMD 0402 125C Automotive T/R'
PRP Mouser_Part_Number '81-GRT155R70J105KE1D'
PRP Operating_Temperature_Range '-55°C to +125°C'
PRP PackageReference '0402'
PRP PartNumber 'GRT155R70J105KE01D'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.55mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '490-18216-1-ND'
PRP Supplier_Part_Number_2 '81-GRT155R70J105KE1D'
PRP TempCo '15%'
PRP Temperature_Characteristic 'X7R'
PRP Tolerance__ '10%'
PRP ValueDisplayed '1uF'
PRP VDC_V '6.3V'
TOP 0 2.1174015 3.8661896 180 N 173 0 1
TOP 1 2.0859084 3.8661896 180 N 424 336 2
#
# CMP 156
CMP 46 2.101655 3.8356584 0 N C103 GRT155R70J105KE01D ;0=1,1=0.0000
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRT155R70J105KE01-01.pdf'
PRP Datasheet 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRT155R70J105KE01-01.pdf'
PRP Datasheet_Path 'datasheets/Cap_GRT155R70J105KE01D.pdf'
PRP Digikey_Description 'CAP CERAMIC 1UF 6.3V X7R 10% PAD'
PRP Digikey_Part_Number '490-18216-1-ND'
PRP helpURL 'https://upverter.com/upn/revision/e7058e337ffa2e70/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Murata'
PRP Mouser_Description 'Cap Ceramic 1uF 6.3V X7R 10% Pad SMD 0402 125C Automotive T/R'
PRP Mouser_Part_Number '81-GRT155R70J105KE1D'
PRP Operating_Temperature_Range '-55°C to +125°C'
PRP PackageReference '0402'
PRP PartNumber 'GRT155R70J105KE01D'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.55mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '490-18216-1-ND'
PRP Supplier_Part_Number_2 '81-GRT155R70J105KE1D'
PRP TempCo '15%'
PRP Temperature_Characteristic 'X7R'
PRP Tolerance__ '10%'
PRP ValueDisplayed '1uF'
PRP VDC_V '6.3V'
TOP 0 2.1174015 3.8356584 180 N 174 0 1
TOP 1 2.0859084 3.8356584 180 N 424 366 2
#
# CMP 157
CMP 44 1.934628 3.7225067 0 N C106 GCM1555C1H3R9BA16D ;0=1,1=0.0000
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP Cap_F '3.9pF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.murata.com/en-us/products/productdetail?partno=GCM1555C1H3R9BA16%23'
PRP Datasheet 'https://www.murata.com/en-us/products/productdetail?partno=GCM1555C1H3R9BA16%23'
PRP Datasheet_Path 'datasheets/Cap-GCM1555C1H3R9BA16D.pdf'
PRP helpURL 'https://upverter.com/upn/revision/a8ea75d1d60bc8eb/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Murata'
PRP Operating_Temperature_Range '-55°C to +125°C'
PRP PackageReference '0402'
PRP Part_Number 'GCM1555C1H3R9BA16D'
PRP PartNumber 'GCM1555C1H3R9BA16D'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.55mm'
PRP TempCo '30ppm/°C'
PRP Temperature_Characteristic 'C0G'
PRP Value '3.9pF'
PRP ValueDisplayed '3.9pF'
PRP VDC_V '50V'
TOP 0 1.950376 3.7225067 180 N 32 3 1
TOP 1 1.91888 3.7225067 180 N 424 369 2
#
# CMP 158
CMP 5 2.1292655 3.9624828 180 N C107 GCM155R71C224KE02D ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM155R71C224KE02%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71C224KE02D'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-10671-1-ND'
PRP Supplier_Part_Number_2 '81-GCM155R71C224KE2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.22uF'
PRP Value1 ''
PRP Value2 '16V'
PRP ValueDisplayed '0.22µF'
PRP VDC_V '16V'
TOP 0 2.1095805 3.9624828 90 N 424 521 1
TOP 1 2.1489506 3.9624828 90 N 457 28 2
#
# CMP 159
CMP 44 2.0688492 3.5954436 90 N C108 GCM1555C1H3R9BA16D ;0=1,1=0.0000
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP Cap_F '3.9pF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.murata.com/en-us/products/productdetail?partno=GCM1555C1H3R9BA16%23'
PRP Datasheet 'https://www.murata.com/en-us/products/productdetail?partno=GCM1555C1H3R9BA16%23'
PRP Datasheet_Path 'datasheets/Cap-GCM1555C1H3R9BA16D.pdf'
PRP helpURL 'https://upverter.com/upn/revision/a8ea75d1d60bc8eb/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Murata'
PRP Operating_Temperature_Range '-55°C to +125°C'
PRP PackageReference '0402'
PRP Part_Number 'GCM1555C1H3R9BA16D'
PRP PartNumber 'GCM1555C1H3R9BA16D'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.55mm'
PRP TempCo '30ppm/°C'
PRP Temperature_Characteristic 'C0G'
PRP Value '3.9pF'
PRP ValueDisplayed '3.9pF'
PRP VDC_V '50V'
TOP 0 2.0688492 3.6111916 90 N 17 3 1
TOP 1 2.0688492 3.5796956 90 N 424 370 2
#
# CMP 160
CMP 5 1.9486305 1.0255569 0 N C109 C0402C103K4RACTU ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '10nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://content.kemet.com/datasheets/KEM_C1002_X7R_SMD.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP IRMS_A ''
PRP Manufacturer 'Kemet'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'C0402C103K4RACTU'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '399-1038-1-ND'
PRP Supplier_Part_Number_2 '66W8706'
PRP Supplier_Part_Number_3 '80-C0402C103K4R'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.01uF'
PRP Value1 ''
PRP Value2 '16V'
PRP ValueDisplayed '0.01µF'
PRP VDC_V '16V'
TOP 0 1.9683155 1.0255569 270 N 424 213 1
TOP 1 1.9289454 1.0255569 270 N 263 0 2
#
# CMP 161
CMP 11 2.2578561 3.5259791 90 N C110 GCM21BR71A106KE22L ;0=1,1=0.0571
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0805'
PRP Cap_F '10µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.murata.com/products/catalog/pdf/c03e.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'GCM21BR71A106KE22L'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10674-1-ND'
PRP Supplier_Part_Number_2 '06AC6014'
PRP Supplier_Part_Number_3 '81-GCM21BR71A106KE2L'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '10uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '10uF'
PRP VDC_V '10V'
TOP 0 2.2578561 3.5555067 180 N 457 6 1
TOP 1 2.2578561 3.4964516 180 N 424 214 2
#
# CMP 162
CMP 5 2.1292655 3.898337 180 N C111 GCM155R71C224KE02D ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM155R71C224KE02%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71C224KE02D'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-10671-1-ND'
PRP Supplier_Part_Number_2 '81-GCM155R71C224KE2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.22uF'
PRP Value1 ''
PRP Value2 '16V'
PRP ValueDisplayed '0.22µF'
PRP VDC_V '16V'
TOP 0 2.1095804 3.898337 90 N 424 215 1
TOP 1 2.1489506 3.898337 90 N 457 7 2
#
# CMP 163
CMP 11 2.0570011 4.1325287 270 N C112 GCM21BR71A106KE22L ;0=1,1=0.0571
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0805'
PRP Cap_F '10µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.murata.com/products/catalog/pdf/c03e.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'GCM21BR71A106KE22L'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10674-1-ND'
PRP Supplier_Part_Number_2 '06AC6014'
PRP Supplier_Part_Number_3 '81-GCM21BR71A106KE2L'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '10uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '10uF'
PRP VDC_V '10V'
TOP 0 2.0570011 4.1030011 180 N 457 8 1
TOP 1 2.0570011 4.1620562 180 N 424 216 2
#
# CMP 164
CMP 5 2.1140011 4.0928437 90 N C113 GCM155R71C224KE02D ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM155R71C224KE02%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71C224KE02D'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-10671-1-ND'
PRP Supplier_Part_Number_2 '81-GCM155R71C224KE2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.22uF'
PRP Value1 ''
PRP Value2 '16V'
PRP ValueDisplayed '0.22µF'
PRP VDC_V '16V'
TOP 0 2.1140011 4.1125287 0 N 424 217 1
TOP 1 2.1140011 4.0731586 0 N 457 9 2
#
# CMP 165
CMP 11 2.0336 4.0018 90 N C114 GCM21BR71A106KE22L ;0=1,1=0.0571
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0805'
PRP Cap_F '10µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.murata.com/products/catalog/pdf/c03e.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'GCM21BR71A106KE22L'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10674-1-ND'
PRP Supplier_Part_Number_2 '06AC6014'
PRP Supplier_Part_Number_3 '81-GCM21BR71A106KE2L'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '10uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '10uF'
PRP VDC_V '10V'
TOP 0 2.0336 4.0313276 180 N 175 4 1
TOP 1 2.0336 3.9722725 180 N 424 218 2
#
# CMP 166
CMP 5 2.1421217 4.0111366 180 N C115 GCM155R71C224KE02D ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM155R71C224KE02%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71C224KE02D'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-10671-1-ND'
PRP Supplier_Part_Number_2 '81-GCM155R71C224KE2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.22uF'
PRP Value1 ''
PRP Value2 '16V'
PRP ValueDisplayed '0.22µF'
PRP VDC_V '16V'
TOP 0 2.1224367 4.0111366 90 N 424 219 1
TOP 1 2.1618068 4.0111366 90 N 175 5 2
#
# CMP 167
CMP 11 2.3470011 3.4264735 90 N C116 GCM21BR71A106KE22L ;0=1,1=0.0571
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0805'
PRP Cap_F '10µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.murata.com/products/catalog/pdf/c03e.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'GCM21BR71A106KE22L'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10674-1-ND'
PRP Supplier_Part_Number_2 '06AC6014'
PRP Supplier_Part_Number_3 '81-GCM21BR71A106KE2L'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '10uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '10uF'
PRP VDC_V '10V'
TOP 0 2.3470011 3.4560011 180 N 175 6 1
TOP 1 2.3470011 3.396946 180 N 424 220 2
#
# CMP 168
CMP 5 2.3436862 3.6180011 0 N C117 GCM155R71C224KE02D ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM155R71C224KE02%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71C224KE02D'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-10671-1-ND'
PRP Supplier_Part_Number_2 '81-GCM155R71C224KE2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.22uF'
PRP Value1 ''
PRP Value2 '16V'
PRP ValueDisplayed '0.22µF'
PRP VDC_V '16V'
TOP 0 2.3633712 3.6180011 270 N 424 221 1
TOP 1 2.3240011 3.6180011 270 N 175 7 2
#
# CMP 169
CMP 2 2.7934628 2.5746792 270 N C119 GCM155R71C224KE02D ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM155R71C224KE02%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71C224KE02D'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-10671-1-ND'
PRP Supplier_Part_Number_2 '81-GCM155R71C224KE2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.22uF'
PRP Value1 ''
PRP Value2 '16V'
PRP ValueDisplayed '0.22µF'
PRP VDC_V '16V'
TOP 0 2.7934628 2.5510572 0 N 309 5 1
TOP 1 2.7934628 2.5983013 0 N 424 222 2
#
# CMP 170
CMP 2 1.9909602 2.5743788 270 N C120 GCM155R71C224KE02D ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM155R71C224KE02%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71C224KE02D'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-10671-1-ND'
PRP Supplier_Part_Number_2 '81-GCM155R71C224KE2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.22uF'
PRP Value1 ''
PRP Value2 '16V'
PRP ValueDisplayed '0.22µF'
PRP VDC_V '16V'
TOP 0 1.9909602 2.5507568 0 N 144 3 1
TOP 1 1.9909602 2.5980009 0 N 424 223 2
#
# CMP 171
CMP 7 1.0719345 3.2128115 270 N C121 CGA3E2C0G1H220J080AA ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '22pF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://product.tdk.com/en/catalog/datasheets/mlcc_automotive_general_en.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'CGA3E2C0G1H220J080AA'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '445-5632-1-ND'
PRP Supplier_Part_Number_2 '12T1569'
PRP Supplier_Part_Number_3 '810-CGA3E2C0G1H220J'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'C0G/NP0'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '22pF'
PRP Value1 'Unknown'
PRP Value2 '50V'
PRP ValueDisplayed '22pF'
PRP VDC_V '50V'
TOP 0 1.0719345 3.1813154 0 N 96 5 1
TOP 1 1.0719345 3.2443075 0 N 424 224 2
#
# CMP 172
CMP 2 2.779528 1.8791895 90 N C122 GCM155R71C224KE02D ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM155R71C224KE02%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71C224KE02D'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-10671-1-ND'
PRP Supplier_Part_Number_2 '81-GCM155R71C224KE2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.22uF'
PRP Value1 ''
PRP Value2 '16V'
PRP ValueDisplayed '0.22µF'
PRP VDC_V '16V'
TOP 0 2.779528 1.9028115 180 N 454 8 1
TOP 1 2.779528 1.8555674 180 N 424 225 2
#
# CMP 173
CMP 8 2.2308916 2.2143425 180 N C123 GCM188R70J225KE22D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '2.2µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM188R70J225KE22%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM188R70J225KE22D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5316-1-ND'
PRP Supplier_Part_Number_2 '81-GCM188R70J225KE2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '2.2uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '2.2uF'
PRP VDC_V '6.3V'
TOP 0 2.2033325 2.2143425 90 N 68 15 1
TOP 1 2.2584506 2.2143425 90 N 158 0 2
#
# CMP 174
CMP 11 2.2035044 2.5743391 270 N C124 GCM21BR71A106KE22L ;0=1,1=0.0571
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0805'
PRP Cap_F '10µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.murata.com/products/catalog/pdf/c03e.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'GCM21BR71A106KE22L'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10674-1-ND'
PRP Supplier_Part_Number_2 '06AC6014'
PRP Supplier_Part_Number_3 '81-GCM21BR71A106KE2L'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '10uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '10uF'
PRP VDC_V '10V'
TOP 0 2.2035044 2.5448115 0 N 144 4 1
TOP 1 2.2035044 2.6038666 0 N 424 226 2
#
# CMP 175
CMP 11 2.7198115 2.5748115 270 N C125 GCM21BR71A106KE22L ;0=1,1=0.0571
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0805'
PRP Cap_F '10µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.murata.com/products/catalog/pdf/c03e.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'GCM21BR71A106KE22L'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10674-1-ND'
PRP Supplier_Part_Number_2 '06AC6014'
PRP Supplier_Part_Number_3 '81-GCM21BR71A106KE2L'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '10uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '10uF'
PRP VDC_V '10V'
TOP 0 2.7198115 2.5452839 0 N 309 6 1
TOP 1 2.7198115 2.604339 0 N 424 227 2
#
# CMP 176
CMP 11 2.6353164 2.5748115 270 N C127 GCM21BR71A106KE22L ;0=1,1=0.0571
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0805'
PRP Cap_F '10µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.murata.com/products/catalog/pdf/c03e.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'GCM21BR71A106KE22L'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10674-1-ND'
PRP Supplier_Part_Number_2 '06AC6014'
PRP Supplier_Part_Number_3 '81-GCM21BR71A106KE2L'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '10uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '10uF'
PRP VDC_V '10V'
TOP 0 2.6353164 2.5452839 0 N 309 7 1
TOP 1 2.6353164 2.604339 0 N 424 228 2
#
# CMP 177
CMP 9 3.0158588 1.8803627 90 N C128 CGA4J1X7T0J226M ;0=1,1=0.0610
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0805'
PRP Cap_F '22µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://sps16.itg.ti.com/sites/KMS/crossdivteams/altium/docs/ComponentDatasheets/TDK datasheet_CGA4J1X7T0J226M (preliminary)_TI 03122019.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'CGA4J1X7T0J226M'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.55'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7T'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '22uF'
PRP Value1 ''
PRP Value2 '6.3V'
PRP ValueDisplayed '22µF'
PRP VDC_V '6.3V'
TOP 0 3.0158588 1.9148115 180 N 16 2 1
TOP 1 3.0158588 1.8459139 180 N 424 229 2
#
# CMP 178
CMP 11 2.7158107 1.8809438 90 N C129 GCM21BR71A106KE22L ;0=1,1=0.0571
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0805'
PRP Cap_F '10µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.murata.com/products/catalog/pdf/c03e.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'GCM21BR71A106KE22L'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10674-1-ND'
PRP Supplier_Part_Number_2 '06AC6014'
PRP Supplier_Part_Number_3 '81-GCM21BR71A106KE2L'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '10uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '10uF'
PRP VDC_V '10V'
TOP 0 2.7158107 1.9104714 180 N 454 9 1
TOP 1 2.7158107 1.8514163 180 N 424 230 2
#
# CMP 179
CMP 11 2.6298107 1.8789438 90 N C130 GCM21BR71A106KE22L ;0=1,1=0.0571
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0805'
PRP Cap_F '10µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.murata.com/products/catalog/pdf/c03e.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'GCM21BR71A106KE22L'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10674-1-ND'
PRP Supplier_Part_Number_2 '06AC6014'
PRP Supplier_Part_Number_3 '81-GCM21BR71A106KE2L'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '10uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '10uF'
PRP VDC_V '10V'
TOP 0 2.6298107 1.9084714 180 N 454 10 1
TOP 1 2.6298107 1.8494163 180 N 424 231 2
#
# CMP 180
CMP 5 1.9986184 4.2658751 270 N C131 GCM155R71C104KA55D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.murata.com/capacitor/product/GCM155R71C104KA55%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71C104KA55D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-4759-2-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '16V'
TOP 0 1.9986184 4.2461901 0 N 424 232 1
TOP 1 1.9986184 4.2855602 0 N 421 0 2
#
# CMP 181
CMP 11 2.0528266 2.5743391 270 N C132 GCM21BR71A106KE22L ;0=1,1=0.0571
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0805'
PRP Cap_F '10µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.murata.com/products/catalog/pdf/c03e.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'GCM21BR71A106KE22L'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10674-1-ND'
PRP Supplier_Part_Number_2 '06AC6014'
PRP Supplier_Part_Number_3 '81-GCM21BR71A106KE2L'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '10uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '10uF'
PRP VDC_V '10V'
TOP 0 2.0528266 2.5448115 0 N 144 5 1
TOP 1 2.0528266 2.6038666 0 N 424 233 2
#
# CMP 182
CMP 5 1.7637394 1.6858115 180 N C133 C0402C104K8RACTU ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://content.kemet.com/datasheets/KEM_C1002_X7R_SMD.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'Kemet'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'C0402C104K8RACTU'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '399-3520-1-ND'
PRP Supplier_Part_Number_2 '68X2393'
PRP Supplier_Part_Number_3 '80-C0402C104K8R'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.1uF'
PRP Value1 ''
PRP Value2 '10V'
PRP ValueDisplayed '0.1µF'
PRP VDC_V '10V'
TOP 0 1.7440544 1.6858115 90 N 308 16 1
TOP 1 1.7834245 1.6858115 90 N 424 234 2
#
# CMP 183
CMP 11 2.1281655 2.5743391 270 N C134 GCM21BR71A106KE22L ;0=1,1=0.0571
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0805'
PRP Cap_F '10µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.murata.com/products/catalog/pdf/c03e.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'GCM21BR71A106KE22L'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-10674-1-ND'
PRP Supplier_Part_Number_2 '06AC6014'
PRP Supplier_Part_Number_3 '81-GCM21BR71A106KE2L'
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '10uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '10uF'
PRP VDC_V '10V'
TOP 0 2.1281655 2.5448115 0 N 144 6 1
TOP 1 2.1281655 2.6038666 0 N 424 235 2
#
# CMP 184
CMP 5 1.8652215 3.9748121 180 N C135 GCM155R71C104KA55D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.murata.com/capacitor/product/GCM155R71C104KA55%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71C104KA55D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-4759-2-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '16V'
TOP 0 1.8455365 3.9748121 90 N 424 236 1
TOP 1 1.8849066 3.9748121 90 N 422 0 2
#
# CMP 185
CMP 5 2.0626097 4.5961271 90 N C136 GCM155R71C104KA55D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.murata.com/capacitor/product/GCM155R71C104KA55%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71C104KA55D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-4759-2-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '16V'
TOP 0 2.0626097 4.6158121 180 N 424 237 1
TOP 1 2.0626097 4.576442 180 N 423 0 2
#
# CMP 186
CMP 8 2.7040011 3.5164421 270 N C137 GCM188R70J225KE22D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '2.2µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM188R70J225KE22%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM188R70J225KE22D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5316-1-ND'
PRP Supplier_Part_Number_2 '81-GCM188R70J225KE2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '2.2uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '2.2uF'
PRP VDC_V '6.3V'
TOP 0 2.7040011 3.488883 0 N 424 238 1
TOP 1 2.7040011 3.5440011 0 N 458 9 2
#
# CMP 187
CMP 5 2.661001 3.547316 270 N C139 GCM155R71C224KE02D ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM155R71C224KE02%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71C224KE02D'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-10671-1-ND'
PRP Supplier_Part_Number_2 '81-GCM155R71C224KE2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.22uF'
PRP Value1 ''
PRP Value2 '16V'
PRP ValueDisplayed '0.22µF'
PRP VDC_V '16V'
TOP 0 2.661001 3.527631 0 N 424 239 1
TOP 1 2.661001 3.5670011 0 N 458 10 2
#
# CMP 188
CMP 5 2.4648561 4.2281918 90 N C140 GCM155R71C224KE02D ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM155R71C224KE02%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71C224KE02D'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-10671-1-ND'
PRP Supplier_Part_Number_2 '81-GCM155R71C224KE2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.22uF'
PRP Value1 ''
PRP Value2 '16V'
PRP ValueDisplayed '0.22µF'
PRP VDC_V '16V'
TOP 0 2.4648561 4.2478768 180 N 424 240 1
TOP 1 2.4648561 4.2085067 180 N 458 11 2
#
# CMP 189
CMP 5 2.6284713 4.2101918 90 N C141 GCM155R71C224KE02D ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM155R71C224KE02%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71C224KE02D'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-10671-1-ND'
PRP Supplier_Part_Number_2 '81-GCM155R71C224KE2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.22uF'
PRP Value1 ''
PRP Value2 '16V'
PRP ValueDisplayed '0.22µF'
PRP VDC_V '16V'
TOP 0 2.6284713 4.2298768 180 N 424 241 1
TOP 1 2.6284713 4.1905067 180 N 458 12 2
#
# CMP 190
CMP 43 2.4632914 2.5504344 90 N C144 GCJ188C70J475KE02J ;0=1,1=0.0000
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP Cap_F '4.7µF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.murata.com/en-us/products/productdetail?partno=GCJ188C70J475KE02%23'
PRP Datasheet 'https://www.murata.com/en-us/products/productdetail?partno=GCJ188C70J475KE02%23'
PRP Datasheet_Path 'datasheets/Cap-GCJ188C70J475KE02J.pdf'
PRP helpURL 'https://upverter.com/upn/revision/50667d1a23a19155/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Murata'
PRP Operating_Temperature_Range '-55°C to +125°C'
PRP PackageReference '0603'
PRP Part_Number 'GCJ188C70J475KE02J'
PRP PartNumber 'GCJ188C70J475KE02J'
PRP RoHS 'TRUE'
PRP SizeZ_mm '1mm'
PRP TempCo '22%'
PRP Temperature_Characteristic 'X7S'
PRP Tolerance__ '10%'
PRP Value '4.7µF'
PRP ValueDisplayed '4.7uF'
PRP VDC_V '6.3V'
TOP 0 2.4632914 2.5809462 90 N 424 242 1
TOP 1 2.4632914 2.5199226 90 N 54 15 2
#
# CMP 191
CMP 8 2.8410011 3.6754421 270 N C146 GCM188R70J225KE22D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '2.2µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM188R70J225KE22%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM188R70J225KE22D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5316-1-ND'
PRP Supplier_Part_Number_2 '81-GCM188R70J225KE2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '2.2uF'
PRP Value1 'Unknown'
PRP Value2 '6.3V'
PRP ValueDisplayed '2.2uF'
PRP VDC_V '6.3V'
TOP 0 2.8410011 3.647883 0 N 424 243 1
TOP 1 2.8410011 3.7030011 0 N 458 13 2
#
# CMP 192
CMP 43 2.2993564 1.9883775 270 N C147 GCJ188C70J475KE02J ;0=1,1=0.0000
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP Cap_F '4.7µF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.murata.com/en-us/products/productdetail?partno=GCJ188C70J475KE02%23'
PRP Datasheet 'https://www.murata.com/en-us/products/productdetail?partno=GCJ188C70J475KE02%23'
PRP Datasheet_Path 'datasheets/Cap-GCJ188C70J475KE02J.pdf'
PRP helpURL 'https://upverter.com/upn/revision/50667d1a23a19155/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Murata'
PRP Operating_Temperature_Range '-55°C to +125°C'
PRP PackageReference '0603'
PRP Part_Number 'GCJ188C70J475KE02J'
PRP PartNumber 'GCJ188C70J475KE02J'
PRP RoHS 'TRUE'
PRP SizeZ_mm '1mm'
PRP TempCo '22%'
PRP Temperature_Characteristic 'X7S'
PRP Tolerance__ '10%'
PRP Value '4.7µF'
PRP ValueDisplayed '4.7uF'
PRP VDC_V '6.3V'
TOP 0 2.2993564 1.9578657 270 N 424 244 1
TOP 1 2.2993564 2.0188893 270 N 13 3 2
#
# CMP 193
CMP 5 2.8385412 3.9865067 0 N C150 GCM155R71C104KA55D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.murata.com/capacitor/product/GCM155R71C104KA55%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71C104KA55D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-4759-2-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '16V'
TOP 0 2.8582262 3.9865067 270 N 424 245 1
TOP 1 2.8188561 3.9865067 270 N 194 1 2
#
# CMP 194
CMP 9 1.9240635 2.5703391 270 N C151 CGA4J1X7T0J226M ;0=1,1=0.0610
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0805'
PRP Cap_F '22µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://sps16.itg.ti.com/sites/KMS/crossdivteams/altium/docs/ComponentDatasheets/TDK datasheet_CGA4J1X7T0J226M (preliminary)_TI 03122019.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'CGA4J1X7T0J226M'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.55'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7T'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '22uF'
PRP Value1 ''
PRP Value2 '6.3V'
PRP ValueDisplayed '22µF'
PRP VDC_V '6.3V'
TOP 0 1.9240635 2.5358903 0 N 57 2 1
TOP 1 1.9240635 2.6047879 0 N 424 246 2
#
# CMP 195
CMP 11 1.7670005 2.5692603 270 N C152 C0805C106J8RACAUTO ;0=1,1=0.0571
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0805'
PRP Cap_F '10µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://content.kemet.com/datasheets/KEM_C1023_X7R_AUTO_SMD.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'Kemet'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'C0805C106J8RACAUTO'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '399-15693-1-ND'
PRP Supplier_Part_Number_2 '80-C0805C106J8RAUTO'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '10uF'
PRP Value1 ''
PRP Value2 '10V'
PRP ValueDisplayed '10µF'
PRP VDC_V '10V'
TOP 0 1.7670005 2.5397327 0 N 57 3 1
TOP 1 1.7670005 2.5987878 0 N 424 247 2
#
# CMP 196
CMP 11 3.1058588 1.8742839 90 N C154 C0805C106J8RACAUTO ;0=1,1=0.0571
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0805'
PRP Cap_F '10µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://content.kemet.com/datasheets/KEM_C1023_X7R_AUTO_SMD.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'Kemet'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'C0805C106J8RACAUTO'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '399-15693-1-ND'
PRP Supplier_Part_Number_2 '80-C0805C106J8RAUTO'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '10uF'
PRP Value1 ''
PRP Value2 '10V'
PRP ValueDisplayed '10µF'
PRP VDC_V '10V'
TOP 0 3.1058588 1.9038115 180 N 16 3 1
TOP 1 3.1058588 1.8447564 180 N 424 248 2
#
# CMP 197
CMP 50 1.4156161 3.6726033 90 N C155 KGM05ACG1H470FH ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP Cap_F '47pF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://spicat.kyocera-avx.com/product/mlcc/chartview/KGM05ACG1H470FH'
PRP Datasheet 'https://spicat.kyocera-avx.com/product/mlcc/chartview/KGM05ACG1H470FH'
PRP Datasheet_Path 'datasheets/Cap-KGM05ACG1H470FH.pdf'
PRP Digikey_Description 'CAP CER 47PF 50V NP0 0402'
PRP Digikey_Part_Number '478-KGM05ACG1H470FHCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/cf39fa6dd43fa591/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'KYOCERA AVX'
PRP Mouser_Part_Number '581-KGM05ACG1H470FH'
PRP Operating_Temperature_Range '-55°C to +125°C'
PRP PackageReference '0402'
PRP Part_Number 'KGM05ACG1H470FH'
PRP PartNumber 'KGM05ACG1H470FH'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.56mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '478-KGM05ACG1H470FHCT-ND'
PRP Supplier_Part_Number_2 '581-KGM05ACG1H470FH'
PRP TempCo '30ppm/°C'
PRP Temperature_Characteristic 'C0G'
PRP Tolerance__ '1%'
PRP Value '47pF'
PRP ValueDisplayed '47pF'
PRP VDC_V '50V'
TOP 0 1.4156161 3.6942568 90 N 424 371 1
TOP 1 1.4156161 3.6509498 90 N 95 2 2
#
# CMP 198
CMP 10 1.0376701 3.6155369 180 N C157 CGA4J2X7R2A104K125AA ;0=1,1=0.0571
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0805'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=CGA4J2X7R2A104K125AA'
PRP CompType 'Capacitor'
PRP ESR_ohm '0.020726'
PRP IRMS_A '1.456A'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'CGA4J2X7R2A104K125AA'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '445-5827-1-ND'
PRP Supplier_Part_Number_2 '810-CGA4J2X7R2A104K125AA'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 '0.020726 ohm'
PRP Value2 '100V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '100V'
TOP 0 0.9976702 3.6155369 0 N 71 1 1
TOP 1 1.0776702 3.6155369 0 N 73 0 2
#
# CMP 199
CMP 8 1.07854 2.8240265 270 N C159 GCM188R71C105KA64D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM188R71C105KA64%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM188R71C105KA64D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5241-6-ND'
PRP Supplier_Part_Number_2 '81-GCM188R71C105K64D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '1uF'
PRP VDC_V '16V'
TOP 0 1.07854 2.7964674 0 N 459 4 1
TOP 1 1.07854 2.8515855 0 N 424 249 2
#
# CMP 200
CMP 10 1.0376701 3.5249874 180 N C161 CGA4J2X7R2A104K125AA ;0=1,1=0.0571
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0805'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=CGA4J2X7R2A104K125AA'
PRP CompType 'Capacitor'
PRP ESR_ohm '0.020726'
PRP IRMS_A '1.456A'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'CGA4J2X7R2A104K125AA'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '445-5827-1-ND'
PRP Supplier_Part_Number_2 '810-CGA4J2X7R2A104K125AA'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 '0.020726 ohm'
PRP Value2 '100V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '100V'
TOP 0 0.9976702 3.5249874 0 N 70 1 1
TOP 1 1.0776702 3.5249874 0 N 72 0 2
#
# CMP 201
CMP 49 1.4543804 3.5220162 0 N C162 KGM05ACG1H220FH ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP Cap_F '22pF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://spicat.kyocera-avx.com/product/mlcc/chartview/KGM05ACG1H220FH'
PRP Datasheet 'https://spicat.kyocera-avx.com/product/mlcc/chartview/KGM05ACG1H220FH'
PRP Datasheet_Path 'datasheets/Cap-KGM05ACG1H220FH.pdf'
PRP Digikey_Description 'CAP CER 22PF 50V C0G/NP0 0402'
PRP Digikey_Part_Number '478-KGM05ACG1H220FHCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/b1505dfd3a8c3c16/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'KYOCERA AVX'
PRP Mouser_Part_Number '581-KGM05ACG1H220FH'
PRP Operating_Temperature_Range '-55°C to +125°C'
PRP PackageReference '0402'
PRP Part_Number 'KGM05ACG1H220FH'
PRP PartNumber 'KGM05ACG1H220FH'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.56mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '478-KGM05ACG1H220FHCT-ND'
PRP Supplier_Part_Number_2 '581-KGM05ACG1H220FH'
PRP TempCo '30ppm/°C'
PRP Temperature_Characteristic 'C0G'
PRP Tolerance__ '1%'
PRP Value '22pF'
PRP ValueDisplayed '22pF'
PRP VDC_V '50V'
TOP 0 1.4760339 3.5220162 180 N 102 1 1
TOP 1 1.4327269 3.5220162 180 N 94 1 2
#
# CMP 202
CMP 5 2.5000099 4.2281918 90 N C163 GCM155R71C224KE02D ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM155R71C224KE02%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71C224KE02D'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-10671-1-ND'
PRP Supplier_Part_Number_2 '81-GCM155R71C224KE2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.22uF'
PRP Value1 ''
PRP Value2 '16V'
PRP ValueDisplayed '0.22µF'
PRP VDC_V '16V'
TOP 0 2.5000099 4.2478768 180 N 424 250 1
TOP 1 2.5000099 4.2085067 180 N 457 10 2
#
# CMP 203
CMP 5 2.584 3.57 270 N C164 GCM155R71C224KE02D ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM155R71C224KE02%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71C224KE02D'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-10671-1-ND'
PRP Supplier_Part_Number_2 '81-GCM155R71C224KE2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.22uF'
PRP Value1 ''
PRP Value2 '16V'
PRP ValueDisplayed '0.22µF'
PRP VDC_V '16V'
TOP 0 2.584 3.550315 0 N 424 368 1
TOP 1 2.584 3.5896851 0 N 457 18 2
#
# CMP 204
CMP 5 2.7898144 4.0964518 90 N C165 GCM155R71C224KE02D ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM155R71C224KE02%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71C224KE02D'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-10671-1-ND'
PRP Supplier_Part_Number_2 '81-GCM155R71C224KE2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.22uF'
PRP Value1 ''
PRP Value2 '16V'
PRP ValueDisplayed '0.22µF'
PRP VDC_V '16V'
TOP 0 2.7898144 4.1161368 180 N 424 251 1
TOP 1 2.7898144 4.0767667 180 N 457 11 2
#
# CMP 205
CMP 50 1.435864 3.4881704 180 N C166 KGM05ACG1H470FH ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP Cap_F '47pF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://spicat.kyocera-avx.com/product/mlcc/chartview/KGM05ACG1H470FH'
PRP Datasheet 'https://spicat.kyocera-avx.com/product/mlcc/chartview/KGM05ACG1H470FH'
PRP Datasheet_Path 'datasheets/Cap-KGM05ACG1H470FH.pdf'
PRP Digikey_Description 'CAP CER 47PF 50V NP0 0402'
PRP Digikey_Part_Number '478-KGM05ACG1H470FHCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/cf39fa6dd43fa591/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'KYOCERA AVX'
PRP Mouser_Part_Number '581-KGM05ACG1H470FH'
PRP Operating_Temperature_Range '-55°C to +125°C'
PRP PackageReference '0402'
PRP Part_Number 'KGM05ACG1H470FH'
PRP PartNumber 'KGM05ACG1H470FH'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.56mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '478-KGM05ACG1H470FHCT-ND'
PRP Supplier_Part_Number_2 '581-KGM05ACG1H470FH'
PRP TempCo '30ppm/°C'
PRP Temperature_Characteristic 'C0G'
PRP Tolerance__ '1%'
PRP Value '47pF'
PRP ValueDisplayed '47pF'
PRP VDC_V '50V'
TOP 0 1.4142105 3.4881704 0 N 94 2 1
TOP 1 1.4575175 3.4881704 0 N 424 372 2
#
# CMP 206
CMP 5 2.2632067 3.6135067 180 N C168 GCM155R71C224KE02D ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM155R71C224KE02%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71C224KE02D'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-10671-1-ND'
PRP Supplier_Part_Number_2 '81-GCM155R71C224KE2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.22uF'
PRP Value1 ''
PRP Value2 '16V'
PRP ValueDisplayed '0.22µF'
PRP VDC_V '16V'
TOP 0 2.2435217 3.6135067 90 N 424 252 1
TOP 1 2.2828918 3.6135067 90 N 457 12 2
#
# CMP 207
CMP 9 2.9053375 2.5728114 270 N C169 CGA4J1X7T0J226M ;0=1,1=0.0610
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0805'
PRP Cap_F '22µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://sps16.itg.ti.com/sites/KMS/crossdivteams/altium/docs/ComponentDatasheets/TDK datasheet_CGA4J1X7T0J226M (preliminary)_TI 03122019.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'CGA4J1X7T0J226M'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.55'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7T'
PRP Tolerance__ '20%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '22uF'
PRP Value1 ''
PRP Value2 '6.3V'
PRP ValueDisplayed '22µF'
PRP VDC_V '6.3V'
TOP 0 2.9053375 2.5383626 0 N 56 3 1
TOP 1 2.9053375 2.6072602 0 N 424 253 2
#
# CMP 208
CMP 5 2.8205412 3.8566577 0 N C170 GCM155R71C224KE02D ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM155R71C224KE02%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71C224KE02D'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-10671-1-ND'
PRP Supplier_Part_Number_2 '81-GCM155R71C224KE2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.22uF'
PRP Value1 ''
PRP Value2 '16V'
PRP ValueDisplayed '0.22µF'
PRP VDC_V '16V'
TOP 0 2.8402262 3.8566577 270 N 424 254 1
TOP 1 2.8008561 3.8566577 270 N 457 13 2
#
# CMP 209
CMP 5 0.7504493 3.166218 180 N C172 GCM155R71C104KA55D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade ''
PRP AEC_Qualified '?'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.murata.com/capacitor/product/GCM155R71C104KA55%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71C104KA55D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-4759-2-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '16V'
TOP 0 0.7307643 3.166218 90 N 424 524 1
TOP 1 0.7701344 3.166218 90 N 19 4 2
#
# CMP 210
CMP 5 2.8505412 4.0305067 0 N C174 GCM155R71C224KE02D ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM155R71C224KE02%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71C224KE02D'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-10671-1-ND'
PRP Supplier_Part_Number_2 '81-GCM155R71C224KE2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.22uF'
PRP Value1 ''
PRP Value2 '16V'
PRP ValueDisplayed '0.22µF'
PRP VDC_V '16V'
TOP 0 2.8702262 4.0305067 270 N 424 255 1
TOP 1 2.8308561 4.0305067 270 N 455 4 2
#
# CMP 211
CMP 5 2.571 3.4811328 0 N C175 GCM155R71C224KE02D ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM155R71C224KE02%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71C224KE02D'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-10671-1-ND'
PRP Supplier_Part_Number_2 '81-GCM155R71C224KE2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.22uF'
PRP Value1 ''
PRP Value2 '16V'
PRP ValueDisplayed '0.22µF'
PRP VDC_V '16V'
TOP 0 2.590685 3.4811328 270 N 424 256 1
TOP 1 2.5513149 3.4811328 270 N 455 5 2
#
# CMP 212
CMP 5 2.5461637 4.2281918 90 N C176 GCM155R71C224KE02D ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM155R71C224KE02%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71C224KE02D'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-10671-1-ND'
PRP Supplier_Part_Number_2 '81-GCM155R71C224KE2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.22uF'
PRP Value1 ''
PRP Value2 '16V'
PRP ValueDisplayed '0.22µF'
PRP VDC_V '16V'
TOP 0 2.5461637 4.2478768 180 N 424 257 1
TOP 1 2.5461637 4.2085067 180 N 455 6 2
#
# CMP 213
CMP 5 2.571 3.516 0 N C177 GCM155R71C224KE02D ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '220nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM155R71C224KE02%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71C224KE02D'
PRP Polarized 'N'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-10671-1-ND'
PRP Supplier_Part_Number_2 '81-GCM155R71C224KE2D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value '0.22uF'
PRP Value1 ''
PRP Value2 '16V'
PRP ValueDisplayed '0.22µF'
PRP VDC_V '16V'
TOP 0 2.590685 3.516 270 N 424 258 1
TOP 1 2.5513149 3.516 270 N 455 7 2
#
# CMP 214
CMP 5 2.1292656 3.9304099 0 N C180 CGA2B3X7R1H473K050BB ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '47nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=CGA2B3X7R1H473K050BB'
PRP CompType 'Capacitor'
PRP ESR_ohm '0.06407'
PRP IRMS_A '646.122mA'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'TDK'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CGA2B3X7R1H473K050BB'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '445-6897-1-ND'
PRP Supplier_Part_Number_2 '810-CGA2B3X7R1H473K050BB'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.047uF'
PRP Value1 '0.06407 ohm'
PRP Value2 '50V'
PRP ValueDisplayed '0.047uF'
PRP VDC_V '50V'
TOP 0 2.1489506 3.9304099 270 N 264 1 1
TOP 1 2.1095805 3.9304099 270 N 424 522 2
#
# CMP 215
CMP 8 1.2453626 2.4360744 180 N C183 GCM188R71C105KA64D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM188R71C105KA64%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM188R71C105KA64D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5241-6-ND'
PRP Supplier_Part_Number_2 '81-GCM188R71C105K64D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '1uF'
PRP VDC_V '16V'
TOP 0 1.2178035 2.4360744 90 N 261 3 1
TOP 1 1.2729216 2.4360744 90 N 424 259 2
#
# CMP 216
CMP 8 1.4405872 2.5135252 180 N C186 GCM188R71C105KA64D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM188R71C105KA64%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM188R71C105KA64D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5241-6-ND'
PRP Supplier_Part_Number_2 '81-GCM188R71C105K64D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '1uF'
PRP VDC_V '16V'
TOP 0 1.4130281 2.5135252 90 N 261 4 1
TOP 1 1.4681462 2.5135252 90 N 424 260 2
#
# CMP 217
CMP 8 0.9250348 2.6451464 0 N C187 GCM188R71C105KA64D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM188R71C105KA64%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM188R71C105KA64D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5241-6-ND'
PRP Supplier_Part_Number_2 '81-GCM188R71C105K64D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '1uF'
PRP VDC_V '16V'
TOP 0 0.9525939 2.6451464 270 N 456 3 1
TOP 1 0.8974758 2.6451464 270 N 424 261 2
#
# CMP 218
CMP 8 1.284196 2.3153188 90 N C190 GCM188R71C105KA64D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM188R71C105KA64%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM188R71C105KA64D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5241-6-ND'
PRP Supplier_Part_Number_2 '81-GCM188R71C105K64D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '1uF'
PRP VDC_V '16V'
TOP 0 1.284196 2.3428779 180 N 459 5 1
TOP 1 1.284196 2.2877598 180 N 424 262 2
#
# CMP 219
CMP 8 1.2850165 2.4970747 0 N C192 GCM188R71C105KA64D ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0603'
PRP Cap_F '1µF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://psearch.en.murata.com/capacitor/product/GCM188R71C105KA64%23.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'GCM188R71C105KA64D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeAreaWB_mm2 '4.68'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '490-5241-6-ND'
PRP Supplier_Part_Number_2 '81-GCM188R71C105K64D'
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '1uF'
PRP Value1 'Unknown'
PRP Value2 '16V'
PRP ValueDisplayed '1uF'
PRP VDC_V '16V'
TOP 0 1.3125756 2.4970747 270 N 459 6 1
TOP 1 1.2574575 2.4970747 270 N 424 263 2
#
# CMP 220
CMP 5 1.2753204 2.6304593 0 N C193 GCM155R71A104KA55D ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case '0402'
PRP Cap_F '100nF'
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GCM155R71A104KA55-01.pdf'
PRP CompType 'Capacitor'
PRP ESR_ohm ''
PRP IRMS_A ''
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'GCM155R71A104KA55D'
PRP Polarized 'N'
PRP Published '2008-06-19'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Mouser'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '81-GCM155R71A104K5D'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-55°C'
PRP Technology 'Ceramic'
PRP TempCo 'X7R'
PRP Tolerance__ '10%'
PRP U/M 'EA'
PRP Value '0.1uF'
PRP Value1 'Unknown'
PRP Value2 '10V'
PRP ValueDisplayed '0.1uF'
PRP VDC_V '10V'
TOP 0 1.2950054 2.6304593 270 N 459 7 1
TOP 1 1.2556353 2.6304593 270 N 424 264 2
#
# CMP 221
CMP 77 1.610482 4.0799415 90 N D5 SMS3923-040LF ;0=1,1=0.0197
PRP AEC_Category 'Q101'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.skyworksinc.com/uploads/documents/SMS392x_Series_200042AC.pdf'
PRP CompType 'Diode'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Io_A '10mA'
PRP Manufacturer 'Skyworks Solutions'
PRP MountType 'SMT'
PRP PackageReference 'SOD-882'
PRP PartNumber 'SMS3923-040LF'
PRP RJC_CperW ''
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.6'
PRP SizeAreaWB_mm2 '3.2'
PRP SizeX_mm '1'
PRP SizeY_mm '0.6'
PRP SizeZ_mm '0.5'
PRP TJmax_C '150°C'
PRP Type 'Schottky'
PRP Value 'V'
PRP Value1 '0.01A'
PRP Value2 '0.34V'
PRP Vf_V '340mV'
PRP Vr_V ''
TOP 0 1.610482 4.0961816 90 N 367 0 1
TOP 1 1.610482 4.0637014 90 N 267 0 2
#
# CMP 222
CMP 72 2.2900011 4.6890011 270 N D6 SML-LXT0805GW-TR ;0=1,1=0.0315
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Angle '140'
PRP Color 'Green'
PRP ColorTemperature ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.lumex.com/content/files/ProductAttachment/SML-LXT0805GW-TR.pdf'
PRP CompType 'LED'
PRP DynamicResistance ''
PRP Family_Io ''
PRP FamilyName ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Io_A '20mA'
PRP Ir_A '100µA'
PRP LambdaD ''
PRP LambdaP ''
PRP Luminance_Lv ''
PRP LuminousFlux_PhiV ''
PRP LuminousIntensity_IV ''
PRP Manufacturer 'Lumex'
PRP MountType 'SMT'
PRP NumParallelLEDs ''
PRP NumSeriesLEDs ''
PRP PackageReference '0805'
PRP PartNumber 'SML-LXT0805GW-TR'
PRP Power_TotalModule '50mW'
PRP RJC_CperW ''
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.5'
PRP SizeAreaWB_mm2 '6.75'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '0.8'
PRP TJmax_C '80°C'
PRP Type '?'
PRP Value 'Green'
PRP Value1 '0.05W'
PRP Value2 '2V'
PRP Vf_V '2V'
PRP Vr_V '5V'
TOP 0 2.2900011 4.6476625 270 N 191 1 1
TOP 1 2.2900011 4.7303397 270 N 424 364 2
#
# CMP 223
CMP 30 2.13 3.407 270 N FID1 Fiducial ;0=1,1=0.0010
PRP ClassName 'FiducialMark'
PRP CompType 'Fiducial'
PRP Manufacturer 'N/A'
PRP MountType 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 2.13 3.407 270 N 0 47 1
#
# CMP 224
CMP 30 2.817 4.266 270 N FID2 Fiducial ;0=1,1=0.0010
PRP ClassName 'FiducialMark'
PRP CompType 'Fiducial'
PRP Manufacturer 'N/A'
PRP MountType 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 2.817 4.266 270 N 0 0 1
#
# CMP 225
CMP 30 0.3610005 0.1118115 270 N FID4 Fiducial ;0=1,1=0.0010
PRP ClassName 'FiducialMark'
PRP CompType 'Fiducial'
PRP Manufacturer 'N/A'
PRP MountType 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 0.3610005 0.1118115 270 N 0 1 1
#
# CMP 226
CMP 30 2.1950005 0.1218115 270 N FID5 Fiducial ;0=1,1=0.0010
PRP ClassName 'FiducialMark'
PRP CompType 'Fiducial'
PRP Manufacturer 'N/A'
PRP MountType 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 2.1950005 0.1218115 270 N 0 2 1
#
# CMP 227
CMP 30 0.2499996 5.0968424 270 N FID7 Fiducial ;0=1,1=0.0010
PRP ClassName 'FiducialMark'
PRP CompType 'Fiducial'
PRP Manufacturer 'N/A'
PRP MountType 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 0.2499996 5.0968424 270 N 0 3 1
#
# CMP 228
CMP 30 0.250001 -0.1755887 270 N FID13 Fiducial ;0=1,1=0.0010
PRP ClassName 'FiducialMark'
PRP CompType 'Fiducial'
PRP Manufacturer 'N/A'
PRP MountType 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 0.250001 -0.1755887 270 N 0 4 1
#
# CMP 229
CMP 30 0.1565493 4.7729139 270 N FID9 Fiducial ;0=1,1=0.0010
PRP ClassName 'FiducialMark'
PRP CompType 'Fiducial'
PRP Manufacturer 'N/A'
PRP MountType 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 0.1565493 4.7729139 270 N 0 5 1
#
# CMP 230
CMP 30 3.0964513 -0.175589 270 N FID15 Fiducial ;0=1,1=0.0010
PRP ClassName 'FiducialMark'
PRP CompType 'Fiducial'
PRP Manufacturer 'N/A'
PRP MountType 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 3.0964513 -0.175589 270 N 0 6 1
#
# CMP 231
CMP 30 3.0964499 5.0968421 270 N FID11 Fiducial ;0=1,1=0.0010
PRP ClassName 'FiducialMark'
PRP CompType 'Fiducial'
PRP Manufacturer 'N/A'
PRP MountType 'N/A'
PRP PackageReference 'N/A'
PRP PartNumber 'N/A'
TOP 0 3.0964499 5.0968421 270 N 0 7 1
#
# CMP 232
CMP 17 3.236215 1.2980426 90 N J8 105017-0001 ;0=1,1=0.1142
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'FALSE'
PRP Color ''
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.molex.com/pdm_docs/sd/1050170001_sd.pdf'
PRP CompType 'USB'
PRP ContactFinish ''
PRP CT 'TRUE'
PRP Current_A ''
PRP Gender 'Female'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Molex'
PRP MountType 'SMT'
PRP Note ''
PRP Orientation ''
PRP PackageReference 'Micro USB receptacle'
PRP PartNumber '105017-0001'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'WM1399CT-ND'
PRP Supplier_Part_Number_2 '78R1699'
PRP Supplier_Part_Number_3 '538-105017-0001'
PRP Voltage_V ''
TOP 0 3.1830653 1.3492236 180 N 348 1 1
TOP 1 3.1830653 1.3236331 180 N 249 0 2
TOP 2 3.1830653 1.2980425 180 N 248 0 3
TOP 3 3.1830653 1.2724519 180 N 247 0 4
TOP 4 3.1830653 1.2468614 180 N 347 1 5
TOP 5 3.2893645 1.4358378 180 N 424 526 6
TOP 6 3.2893645 1.3374126 180 N 0 44 7
TOP 7 3.2893645 1.2586724 180 N 0 43 8
TOP 8 3.2893645 1.1602472 180 N 424 527 9
TOP 9 3.1830653 1.1996173 90 N 424 528 10
TOP 10 3.1830653 1.3964677 90 N 424 529 11
#
# CMP 233
CMP 51 0.2792547 2.5529326 270 N J9 LPJG16414A4NL ;0=2,1=0.0010
PRP AEC_Qualified 'No'
PRP Conn_Gender 'Female'
PRP Conn_Orientation 'Horizontal'
PRP ContactFinish 'Gold'
PRP Datasheet_Path 'datasheets/Conn_LPJG16414A4NL.pdf'
PRP DUT-Pitch_mm '1.27mm'
PRP helpURL 'https://upverter.com/upn/revision/c539a529bedc0c6c/'
PRP Is_Female 'yes'
PRP Lead_Free 'Yes'
PRP Manufacturer 'LINK-PP'
PRP Operating_Temperature_Range '-40°C to +85°C'
PRP PackageReference 'CONN_RJ45'
PRP PartNumber 'LPJG16414A4NL'
PRP PinCount '8'
PRP RoHS 'TRUE'
PRP Shrouded 'true'
TOP 0 0.634176 2.3279326 270 N 205 1 1
TOP 1 0.534176 2.3779326 270 N 204 0 2
TOP 2 0.634176 2.4279326 270 N 276 0 3
TOP 3 0.534176 2.4779326 270 N 277 0 4
TOP 4 0.634176 2.5279326 270 N 278 0 5
TOP 5 0.534176 2.5779326 270 N 279 0 6
TOP 6 0.634176 2.6279326 270 N 280 0 7
TOP 7 0.534176 2.6779326 270 N 281 0 8
TOP 8 0.634176 2.7279326 270 N 282 0 9
TOP 9 0.534176 2.7779326 270 N 283 0 10
TOP 10 0.184176 2.8176964 270 N 203 1 11
TOP 11 0.1042547 2.8176964 270 N 424 534 12
TOP 12 0.184176 2.2881688 270 N 424 533 13
TOP 13 0.1042547 2.2881688 270 N 224 1 14
TOP 14 0.4042547 2.2428932 270 N 202 2 15
TOP 15 0.4042547 2.862972 270 N 182 2 16
TOP 16 0.284176 2.7779326 270 N 0 149 empty-1
TOP 17 0.284176 2.3279326 270 N 0 148 empty-2
#
# CMP 234
CMP 17 0.1102366 4.3862128 270 N J10 105017-0001 ;0=1,1=0.1142
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'FALSE'
PRP Color ''
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.molex.com/pdm_docs/sd/1050170001_sd.pdf'
PRP CompType 'USB'
PRP ContactFinish ''
PRP CT 'TRUE'
PRP Current_A ''
PRP Gender 'Female'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Molex'
PRP MountType 'SMT'
PRP Note ''
PRP Orientation ''
PRP PackageReference 'Micro USB receptacle'
PRP PartNumber '105017-0001'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'WM1399CT-ND'
PRP Supplier_Part_Number_2 '78R1699'
PRP Supplier_Part_Number_3 '538-105017-0001'
PRP Voltage_V ''
TOP 0 0.1633863 4.3350318 0 N 346 1 1
TOP 1 0.1633863 4.3606223 0 N 429 0 2
TOP 2 0.1633863 4.3862129 0 N 428 0 3
TOP 3 0.1633863 4.4118035 0 N 427 0 4
TOP 4 0.1633863 4.437394 0 N 424 265 5
TOP 5 0.0570871 4.2484176 0 N 345 6 6
TOP 6 0.0570871 4.3468428 0 N 345 4 7
TOP 7 0.0570871 4.425583 0 N 345 5 8
TOP 8 0.0570871 4.5240082 0 N 345 7 9
TOP 9 0.1633863 4.4846381 270 N 345 8 10
TOP 10 0.1633863 4.2877877 270 N 345 9 11
#
# CMP 235
CMP 18 3.0905755 0.3274885 180 N J12 PJ-063AH ;0=2,1=0.3622
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL 'Y'
PRP Cert_VDE ''
PRP ClassName ''
PRP Color 'Black'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.cui.com/product/resource/pj-063ah.pdf'
PRP CompType 'Power Jack'
PRP ContactFinish ''
PRP Current_A '8A'
PRP Gender 'Male'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'CUI Inc.'
PRP MountType 'TH'
PRP Note ''
PRP Orientation 'R/A'
PRP PackageReference 'DC POWER JACK, R/A, TH'
PRP PartNumber 'PJ-063AH'
PRP PinCount '2'
PRP Pitch_mm ''
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded 'Y'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'CP-063AH-ND'
PRP Supplier_Part_Number_2 '490-PJ-063AH'
PRP Supplier_Part_Number_3 ''
PRP Voltage_V '24V'
TOP 0 2.9134102 0.3274885 90 N 370 1 1
TOP 1 3.1496306 0.3274885 90 N 424 530 2
TOP 2 3.2677409 0.3274885 180 N 0 147 ALIGN
TOP 3 3.1890007 0.5046539 180 N 424 531 S1
TOP 4 3.1890007 0.1503231 180 N 424 532 S2
#
# CMP 236
CMP 14 3.1335011 4.7095011 0 N J13 142-0711-201 ;0=1,1=0.3530
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP Color 'Gold'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'https://belfuse.com/resources/Johnson/productinformation/pi-142-0711-201.pdf'
PRP CompType 'SMA'
PRP ContactFinish 'Gold'
PRP Current_A ''
PRP Gender 'Female'
PRP Green_EU_RoHS 'Incomplete'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Not Set'
PRP Green_REACh 'Incomplete'
PRP Manufacturer 'Cinch Connectivity'
PRP MountType 'SMT'
PRP Note ''
PRP Orientation 'Vertical'
PRP PackageReference 'SMA'
PRP PartNumber '142-0711-201'
PRP PinCount '2'
PRP Pitch_mm ''
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Voltage_V ''
TOP 0 3.1335011 4.7095011 180 N 275 0 1
TOP 1 3.0400011 4.6160011 180 N 424 318 2
TOP 2 3.0400011 4.8030011 180 N 424 319 2
TOP 3 3.2270011 4.6160011 180 N 424 320 2
TOP 4 3.2270011 4.8030011 180 N 424 321 2
#
# CMP 237
CMP 70 0.5102892 1.6511308 180 N J19 Receptacle_30x2_4MP_LeftRight ;0=1,1=0.1310
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'False'
PRP Color 'Black'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.samtec.com/ftppub/cpdf/QSH-XXX-01-X-D-XX-MKT.pdf'
PRP CompType 'Receptacle'
PRP ContactFinish 'Gold'
PRP CT 'False'
PRP Current_A ''
PRP Gender 'Female'
PRP Green_EU_RoHS 'Passed with Exemption'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '2017-07-12'
PRP Manufacturer 'Samtec'
PRP MountType 'SMT'
PRP Note ''
PRP Orientation 'Vertical'
PRP PackageReference 'Receptacle, 0.5 mm, 30x2, TH'
PRP PartNumber 'QSH-030-01-L-D-A'
PRP PinCount '60'
PRP Pitch_mm '0.5'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count '2'
PRP RowSpacing_mm '5.73'
PRP Shrouded 'N'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 'SAM8180-ND'
PRP Supplier_Part_Number_2 '19M9181'
PRP Supplier_Part_Number_3 '1667876'
PRP Voltage_V ''
TOP 0 0.3974939 1.3656977 270 N 409 1 1
TOP 1 0.6230845 1.3656977 270 N 226 0 2
TOP 2 0.3974939 1.3853827 270 N 411 0 3
TOP 3 0.6230845 1.3853827 270 N 448 0 4
TOP 4 0.3974939 1.4050678 270 N 227 0 5
TOP 5 0.6230845 1.4050678 270 N 412 0 6
TOP 6 0.3974939 1.4247528 270 N 184 0 7
TOP 7 0.6230845 1.4247528 270 N 410 0 8
TOP 8 0.3974939 1.4444379 270 N 413 0 9
TOP 9 0.6230845 1.4444379 270 N 0 21 10
TOP 10 0.3974939 1.4641229 270 N 0 8 11
TOP 11 0.6230845 1.4641229 270 N 409 0 12
TOP 12 0.3974939 1.4838079 270 N 58 0 13
TOP 13 0.6230845 1.4838079 270 N 0 22 14
TOP 14 0.3974939 1.503493 270 N 414 0 15
TOP 15 0.6230845 1.503493 270 N 424 270 16
TOP 16 0.3974939 1.523178 270 N 123 0 17
TOP 17 0.6230845 1.523178 270 N 0 23 18
TOP 18 0.3974939 1.5428631 270 N 122 0 19
TOP 19 0.6230845 1.5428631 270 N 0 24 20
TOP 20 0.3974939 1.5625481 270 N 121 0 21
TOP 21 0.6230845 1.5625481 270 N 0 25 22
TOP 22 0.3974939 1.5822331 270 N 120 0 23
TOP 23 0.6230845 1.5822331 270 N 0 26 24
TOP 24 0.3974939 1.6019182 270 N 119 0 25
TOP 25 0.6230845 1.6019182 270 N 0 27 26
TOP 26 0.3974939 1.6216032 270 N 118 0 27
TOP 27 0.6230845 1.6216032 270 N 0 28 28
TOP 28 0.3974939 1.6412883 270 N 117 0 29
TOP 29 0.6230845 1.6412883 270 N 0 29 30
TOP 30 0.3974939 1.6609733 270 N 116 0 31
TOP 31 0.6230845 1.6609733 270 N 0 30 32
TOP 32 0.3974939 1.6806583 270 N 115 0 33
TOP 33 0.6230845 1.6806583 270 N 0 31 34
TOP 34 0.3974939 1.7003434 270 N 0 9 35
TOP 35 0.6230845 1.7003434 270 N 0 32 36
TOP 36 0.3974939 1.7200284 270 N 0 10 37
TOP 37 0.6230845 1.7200284 270 N 0 33 38
TOP 38 0.3974939 1.7397135 270 N 0 11 39
TOP 39 0.6230845 1.7397135 270 N 0 34 40
TOP 40 0.3974939 1.7593985 270 N 0 12 41
TOP 41 0.6230845 1.7593985 270 N 424 269 42
TOP 42 0.3974939 1.7790835 270 N 0 13 43
TOP 43 0.6230845 1.7790835 270 N 0 35 44
TOP 44 0.3974939 1.7987685 270 N 0 14 45
TOP 45 0.6230845 1.7987685 270 N 0 36 46
TOP 46 0.3974939 1.8184536 270 N 0 15 47
TOP 47 0.6230845 1.8184536 270 N 424 268 48
TOP 48 0.3974939 1.8381387 270 N 0 16 49
TOP 49 0.6230845 1.8381387 270 N 0 37 50
TOP 50 0.3974939 1.8578237 270 N 0 17 51
TOP 51 0.6230845 1.8578237 270 N 0 38 52
TOP 52 0.3974939 1.8775087 270 N 0 18 53
TOP 53 0.6230845 1.8775087 270 N 424 267 54
TOP 54 0.3974939 1.8971937 270 N 0 19 55
TOP 55 0.6230845 1.8971937 270 N 0 39 56
TOP 56 0.3974939 1.9168788 270 N 424 271 57
TOP 57 0.6230845 1.9168788 270 N 28 0 58
TOP 58 0.3974939 1.9365639 270 N 0 20 59
TOP 59 0.6230845 1.9365639 270 N 424 266 60
TOP 60 0.6154073 1.254871 270 N 0 145 MH1
TOP 61 0.6154073 2.0473906 270 N 0 146 MH2
TOP 62 0.5102892 1.3336111 270 N 424 272 MP1
TOP 63 0.5102892 1.5261309 270 N 424 273 MP2
TOP 64 0.5102892 1.7761307 90 N 424 274 MP3
TOP 65 0.5102892 1.9686505 90 N 424 275 MP4
#
# CMP 238
CMP 80 1.3870005 1.6888115 0 N J21 GBC01SFBN-M30 ;0=1,1=0.4925
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL 'Y'
PRP Cert_VDE ''
PRP ClassName 'Header'
PRP Color 'Black'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'https://drawings-pdf.s3.amazonaws.com/C10058.pdf'
PRP CompType 'Header'
PRP ContactFinish 'Gold'
PRP Current_A '3A'
PRP Gender 'Male'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Sullins Connector Solutions'
PRP MountType 'SMT'
PRP Note ''
PRP Orientation 'Vertical'
PRP PackageReference 'Header, 1x1, SMT'
PRP PartNumber 'GBC01SFBN-M30'
PRP PinCount '1'
PRP Pitch_mm ''
PRP RoHS 'Y'
PRP Row_Count '1'
PRP RowSpacing_mm ''
PRP Shrouded 'N'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Voltage_V ''
TOP 0 1.3870005 1.7888115 180 N 424 365 1
#
# CMP 239
CMP 88 2.5463564 2.0678814 90 N L2 VCTA20161B-R47MS6 ;0=1,1=0.0472
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.cyntec.com/upfile/products/download/VCTA20161B.pdf'
PRP CompType 'Inductor'
PRP DCR_ohm '0.025'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Imax_A '4A'
PRP Ind_H '470nH'
PRP Irms '4A @ 40C rise'
PRP Isat '4.8A @ 30% inductance drop'
PRP LatestRevisionDate '2017-06-02'
PRP Manufacturer 'Cyntec'
PRP Material '?'
PRP MountType 'SMT'
PRP PackageReference '2.0x1.6x1.2mm'
PRP PartNumber 'VCTA20161B-R47MS6'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '3.2'
PRP SizeAreaWB_mm2 '7.8'
PRP SizeX_mm '2'
PRP SizeY_mm '1.6'
PRP SizeZ_mm '1.2'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology '?'
PRP Value '470nH'
PRP Value1 '0.025 ohm'
PRP Value2 '4A'
PRP ValueDisplayed '470nH'
TOP 0 2.5463564 2.0993775 90 N 142 1 1
TOP 1 2.5463564 2.0363853 90 N 454 11 2
#
# CMP 240
CMP 5 0.5837885 4.2211046 180 N L3 BLM15HG601SN1D ;0=1,1=0.0236
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://www.murata.com/en-global/products/productdata/8796740223006/ENFA0024.pdf'
PRP CompType 'Ferrite Bead'
PRP DCR_ohm '7d'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Imax_A '3dA'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'BLM15HG601SN1D'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-3998-1-ND'
PRP Supplier_Part_Number_2 '73M9049'
PRP Supplier_Part_Number_3 '81-BLM15HG601SN1D'
PRP Value '600 ohm'
PRP Value1 '0.7 ohm'
PRP Value2 '0.3A'
PRP ValueDisplayed '600 ohm'
PRP Ztyp@1GHz_Ohm '1k'
PRP ZTyp@100MHz_Ohm '600'
TOP 0 0.5641035 4.2211046 90 N 436 7 1
TOP 1 0.6034736 4.2211046 90 N 259 1 2
#
# CMP 241
CMP 5 0.5845365 4.3195298 180 N L4 BLM15HG601SN1D ;0=1,1=0.0236
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://www.murata.com/en-global/products/productdata/8796740223006/ENFA0024.pdf'
PRP CompType 'Ferrite Bead'
PRP DCR_ohm '7d'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Imax_A '3dA'
PRP Manufacturer 'MuRata'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'BLM15HG601SN1D'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeAreaWB_mm2 '3'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '490-3998-1-ND'
PRP Supplier_Part_Number_2 '73M9049'
PRP Supplier_Part_Number_3 '81-BLM15HG601SN1D'
PRP Value '600 ohm'
PRP Value1 '0.7 ohm'
PRP Value2 '0.3A'
PRP ValueDisplayed '600 ohm'
PRP Ztyp@1GHz_Ohm '1k'
PRP ZTyp@100MHz_Ohm '600'
TOP 0 0.5648515 4.3195298 90 N 436 8 1
TOP 1 0.6042216 4.3195298 90 N 258 1 2
#
# CMP 242
CMP 40 1.2142291 3.5702625 0 N L7 DLW32MH101XT2 ;0=1,1=0.0000
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.murata.com/en-global/products/productdetail?partno=DLW32MH101XT2%23'
PRP Datasheet 'https://www.murata.com/en-global/products/productdetail?partno=DLW32MH101XT2%23'
PRP Datasheet_Path 'datasheets/Ind-DLW32MH101XT2.pdf'
PRP DCR_ohm '3.12'
PRP helpURL 'https://upverter.com/upn/revision/cff661865344cba9/'
PRP Imax_A '100mA'
PRP Ind_H '100µH'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Murata'
PRP Mouser_Part_Number '81-DLW32MH101XT2L'
PRP Operating_Temperature_Range '-40°C to +125°C'
PRP PackageReference '1210'
PRP Part_Number 'DLW32MH101XT2'
PRP PartNumber 'DLW32MH101XT2'
PRP RoHS 'TRUE'
PRP SizeZ_mm '2.5mm'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_2 '81-DLW32MH101XT2L'
PRP Technology 'Wirewound'
PRP Test_Frequency '100kHz'
PRP Tolerance__ '-25/+50%'
TOP 0 1.2742685 3.5505775 180 N 74 2 1
TOP 1 1.1541897 3.5505775 180 N 72 1 2
TOP 2 1.1541897 3.5899475 180 N 73 1 3
TOP 3 1.2742685 3.5899475 180 N 75 2 4
#
# CMP 243
CMP 88 2.23478 2.4550011 0 N L8 VCTA20161B-R47MS6 ;0=1,1=0.0472
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.cyntec.com/upfile/products/download/VCTA20161B.pdf'
PRP CompType 'Inductor'
PRP DCR_ohm '0.025'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Imax_A '4A'
PRP Ind_H '470nH'
PRP Irms '4A @ 40C rise'
PRP Isat '4.8A @ 30% inductance drop'
PRP LatestRevisionDate '2017-06-02'
PRP Manufacturer 'Cyntec'
PRP Material '?'
PRP MountType 'SMT'
PRP PackageReference '2.0x1.6x1.2mm'
PRP PartNumber 'VCTA20161B-R47MS6'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '3.2'
PRP SizeAreaWB_mm2 '7.8'
PRP SizeX_mm '2'
PRP SizeY_mm '1.6'
PRP SizeZ_mm '1.2'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology '?'
PRP Value '470nH'
PRP Value1 '0.025 ohm'
PRP Value2 '4A'
PRP ValueDisplayed '470nH'
TOP 0 2.2662761 2.4550011 180 N 143 1 1
TOP 1 2.2032839 2.4550011 180 N 144 7 2
#
# CMP 244
CMP 88 2.5900408 2.4550011 180 N L9 VCTA20161B-R47MS6 ;0=1,1=0.0472
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.cyntec.com/upfile/products/download/VCTA20161B.pdf'
PRP CompType 'Inductor'
PRP DCR_ohm '0.025'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Imax_A '4A'
PRP Ind_H '470nH'
PRP Irms '4A @ 40C rise'
PRP Isat '4.8A @ 30% inductance drop'
PRP LatestRevisionDate '2017-06-02'
PRP Manufacturer 'Cyntec'
PRP Material '?'
PRP MountType 'SMT'
PRP PackageReference '2.0x1.6x1.2mm'
PRP PartNumber 'VCTA20161B-R47MS6'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '3.2'
PRP SizeAreaWB_mm2 '7.8'
PRP SizeX_mm '2'
PRP SizeY_mm '1.6'
PRP SizeZ_mm '1.2'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology '?'
PRP Value '470nH'
PRP Value1 '0.025 ohm'
PRP Value2 '4A'
PRP ValueDisplayed '470nH'
TOP 0 2.5585447 2.4550011 0 N 76 1 1
TOP 1 2.6215369 2.4550011 0 N 309 8 2
#
# CMP 245
CMP 5 2.5956362 0.8419953 270 N R2 CRCW04027K50FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04027K50FKED'
PRP Power_W '63mW'
PRP Res_ohm '7.5k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-7.50KLCT-ND'
PRP Supplier_Part_Number_2 '52K7245'
PRP Supplier_Part_Number_3 '71-CRCW0402-7.5K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '7.50k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '7k50'
PRP ValueDisplayed '7.50k'
PRP VDC_V '50V'
TOP 0 2.5956362 0.8223103 0 N 424 276 1
TOP 1 2.5956362 0.8616804 0 N 153 0 2
#
# CMP 246
CMP 42 2.5230011 4.3586862 90 N R3 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 2.5230011 4.3788633 90 N 406 1 1
TOP 1 2.5230011 4.338509 90 N 152 1 2
#
# CMP 247
CMP 1 2.5825772 3.097 180 N R5 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 2.5715536 3.097 90 N 29 0 1
TOP 1 2.5936008 3.097 90 N 168 0 2
#
# CMP 248
CMP 42 2.5739158 3.132 0 N R6 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 2.5940929 3.132 180 N 168 2 1
TOP 1 2.5537386 3.132 180 N 11 1 2
#
# CMP 249
CMP 5 1.1617484 3.2222836 180 N R11 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 1.1420634 3.2222836 90 N 308 17 1
TOP 1 1.1814335 3.2222836 90 N 44 1 2
#
# CMP 250
CMP 1 1.2080005 3.3448351 90 N R12 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 1.2080005 3.3558587 180 N 145 2 1
TOP 1 1.2080005 3.3338115 180 N 43 0 2
#
# CMP 251
CMP 5 2.9790011 3.3969775 270 N R17 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP INSTALLATION 'DNP'
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 2.9790011 3.3772925 0 N 424 277 1
TOP 1 2.9790011 3.4166626 0 N 53 0 2
#
# CMP 252
CMP 42 1.9819775 4.4558096 180 N R18 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 1.9618004 4.4558096 0 N 388 1 1
TOP 1 2.0021547 4.4558096 0 N 22 1 2
#
# CMP 253
CMP 42 2.6491971 3.3983263 90 N R19 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 2.6491971 3.4185034 90 N 130 2 1
TOP 1 2.6491971 3.3781491 90 N 167 0 2
#
# CMP 254
CMP 42 2.1333154 2.3578115 0 N R20 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 2.1534925 2.3578115 180 N 100 1 1
TOP 1 2.1131382 2.3578115 180 N 175 17 2
#
# CMP 255
CMP 42 2.3446114 3.2277548 90 N R21 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 2.3446114 3.2479319 90 N 37 2 1
TOP 1 2.3446114 3.2075776 90 N 237 0 2
#
# CMP 256
CMP 42 2.1850011 3.276316 270 N R22 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 2.1850011 3.2561389 270 N 107 2 1
TOP 1 2.1850011 3.2964932 270 N 128 3 2
#
# CMP 257
CMP 42 2.3879864 3.2277548 90 N R24 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 2.3879864 3.2479319 90 N 37 3 1
TOP 1 2.3879864 3.2075776 90 N 166 0 2
#
# CMP 258
CMP 42 2.516 3.225 90 N R25 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 2.516 3.2451771 90 N 36 2 1
TOP 1 2.516 3.2048228 90 N 238 0 2
#
# CMP 259
CMP 5 3.1625045 2.0271981 0 N R32 CRCW040210R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '10.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '541-10.2LCT-ND'
PRP Supplier_Part_Number_2 '71-CRCW0402-10.2-E3'
PRP Supplier_Part_Number_3 '1158303'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10R2'
PRP ValueDisplayed '10.2'
PRP VDC_V '50V'
TOP 0 3.1821895 2.0271981 270 N 16 4 1
TOP 1 3.1428194 2.0271981 270 N 381 1 2
#
# CMP 260
CMP 42 2.7468378 2.12582 0 N R27 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 2.7670149 2.12582 180 N 343 1 1
TOP 1 2.7266606 2.12582 180 N 406 2 2
#
# CMP 261
CMP 42 2.6740011 3.2417389 90 N R28 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 2.6740011 3.261916 90 N 131 2 1
TOP 1 2.6740011 3.2215617 90 N 408 0 2
#
# CMP 262
CMP 42 2.7465518 2.092894 0 N R29 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 2.7667289 2.092894 180 N 342 1 1
TOP 1 2.7263746 2.092894 180 N 405 2 2
#
# CMP 263
CMP 13 3.2499844 2.0482296 90 N R30 CSNL1206FT1L00 ;0=1,1=0.0531
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://www.seielect.com/Catalog/SEI-csnl.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Stackpole Electronics Inc'
PRP MountType 'SMT'
PRP PackageReference '1206'
PRP PartNumber 'CSNL1206FT1L00'
PRP Power_W '1W'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '1m'
PRP RoHS 'Y'
PRP SizeArea_mm2 '5.12'
PRP SizeX_mm '3.2'
PRP SizeY_mm '1.6'
PRP SizeZ_mm '1.35'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'CSNL1206FT1L00CT-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Metal Element'
PRP TempCo '50 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '0.001'
PRP Value1 '1%'
PRP Value2 '1W'
PRP Value_Code '1L000'
PRP ValueDisplayed '0.001'
PRP VDC_V ''
TOP 0 3.2499844 2.1013792 180 N 458 14 1
TOP 1 3.2499844 1.99508 180 N 16 5 2
#
# CMP 264
CMP 5 3.1625045 2.0692611 0 N R26 CRCW040210R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '10.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '541-10.2LCT-ND'
PRP Supplier_Part_Number_2 '71-CRCW0402-10.2-E3'
PRP Supplier_Part_Number_3 '1158303'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10R2'
PRP ValueDisplayed '10.2'
PRP VDC_V '50V'
TOP 0 3.1821895 2.0692611 270 N 458 15 1
TOP 1 3.1428194 2.0692611 270 N 380 1 2
#
# CMP 265
CMP 42 3.2666855 2.2263863 180 N R33 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 3.2465084 2.2263863 0 N 341 1 1
TOP 1 3.2868627 2.2263863 0 N 406 3 2
#
# CMP 266
CMP 5 1.162885 3.0522102 180 N R34 CRCW04022K20JNED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K20JNED'
PRP Power_W '63mW'
PRP Res_ohm '2.2k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.2KJCT-ND'
PRP Supplier_Part_Number_2 '59M6710'
PRP Supplier_Part_Number_3 '71-CRCW0402J-2.2K-E3'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP Value '2.2k'
PRP Value1 '5%'
PRP Value2 '0.063W'
PRP Value_Code '2k20'
PRP ValueDisplayed '2.2k'
PRP VDC_V '50V'
TOP 0 1.1432 3.0522102 90 N 69 12 1
TOP 1 1.1825701 3.0522102 90 N 107 0 2
#
# CMP 267
CMP 42 3.2666855 2.2663863 180 N R35 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 3.2465084 2.2663863 0 N 340 1 1
TOP 1 3.2868627 2.2663863 0 N 405 4 2
#
# CMP 268
CMP 42 2.413316 4.7033318 180 N R37 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 2.3931389 4.7033318 0 N 109 20 1
TOP 1 2.4334932 4.7033318 0 N 382 4 2
#
# CMP 269
CMP 41 2.8064529 4.6443317 0 N R39 ERJ-1GNF33R2C ;0=1,1=0.0000
PRP AEC_Category ''
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP CompType ''
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-1GNF33R2C.pdf'
PRP Digikey_Description 'RES SMD 33.2 OHM 1% 1/20W 0201'
PRP Digikey_Part_Number 'P122945CT-ND'
PRP EIA_Code ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP helpURL 'https://upverter.com/upn/revision/804e6f7ea13c6b2c/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP MountType ''
PRP Mouser_Description 'Thick Film Resistors - SMD 0201 33.2ohm 1% HalogenFree AEC-Q200'
PRP Mouser_Part_Number '667-ERJ-1GNF33R2C'
PRP Operating_Temperature_Range '-55°C to +125°C'
PRP PackageReference '0201'
PRP Part_Number 'ERJ-1GNF33R2C'
PRP PartNumber 'ERJ-1GNF33R2C'
PRP Power_W '50mW'
PRP Res_ohm '33.2'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm '0.26mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'P122945CT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-1GNF33R2C'
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo '200ppm/°C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 ''
PRP Value2 ''
PRP Value_Code ''
PRP ValueDisplayed ''
PRP VDC_V '25V'
TOP 0 2.8182639 4.6443317 180 N 305 0 1
TOP 1 2.7946419 4.6443317 180 N 339 0 2
#
# CMP 270
CMP 41 2.4220833 4.6443318 0 N R40 ERJ-1GNF33R2C ;0=1,1=0.0000
PRP AEC_Category ''
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP CompType ''
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-1GNF33R2C.pdf'
PRP Digikey_Description 'RES SMD 33.2 OHM 1% 1/20W 0201'
PRP Digikey_Part_Number 'P122945CT-ND'
PRP EIA_Code ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP helpURL 'https://upverter.com/upn/revision/804e6f7ea13c6b2c/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP MountType ''
PRP Mouser_Description 'Thick Film Resistors - SMD 0201 33.2ohm 1% HalogenFree AEC-Q200'
PRP Mouser_Part_Number '667-ERJ-1GNF33R2C'
PRP Operating_Temperature_Range '-55°C to +125°C'
PRP PackageReference '0201'
PRP Part_Number 'ERJ-1GNF33R2C'
PRP PartNumber 'ERJ-1GNF33R2C'
PRP Power_W '50mW'
PRP Res_ohm '33.2'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm '0.26mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'P122945CT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-1GNF33R2C'
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo '200ppm/°C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 ''
PRP Value2 ''
PRP Value_Code ''
PRP ValueDisplayed ''
PRP VDC_V '25V'
TOP 0 2.4338943 4.6443318 180 N 338 0 1
TOP 1 2.4102723 4.6443318 180 N 303 0 2
#
# CMP 271
CMP 41 2.8064529 4.5940275 0 N R42 ERJ-1GNF33R2C ;0=1,1=0.0000
PRP AEC_Category ''
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP CompType ''
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-1GNF33R2C.pdf'
PRP Digikey_Description 'RES SMD 33.2 OHM 1% 1/20W 0201'
PRP Digikey_Part_Number 'P122945CT-ND'
PRP EIA_Code ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP helpURL 'https://upverter.com/upn/revision/804e6f7ea13c6b2c/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP MountType ''
PRP Mouser_Description 'Thick Film Resistors - SMD 0201 33.2ohm 1% HalogenFree AEC-Q200'
PRP Mouser_Part_Number '667-ERJ-1GNF33R2C'
PRP Operating_Temperature_Range '-55°C to +125°C'
PRP PackageReference '0201'
PRP Part_Number 'ERJ-1GNF33R2C'
PRP PartNumber 'ERJ-1GNF33R2C'
PRP Power_W '50mW'
PRP Res_ohm '33.2'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm '0.26mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'P122945CT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-1GNF33R2C'
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo '200ppm/°C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 ''
PRP Value2 ''
PRP Value_Code ''
PRP ValueDisplayed ''
PRP VDC_V '25V'
TOP 0 2.8182639 4.5940275 180 N 304 0 1
TOP 1 2.7946419 4.5940275 180 N 337 0 2
#
# CMP 272
CMP 41 2.4220833 4.5943318 0 N R44 ERJ-1GNF33R2C ;0=1,1=0.0000
PRP AEC_Category ''
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP CompType ''
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-1GNF33R2C.pdf'
PRP Digikey_Description 'RES SMD 33.2 OHM 1% 1/20W 0201'
PRP Digikey_Part_Number 'P122945CT-ND'
PRP EIA_Code ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP helpURL 'https://upverter.com/upn/revision/804e6f7ea13c6b2c/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP MountType ''
PRP Mouser_Description 'Thick Film Resistors - SMD 0201 33.2ohm 1% HalogenFree AEC-Q200'
PRP Mouser_Part_Number '667-ERJ-1GNF33R2C'
PRP Operating_Temperature_Range '-55°C to +125°C'
PRP PackageReference '0201'
PRP Part_Number 'ERJ-1GNF33R2C'
PRP PartNumber 'ERJ-1GNF33R2C'
PRP Power_W '50mW'
PRP Res_ohm '33.2'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm '0.26mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'P122945CT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-1GNF33R2C'
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo '200ppm/°C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 ''
PRP Value2 ''
PRP Value_Code ''
PRP ValueDisplayed ''
PRP VDC_V '25V'
TOP 0 2.4338943 4.5943318 180 N 336 0 1
TOP 1 2.4102723 4.5943318 180 N 302 0 2
#
# CMP 273
CMP 41 2.4220833 4.5443318 0 N R45 ERJ-1GNF33R2C ;0=1,1=0.0000
PRP AEC_Category ''
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP CompType ''
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-1GNF33R2C.pdf'
PRP Digikey_Description 'RES SMD 33.2 OHM 1% 1/20W 0201'
PRP Digikey_Part_Number 'P122945CT-ND'
PRP EIA_Code ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP helpURL 'https://upverter.com/upn/revision/804e6f7ea13c6b2c/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP MountType ''
PRP Mouser_Description 'Thick Film Resistors - SMD 0201 33.2ohm 1% HalogenFree AEC-Q200'
PRP Mouser_Part_Number '667-ERJ-1GNF33R2C'
PRP Operating_Temperature_Range '-55°C to +125°C'
PRP PackageReference '0201'
PRP Part_Number 'ERJ-1GNF33R2C'
PRP PartNumber 'ERJ-1GNF33R2C'
PRP Power_W '50mW'
PRP Res_ohm '33.2'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm '0.26mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'P122945CT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-1GNF33R2C'
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo '200ppm/°C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 ''
PRP Value2 ''
PRP Value_Code ''
PRP ValueDisplayed ''
PRP VDC_V '25V'
TOP 0 2.4338943 4.5443318 180 N 335 0 1
TOP 1 2.4102723 4.5443318 180 N 306 0 2
#
# CMP 274
CMP 5 2.8517402 2.3264729 180 N R65 CRCW040210R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '10.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '541-10.2LCT-ND'
PRP Supplier_Part_Number_2 '71-CRCW0402-10.2-E3'
PRP Supplier_Part_Number_3 '1158303'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10R2'
PRP ValueDisplayed '10.2'
PRP VDC_V '50V'
TOP 0 2.8320552 2.3264729 90 N 56 4 1
TOP 1 2.8714253 2.3264729 90 N 379 1 2
#
# CMP 275
CMP 37 2.2323784 2.3218115 180 N R48 CRCW04020000Z0EDHP ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.vishay.com/docs/20043/crcwhpe3.pdf'
PRP Datasheet 'https://www.vishay.com/docs/20043/crcwhpe3.pdf'
PRP Datasheet_Path 'datasheets/Res-CRCW04020000Z0EDHP.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/5W 0402'
PRP Digikey_Part_Number '541-0.0YBCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/5e0a18f71149352e/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Vishay Dale'
PRP Mouser_Description 'Resistor; Thick Film; 0 Ohms; 0.125 W; 0 Ohms Jumper; SMT; 0402; TCR 0 ppm/DegC'
PRP Mouser_Part_Number '71-CRCW04020000Z0EDH'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'CRCW04020000Z0EDHP'
PRP PartNumber 'CRCW04020000Z0EDHP'
PRP Power_W '200mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'CRCW-HP e3'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '541-0.0YBCT-ND'
PRP Supplier_Part_Number_2 '71-CRCW04020000Z0EDH'
PRP Technology 'Thick Film'
PRP Value '0'
PRP VDC_V '50V'
TOP 0 2.2117091 2.3218115 0 N 54 24 1
TOP 1 2.2530477 2.3218115 0 N 31 1 2
#
# CMP 276
CMP 37 2.622413 2.2996168 0 N R53 CRCW04020000Z0EDHP ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.vishay.com/docs/20043/crcwhpe3.pdf'
PRP Datasheet 'https://www.vishay.com/docs/20043/crcwhpe3.pdf'
PRP Datasheet_Path 'datasheets/Res-CRCW04020000Z0EDHP.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/5W 0402'
PRP Digikey_Part_Number '541-0.0YBCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/5e0a18f71149352e/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Vishay Dale'
PRP Mouser_Description 'Resistor; Thick Film; 0 Ohms; 0.125 W; 0 Ohms Jumper; SMT; 0402; TCR 0 ppm/DegC'
PRP Mouser_Part_Number '71-CRCW04020000Z0EDH'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'CRCW04020000Z0EDHP'
PRP PartNumber 'CRCW04020000Z0EDHP'
PRP Power_W '200mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'CRCW-HP e3'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '541-0.0YBCT-ND'
PRP Supplier_Part_Number_2 '71-CRCW04020000Z0EDH'
PRP Technology 'Thick Film'
PRP Value '0'
PRP VDC_V '50V'
TOP 0 2.6430823 2.2996168 180 N 405 1 1
TOP 1 2.6017437 2.2996168 180 N 151 0 2
#
# CMP 277
CMP 42 1.9819775 4.4990011 180 N R55 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 1.9618004 4.4990011 0 N 386 0 1
TOP 1 2.0021547 4.4990011 0 N 22 2 2
#
# CMP 278
CMP 5 1.9836183 2.2377277 90 N R66 CRCW040210R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '10.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '541-10.2LCT-ND'
PRP Supplier_Part_Number_2 '71-CRCW0402-10.2-E3'
PRP Supplier_Part_Number_3 '1158303'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10R2'
PRP ValueDisplayed '10.2'
PRP VDC_V '50V'
TOP 0 1.9836183 2.2574127 180 N 57 4 1
TOP 1 1.9836183 2.2180426 180 N 159 1 2
#
# CMP 279
CMP 42 1.8825322 1.8171265 90 N R57 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 1.8825322 1.8373036 90 N 150 1 1
TOP 1 1.8825322 1.7969493 90 N 406 4 2
#
# CMP 280
CMP 42 2.0335674 1.2989859 90 N R58 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 2.0335674 1.319163 90 N 334 1 1
TOP 1 2.0335674 1.2788087 90 N 406 5 2
#
# CMP 281
CMP 42 2.0755674 1.2989859 90 N R59 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 2.0755674 1.319163 90 N 333 1 1
TOP 1 2.0755674 1.2788087 90 N 405 5 2
#
# CMP 282
CMP 13 2.7642603 2.3054414 270 N R60 CSNL1206FT1L00 ;0=1,1=0.0531
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://www.seielect.com/Catalog/SEI-csnl.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Stackpole Electronics Inc'
PRP MountType 'SMT'
PRP PackageReference '1206'
PRP PartNumber 'CSNL1206FT1L00'
PRP Power_W '1W'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '1m'
PRP RoHS 'Y'
PRP SizeArea_mm2 '5.12'
PRP SizeX_mm '3.2'
PRP SizeY_mm '1.6'
PRP SizeZ_mm '1.35'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'CSNL1206FT1L00CT-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Metal Element'
PRP TempCo '50 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '0.001'
PRP Value1 '1%'
PRP Value2 '1W'
PRP Value_Code '1L000'
PRP ValueDisplayed '0.001'
PRP VDC_V ''
TOP 0 2.7642603 2.2522918 0 N 457 14 1
TOP 1 2.7642603 2.358591 0 N 56 5 2
#
# CMP 283
CMP 42 1.9245322 1.8171265 90 N R62 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 1.9245322 1.8373036 90 N 149 2 1
TOP 1 1.9245322 1.7969493 90 N 405 6 2
#
# CMP 284
CMP 37 1.1310005 3.3318115 180 N R63 CRCW04020000Z0EDHP ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.vishay.com/docs/20043/crcwhpe3.pdf'
PRP Datasheet 'https://www.vishay.com/docs/20043/crcwhpe3.pdf'
PRP Datasheet_Path 'datasheets/Res-CRCW04020000Z0EDHP.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/5W 0402'
PRP Digikey_Part_Number '541-0.0YBCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/5e0a18f71149352e/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Vishay Dale'
PRP Mouser_Description 'Resistor; Thick Film; 0 Ohms; 0.125 W; 0 Ohms Jumper; SMT; 0402; TCR 0 ppm/DegC'
PRP Mouser_Part_Number '71-CRCW04020000Z0EDH'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'CRCW04020000Z0EDHP'
PRP PartNumber 'CRCW04020000Z0EDHP'
PRP Power_W '200mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'CRCW-HP e3'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '541-0.0YBCT-ND'
PRP Supplier_Part_Number_2 '71-CRCW04020000Z0EDH'
PRP Technology 'Thick Film'
PRP Value '0'
PRP VDC_V '50V'
TOP 0 1.1103312 3.3318115 0 N 18 8 1
TOP 1 1.1516698 3.3318115 0 N 26 1 2
#
# CMP 285
CMP 13 1.9625868 2.3252076 180 N R64 CSNL1206FT1L00 ;0=1,1=0.0531
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://www.seielect.com/Catalog/SEI-csnl.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Stackpole Electronics Inc'
PRP MountType 'SMT'
PRP PackageReference '1206'
PRP PartNumber 'CSNL1206FT1L00'
PRP Power_W '1W'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '1m'
PRP RoHS 'Y'
PRP SizeArea_mm2 '5.12'
PRP SizeX_mm '3.2'
PRP SizeY_mm '1.6'
PRP SizeZ_mm '1.35'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'CSNL1206FT1L00CT-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Metal Element'
PRP TempCo '50 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '0.001'
PRP Value1 '1%'
PRP Value2 '1W'
PRP Value_Code '1L000'
PRP ValueDisplayed '0.001'
PRP VDC_V ''
TOP 0 1.9094372 2.3252076 90 N 175 8 1
TOP 1 2.0157364 2.3252076 90 N 57 5 2
#
# CMP 286
CMP 5 2.8517402 2.2844099 180 N R47 CRCW040210R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '10.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '541-10.2LCT-ND'
PRP Supplier_Part_Number_2 '71-CRCW0402-10.2-E3'
PRP Supplier_Part_Number_3 '1158303'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10R2'
PRP ValueDisplayed '10.2'
PRP VDC_V '50V'
TOP 0 2.8320552 2.2844099 90 N 457 15 1
TOP 1 2.8714253 2.2844099 90 N 378 1 2
#
# CMP 287
CMP 5 1.9415553 2.2377277 90 N R56 CRCW040210R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '10.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '541-10.2LCT-ND'
PRP Supplier_Part_Number_2 '71-CRCW0402-10.2-E3'
PRP Supplier_Part_Number_3 '1158303'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10R2'
PRP ValueDisplayed '10.2'
PRP VDC_V '50V'
TOP 0 1.9415553 2.2574127 180 N 175 9 1
TOP 1 1.9415553 2.2180426 180 N 199 1 2
#
# CMP 288
CMP 42 2.6224129 2.3748114 180 N R14 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 2.6022358 2.3748114 0 N 101 0 1
TOP 1 2.6425901 2.3748114 0 N 309 10 2
#
# CMP 289
CMP 5 0.1042547 2.1005372 270 N R68 CRCW0402220RJNED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW0402220RJNED'
PRP Power_W '63mW'
PRP Res_ohm '220'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-220JCT-ND'
PRP Supplier_Part_Number_2 '59M6718'
PRP Supplier_Part_Number_3 '71-CRCW0402J-220-E3'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP Value '220'
PRP Value1 '5%'
PRP Value2 '0.063W'
PRP Value_Code '220R'
PRP ValueDisplayed '220'
PRP VDC_V '50V'
TOP 0 0.1042547 2.0808522 0 N 442 0 1
TOP 1 0.1042547 2.1202223 0 N 224 0 2
#
# CMP 290
CMP 5 0.3200924 2.9704062 180 N R69 CRCW0402220RJNED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW0402220RJNED'
PRP Power_W '63mW'
PRP Res_ohm '220'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-220JCT-ND'
PRP Supplier_Part_Number_2 '59M6718'
PRP Supplier_Part_Number_3 '71-CRCW0402J-220-E3'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP Value '220'
PRP Value1 '5%'
PRP Value2 '0.063W'
PRP Value_Code '220R'
PRP ValueDisplayed '220'
PRP VDC_V '50V'
TOP 0 0.3004074 2.9704062 90 N 203 0 1
TOP 1 0.3397775 2.9704062 90 N 440 0 2
#
# CMP 291
CMP 42 2.6226855 2.2608115 180 N R70 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 2.6025084 2.2608115 0 N 99 0 1
TOP 1 2.6428627 2.2608115 0 N 458 31 2
#
# CMP 292
CMP 42 2.1330005 2.3978115 0 N R71 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 2.1531776 2.3978115 180 N 100 2 1
TOP 1 2.1128233 2.3978115 180 N 144 10 2
#
# CMP 293
CMP 5 1.5506057 3.3348115 270 N R75 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 1.5506057 3.3151265 0 N 25 0 1
TOP 1 1.5506057 3.3544966 0 N 109 8 2
#
# CMP 294
CMP 42 0.7504493 3.166218 180 N R76 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 0.7302722 3.166218 0 N 424 523 1
TOP 1 0.7706265 3.166218 0 N 19 3 2
#
# CMP 295
CMP 1 2.9440011 3.3983262 270 N R78 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 2.9440011 3.3873026 0 N 21 1 1
TOP 1 2.9440011 3.4093498 0 N 53 1 2
#
# CMP 296
CMP 42 0.7504493 3.121718 180 N R79 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 0.7302722 3.121718 0 N 109 21 1
TOP 1 0.7706265 3.121718 0 N 19 2 2
#
# CMP 297
CMP 1 1.9913832 4.5874656 270 N R80 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 1.9913832 4.576442 0 N 423 1 1
TOP 1 1.9913832 4.5984892 0 N 356 0 2
#
# CMP 298
CMP 1 1.873883 3.9409696 0 N R82 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 1.8849066 3.9409696 270 N 422 1 1
TOP 1 1.8628594 3.9409696 270 N 355 0 2
#
# CMP 299
CMP 5 2.0175412 3.7225067 0 N R83 ERJ-2GEJ101X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C84.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GEJ101X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '100'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 'P100JCT-ND'
PRP Supplier_Part_Number_2 '65T8246'
PRP Supplier_Part_Number_3 '2059210'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '100'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '100R'
PRP ValueDisplayed '100'
PRP VDC_V ''
TOP 0 2.0372262 3.7225067 270 N 266 0 1
TOP 1 1.9978561 3.7225067 270 N 32 0 2
#
# CMP 300
CMP 42 2.1405412 3.6145067 0 N R85 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 2.1607183 3.6145067 180 N 137 1 1
TOP 1 2.120364 3.6145067 180 N 17 4 2
#
# CMP 301
CMP 42 1.9533561 3.5519354 0 N R86 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 1.9735332 3.5519354 180 N 424 517 1
TOP 1 1.9331789 3.5519354 180 N 20 3 2
#
# CMP 302
CMP 42 1.8798878 3.6686205 90 N R87 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 1.8798878 3.6887976 90 N 309 11 1
TOP 1 1.8798878 3.6484433 90 N 20 4 2
#
# CMP 303
CMP 1 0.408155 0.9683632 90 N R91 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 0.408155 0.9793868 180 N 421 1 1
TOP 1 0.408155 0.9573396 180 N 354 0 2
#
# CMP 304
CMP 1 2.0659775 4.2880011 0 N R94 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 2.0770011 4.2880011 270 N 420 0 1
TOP 1 2.0549539 4.2880011 270 N 353 0 2
#
# CMP 305
CMP 5 3.1802834 4.3088425 180 N R96 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 3.1605984 4.3088425 90 N 394 0 1
TOP 1 3.1999685 4.3088425 90 N 88 0 2
#
# CMP 306
CMP 5 3.1389449 4.019 0 N R98 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 3.1586299 4.019 270 N 396 1 1
TOP 1 3.1192598 4.019 270 N 296 0 2
#
# CMP 307
CMP 5 3.1783149 4.250874 180 N R100 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 3.1586299 4.250874 90 N 393 0 1
TOP 1 3.198 4.250874 90 N 87 0 2
#
# CMP 308
CMP 5 3.1389449 4.0769685 0 N R101 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 3.1586299 4.0769685 270 N 395 1 1
TOP 1 3.1192598 4.0769685 270 N 186 0 2
#
# CMP 309
CMP 5 3.1409134 4.3088425 0 N R103 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 3.1605984 4.3088425 270 N 394 1 1
TOP 1 3.1212283 4.3088425 270 N 295 0 2
#
# CMP 310
CMP 42 2.9190404 3.2412468 90 N R104 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 2.9190404 3.2614239 90 N 125 1 1
TOP 1 2.9190404 3.2210696 90 N 12 3 2
#
# CMP 311
CMP 5 3.1389449 4.250874 0 N R105 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 3.1586299 4.250874 270 N 393 2 1
TOP 1 3.1192598 4.250874 270 N 294 0 2
#
# CMP 312
CMP 13 0.4085224 3.1238114 0 N R119 CRCW12061M00JNEA ;0=1,1=0.0531
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '1206'
PRP PartNumber 'CRCW12061M00JNEA'
PRP Power_W '250mW'
PRP Res_ohm '1M'
PRP RoHS 'E'
PRP SizeArea_mm2 '5.12'
PRP SizeX_mm '3.2'
PRP SizeY_mm '1.6'
PRP SizeZ_mm '1.35'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-1.0MECT-ND'
PRP Supplier_Part_Number_2 '59M6941'
PRP Supplier_Part_Number_3 '71-CRCW1206J-1M-E3'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP Value '1.0Meg'
PRP Value1 '5%'
PRP Value2 '0.25W'
PRP Value_Code '1M00'
PRP ValueDisplayed '1.0M'
PRP VDC_V '200V'
TOP 0 0.461672 3.1238114 270 N 446 6 1
TOP 1 0.3553728 3.1238114 270 N 424 278 2
#
# CMP 313
CMP 5 3.1389449 4.1929055 0 N R121 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 3.1586299 4.1929055 270 N 392 1 1
TOP 1 3.1192598 4.1929055 270 N 293 0 2
#
# CMP 314
CMP 5 3.1389449 4.134937 0 N R122 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 3.1586299 4.134937 270 N 391 1 1
TOP 1 3.1192598 4.134937 270 N 292 0 2
#
# CMP 315
CMP 5 1.2775929 0.3461751 90 N R123 CRCW04021K00FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04021K00FKED'
PRP Power_W '63mW'
PRP Res_ohm '1k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-1.00KLCT-ND'
PRP Supplier_Part_Number_2 '52K6545'
PRP Supplier_Part_Number_3 '71-CRCW0402-1.0K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '1.00k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '1k00'
PRP ValueDisplayed '1.00k'
PRP VDC_V '50V'
TOP 0 1.2775929 0.3658601 180 N 331 0 1
TOP 1 1.2775929 0.32649 180 N 424 279 2
#
# CMP 316
CMP 5 1.3469318 0.3461751 90 N R124 CRCW04021K00FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04021K00FKED'
PRP Power_W '63mW'
PRP Res_ohm '1k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-1.00KLCT-ND'
PRP Supplier_Part_Number_2 '52K6545'
PRP Supplier_Part_Number_3 '71-CRCW0402-1.0K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '1.00k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '1k00'
PRP ValueDisplayed '1.00k'
PRP VDC_V '50V'
TOP 0 1.3469318 0.3658601 180 N 330 0 1
TOP 1 1.3469318 0.32649 180 N 308 18 2
#
# CMP 317
CMP 5 1.3131902 0.3461751 90 N R126 CRCW04021K00FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04021K00FKED'
PRP Power_W '63mW'
PRP Res_ohm '1k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-1.00KLCT-ND'
PRP Supplier_Part_Number_2 '52K6545'
PRP Supplier_Part_Number_3 '71-CRCW0402-1.0K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '1.00k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '1k00'
PRP ValueDisplayed '1.00k'
PRP VDC_V '50V'
TOP 0 1.3131902 0.3658601 180 N 329 0 1
TOP 1 1.3131902 0.32649 180 N 424 280 2
#
# CMP 318
CMP 5 1.3815114 0.3461751 90 N R127 CRCW04021K00FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04021K00FKED'
PRP Power_W '63mW'
PRP Res_ohm '1k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-1.00KLCT-ND'
PRP Supplier_Part_Number_2 '52K6545'
PRP Supplier_Part_Number_3 '71-CRCW0402-1.0K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '1.00k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '1k00'
PRP ValueDisplayed '1.00k'
PRP VDC_V '50V'
TOP 0 1.3815114 0.3658601 180 N 328 0 1
TOP 1 1.3815114 0.32649 180 N 308 19 2
#
# CMP 319
CMP 42 1.8531497 0.3308757 270 N R128 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 1.8531497 0.3106986 270 N 284 3 1
TOP 1 1.8531497 0.3510529 270 N 251 1 2
#
# CMP 320
CMP 42 1.8057551 0.3303029 270 N R129 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 1.8057551 0.3101258 270 N 383 1 1
TOP 1 1.8057551 0.3504801 270 N 252 1 2
#
# CMP 321
CMP 13 0.24833 2.0306394 0 N R130 CRCW12061M00JNEA ;0=1,1=0.0531
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '1206'
PRP PartNumber 'CRCW12061M00JNEA'
PRP Power_W '250mW'
PRP Res_ohm '1M'
PRP RoHS 'E'
PRP SizeArea_mm2 '5.12'
PRP SizeX_mm '3.2'
PRP SizeY_mm '1.6'
PRP SizeZ_mm '1.35'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-1.0MECT-ND'
PRP Supplier_Part_Number_2 '59M6941'
PRP Supplier_Part_Number_3 '71-CRCW1206J-1M-E3'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP Value '1.0Meg'
PRP Value1 '5%'
PRP Value2 '0.25W'
PRP Value_Code '1M00'
PRP ValueDisplayed '1.0M'
PRP VDC_V '200V'
TOP 0 0.3014796 2.0306394 270 N 446 7 1
TOP 1 0.1951804 2.0306394 270 N 424 281 2
#
# CMP 322
CMP 42 1.4807463 4.3399592 0 N R131 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 1.5009234 4.3399592 180 N 169 2 1
TOP 1 1.4605691 4.3399592 180 N 265 1 2
#
# CMP 323
CMP 5 1.9607052 4.2658752 90 N R133 CRCW04021K00FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04021K00FKED'
PRP Power_W '63mW'
PRP Res_ohm '1k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-1.00KLCT-ND'
PRP Supplier_Part_Number_2 '52K6545'
PRP Supplier_Part_Number_3 '71-CRCW0402-1.0K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '1.00k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '1k00'
PRP ValueDisplayed '1.00k'
PRP VDC_V '50V'
TOP 0 1.9607052 4.2855602 180 N 421 2 1
TOP 1 1.9607052 4.2461901 180 N 175 10 2
#
# CMP 324
CMP 5 1.123527 0.5139695 0 N R134 CRCW040249R9FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040249R9FKED'
PRP Power_W '63mW'
PRP Res_ohm '49.9'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-49.9LCT-ND'
PRP Supplier_Part_Number_2 '52K7114'
PRP Supplier_Part_Number_3 '71-CRCW0402-49.9-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '49.9'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '49R9'
PRP ValueDisplayed '49.9'
PRP VDC_V '50V'
TOP 0 1.143212 0.5139695 270 N 242 1 1
TOP 1 1.1038419 0.5139695 270 N 308 20 2
#
# CMP 325
CMP 42 1.9499963 0.6115359 0 N R136 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 1.9701734 0.6115359 180 N 285 3 1
TOP 1 1.9298191 0.6115359 180 N 250 1 2
#
# CMP 326
CMP 5 1.2274285 2.7304551 0 N R139 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 1.2471135 2.7304551 270 N 445 0 1
TOP 1 1.2077434 2.7304551 270 N 261 5 2
#
# CMP 327
CMP 5 1.950579 0.7690162 180 N R140 CRCW04021K00FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04021K00FKED'
PRP Power_W '63mW'
PRP Res_ohm '1k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-1.00KLCT-ND'
PRP Supplier_Part_Number_2 '52K6545'
PRP Supplier_Part_Number_3 '71-CRCW0402-1.0K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '1.00k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '1k00'
PRP ValueDisplayed '1.00k'
PRP VDC_V '50V'
TOP 0 1.930894 0.7690162 90 N 241 2 1
TOP 1 1.9702641 0.7690162 90 N 308 21 2
#
# CMP 328
CMP 5 1.2840927 2.7112475 270 N R143 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 1.2840927 2.6915625 0 N 424 282 1
TOP 1 1.2840927 2.7309326 0 N 445 1 2
#
# CMP 329
CMP 5 0.7414445 4.4653992 0 N R144 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 0.7611295 4.4653992 270 N 432 0 1
TOP 1 0.7217594 4.4653992 270 N 41 0 2
#
# CMP 330
CMP 5 0.9009536 4.6762684 270 N R145 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 0.9009536 4.6565834 0 N 433 0 1
TOP 1 0.9009536 4.6959535 0 N 38 0 2
#
# CMP 331
CMP 42 0.9541552 4.6762386 270 N R146 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 0.9541552 4.6560615 270 N 434 1 1
TOP 1 0.9541552 4.6964158 270 N 39 0 2
#
# CMP 332
CMP 5 1.0062688 4.6769753 270 N R147 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 1.0062688 4.6572903 0 N 431 0 1
TOP 1 1.0062688 4.6966604 0 N 40 0 2
#
# CMP 333
CMP 42 1.1068856 4.6770149 270 N R148 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 1.1068856 4.6568378 270 N 417 1 1
TOP 1 1.1068856 4.6971921 270 N 406 6 2
#
# CMP 334
CMP 42 1.1628851 4.6770149 270 N R149 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 1.1628851 4.6568378 270 N 416 1 1
TOP 1 1.1628851 4.6971921 270 N 405 7 2
#
# CMP 335
CMP 42 1.2158053 4.6770149 270 N R150 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 1.2158053 4.6568378 270 N 415 1 1
TOP 1 1.2158053 4.6971921 270 N 405 8 2
#
# CMP 336
CMP 42 1.480115 4.5310102 180 N R151 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 1.4599379 4.5310102 0 N 419 1 1
TOP 1 1.5002922 4.5310102 0 N 388 2 2
#
# CMP 337
CMP 42 1.1254955 1.067795 180 N R152 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 1.1053184 1.067795 0 N 247 2 1
TOP 1 1.1456727 1.067795 0 N 189 1 2
#
# CMP 338
CMP 42 1.480115 4.4798291 180 N R153 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 1.4599379 4.4798291 0 N 418 1 1
TOP 1 1.5002922 4.4798291 0 N 388 3 2
#
# CMP 339
CMP 5 1.2783424 1.1725152 270 N R154 ERJ-2GEJ101X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C84.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GEJ101X'
PRP Power_W '100mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '100'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 'P100JCT-ND'
PRP Supplier_Part_Number_2 '65T8246'
PRP Supplier_Part_Number_3 '2059210'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '100'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '100R'
PRP ValueDisplayed '100'
PRP VDC_V ''
TOP 0 1.2783424 1.1528302 0 N 374 1 1
TOP 1 1.2783424 1.1922003 0 N 246 2 2
#
# CMP 340
CMP 5 1.1563416 0.6179888 270 N R155 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 1.1563416 0.5983038 0 N 245 0 1
TOP 1 1.1563416 0.6376739 0 N 308 22 2
#
# CMP 341
CMP 5 1.977974 4.6589474 0 N R156 CRCW04026K04FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04026K04FKED'
PRP Power_W '63mW'
PRP Res_ohm '6.04k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-6.04KLCT-ND'
PRP Supplier_Part_Number_2 '52K7180'
PRP Supplier_Part_Number_3 '71-CRCW0402-6.04K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '6.04k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '6k04'
PRP ValueDisplayed '6.04k'
PRP VDC_V '50V'
TOP 0 1.997659 4.6589474 270 N 148 0 1
TOP 1 1.9582889 4.6589474 270 N 457 16 2
#
# CMP 342
CMP 5 0.7414445 4.2707884 180 N R157 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 0.7217595 4.2707884 90 N 424 283 1
TOP 1 0.7611296 4.2707884 90 N 301 0 2
#
# CMP 343
CMP 42 1.4789815 4.1028582 180 N R158 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 1.4588044 4.1028582 0 N 134 1 1
TOP 1 1.4991587 4.1028582 0 N 390 2 2
#
# CMP 344
CMP 8 3.060956 1.3811741 0 N R161 MCT06030Z0000ZP500 ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/28705/mcx0x0xpro.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Vishay/Beyschlag'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'MCT06030Z0000ZP500'
PRP Power_W '125mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'MCT0603-0.0-ZZCT-ND'
PRP Supplier_Part_Number_2 '96Y9454'
PRP Supplier_Part_Number_3 '594-MCT06030Z0000ZP5'
PRP Technology 'Thin Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.125W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 3.0885151 1.3811741 270 N 348 0 1
TOP 1 3.033397 1.3811741 270 N 246 3 2
#
# CMP 345
CMP 42 1.2178605 3.9265673 90 N R162 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 1.2178605 3.9467444 90 N 133 1 1
TOP 1 1.2178605 3.9063901 90 N 389 2 2
#
# CMP 346
CMP 5 0.7414445 4.4150345 180 N R163 CRCW04021K00FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04021K00FKED'
PRP Power_W '63mW'
PRP Res_ohm '1k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-1.00KLCT-ND'
PRP Supplier_Part_Number_2 '52K6545'
PRP Supplier_Part_Number_3 '71-CRCW0402-1.0K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '1.00k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '1k00'
PRP ValueDisplayed '1.00k'
PRP VDC_V '50V'
TOP 0 0.7217595 4.4150345 90 N 436 9 1
TOP 1 0.7611296 4.4150345 90 N 176 0 2
#
# CMP 347
CMP 42 1.480115 4.2006046 180 N R166 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 1.4599379 4.2006046 0 N 310 1 1
TOP 1 1.5002922 4.2006046 0 N 273 0 2
#
# CMP 348
CMP 5 1.1644909 3.9265673 90 N R169 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 1.1644909 3.9462523 180 N 291 0 1
TOP 1 1.1644909 3.9068822 180 N 269 0 2
#
# CMP 349
CMP 5 1.1111213 3.9265673 90 N R170 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 1.1111213 3.9462523 180 N 289 0 1
TOP 1 1.1111213 3.9068822 180 N 270 0 2
#
# CMP 350
CMP 5 1.0589077 3.9265673 90 N R171 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 1.0589077 3.9462523 180 N 287 0 1
TOP 1 1.0589077 3.9068822 180 N 271 0 2
#
# CMP 351
CMP 5 1.9779739 4.6969474 180 N R172 CRCW040210K5FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K5FKED'
PRP Power_W '63mW'
PRP Res_ohm '10.5k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.5KLCT-ND'
PRP Supplier_Part_Number_2 '52K6597'
PRP Supplier_Part_Number_3 '71-CRCW0402-10.5K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.5k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k5'
PRP ValueDisplayed '10.5k'
PRP VDC_V '50V'
TOP 0 1.9582889 4.6969474 90 N 424 284 1
TOP 1 1.997659 4.6969474 90 N 148 1 2
#
# CMP 352
CMP 5 1.41321 2.6523649 270 N R173 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 1.41321 2.6326799 0 N 300 0 1
TOP 1 1.41321 2.67205 0 N 261 6 2
#
# CMP 353
CMP 5 3.0004975 1.3009953 180 N R174 CRCW040230K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code ''
PRP Green_EU_RoHS 'Passed with Exemption'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040230K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '30k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-30.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6953'
PRP Supplier_Part_Number_3 '71-CRCW0402-30K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '30.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '30k0'
PRP ValueDisplayed '30.0k'
PRP VDC_V '50V'
TOP 0 2.9808125 1.3009953 90 N 424 285 1
TOP 1 3.0201826 1.3009953 90 N 195 0 2
#
# CMP 354
CMP 8 3.0304535 1.1876868 180 N R175 MCT06030Z0000ZP500 ;0=1,1=0.0394
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/28705/mcx0x0xpro.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Vishay/Beyschlag'
PRP MountType 'SMT'
PRP PackageReference '0603'
PRP PartNumber 'MCT06030Z0000ZP500'
PRP Power_W '125mW'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '0'
PRP RoHS 'Y'
PRP SizeArea_mm2 '1.28'
PRP SizeX_mm '1.6'
PRP SizeY_mm '0.8'
PRP SizeZ_mm '1'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'MCT0603-0.0-ZZCT-ND'
PRP Supplier_Part_Number_2 '96Y9454'
PRP Supplier_Part_Number_3 '594-MCT06030Z0000ZP5'
PRP Technology 'Thin Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.125W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 3.0028944 1.1876868 90 N 424 286 1
TOP 1 3.0580125 1.1876868 90 N 347 0 2
#
# CMP 355
CMP 11 1.480135 4.6170065 0 N R182 CRCW08050000Z0EA ;0=1,1=0.0571
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'CRCW08050000Z0EA'
PRP Power_W '125mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '2.5'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-0.0ACT-ND'
PRP Supplier_Part_Number_2 '52K9721'
PRP Supplier_Part_Number_3 '71-CRCW0805-0-E3'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.125W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '150V'
TOP 0 1.5096626 4.6170065 270 N 260 3 1
TOP 1 1.4506075 4.6170065 270 N 436 10 2
#
# CMP 356
CMP 5 1.7803471 4.4235641 180 N R183 CRCW0402100KFKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP INSTALLATION 'DNP'
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW0402100KFKED'
PRP Power_W '63mW'
PRP Res_ohm '100k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-100KLCT-ND'
PRP Supplier_Part_Number_2 '52K6607'
PRP Supplier_Part_Number_3 '71-CRCW0402-100K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '100k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '100k'
PRP ValueDisplayed '100k'
PRP VDC_V '50V'
TOP 0 1.7606621 4.4235641 90 N 435 1 1
TOP 1 1.8000322 4.4235641 90 N 426 6 2
#
# CMP 357
CMP 5 1.4175372 0.3455845 270 N R194 CRCW04024K87FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04024K87FKED'
PRP Power_W '63mW'
PRP Res_ohm '4.87k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-4.87KLCT-ND'
PRP Supplier_Part_Number_2 '52K7047'
PRP Supplier_Part_Number_3 '71-CRCW0402-4.87K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '4.87k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '4k87'
PRP ValueDisplayed '4.87k'
PRP VDC_V '50V'
TOP 0 1.4175372 0.3258995 0 N 424 287 1
TOP 1 1.4175372 0.3652696 0 N 326 0 2
#
# CMP 358
CMP 1 0.7168645 1.9279024 270 N R196 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 0.7168645 1.9168788 0 N 28 1 1
TOP 1 0.7168645 1.938926 0 N 424 288 2
#
# CMP 359
CMP 5 1.7803471 4.6032269 180 N R202 CRCW040249K9FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040249K9FKED'
PRP Power_W '63mW'
PRP Res_ohm '49.9k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-49.9KLCT-ND'
PRP Supplier_Part_Number_2 '52K7113'
PRP Supplier_Part_Number_3 '71-CRCW0402-49.9K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '49.9k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '49k9'
PRP ValueDisplayed '49.9k'
PRP VDC_V '50V'
TOP 0 1.7606621 4.6032269 90 N 325 0 1
TOP 1 1.8000322 4.6032269 90 N 260 4 2
#
# CMP 360
CMP 5 1.7803471 4.5501939 180 N R203 CRCW040229K4FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040229K4FKED'
PRP Power_W '63mW'
PRP Res_ohm '29.4k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-29.4KLCT-ND'
PRP Supplier_Part_Number_2 '52K6927'
PRP Supplier_Part_Number_3 '71-CRCW0402-29.4K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '29.4k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '29k4'
PRP ValueDisplayed '29.4k'
PRP VDC_V '50V'
TOP 0 1.7606621 4.5501939 90 N 325 1 1
TOP 1 1.8000322 4.5501939 90 N 424 289 2
#
# CMP 361
CMP 5 1.7803471 4.4734222 0 N R204 CRCW0402200KFKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW0402200KFKED'
PRP Power_W '63mW'
PRP Res_ohm '200k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-200KLCT-ND'
PRP Supplier_Part_Number_2 '52K6825'
PRP Supplier_Part_Number_3 '71-CRCW0402-200K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '200k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '200k'
PRP ValueDisplayed '200k'
PRP VDC_V '50V'
TOP 0 1.8000321 4.4734222 270 N 424 290 1
TOP 1 1.760662 4.4734222 270 N 435 2 2
#
# CMP 362
CMP 11 0.261154 4.2191528 90 N R206 CRCW08050000Z0EA ;0=1,1=0.0571
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'CRCW08050000Z0EA'
PRP Power_W '125mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '2.5'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-0.0ACT-ND'
PRP Supplier_Part_Number_2 '52K9721'
PRP Supplier_Part_Number_3 '71-CRCW0805-0-E3'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.125W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '150V'
TOP 0 0.261154 4.2486804 180 N 346 2 1
TOP 1 0.261154 4.1896253 180 N 426 7 2
#
# CMP 363
CMP 11 0.3631668 4.2183232 90 N R207 CRCW08050000Z0EA ;0=1,1=0.0571
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0805'
PRP PartNumber 'CRCW08050000Z0EA'
PRP Power_W '125mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '2.5'
PRP SizeX_mm '2'
PRP SizeY_mm '1.25'
PRP SizeZ_mm '1.45'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-0.0ACT-ND'
PRP Supplier_Part_Number_2 '52K9721'
PRP Supplier_Part_Number_3 '71-CRCW0805-0-E3'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.125W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V '150V'
TOP 0 0.3631668 4.2478508 180 N 372 2 1
TOP 1 0.3631668 4.1887957 180 N 426 8 2
#
# CMP 364
CMP 5 0.3782532 4.3811594 0 N R208 CRCW040230K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code ''
PRP Green_EU_RoHS 'Passed with Exemption'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040230K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '30k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-30.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6953'
PRP Supplier_Part_Number_3 '71-CRCW0402-30K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '30.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '30k0'
PRP ValueDisplayed '30.0k'
PRP VDC_V '50V'
TOP 0 0.3979382 4.3811594 270 N 424 291 1
TOP 1 0.3585681 4.3811594 270 N 323 0 2
#
# CMP 365
CMP 5 1.5597012 1.7164644 0 N R222 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 1.5793862 1.7164644 270 N 322 0 1
TOP 1 1.5400161 1.7164644 270 N 308 23 2
#
# CMP 366
CMP 0 0.7402896 1.4050924 180 N R243 CRCW02014K70FKED ;0=1,1=0.0130
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02014K70FKED'
PRP Power_W '50mW'
PRP Res_ohm '4.7k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.33'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-4.70KAABCT-ND'
PRP Supplier_Part_Number_2 '87W8644'
PRP Supplier_Part_Number_3 '71-CRCW02014K70FKED'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '4.70k'
PRP Value1 '1%'
PRP Value2 '0.05W'
PRP Value_Code '4k70'
PRP ValueDisplayed '4.70k'
PRP VDC_V '30V'
TOP 0 0.729266 1.4050924 90 N 412 1 1
TOP 1 0.7513132 1.4050924 90 N 308 33 2
#
# CMP 367
CMP 1 0.2926613 1.4278089 180 N R244 ERJ-1GNJ220C ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://industrial.panasonic.com/lecs/www-data/pdf/AOA0000/AOA0000CE1.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'ERJ-1GNJ220C'
PRP Power_W '50mW'
PRP Published '2016-10-14'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '22'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'ERJ-1GNJ220C-ND'
PRP Supplier_Part_Number_2 '667-ERJ-1GNJ220C'
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '22'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '22R0'
PRP ValueDisplayed '22'
PRP VDC_V ''
TOP 0 0.2816377 1.4278089 90 N 450 0 1
TOP 1 0.3036849 1.4278089 90 N 184 1 2
#
# CMP 368
CMP 42 2.1148561 3.7361917 270 N R269 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 2.1148561 3.7160146 270 N 266 3 1
TOP 1 2.1148561 3.7563689 270 N 275 1 2
#
# CMP 369
CMP 5 2.8113343 3.3983263 90 N R271 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP INSTALLATION 'DNP'
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 2.8113343 3.4180113 180 N 274 0 1
TOP 1 2.8113343 3.3786412 180 N 109 9 2
#
# CMP 370
CMP 5 2.8460009 3.3983263 90 N R272 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP INSTALLATION 'DNP'
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 2.8460009 3.4180113 180 N 267 1 1
TOP 1 2.8460009 3.3786412 180 N 109 10 2
#
# CMP 371
CMP 5 1.5183516 4.0472446 180 N R278 CRCW0402100KFKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW0402100KFKED'
PRP Power_W '63mW'
PRP Res_ohm '100k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-100KLCT-ND'
PRP Supplier_Part_Number_2 '52K6607'
PRP Supplier_Part_Number_3 '71-CRCW0402-100K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '100k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '100k'
PRP ValueDisplayed '100k'
PRP VDC_V '50V'
TOP 0 1.4986666 4.0472446 90 N 390 0 1
TOP 1 1.5380367 4.0472446 90 N 109 11 2
#
# CMP 372
CMP 5 2.7420011 3.3983263 90 N R279 CRCW0402100KFKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW0402100KFKED'
PRP Power_W '63mW'
PRP Res_ohm '100k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-100KLCT-ND'
PRP Supplier_Part_Number_2 '52K6607'
PRP Supplier_Part_Number_3 '71-CRCW0402-100K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '100k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '100k'
PRP ValueDisplayed '100k'
PRP VDC_V '50V'
TOP 0 2.7420011 3.4180113 180 N 389 0 1
TOP 1 2.7420011 3.3786412 180 N 109 12 2
#
# CMP 373
CMP 5 1.1927149 2.1817 180 N R280 CRCW04022K20JNED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K20JNED'
PRP Power_W '63mW'
PRP Res_ohm '2.2k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.2KJCT-ND'
PRP Supplier_Part_Number_2 '59M6710'
PRP Supplier_Part_Number_3 '71-CRCW0402J-2.2K-E3'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP Value '2.2k'
PRP Value1 '5%'
PRP Value2 '0.063W'
PRP Value_Code '2k20'
PRP ValueDisplayed '2.2k'
PRP VDC_V '50V'
TOP 0 1.1730299 2.1817 90 N 403 0 1
TOP 1 1.2124 2.1817 90 N 109 18 2
#
# CMP 374
CMP 5 1.9486304 1.0619102 180 N R284 CRCW0402330KFKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW0402330KFKED'
PRP Power_W '63mW'
PRP Res_ohm '330k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-330KLCT-ND'
PRP Supplier_Part_Number_2 '72M6783'
PRP Supplier_Part_Number_3 '71-CRCW0402-330K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '330k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '330k'
PRP ValueDisplayed '330k'
PRP VDC_V '50V'
TOP 0 1.9289454 1.0619102 90 N 263 1 1
TOP 1 1.9683155 1.0619102 90 N 246 4 2
#
# CMP 375
CMP 5 1.9486305 0.9894883 0 N R285 CRCW0402330KFKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW0402330KFKED'
PRP Power_W '63mW'
PRP Res_ohm '330k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-330KLCT-ND'
PRP Supplier_Part_Number_2 '72M6783'
PRP Supplier_Part_Number_3 '71-CRCW0402-330K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '330k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '330k'
PRP ValueDisplayed '330k'
PRP VDC_V '50V'
TOP 0 1.9683155 0.9894883 270 N 424 292 1
TOP 1 1.9289454 0.9894883 270 N 263 2 2
#
# CMP 376
CMP 5 1.414482 2.7475414 270 N R286 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 1.414482 2.7278564 0 N 298 0 1
TOP 1 1.414482 2.7672265 0 N 261 7 2
#
# CMP 377
CMP 5 1.4870005 2.6129948 270 N R287 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 1.4870005 2.5933098 0 N 424 293 1
TOP 1 1.4870005 2.6326799 0 N 300 1 2
#
# CMP 378
CMP 5 1.4928007 2.7475415 90 N R288 CRCW04022K49FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04022K49FKED'
PRP Power_W '63mW'
PRP Res_ohm '2.49k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-2.49KLCT-ND'
PRP Supplier_Part_Number_2 '52K6803'
PRP Supplier_Part_Number_3 '71-CRCW0402-2.49K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '2.49k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '2k49'
PRP ValueDisplayed '2.49k'
PRP VDC_V '50V'
TOP 0 1.4928007 2.7672265 180 N 424 294 1
TOP 1 1.4928007 2.7278564 180 N 298 1 2
#
# CMP 379
CMP 5 2.046152 0.647916 180 N R301 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP INSTALLATION 'DNP'
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 2.026467 0.647916 90 N 285 0 1
TOP 1 2.0658371 0.647916 90 N 109 13 2
#
# CMP 380
CMP 5 2.0461521 0.6115359 0 N R303 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP INSTALLATION 'DNP'
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 2.0658371 0.6115359 270 N 424 295 1
TOP 1 2.026467 0.6115359 270 N 285 1 2
#
# CMP 381
CMP 5 1.9010005 0.3308757 270 N R309 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP INSTALLATION 'DNP'
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 1.9010005 0.3111907 0 N 284 0 1
TOP 1 1.9010005 0.3505608 0 N 109 14 2
#
# CMP 382
CMP 5 1.9480005 0.3308758 90 N R312 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP INSTALLATION 'DNP'
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 1.9480005 0.3505608 180 N 424 296 1
TOP 1 1.9480005 0.3111907 180 N 284 1 2
#
# CMP 383
CMP 5 1.8644342 4.0089696 0 N R315 CRCW04021K00FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW04021K00FKED'
PRP Power_W '63mW'
PRP Res_ohm '1k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-1.00KLCT-ND'
PRP Supplier_Part_Number_2 '52K6545'
PRP Supplier_Part_Number_3 '71-CRCW0402-1.0K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '1.00k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '1k00'
PRP ValueDisplayed '1.00k'
PRP VDC_V '50V'
TOP 0 1.8841192 4.0089696 270 N 422 2 1
TOP 1 1.8447491 4.0089696 270 N 458 16 2
#
# CMP 384
CMP 42 2.0237494 4.596127 270 N R316 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 2.0237494 4.5759499 270 N 423 3 1
TOP 1 2.0237494 4.6163042 270 N 148 2 2
#
# CMP 385
CMP 1 1.755078 1.718433 0 N R317 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 1.7661016 1.718433 270 N 308 24 1
TOP 1 1.7440544 1.718433 270 N 316 0 2
#
# CMP 386
CMP 1 1.7546372 1.63228 180 N R319 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 1.7436136 1.63228 90 N 314 0 1
TOP 1 1.7656608 1.63228 90 N 405 0 2
#
# CMP 387
CMP 1 0.2444477 1.5147133 180 N R321 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 0.2334241 1.5147133 90 N 424 297 1
TOP 1 0.2554713 1.5147133 90 N 414 1 2
#
# CMP 388
CMP 5 0.7320005 1.1478115 180 N R326 CRCW040210K0FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP INSTALLATION 'DNP'
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210K0FKED'
PRP Power_W '63mW'
PRP Res_ohm '10k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-10.0KLCT-ND'
PRP Supplier_Part_Number_2 '52K6595'
PRP Supplier_Part_Number_3 '71-CRCW0402-10K-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.0k'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10k0'
PRP ValueDisplayed '10.0k'
PRP VDC_V '50V'
TOP 0 0.7123155 1.1478115 90 N 424 298 1
TOP 1 0.7516856 1.1478115 90 N 388 0 2
#
# CMP 389
CMP 42 1.480135 4.1521869 180 N R330 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 1.4599579 4.1521869 0 N 257 1 1
TOP 1 1.5003122 4.1521869 0 N 268 1 2
#
# CMP 390
CMP 13 2.1136225 1.7889859 180 N R346 CSNL1206FT1L00 ;0=1,1=0.0531
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://www.seielect.com/Catalog/SEI-csnl.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Stackpole Electronics Inc'
PRP MountType 'SMT'
PRP PackageReference '1206'
PRP PartNumber 'CSNL1206FT1L00'
PRP Power_W '1W'
PRP Published '2008-06-26'
PRP Publisher 'Texas Instruments'
PRP Res_ohm '1m'
PRP RoHS 'Y'
PRP SizeArea_mm2 '5.12'
PRP SizeX_mm '3.2'
PRP SizeY_mm '1.6'
PRP SizeZ_mm '1.35'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'CSNL1206FT1L00CT-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Metal Element'
PRP TempCo '50 ppm/C'
PRP Tolerance__ '1%'
PRP U/M 'EA'
PRP Value '0.001'
PRP Value1 '1%'
PRP Value2 '1W'
PRP Value_Code '1L000'
PRP ValueDisplayed '0.001'
PRP VDC_V ''
TOP 0 2.0604729 1.7889859 90 N 455 8 1
TOP 1 2.1667721 1.7889859 90 N 109 15 2
#
# CMP 391
CMP 5 2.2900011 4.5583161 90 N R347 ERJ-2GEJ511X ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/DMA0000COL9.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP LatestRevisionDate ''
PRP Manufacturer 'Panasonic'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'ERJ-2GEJ511X'
PRP Power_W '100mW'
PRP Published ''
PRP Publisher ''
PRP Res_ohm '510'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 'P510JCT-ND'
PRP Supplier_Part_Number_2 '65T8293'
PRP Supplier_Part_Number_3 '667-ERJ-2GEJ511X'
PRP Technology 'Thick Film'
PRP TempCo '200 ppm/C'
PRP Tolerance__ '5%'
PRP U/M 'EA'
PRP Value '510'
PRP Value1 '5%'
PRP Value2 '0.1W'
PRP Value_Code '510R'
PRP ValueDisplayed '510'
PRP VDC_V '50V'
TOP 0 2.2900011 4.5780011 180 N 191 0 1
TOP 1 2.2900011 4.538631 180 N 407 0 2
#
# CMP 392
CMP 5 2.1336225 1.697671 90 N R352 CRCW040210R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '10.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '541-10.2LCT-ND'
PRP Supplier_Part_Number_2 '71-CRCW0402-10.2-E3'
PRP Supplier_Part_Number_3 '1158303'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10R2'
PRP ValueDisplayed '10.2'
PRP VDC_V '50V'
TOP 0 2.1336225 1.717356 180 N 109 16 1
TOP 1 2.1336225 1.6779859 180 N 201 1 2
#
# CMP 393
CMP 5 2.0936225 1.697671 90 N R348 CRCW040210R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '10.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '541-10.2LCT-ND'
PRP Supplier_Part_Number_2 '71-CRCW0402-10.2-E3'
PRP Supplier_Part_Number_3 '1158303'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10R2'
PRP ValueDisplayed '10.2'
PRP VDC_V '50V'
TOP 0 2.0936225 1.717356 180 N 455 9 1
TOP 1 2.0936225 1.6779859 180 N 200 1 2
#
# CMP 394
CMP 5 1.58686 4.1521869 180 N R362 CRCW040210R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040210R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '10.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 'Farnell'
PRP Supplier_Part_Number_1 '541-10.2LCT-ND'
PRP Supplier_Part_Number_2 '71-CRCW0402-10.2-E3'
PRP Supplier_Part_Number_3 '1158303'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '10.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '10R2'
PRP ValueDisplayed '10.2'
PRP VDC_V '50V'
TOP 0 1.567175 4.1521869 90 N 268 0 1
TOP 1 1.6065451 4.1521869 90 N 367 1 2
#
# CMP 395
CMP 1 2.8800011 3.3983262 90 N R371 CRCW02010000Z0ED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E24'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02010000Z0ED'
PRP Power_W '50mW'
PRP Res_ohm '0'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 'Newark'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '72M6743'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo 'ppm/C'
PRP Tolerance__ '5%'
PRP Value '0'
PRP Value1 '5%'
PRP Value2 '0.05W'
PRP Value_Code '0000'
PRP ValueDisplayed '0'
PRP VDC_V ''
TOP 0 2.8800011 3.4093498 180 N 267 2 1
TOP 1 2.8800011 3.3873026 180 N 229 0 2
#
# CMP 396
CMP 41 0.7391085 1.359565 0 N R374 ERJ-1GNF33R2C ;0=1,1=0.0000
PRP AEC_Category ''
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP CompType ''
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-1GNF33R2C.pdf'
PRP Digikey_Description 'RES SMD 33.2 OHM 1% 1/20W 0201'
PRP Digikey_Part_Number 'P122945CT-ND'
PRP EIA_Code ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP helpURL 'https://upverter.com/upn/revision/804e6f7ea13c6b2c/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP MountType ''
PRP Mouser_Description 'Thick Film Resistors - SMD 0201 33.2ohm 1% HalogenFree AEC-Q200'
PRP Mouser_Part_Number '667-ERJ-1GNF33R2C'
PRP Operating_Temperature_Range '-55°C to +125°C'
PRP PackageReference '0201'
PRP Part_Number 'ERJ-1GNF33R2C'
PRP PartNumber 'ERJ-1GNF33R2C'
PRP Power_W '50mW'
PRP Res_ohm '33.2'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm '0.26mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'P122945CT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-1GNF33R2C'
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo '200ppm/°C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 ''
PRP Value2 ''
PRP Value_Code ''
PRP ValueDisplayed ''
PRP VDC_V '25V'
TOP 0 0.7509195 1.359565 180 N 447 0 1
TOP 1 0.7272975 1.359565 180 N 226 1 2
#
# CMP 397
CMP 41 0.2926613 1.3460345 0 N R375 ERJ-1GNF33R2C ;0=1,1=0.0000
PRP AEC_Category ''
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP CompType ''
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-1GNF33R2C.pdf'
PRP Digikey_Description 'RES SMD 33.2 OHM 1% 1/20W 0201'
PRP Digikey_Part_Number 'P122945CT-ND'
PRP EIA_Code ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP helpURL 'https://upverter.com/upn/revision/804e6f7ea13c6b2c/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP MountType ''
PRP Mouser_Description 'Thick Film Resistors - SMD 0201 33.2ohm 1% HalogenFree AEC-Q200'
PRP Mouser_Part_Number '667-ERJ-1GNF33R2C'
PRP Operating_Temperature_Range '-55°C to +125°C'
PRP PackageReference '0201'
PRP Part_Number 'ERJ-1GNF33R2C'
PRP PartNumber 'ERJ-1GNF33R2C'
PRP Power_W '50mW'
PRP Res_ohm '33.2'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm '0.26mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'P122945CT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-1GNF33R2C'
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo '200ppm/°C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 ''
PRP Value2 ''
PRP Value_Code ''
PRP ValueDisplayed ''
PRP VDC_V '25V'
TOP 0 0.3044723 1.3460345 180 N 411 1 1
TOP 1 0.2808503 1.3460345 180 N 450 1 2
#
# CMP 398
CMP 41 0.2926613 1.3881028 0 N R376 ERJ-1GNF33R2C ;0=1,1=0.0000
PRP AEC_Category ''
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP CompType ''
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-1GNF33R2C.pdf'
PRP Digikey_Description 'RES SMD 33.2 OHM 1% 1/20W 0201'
PRP Digikey_Part_Number 'P122945CT-ND'
PRP EIA_Code ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP helpURL 'https://upverter.com/upn/revision/804e6f7ea13c6b2c/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP MountType ''
PRP Mouser_Description 'Thick Film Resistors - SMD 0201 33.2ohm 1% HalogenFree AEC-Q200'
PRP Mouser_Part_Number '667-ERJ-1GNF33R2C'
PRP Operating_Temperature_Range '-55°C to +125°C'
PRP PackageReference '0201'
PRP Part_Number 'ERJ-1GNF33R2C'
PRP PartNumber 'ERJ-1GNF33R2C'
PRP Power_W '50mW'
PRP Res_ohm '33.2'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm '0.26mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 'P122945CT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-1GNF33R2C'
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo '200ppm/°C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 ''
PRP Value2 ''
PRP Value_Code ''
PRP ValueDisplayed ''
PRP VDC_V '25V'
TOP 0 0.3044723 1.3881028 180 N 227 1 1
TOP 1 0.2808503 1.3881028 180 N 449 0 2
#
# CMP 399
CMP 5 2.437 3.224 270 N R386 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 2.437 3.204315 0 N 290 0 1
TOP 1 2.437 3.2436851 0 N 211 0 2
#
# CMP 400
CMP 5 1.756381 0.3303029 270 N R387 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 1.756381 0.3106179 0 N 256 0 1
TOP 1 1.756381 0.349988 0 N 208 0 2
#
# CMP 401
CMP 5 1.7048161 0.3308757 270 N R388 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 1.7048161 0.3111907 0 N 253 0 1
TOP 1 1.7048161 0.3505608 0 N 206 0 2
#
# CMP 402
CMP 5 1.6540533 0.3314663 270 N R389 CRCW040233R2FKED ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '0'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20035/dcrcwe3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0402'
PRP PartNumber 'CRCW040233R2FKED'
PRP Power_W '63mW'
PRP Res_ohm '33.2'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.5'
PRP SizeX_mm '1'
PRP SizeY_mm '0.5'
PRP SizeZ_mm '0.6'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-33.2LCT-ND'
PRP Supplier_Part_Number_2 '52K6980'
PRP Supplier_Part_Number_3 '71-CRCW0402-33.2-E3'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '33.2'
PRP Value1 '1%'
PRP Value2 '0.063W'
PRP Value_Code '33R2'
PRP ValueDisplayed '33.2'
PRP VDC_V '50V'
TOP 0 1.6540533 0.3117813 0 N 255 0 1
TOP 1 1.6540533 0.3511514 0 N 207 0 2
#
# CMP 403
CMP 42 0.7905231 2.3279326 180 N R400 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 0.770346 2.3279326 0 N 205 0 1
TOP 1 0.8107003 2.3279326 0 N 424 518 2
#
# CMP 404
CMP 42 0.3606331 2.1221908 0 N R401 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 0.3808102 2.1221908 180 N 202 1 1
TOP 1 0.3404559 2.1221908 180 N 446 9 2
#
# CMP 405
CMP 42 0.4038638 3.009183 270 N R419 ERJ-2GE0R00X ;0=1,1=0.0000
PRP AEC_Grade 'Grade 0'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet 'https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf'
PRP Datasheet_Path 'datasheets/Res-ERJ-2GE0R00X.pdf'
PRP Digikey_Description 'RES SMD 0 OHM JUMPER 1/10W 0402'
PRP Digikey_Part_Number 'P0.0JCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/2cded3eb4b39bf91/'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Panasonic'
PRP Mouser_Description 'Thick Film Resistors - SMD 0402 Zero ohms 5% Tol'
PRP Mouser_Part_Number '667-ERJ-2GE0R00X'
PRP Operating_Temperature_Range '-55°C to +155°C'
PRP PackageReference '0402'
PRP Part_Number 'ERJ-2GE0R00X'
PRP PartNumber 'ERJ-2GE0R00X'
PRP Power '100mW'
PRP Res_ohm '0'
PRP RoHS 'TRUE'
PRP Series 'ERJ'
PRP SizeZ_mm '0.4mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 'P0.0JCT-ND'
PRP Supplier_Part_Number_2 '667-ERJ-2GE0R00X'
PRP Technology 'Thick Film'
PRP Value '0'
TOP 0 0.4038638 2.9890059 270 N 182 1 1
TOP 1 0.4038638 3.0293602 270 N 446 10 2
#
# CMP 406
CMP 1 0.2918886 1.2973527 180 N R503 CRCW0201100RFKED ;0=1,1=0.0102
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code 'E96'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Semiconductor'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW0201100RFKED'
PRP Power_W '50mW'
PRP Res_ohm '100'
PRP RoHS 'Y'
PRP SizeArea_mm2 '0.18'
PRP SizeAreaWB_mm2 '2.08'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.26'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '100'
PRP Value1 '1%'
PRP Value2 '0.05W'
PRP Value_Code '100R'
PRP ValueDisplayed '100'
PRP VDC_V ''
TOP 0 0.280865 1.2973527 90 N 308 25 1
TOP 1 0.3029122 1.2973527 90 N 409 2 2
#
# CMP 407
CMP 0 0.2444477 1.4676121 180 N R508 CRCW02014K70FKED ;0=1,1=0.0130
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02014K70FKED'
PRP Power_W '50mW'
PRP Res_ohm '4.7k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.33'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-4.70KAABCT-ND'
PRP Supplier_Part_Number_2 '87W8644'
PRP Supplier_Part_Number_3 '71-CRCW02014K70FKED'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '4.70k'
PRP Value1 '1%'
PRP Value2 '0.05W'
PRP Value_Code '4k70'
PRP ValueDisplayed '4.70k'
PRP VDC_V '30V'
TOP 0 0.2334241 1.4676121 90 N 308 26 1
TOP 1 0.2554713 1.4676121 90 N 413 1 2
#
# CMP 408
CMP 0 0.7402896 1.478226 180 N R512 CRCW02014K70FKED ;0=1,1=0.0130
PRP AEC_Category 'Q200'
PRP AEC_Grade 'N/A'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet link'
PRP ComponentLink1URL 'http://www.vishay.com/docs/20052/crcw0201e3.pdf'
PRP CompType 'Resistor'
PRP EIA_Code ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Vishay-Dale'
PRP MountType 'SMT'
PRP PackageReference '0201'
PRP PartNumber 'CRCW02014K70FKED'
PRP Power_W '50mW'
PRP Res_ohm '4.7k'
PRP RoHS 'E'
PRP SizeArea_mm2 '0.18'
PRP SizeX_mm '0.6'
PRP SizeY_mm '0.3'
PRP SizeZ_mm '0.33'
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '541-4.70KAABCT-ND'
PRP Supplier_Part_Number_2 '87W8644'
PRP Supplier_Part_Number_3 '71-CRCW02014K70FKED'
PRP Technology 'Thick Film'
PRP TempCo '100 ppm/C'
PRP Tolerance__ '1%'
PRP Value '4.70k'
PRP Value1 '1%'
PRP Value2 '0.05W'
PRP Value_Code '4k70'
PRP ValueDisplayed '4.70k'
PRP VDC_V '30V'
TOP 0 0.729266 1.478226 90 N 410 1 1
TOP 1 0.7513132 1.478226 90 N 424 299 2
#
# CMP 409
CMP 81 1.2504336 1.461402 0 N S2 CJS-1201TA ;0=1,1=0.0984
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Circuit 'SPDT'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://copal-electronics.info/en/0008e/02461.pdf'
PRP CompType 'Switch'
PRP CurrentRating_mA '100A'
PRP LatestRevisionDate '2017-03-09'
PRP Manufacturer 'Copal Electronics'
PRP MountType 'SMT'
PRP Orientation 'Side Actuated'
PRP PackageReference 'SW, 3.1x2.5x6 mm'
PRP PartNumber 'CJS-1201TA'
PRP PositionCount '1'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '563-1023-1-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP SwitchFunction 'On-Off-On'
PRP VDC_V '50V'
TOP 0 1.3193312 1.4161264 180 N 308 27 1
TOP 1 1.2504336 1.5066776 180 N 209 0 2
TOP 2 1.181536 1.4161264 180 N 424 300 3
#
# CMP 410
CMP 60 0.7178224 4.6375065 270 N TP7 5001 ;0=2,1=0.1811
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cert_CSA ''
PRP Cert_CULUS ''
PRP Cert_UL ''
PRP Cert_VDE ''
PRP ClassName ''
PRP CNHeader 'FALSE'
PRP Color 'Black'
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.keyelco.com/userAssets/file/M60-2p60.pdf'
PRP CompType 'Test Point'
PRP ContactFinish 'Silver'
PRP CT 'TRUE'
PRP Current_A ''
PRP Gender ''
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Incomplete'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '26/05/2017'
PRP Manufacturer 'Keystone Electronics'
PRP MountType 'TH'
PRP Note ''
PRP Orientation ''
PRP PackageReference 'Black Miniature Testpoint'
PRP PartNumber '5001'
PRP PinCount ''
PRP Pitch_mm ''
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP Row_Count ''
PRP RowSpacing_mm ''
PRP Shrouded ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Mouser'
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '36-5001-ND'
PRP Supplier_Part_Number_2 '534-5001'
PRP Supplier_Part_Number_3 ''
PRP Voltage_V ''
TOP 0 0.7178224 4.6375065 270 N 424 535 1
#
# CMP 411
CMP 45 2.6161428 4.6193318 0 N U1 GD25B64CWAG ;0=1,1=0.0010
PRP Access_Time '7ns'
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.gigadevice.com/datasheet/gd25b64c/'
PRP Datasheet 'https://www.gigadevice.com/datasheet/gd25b64c/'
PRP Datasheet_Path 'datasheets/IC-GD25B64CWAG.pdf'
PRP Frequency_Fixed '120MHz'
PRP helpURL 'https://upverter.com/upn/revision/4df42c5e97fa062f/'
PRP Interface 'SPI,Other'
PRP Lead_Free 'Yes'
PRP Manufacturer 'GigaDevice'
PRP Max_Supply_Voltage '3.6V'
PRP Memory_Size '64Mbits'
PRP Memory_Type 'FLASH'
PRP Min_Supply_Voltage '2.7V'
PRP Nominal_Supply_Current '13-15mA'
PRP Operating_Temperature_Range '-40°C to +125°C'
PRP PackageReference 'WSON8'
PRP Part_Number 'GD25B64CWAG'
PRP PartNumber 'GD25B64CWAG'
PRP RoHS 'TRUE'
PRP SizeZ_mm '0.8mm'
PRP Standoff_Height '0mm'
PRP TaMax_C '+125°C'
PRP TaMin_C '-40°C'
TOP 0 2.7234855 4.6943318 180 N 307 0 1
TOP 1 2.7234855 4.6443318 180 N 339 1 2
TOP 2 2.7234855 4.5943318 180 N 337 1 3
TOP 3 2.7234855 4.5443318 180 N 424 335 4
TOP 4 2.5088001 4.5443318 180 N 335 1 5
TOP 5 2.5088001 4.5943318 180 N 336 1 6
TOP 6 2.5088001 4.6443318 180 N 338 1 7
TOP 7 2.5088001 4.6943318 180 N 382 3 8
TOP 8 2.6161428 4.6193318 180 N 424 334 9
#
# CMP 412
CMP 68 1.3762045 3.1475661 180 N U4 DP83TG720SWRNDRQ1 ;0=1,1=0.0354
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer 'Texas Instruments'
PRP Alternate_PartNumber 'DP83TG720SWRNDTQ1'
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/dp83tg720s-q1.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/dp83tg720s-q1'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/dp83tg720s-q1/datasheet'
PRP CompType 'IC'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP Operating_Temperature_Range ''
PRP PackageDescription 'VQFNP-36'
PRP PackageReference 'RND0036A'
PRP PartNumber 'DP83TG720SWRNDRQ1'
PRP Rating ''
PRP RoHS ''
PRP SizeArea_mm2 '36'
PRP SizeAreaWB_mm2 '64'
PRP SizeX_mm '6'
PRP SizeY_mm '6'
PRP SizeZ_mm '0.9'
TOP 0 1.2620314 3.0688259 0 N 82 0 1
TOP 1 1.2620314 3.088511 0 N 107 1 2
TOP 2 1.2620314 3.108196 0 N 106 0 3
TOP 3 1.2620314 3.1278811 0 N 104 0 4
TOP 4 1.2620314 3.1475661 0 N 105 1 5
TOP 5 1.2620314 3.1672511 0 N 34 0 6
TOP 6 1.2620314 3.1869362 0 N 44 2 7
TOP 7 1.2620314 3.2066212 0 N 90 0 8
TOP 8 1.2620314 3.2263063 0 N 26 0 9
TOP 9 1.2974644 3.2617393 90 N 43 1 10
TOP 10 1.3171495 3.2617393 90 N 98 3 11
TOP 11 1.3368345 3.2617393 90 N 102 0 12
TOP 12 1.3565196 3.2617393 90 N 103 0 13
TOP 13 1.3762046 3.2617393 90 N 21 2 14
TOP 14 1.3958896 3.2617393 90 N 77 0 15
TOP 15 1.4155747 3.2617393 90 N 108 0 16
TOP 16 1.4352597 3.2617393 90 N 0 143 17
TOP 17 1.4549448 3.2617393 90 N 11 0 18
TOP 18 1.4903778 3.2263063 0 N 25 1 19
TOP 19 1.4903778 3.2066212 0 N 0 144 20
TOP 20 1.4903778 3.1869362 0 N 18 7 21
TOP 21 1.4903778 3.1672511 0 N 69 13 22
TOP 22 1.4903778 3.1475661 0 N 78 0 23
TOP 23 1.4903778 3.1278811 0 N 79 0 24
TOP 24 1.4903778 3.108196 0 N 80 0 25
TOP 25 1.4903778 3.088511 0 N 81 0 26
TOP 26 1.4903778 3.0688259 0 N 42 0 27
TOP 27 1.4549448 3.0333929 90 N 89 1 28
TOP 28 1.4352597 3.0333929 90 N 84 1 29
TOP 29 1.4155747 3.0333929 90 N 85 1 30
TOP 30 1.3958896 3.0333929 90 N 86 1 31
TOP 31 1.3762046 3.0333929 90 N 87 1 32
TOP 32 1.3565196 3.0333929 90 N 88 1 33
TOP 33 1.3368345 3.0333929 90 N 69 14 34
TOP 34 1.3171495 3.0333929 90 N 35 0 35
TOP 35 1.2974644 3.0333929 90 N 83 0 36
TOP 36 1.3762046 3.1475661 0 N 424 363 37
#
# CMP 413
CMP 65 1.5437826 0.7453942 0 N U6 TM4C1294NCPDTT3 ;0=1,1=0.0472
PRP ADC_Channels '20'
PRP ADC_Resolution '12 Bits'
PRP ComponentLink1Description 'Manufacturer URL'
PRP ComponentLink1URL 'http://www.ti.com/'
PRP ComponentLink2Description 'Datasheet'
PRP ComponentLink2URL 'http://www.ti.com/lit/ds/symlink/tm4c1294ncpdt.pdf'
PRP ComponentLink3Description 'Package Specification'
PRP ComponentLink3URL 'http://www.ti.com/lit/ml/mpqf013/mpqf013.pdf'
PRP CompType 'IC'
PRP CPU 'ARM Cortex-M4'
PRP DatasheetVersion '15863.2743'
PRP Eco-Plan 'Green (RoHS & no Sb/Br)'
PRP Flash '1024 KB'
PRP Manufacturer 'Texas Instruments'
PRP Max_Speed '120 MHz'
PRP Mounting_Technology 'Surface Mount'
PRP MountType 'SMT'
PRP PackageDescription '128-Pin Thin Quad Flat Package, Body 14 x 14 mm, Pitch 0.4 mm'
PRP PackageReference 'PDT0128A'
PRP PackageVersion '4087726/A'
PRP Packing 'Tray'
PRP PartId '1'
PRP PartNumber 'TM4C1294NCPDTT3'
PRP SizeArea_mm2 '256.0'
PRP SizeAreaWB_mm2 '324.0'
PRP SizeX_mm '16.0'
PRP SizeY_mm '16.0'
PRP SizeZ_mm '1.2'
PRP SRAM '256 KB'
PRP Temperature_Range '-40 to 105 degC'
TOP 0 1.8469322 0.9894887 270 N 263 3 1
TOP 1 1.8469322 0.9737407 270 N 0 142 2
TOP 2 1.8469322 0.9579926 270 N 0 141 3
TOP 3 1.8469322 0.9422446 270 N 0 140 4
TOP 4 1.8469322 0.9264966 270 N 0 139 5
TOP 5 1.8469322 0.9107485 270 N 0 138 6
TOP 6 1.8469322 0.8950005 270 N 308 51 7
TOP 7 1.8469322 0.8792525 270 N 308 52 8
TOP 8 1.8469322 0.8635044 270 N 241 3 9
TOP 9 1.8469322 0.8477564 270 N 424 354 10
TOP 10 1.8469322 0.8320084 270 N 0 137 11
TOP 11 1.8469322 0.8162603 270 N 0 136 12
TOP 12 1.8469322 0.8005123 270 N 0 135 13
TOP 13 1.8469322 0.7847643 270 N 0 134 14
TOP 14 1.8469322 0.7690162 270 N 0 133 15
TOP 15 1.8469322 0.7532682 270 N 308 48 16
TOP 16 1.8469322 0.7375202 270 N 424 355 17
TOP 17 1.8469322 0.7217721 270 N 0 132 18
TOP 18 1.8469322 0.7060241 270 N 0 131 19
TOP 19 1.8469322 0.6902761 270 N 0 130 20
TOP 20 1.8469322 0.6745281 270 N 0 129 21
TOP 21 1.8469322 0.65878 270 N 0 128 22
TOP 22 1.8469322 0.643032 270 N 0 127 23
TOP 23 1.8469322 0.627284 270 N 0 126 24
TOP 24 1.8469322 0.6115359 270 N 250 0 25
TOP 25 1.8469322 0.5957879 270 N 308 49 26
TOP 26 1.8469322 0.5800399 270 N 0 125 27
TOP 27 1.8469322 0.5642918 270 N 308 50 28
TOP 28 1.8469322 0.5485438 270 N 0 124 29
TOP 29 1.8469322 0.5327958 270 N 0 123 30
TOP 30 1.8469322 0.5170477 270 N 0 122 31
TOP 31 1.8469322 0.5012997 270 N 0 121 32
TOP 32 1.7878771 0.4422446 180 N 251 0 33
TOP 33 1.7721291 0.4422446 180 N 252 0 34
TOP 34 1.756381 0.4422446 180 N 208 1 35
TOP 35 1.740633 0.4422446 180 N 206 1 36
TOP 36 1.724885 0.4422446 180 N 254 0 37
TOP 37 1.7091369 0.4422446 180 N 207 1 38
TOP 38 1.6933889 0.4422446 180 N 308 45 39
TOP 39 1.6776409 0.4422446 180 N 111 0 40
TOP 40 1.6618928 0.4422446 180 N 0 120 41
TOP 41 1.6461448 0.4422446 180 N 0 119 42
TOP 42 1.6303968 0.4422446 180 N 0 118 43
TOP 43 1.6146487 0.4422446 180 N 0 117 44
TOP 44 1.5989007 0.4422446 180 N 0 116 45
TOP 45 1.5831527 0.4422446 180 N 0 115 46
TOP 46 1.5674046 0.4422446 180 N 308 43 47
TOP 47 1.5516566 0.4422446 180 N 424 356 48
TOP 48 1.5359086 0.4422446 180 N 0 114 49
TOP 49 1.5201605 0.4422446 180 N 0 113 50
TOP 50 1.5044125 0.4422446 180 N 308 44 51
TOP 51 1.4886645 0.4422446 180 N 308 39 52
TOP 52 1.4729165 0.4422446 180 N 0 112 53
TOP 53 1.4571684 0.4422446 180 N 0 111 54
TOP 54 1.4414204 0.4422446 180 N 424 357 55
TOP 55 1.4256724 0.4422446 180 N 0 110 56
TOP 56 1.4099243 0.4422446 180 N 0 109 57
TOP 57 1.3941763 0.4422446 180 N 424 358 58
TOP 58 1.3784283 0.4422446 180 N 326 1 59
TOP 59 1.3626802 0.4422446 180 N 328 1 60
TOP 60 1.3469322 0.4422446 180 N 330 1 61
TOP 61 1.3311842 0.4422446 180 N 329 1 62
TOP 62 1.3154361 0.4422446 180 N 331 1 63
TOP 63 1.2996881 0.4422446 180 N 424 359 64
TOP 64 1.240633 0.5012997 270 N 0 108 65
TOP 65 1.240633 0.5170477 270 N 424 360 66
TOP 66 1.240633 0.5327958 270 N 0 107 67
TOP 67 1.240633 0.5485438 270 N 242 2 68
TOP 68 1.240633 0.5642918 270 N 308 38 69
TOP 69 1.240633 0.5800399 270 N 245 1 70
TOP 70 1.240633 0.5957879 270 N 0 106 71
TOP 71 1.240633 0.6115359 270 N 0 105 72
TOP 72 1.240633 0.627284 270 N 0 104 73
TOP 73 1.240633 0.643032 270 N 0 103 74
TOP 74 1.240633 0.65878 270 N 0 102 75
TOP 75 1.240633 0.6745281 270 N 0 101 76
TOP 76 1.240633 0.6902761 270 N 0 100 77
TOP 77 1.240633 0.7060241 270 N 0 99 78
TOP 78 1.240633 0.7217721 270 N 308 40 79
TOP 79 1.240633 0.7375202 270 N 424 361 80
TOP 80 1.240633 0.7532682 270 N 0 98 81
TOP 81 1.240633 0.7690162 270 N 0 97 82
TOP 82 1.240633 0.7847643 270 N 0 96 83
TOP 83 1.240633 0.8005123 270 N 0 95 84
TOP 84 1.240633 0.8162603 270 N 0 94 85
TOP 85 1.240633 0.8320084 270 N 0 93 86
TOP 86 1.240633 0.8477564 270 N 262 2 87
TOP 87 1.240633 0.8635044 270 N 244 2 88
TOP 88 1.240633 0.8792525 270 N 243 2 89
TOP 89 1.240633 0.8950005 270 N 308 41 90
TOP 90 1.240633 0.9107485 270 N 0 92 91
TOP 91 1.240633 0.9264966 270 N 0 91 92
TOP 92 1.240633 0.9422446 270 N 249 2 93
TOP 93 1.240633 0.9579926 270 N 248 2 94
TOP 94 1.240633 0.9737407 270 N 189 0 95
TOP 95 1.240633 0.9894887 270 N 374 2 96
TOP 96 1.2996881 1.0485438 180 N 0 90 97
TOP 97 1.3154361 1.0485438 180 N 0 89 98
TOP 98 1.3311842 1.0485438 180 N 0 88 99
TOP 99 1.3469322 1.0485438 180 N 0 87 100
TOP 100 1.3626802 1.0485438 180 N 308 42 101
TOP 101 1.3784283 1.0485438 180 N 0 86 102
TOP 102 1.3941763 1.0485438 180 N 0 85 103
TOP 103 1.4099243 1.0485438 180 N 0 84 104
TOP 104 1.4256724 1.0485438 180 N 0 83 105
TOP 105 1.4414204 1.0485438 180 N 0 82 106
TOP 106 1.4571684 1.0485438 180 N 0 81 107
TOP 107 1.4729165 1.0485438 180 N 0 80 108
TOP 108 1.4886645 1.0485438 180 N 0 79 109
TOP 109 1.5044125 1.0485438 180 N 0 78 110
TOP 110 1.5201605 1.0485438 180 N 0 77 111
TOP 111 1.5359086 1.0485438 180 N 0 76 112
TOP 112 1.5516566 1.0485438 180 N 308 46 113
TOP 113 1.5674046 1.0485438 180 N 424 362 114
TOP 114 1.5831527 1.0485438 180 N 262 3 115
TOP 115 1.5989007 1.0485438 180 N 0 75 116
TOP 116 1.6146487 1.0485438 180 N 0 74 117
TOP 117 1.6303968 1.0485438 180 N 0 73 118
TOP 118 1.6461448 1.0485438 180 N 0 72 119
TOP 119 1.6618928 1.0485438 180 N 0 71 120
TOP 120 1.6776409 1.0485438 180 N 0 70 121
TOP 121 1.6933889 1.0485438 180 N 308 47 122
TOP 122 1.7091369 1.0485438 180 N 0 69 123
TOP 123 1.724885 1.0485438 180 N 0 68 124
TOP 124 1.740633 1.0485438 180 N 0 67 125
TOP 125 1.756381 1.0485438 180 N 0 66 126
TOP 126 1.7721291 1.0485438 180 N 0 65 127
TOP 127 1.7878771 1.0485438 180 N 0 64 128
#
# CMP 414
CMP 21 2.9265716 2.0788648 180 N U9 INA228AIDGST ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.ti.com/lit/ds/symlink/ina228.pdf?ts=1623689466455&ref_url=https%253A%252F%252Fwww.ti.com%252Fproduct%252FINA228%253FkeyMatch%253DINA228AIDGST%2526tisearch%253Dsearch-everything%2526usecase%253DOPN'
PRP Datasheet 'https://www.ti.com/lit/ds/symlink/ina228.pdf?ts=1623689466455&ref_url=https%253A%252F%252Fwww.ti.com%252Fproduct%252FINA228%253FkeyMatch%253DINA228AIDGST%2526tisearch%253Dsearch-everything%2526usecase%253DOPN'
PRP Datasheet_Path 'datasheets/IC-INA228AIDGST.pdf'
PRP Digikey_Description '85-V, 20-BIT, ULTRA-PRECISE, I2C'
PRP Digikey_Part_Number '296-INA228AIDGSTCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/fd3a73c0321b44f2/'
PRP Input_Bias_Current '0.01uA'
PRP Input_Offset_Voltage '1mV'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Texas Instruments'
PRP Max_Supply_Voltage '5.5V'
PRP Min_Supply_Voltage '2.7V'
PRP Mouser_Part_Number '595-INA228AIDGST'
PRP Nominal_Supply_Current '640uA'
PRP Number_Of_Channels '1'
PRP Operating_Temperature_Range '-40°C to +125°C'
PRP PackageReference 'VSSOP10'
PRP Part_Number 'INA228AIDGST'
PRP PartNumber 'INA228AIDGST'
PRP RoHS 'TRUE'
PRP SizeZ_mm '1.1mm'
PRP Standoff_Height '0.05mm'
PRP TaMax_C '+125°C'
PRP TaMin_C '-40°C'
PRP TJmax_C '+150°C'
TOP 0 2.8399574 2.0394947 0 N 424 323 1
TOP 1 2.8399574 2.0591798 0 N 424 324 2
TOP 2 2.8399574 2.0788648 0 N 0 45 3
TOP 3 2.8399574 2.0985498 0 N 342 0 4
TOP 4 2.8399574 2.1182349 0 N 343 0 5
TOP 5 3.0131858 2.1182349 0 N 308 35 6
TOP 6 3.0131858 2.0985498 0 N 424 325 7
TOP 7 3.0131858 2.0788648 0 N 458 17 8
TOP 8 3.0131858 2.0591798 0 N 380 2 9
TOP 9 3.0131858 2.0394947 0 N 381 2 10
#
# CMP 415
CMP 29 3.0758171 1.3009952 0 N U10 TPD4E004DRYR ;0=1,1=0.0236
PRP 1394_/_Firewire 'TRUE'
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Breakdown_Voltage(Min)(V) '6'
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/tpd4e004.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/tpd4e004'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/tpd4e004/datasheet'
PRP CompType 'IC'
PRP Ctotal(Typ)(pF) ''
PRP Differential_Capacitance(pF) ''
PRP Eco-Plan 'Green (RoHS & no Sb/Br)'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP HDMI ''
PRP IEC_61000-4-2_Air-Gap(+/-_kV) '12'
PRP IEC_61000-4-2_Air-Gap(Typ)(+/-_kV) ''
PRP IEC_61000-4-2_Contact(+/-_kV) '8'
PRP IEC_61000-4-2_Contact(Typ)(+/-_kV) ''
PRP IO_Capacitance(Typ)(pF) '1.6'
PRP IO_Leakage_Current(nA) '1'
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP Number_Of_Channels ''
PRP Operating_Temperature_Range '-40 to 85 C'
PRP PackageDescription 'USON-6'
PRP PackageReference 'DRY0006A'
PRP PartNumber 'TPD4E004DRYR'
PRP Rating 'Catalog'
PRP RoHS 'Y'
PRP Serial_ATA_/_eSATA 'TRUE'
PRP SizeArea_mm2 '1.45'
PRP SizeAreaWB_mm2 '4.9'
PRP SizeX_mm '1.0'
PRP SizeY_mm '1.45'
PRP SizeZ_mm '0.6'
PRP USB_Full_Speed ''
PRP USB_High_Speed 'TRUE'
PRP USB_Super_Speed ''
TOP 0 3.0866439 1.3206803 270 N 249 1 1
TOP 1 3.0876281 1.3009953 270 N 248 1 2
TOP 2 3.0876281 1.2813102 270 N 424 331 3
TOP 3 3.0640061 1.2813102 270 N 247 1 4
TOP 4 3.0640061 1.3009953 270 N 195 1 5
TOP 5 3.0640061 1.3206803 270 N 246 5 6
#
# CMP 416
CMP 21 3.0800005 2.2759139 0 N U11 INA228AIDGST ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.ti.com/lit/ds/symlink/ina228.pdf?ts=1623689466455&ref_url=https%253A%252F%252Fwww.ti.com%252Fproduct%252FINA228%253FkeyMatch%253DINA228AIDGST%2526tisearch%253Dsearch-everything%2526usecase%253DOPN'
PRP Datasheet 'https://www.ti.com/lit/ds/symlink/ina228.pdf?ts=1623689466455&ref_url=https%253A%252F%252Fwww.ti.com%252Fproduct%252FINA228%253FkeyMatch%253DINA228AIDGST%2526tisearch%253Dsearch-everything%2526usecase%253DOPN'
PRP Datasheet_Path 'datasheets/IC-INA228AIDGST.pdf'
PRP Digikey_Description '85-V, 20-BIT, ULTRA-PRECISE, I2C'
PRP Digikey_Part_Number '296-INA228AIDGSTCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/fd3a73c0321b44f2/'
PRP Input_Bias_Current '0.01uA'
PRP Input_Offset_Voltage '1mV'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Texas Instruments'
PRP Max_Supply_Voltage '5.5V'
PRP Min_Supply_Voltage '2.7V'
PRP Mouser_Part_Number '595-INA228AIDGST'
PRP Nominal_Supply_Current '640uA'
PRP Number_Of_Channels '1'
PRP Operating_Temperature_Range '-40°C to +125°C'
PRP PackageReference 'VSSOP10'
PRP Part_Number 'INA228AIDGST'
PRP PartNumber 'INA228AIDGST'
PRP RoHS 'TRUE'
PRP SizeZ_mm '1.1mm'
PRP Standoff_Height '0.05mm'
PRP TaMax_C '+125°C'
PRP TaMin_C '-40°C'
PRP TJmax_C '+150°C'
TOP 0 3.1666147 2.315284 180 N 424 301 1
TOP 1 3.1666147 2.2955989 180 N 308 29 2
TOP 2 3.1666147 2.2759139 180 N 0 40 3
TOP 3 3.1666147 2.2562289 180 N 340 0 4
TOP 4 3.1666147 2.2365438 180 N 341 0 5
TOP 5 2.9933863 2.2365438 180 N 308 28 6
TOP 6 2.9933863 2.2562289 180 N 424 302 7
TOP 7 2.9933863 2.2759139 180 N 457 17 8
TOP 8 2.9933863 2.2955989 180 N 378 2 9
TOP 9 2.9933863 2.315284 180 N 379 2 10
#
# CMP 417
CMP 21 2.084095 1.4778049 270 N U12 INA228AIDGST ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.ti.com/lit/ds/symlink/ina228.pdf?ts=1623689466455&ref_url=https%253A%252F%252Fwww.ti.com%252Fproduct%252FINA228%253FkeyMatch%253DINA228AIDGST%2526tisearch%253Dsearch-everything%2526usecase%253DOPN'
PRP Datasheet 'https://www.ti.com/lit/ds/symlink/ina228.pdf?ts=1623689466455&ref_url=https%253A%252F%252Fwww.ti.com%252Fproduct%252FINA228%253FkeyMatch%253DINA228AIDGST%2526tisearch%253Dsearch-everything%2526usecase%253DOPN'
PRP Datasheet_Path 'datasheets/IC-INA228AIDGST.pdf'
PRP Digikey_Description '85-V, 20-BIT, ULTRA-PRECISE, I2C'
PRP Digikey_Part_Number '296-INA228AIDGSTCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/fd3a73c0321b44f2/'
PRP Input_Bias_Current '0.01uA'
PRP Input_Offset_Voltage '1mV'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Texas Instruments'
PRP Max_Supply_Voltage '5.5V'
PRP Min_Supply_Voltage '2.7V'
PRP Mouser_Part_Number '595-INA228AIDGST'
PRP Nominal_Supply_Current '640uA'
PRP Number_Of_Channels '1'
PRP Operating_Temperature_Range '-40°C to +125°C'
PRP PackageReference 'VSSOP10'
PRP Part_Number 'INA228AIDGST'
PRP PartNumber 'INA228AIDGST'
PRP RoHS 'TRUE'
PRP SizeZ_mm '1.1mm'
PRP Standoff_Height '0.05mm'
PRP TaMax_C '+125°C'
PRP TaMin_C '-40°C'
PRP TJmax_C '+150°C'
TOP 0 2.1234651 1.3911907 270 N 308 31 1
TOP 1 2.10378 1.3911907 270 N 424 303 2
TOP 2 2.084095 1.3911907 270 N 0 41 3
TOP 3 2.06441 1.3911907 270 N 333 0 4
TOP 4 2.0447249 1.3911907 270 N 334 0 5
TOP 5 2.0447249 1.5644191 270 N 308 30 6
TOP 6 2.06441 1.5644191 270 N 424 304 7
TOP 7 2.084095 1.5644191 270 N 455 10 8
TOP 8 2.10378 1.5644191 270 N 200 2 9
TOP 9 2.1234651 1.5644191 270 N 201 2 10
#
# CMP 418
CMP 61 1.1136725 4.3096873 180 N U18 FT4232HL ;0=1,1=0.0630
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet URL'
PRP ComponentLink1URL 'http://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT4232H.pdf'
PRP LatestRevisionDate '09/03/2017'
PRP Manufacturer 'FTDI'
PRP MountType 'SMT'
PRP PackageReference 'LQFP_10x10mm'
PRP PartNumber 'FT4232HL'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 'Newark'
PRP Supplier_3 'Mouser'
PRP Supplier_Part_Number_1 '768-1026-1-ND'
PRP Supplier_Part_Number_2 '80P4241'
PRP Supplier_Part_Number_3 '895-FT4232HL'
TOP 0 0.8951686 4.1620494 90 N 424 351 1
TOP 1 0.8951686 4.1817345 90 N 240 1 2
TOP 2 0.8951686 4.2014195 90 N 239 1 3
TOP 3 0.8951686 4.2211046 90 N 259 2 4
TOP 4 0.8951686 4.2407896 90 N 424 350 5
TOP 5 0.8951686 4.2604746 90 N 301 1 6
TOP 6 0.8951686 4.2801597 90 N 429 2 7
TOP 7 0.8951686 4.2998447 90 N 428 2 8
TOP 8 0.8951686 4.3195298 90 N 258 2 9
TOP 9 0.8951686 4.3392148 90 N 424 349 10
TOP 10 0.8951686 4.3588998 90 N 424 348 11
TOP 11 0.8951686 4.3785849 90 N 425 7 12
TOP 12 0.8951686 4.3982699 90 N 424 347 13
TOP 13 0.8951686 4.417955 90 N 176 1 14
TOP 14 0.8951686 4.43764 90 N 424 346 15
TOP 15 0.8951686 4.457325 90 N 432 1 16
TOP 16 0.9660347 4.5281912 0 N 433 1 17
TOP 17 0.9857198 4.5281912 0 N 434 0 18
TOP 18 1.0054048 4.5281912 0 N 431 1 19
TOP 19 1.0250899 4.5281912 0 N 436 15 20
TOP 20 1.0447749 4.5281912 0 N 0 48 21
TOP 21 1.0644599 4.5281912 0 N 0 49 22
TOP 22 1.084145 4.5281912 0 N 0 50 23
TOP 23 1.10383 4.5281912 0 N 0 51 24
TOP 24 1.1235151 4.5281912 0 N 424 345 25
TOP 25 1.1432001 4.5281912 0 N 417 0 26
TOP 26 1.1628851 4.5281912 0 N 416 0 27
TOP 27 1.1825702 4.5281912 0 N 415 0 28
TOP 28 1.2022552 4.5281912 0 N 0 52 29
TOP 29 1.2219403 4.5281912 0 N 0 53 30
TOP 30 1.2416253 4.5281912 0 N 436 14 31
TOP 31 1.2613103 4.5281912 0 N 419 0 32
TOP 32 1.3321765 4.457325 90 N 0 54 33
TOP 33 1.3321765 4.43764 90 N 418 0 34
TOP 34 1.3321765 4.417955 90 N 424 344 35
TOP 35 1.3321765 4.3982699 90 N 327 0 36
TOP 36 1.3321765 4.3785849 90 N 425 6 37
TOP 37 1.3321765 4.3588998 90 N 0 55 38
TOP 38 1.3321765 4.3392148 90 N 265 0 39
TOP 39 1.3321765 4.3195298 90 N 0 56 40
TOP 40 1.3321765 4.2998447 90 N 0 57 41
TOP 41 1.3321765 4.2801597 90 N 436 13 42
TOP 42 1.3321765 4.2604746 90 N 0 58 43
TOP 43 1.3321765 4.2407896 90 N 0 59 44
TOP 44 1.3321765 4.2211046 90 N 310 0 45
TOP 45 1.3321765 4.2014195 90 N 257 0 46
TOP 46 1.3321765 4.1817345 90 N 424 343 47
TOP 47 1.3321765 4.1620494 90 N 134 0 48
TOP 48 1.2613103 4.0911833 0 N 425 5 49
TOP 49 1.2416253 4.0911833 0 N 436 12 50
TOP 50 1.2219403 4.0911833 0 N 424 342 51
TOP 51 1.2022552 4.0911833 0 N 133 0 52
TOP 52 1.1825702 4.0911833 0 N 291 1 53
TOP 53 1.1628851 4.0911833 0 N 289 1 54
TOP 54 1.1432001 4.0911833 0 N 287 1 55
TOP 55 1.1235151 4.0911833 0 N 436 11 56
TOP 56 1.10383 4.0911833 0 N 0 60 57
TOP 57 1.084145 4.0911833 0 N 0 61 58
TOP 58 1.0644599 4.0911833 0 N 0 62 59
TOP 59 1.0447749 4.0911833 0 N 0 63 60
TOP 60 1.0250899 4.0911833 0 N 451 0 61
TOP 61 1.0054048 4.0911833 0 N 453 0 62
TOP 62 0.9857198 4.0911833 0 N 452 0 63
TOP 63 0.9660347 4.0911833 0 N 425 4 64
#
# CMP 419
CMP 25 1.6458951 4.5118081 180 N U20 TPS79601DRBR ;0=1,1=0.0394
PRP Accuracy(_) '2'
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Manufacturer URL'
PRP ComponentLink1URL 'http://www.ti.com/'
PRP ComponentLink2Description 'Datasheet'
PRP ComponentLink2URL 'http://www.ti.com/general/docs/lit/getliterature.tsp?genericPartNumber=TPS79601&fileType=pdf'
PRP ComponentLink3Description 'Package Specification'
PRP ComponentLink3URL 'http://www.ti.com/litv/pdf/mpds118h'
PRP CompType 'IC'
PRP DatasheetVersion 'SLVS351N'
PRP Eco-Plan 'Green (RoHS & no Sb/Br)'
PRP Iout(Max)(A) '1'
PRP Iq(Typ)(mA) '0.26'
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP PackageDescription 'VSON-8'
PRP PackageReference 'DRB0008B'
PRP PackageVersion '4203482-2/K'
PRP PartNumber 'TPS79601DRBR'
PRP RoHS 'Y'
PRP SizeArea_mm2 '9.0'
PRP SizeAreaWB_mm2 '16.0'
PRP SizeX_mm '3.0'
PRP SizeY_mm '3.0'
PRP SizeZ_mm '1.0'
PRP SubFamily 'Single Channel LDO'
PRP U/M ''
PRP Vdo(Typ)(mV) '250'
PRP Vin(Max)(V) '5.5'
PRP Vin(Min)(V) '2.7'
PRP Vout_Adj(Max)(V) '5.5'
PRP Vout_Adj(Min)(V) '1.2'
TOP 0 1.5907769 4.4734222 90 N 426 10 1
TOP 1 1.5907769 4.4990128 90 N 426 9 2
TOP 2 1.5907769 4.5246033 90 N 260 6 3
TOP 3 1.5907769 4.5501939 90 N 260 5 4
TOP 4 1.7010131 4.5501939 90 N 325 2 5
TOP 5 1.7010131 4.5246033 90 N 424 329 6
TOP 6 1.7010131 4.4990128 90 N 0 46 7
TOP 7 1.7010131 4.4734222 90 N 435 3 8
TOP 8 1.6458951 4.5118081 0 N 424 328 9
#
# CMP 420
CMP 29 0.2768169 4.3837523 180 N U21 TPD4E004DRYR ;0=1,1=0.0236
PRP 1394_/_Firewire 'TRUE'
PRP AEC_Category 'Q200'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Breakdown_Voltage(Min)(V) '6'
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/tpd4e004.pdf'
PRP ComponentLink2Description 'Product Folder'
PRP ComponentLink2URL 'http://www.ti.com/product/tpd4e004'
PRP ComponentLink3Description 'Online Datasheet'
PRP ComponentLink3URL 'http://www.ti.com/product/tpd4e004/datasheet'
PRP CompType 'IC'
PRP Ctotal(Typ)(pF) ''
PRP Differential_Capacitance(pF) ''
PRP Eco-Plan 'Green (RoHS & no Sb/Br)'
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP HDMI ''
PRP IEC_61000-4-2_Air-Gap(+/-_kV) '12'
PRP IEC_61000-4-2_Air-Gap(Typ)(+/-_kV) ''
PRP IEC_61000-4-2_Contact(+/-_kV) '8'
PRP IEC_61000-4-2_Contact(Typ)(+/-_kV) ''
PRP IO_Capacitance(Typ)(pF) '1.6'
PRP IO_Leakage_Current(nA) '1'
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP Number_Of_Channels ''
PRP Operating_Temperature_Range '-40 to 85 C'
PRP PackageDescription 'USON-6'
PRP PackageReference 'DRY0006A'
PRP PartNumber 'TPD4E004DRYR'
PRP Rating 'Catalog'
PRP RoHS 'Y'
PRP Serial_ATA_/_eSATA 'TRUE'
PRP SizeArea_mm2 '1.45'
PRP SizeAreaWB_mm2 '4.9'
PRP SizeX_mm '1.0'
PRP SizeY_mm '1.45'
PRP SizeZ_mm '0.6'
PRP USB_Full_Speed ''
PRP USB_High_Speed 'TRUE'
PRP USB_Super_Speed ''
TOP 0 0.2659901 4.3640672 90 N 429 1 1
TOP 1 0.2650059 4.3837522 90 N 428 1 2
TOP 2 0.2650059 4.4034373 90 N 424 305 3
TOP 3 0.2886279 4.4034373 90 N 427 1 4
TOP 4 0.2886279 4.3837522 90 N 323 1 5
TOP 5 0.2886279 4.3640672 90 N 372 3 6
#
# CMP 421
CMP 21 1.9330598 2.0035522 270 N U22 INA228AIDGST ;0=1,1=0.0000
PRP AEC_Qualified 'No'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.ti.com/lit/ds/symlink/ina228.pdf?ts=1623689466455&ref_url=https%253A%252F%252Fwww.ti.com%252Fproduct%252FINA228%253FkeyMatch%253DINA228AIDGST%2526tisearch%253Dsearch-everything%2526usecase%253DOPN'
PRP Datasheet 'https://www.ti.com/lit/ds/symlink/ina228.pdf?ts=1623689466455&ref_url=https%253A%252F%252Fwww.ti.com%252Fproduct%252FINA228%253FkeyMatch%253DINA228AIDGST%2526tisearch%253Dsearch-everything%2526usecase%253DOPN'
PRP Datasheet_Path 'datasheets/IC-INA228AIDGST.pdf'
PRP Digikey_Description '85-V, 20-BIT, ULTRA-PRECISE, I2C'
PRP Digikey_Part_Number '296-INA228AIDGSTCT-ND'
PRP helpURL 'https://upverter.com/upn/revision/fd3a73c0321b44f2/'
PRP Input_Bias_Current '0.01uA'
PRP Input_Offset_Voltage '1mV'
PRP Lead_Free 'Yes'
PRP Manufacturer 'Texas Instruments'
PRP Max_Supply_Voltage '5.5V'
PRP Min_Supply_Voltage '2.7V'
PRP Mouser_Part_Number '595-INA228AIDGST'
PRP Nominal_Supply_Current '640uA'
PRP Number_Of_Channels '1'
PRP Operating_Temperature_Range '-40°C to +125°C'
PRP PackageReference 'VSSOP10'
PRP Part_Number 'INA228AIDGST'
PRP PartNumber 'INA228AIDGST'
PRP RoHS 'TRUE'
PRP SizeZ_mm '1.1mm'
PRP Standoff_Height '0.05mm'
PRP TaMax_C '+125°C'
PRP TaMin_C '-40°C'
PRP TJmax_C '+150°C'
TOP 0 1.9724299 1.916938 270 N 424 307 1
TOP 1 1.9527448 1.916938 270 N 149 1 2
TOP 2 1.9330598 1.916938 270 N 0 42 3
TOP 3 1.9133748 1.916938 270 N 149 0 4
TOP 4 1.8936897 1.916938 270 N 150 0 5
TOP 5 1.8936897 2.0901664 270 N 308 32 6
TOP 6 1.9133748 2.0901664 270 N 424 306 7
TOP 7 1.9330598 2.0901664 270 N 175 11 8
TOP 8 1.9527448 2.0901664 270 N 199 2 9
TOP 9 1.9724299 2.0901664 270 N 159 2 10
#
# CMP 422
CMP 26 1.6604784 1.6736501 180 N U24 TMP112AIDRLR ;0=1,1=0.0236
PRP Alternate_Manufacturer 'Texas Instruments'
PRP Alternate_PartNumber 'TMP112AIDRLT'
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ti.com/lit/ds/symlink/tmp112.pdf'
PRP CompType 'IC'
PRP Green_EU_RoHS 'Passed'
PRP Green_EU_RoHS-2 'Passed'
PRP Green_Lifecycle 'Active'
PRP Green_REACh 'Passed'
PRP LatestRevisionDate '2017-06-09'
PRP Manufacturer 'Texas Instruments'
PRP MountType 'SMT'
PRP PackageDescription 'SOT-OTHER-6'
PRP PackageReference 'DRL0006A'
PRP PartNumber 'TMP112AIDRLR'
PRP Publisher 'Texas Instruments'
PRP RoHS 'Y'
PRP SizeArea_mm2 '2.56'
PRP SizeAreaWB_mm2 '6.76'
PRP SizeX_mm '1.6'
PRP SizeY_mm '1.6'
PRP SizeZ_mm '0.6'
PRP U/M 'EA'
TOP 0 1.6313445 1.653965 90 N 315 1 1
TOP 1 1.6313445 1.67365 90 N 424 330 2
TOP 2 1.6313445 1.6933351 90 N 322 1 3
TOP 3 1.6896123 1.6933351 90 N 316 1 4
TOP 4 1.6896123 1.67365 90 N 308 36 5
TOP 5 1.6896123 1.653965 90 N 314 1 6
#
# CMP 423
CMP 16 2.4828209 3.8982484 180 N U29 xWR2544LOP ;0=1,1=0.0000
PRP Datasheet_Path 'datasheets/IC-xWR2544LOP.pdf'
PRP helpURL 'https://upverter.com/upn/revision/24a70004bd76e0a8/'
PRP Manufacturer 'Texas Instruments'
PRP Operating_Temperature_Range 'to'
PRP PackageReference 'FCCSP248'
PRP Part_Number 'xWR2544LOP'
PRP PartNumber 'xWR2544LOP'
PRP RoHS 'UNKNOWN'
PRP SizeZ_mm '1.234mm'
PRP Standoff_Height '0.216mm'
TOP 0 2.2653012 3.693524 0 N 424 516 A1
TOP 1 2.2908918 3.693524 0 N 457 26 A2
TOP 2 2.3164823 3.693524 0 N 175 16 A3
TOP 3 2.3420729 3.693524 0 N 175 15 A4
TOP 4 2.3676634 3.693524 0 N 424 515 A5
TOP 5 2.393254 3.693524 0 N 128 0 A6
TOP 6 2.4188445 3.693524 0 N 37 0 A7
TOP 7 2.4444351 3.693524 0 N 36 0 A8
TOP 8 2.4700256 3.693524 0 N 127 0 A9
TOP 9 2.4956162 3.693524 0 N 129 0 A10
TOP 10 2.5212067 3.693524 0 N 390 1 A11
TOP 11 2.5467973 3.693524 0 N 455 13 A12
TOP 12 2.5723878 3.693524 0 N 457 25 A13
TOP 13 2.5979784 3.693524 0 N 424 514 A14
TOP 14 2.6235689 3.693524 0 N 458 30 A15
TOP 15 2.6491595 3.693524 0 N 389 1 A16
TOP 16 2.67475 3.693524 0 N 126 0 A17
TOP 17 2.7003406 3.693524 0 N 424 513 A18
TOP 18 2.2653012 3.7191145 0 N 424 512 B1
TOP 19 2.2908918 3.7191145 0 N 424 511 B2
TOP 20 2.3164823 3.7191145 0 N 424 510 B3
TOP 21 2.3420729 3.7191145 0 N 424 509 B4
TOP 22 2.3676634 3.7191145 0 N 139 0 B5
TOP 23 2.393254 3.7191145 0 N 141 0 B6
TOP 24 2.4188445 3.7191145 0 N 211 1 B7
TOP 25 2.4444351 3.7191145 0 N 140 0 B8
TOP 26 2.4700256 3.7191145 0 N 131 0 B9
TOP 27 2.4956162 3.7191145 0 N 125 0 B10
TOP 28 2.5212067 3.7191145 0 N 130 0 B11
TOP 29 2.5467973 3.7191145 0 N 424 508 B12
TOP 30 2.5723878 3.7191145 0 N 424 507 B13
TOP 31 2.5979784 3.7191145 0 N 424 506 B14
TOP 32 2.6235689 3.7191145 0 N 424 505 B15
TOP 33 2.6491595 3.7191145 0 N 424 504 B16
TOP 34 2.67475 3.7191145 0 N 267 3 B17
TOP 35 2.7003406 3.7191145 0 N 169 0 B18
TOP 36 2.2653012 3.7447051 0 N 24 0 C1
TOP 37 2.2908918 3.7447051 0 N 146 0 C2
TOP 38 2.3164823 3.7447051 0 N 424 503 C3
TOP 39 2.3420729 3.7447051 0 N 424 502 C4
TOP 40 2.3676634 3.7447051 0 N 424 501 C5
TOP 41 2.393254 3.7447051 0 N 424 500 C6
TOP 42 2.4188445 3.7447051 0 N 424 499 C7
TOP 43 2.4444351 3.7447051 0 N 424 498 C8
TOP 44 2.4700256 3.7447051 0 N 424 497 C9
TOP 45 2.4956162 3.7447051 0 N 424 496 C10
TOP 46 2.5212067 3.7447051 0 N 424 495 C11
TOP 47 2.5467973 3.7447051 0 N 424 494 C12
TOP 48 2.6491595 3.7447051 0 N 424 493 C16
TOP 49 2.67475 3.7447051 0 N 53 2 C17
TOP 50 2.7003406 3.7447051 0 N 458 29 C18
TOP 51 2.2653012 3.7702956 0 N 424 492 D1
TOP 52 2.2908918 3.7702956 0 N 424 491 D2
TOP 53 2.3164823 3.7702956 0 N 424 490 D3
TOP 54 2.4188445 3.7702956 0 N 424 489 D7
TOP 55 2.4444351 3.7702956 0 N 424 488 D8
TOP 56 2.5212067 3.7702956 0 N 424 487 D11
TOP 57 2.5467973 3.7702956 0 N 424 486 D12
TOP 58 2.6491595 3.7702956 0 N 424 485 D16
TOP 59 2.67475 3.7702956 0 N 274 1 D17
TOP 60 2.7003406 3.7702956 0 N 458 28 D18
TOP 61 2.2653012 3.7958862 0 N 137 0 E1
TOP 62 2.2908918 3.7958862 0 N 424 484 E2
TOP 63 2.3164823 3.7958862 0 N 424 483 E3
TOP 64 2.4188445 3.7958862 0 N 424 482 E7
TOP 65 2.4444351 3.7958862 0 N 424 481 E8
TOP 66 2.5212067 3.7958862 0 N 424 480 E11
TOP 67 2.5467973 3.7958862 0 N 424 479 E12
TOP 68 2.5723878 3.7958862 0 N 424 478 E13
TOP 69 2.5979784 3.7958862 0 N 424 477 E14
TOP 70 2.6235689 3.7958862 0 N 424 476 E15
TOP 71 2.6491595 3.7958862 0 N 424 475 E16
TOP 72 2.67475 3.7958862 0 N 272 0 E17
TOP 73 2.7003406 3.7958862 0 N 424 474 E18
TOP 74 2.2653012 3.8214767 0 N 424 473 F1
TOP 75 2.2908918 3.8214767 0 N 266 2 F2
TOP 76 2.3164823 3.8214767 0 N 424 472 F3
TOP 77 2.3420729 3.8214767 0 N 424 471 F4
TOP 78 2.3676634 3.8214767 0 N 424 470 F5
TOP 79 2.393254 3.8214767 0 N 424 469 F6
TOP 80 2.4188445 3.8214767 0 N 424 468 F7
TOP 81 2.4444351 3.8214767 0 N 424 467 F8
TOP 82 2.5212067 3.8214767 0 N 424 466 F11
TOP 83 2.5467973 3.8214767 0 N 424 465 F12
TOP 84 2.5723878 3.8214767 0 N 424 464 F13
TOP 85 2.5979784 3.8214767 0 N 424 463 F14
TOP 86 2.6235689 3.8214767 0 N 424 462 F15
TOP 87 2.6491595 3.8214767 0 N 424 461 F16
TOP 88 2.67475 3.8214767 0 N 48 2 F17
TOP 89 2.7003406 3.8214767 0 N 47 2 F18
TOP 90 2.2653012 3.8470673 0 N 424 460 G1
TOP 91 2.2908918 3.8470673 0 N 424 459 G2
TOP 92 2.3164823 3.8470673 0 N 424 458 G3
TOP 93 2.3420729 3.8470673 0 N 424 457 G4
TOP 94 2.3676634 3.8470673 0 N 424 456 G5
TOP 95 2.393254 3.8470673 0 N 424 455 G6
TOP 96 2.4188445 3.8470673 0 N 424 454 G7
TOP 97 2.4444351 3.8470673 0 N 424 453 G8
TOP 98 2.4700256 3.8470673 0 N 424 452 G9
TOP 99 2.4956162 3.8470673 0 N 424 451 G10
TOP 100 2.5212067 3.8470673 0 N 424 450 G11
TOP 101 2.5467973 3.8470673 0 N 424 449 G12
TOP 102 2.5723878 3.8470673 0 N 424 448 G13
TOP 103 2.6491595 3.8470673 0 N 424 447 G16
TOP 104 2.67475 3.8470673 0 N 46 1 G17
TOP 105 2.7003406 3.8470673 0 N 45 1 G18
TOP 106 2.2653012 3.8726578 0 N 173 1 H1
TOP 107 2.2908918 3.8726578 0 N 174 2 H2
TOP 108 2.3164823 3.8726578 0 N 424 446 H3
TOP 109 2.393254 3.8726578 0 N 424 445 H6
TOP 110 2.4188445 3.8726578 0 N 424 444 H7
TOP 111 2.4444351 3.8726578 0 N 424 443 H8
TOP 112 2.4700256 3.8726578 0 N 424 442 H9
TOP 113 2.4956162 3.8726578 0 N 424 441 H10
TOP 114 2.5212067 3.8726578 0 N 424 440 H11
TOP 115 2.5467973 3.8726578 0 N 424 439 H12
TOP 116 2.5723878 3.8726578 0 N 424 438 H13
TOP 117 2.6491595 3.8726578 0 N 424 437 H16
TOP 118 2.67475 3.8726578 0 N 424 436 H17
TOP 119 2.7003406 3.8726578 0 N 457 24 H18
TOP 120 2.2653012 3.8982484 0 N 424 435 J1
TOP 121 2.2908918 3.8982484 0 N 457 23 J2
TOP 122 2.3164823 3.8982484 0 N 424 434 J3
TOP 123 2.393254 3.8982484 0 N 424 433 J6
TOP 124 2.4188445 3.8982484 0 N 424 432 J7
TOP 125 2.5212067 3.8982484 0 N 424 431 J11
TOP 126 2.5467973 3.8982484 0 N 424 430 J12
TOP 127 2.5723878 3.8982484 0 N 424 429 J13
TOP 128 2.6491595 3.8982484 0 N 424 428 J16
TOP 129 2.67475 3.8982484 0 N 50 0 J17
TOP 130 2.7003406 3.8982484 0 N 49 0 J18
TOP 131 2.2653012 3.923839 0 N 264 0 K1
TOP 132 2.2908918 3.923839 0 N 457 22 K2
TOP 133 2.3164823 3.923839 0 N 424 427 K3
TOP 134 2.393254 3.923839 0 N 424 426 K6
TOP 135 2.4188445 3.923839 0 N 424 425 K7
TOP 136 2.5212067 3.923839 0 N 424 424 K11
TOP 137 2.5467973 3.923839 0 N 424 423 K12
TOP 138 2.5723878 3.923839 0 N 424 422 K13
TOP 139 2.5979784 3.923839 0 N 424 421 K14
TOP 140 2.6235689 3.923839 0 N 424 420 K15
TOP 141 2.6491595 3.923839 0 N 424 419 K16
TOP 142 2.67475 3.923839 0 N 52 0 K17
TOP 143 2.7003406 3.923839 0 N 51 0 K18
TOP 144 2.2653012 3.9494295 0 N 422 3 L1
TOP 145 2.2908918 3.9494295 0 N 423 2 L2
TOP 146 2.3164823 3.9494295 0 N 424 418 L3
TOP 147 2.3420729 3.9494295 0 N 424 417 L4
TOP 148 2.3676634 3.9494295 0 N 424 416 L5
TOP 149 2.393254 3.9494295 0 N 424 415 L6
TOP 150 2.4188445 3.9494295 0 N 424 414 L7
TOP 151 2.4444351 3.9494295 0 N 424 413 L8
TOP 152 2.4700256 3.9494295 0 N 424 412 L9
TOP 153 2.4956162 3.9494295 0 N 424 411 L10
TOP 154 2.5212067 3.9494295 0 N 424 410 L11
TOP 155 2.5723878 3.9494295 0 N 424 409 L13
TOP 156 2.5979784 3.9494295 0 N 424 408 L14
TOP 157 2.6491595 3.9494295 0 N 424 407 L16
TOP 158 2.67475 3.9494295 0 N 10 1 L17
TOP 159 2.7003406 3.9494295 0 N 9 1 L18
TOP 160 2.2653012 3.9750201 0 N 175 14 M1
TOP 161 2.2908918 3.9750201 0 N 420 1 M2
TOP 162 2.3164823 3.9750201 0 N 424 406 M3
TOP 163 2.3420729 3.9750201 0 N 424 405 M4
TOP 164 2.3676634 3.9750201 0 N 424 404 M5
TOP 165 2.393254 3.9750201 0 N 424 403 M6
TOP 166 2.4188445 3.9750201 0 N 424 402 M7
TOP 167 2.4444351 3.9750201 0 N 424 401 M8
TOP 168 2.4700256 3.9750201 0 N 424 400 M9
TOP 169 2.4956162 3.9750201 0 N 424 399 M10
TOP 170 2.5212067 3.9750201 0 N 424 398 M11
TOP 171 2.5467973 3.9750201 0 N 424 397 M12
TOP 172 2.5979784 3.9750201 0 N 458 27 M14
TOP 173 2.6235689 3.9750201 0 N 458 26 M15
TOP 174 2.6491595 3.9750201 0 N 458 18 M16
TOP 175 2.67475 3.9750201 0 N 395 2 M17
TOP 176 2.7003406 3.9750201 0 N 194 2 M18
TOP 177 2.2653012 4.0006106 0 N 457 21 N1
TOP 178 2.2908918 4.0006106 0 N 421 3 N2
TOP 179 2.3164823 4.0006106 0 N 424 396 N3
TOP 180 2.4188445 4.0006106 0 N 424 395 N7
TOP 181 2.4444351 4.0006106 0 N 424 394 N8
TOP 182 2.5212067 4.0006106 0 N 424 393 N11
TOP 183 2.5723878 4.0006106 0 N 458 25 N13
TOP 184 2.6235689 4.0006106 0 N 458 24 N15
TOP 185 2.67475 4.0006106 0 N 391 2 N17
TOP 186 2.7003406 4.0006106 0 N 455 12 N18
TOP 187 2.2653012 4.0262012 0 N 383 0 P1
TOP 188 2.2908918 4.0262012 0 N 285 2 P2
TOP 189 2.3164823 4.0262012 0 N 424 392 P3
TOP 190 2.4188445 4.0262012 0 N 424 391 P7
TOP 191 2.4444351 4.0262012 0 N 424 390 P8
TOP 192 2.5212067 4.0262012 0 N 424 389 P11
TOP 193 2.5467973 4.0262012 0 N 424 388 P12
TOP 194 2.5723878 4.0262012 0 N 458 23 P13
TOP 195 2.6235689 4.0262012 0 N 458 22 P15
TOP 196 2.67475 4.0262012 0 N 393 1 P17
TOP 197 2.7003406 4.0262012 0 N 424 387 P18
TOP 198 2.2653012 4.0517917 0 N 387 0 R1
TOP 199 2.2908918 4.0517917 0 N 284 2 R2
TOP 200 2.3164823 4.0517917 0 N 424 386 R3
TOP 201 2.3420729 4.0517917 0 N 424 385 R4
TOP 202 2.3676634 4.0517917 0 N 424 384 R5
TOP 203 2.393254 4.0517917 0 N 424 383 R6
TOP 204 2.4188445 4.0517917 0 N 424 382 R7
TOP 205 2.4444351 4.0517917 0 N 424 381 R8
TOP 206 2.5212067 4.0517917 0 N 424 380 R11
TOP 207 2.5467973 4.0517917 0 N 152 0 R12
TOP 208 2.5979784 4.0517917 0 N 458 21 R14
TOP 209 2.6491595 4.0517917 0 N 398 0 R16
TOP 210 2.67475 4.0517917 0 N 394 2 R17
TOP 211 2.7003406 4.0517917 0 N 457 20 R18
TOP 212 2.2653012 4.0773823 0 N 225 1 T1
TOP 213 2.2908918 4.0773823 0 N 288 0 T2
TOP 214 2.3164823 4.0773823 0 N 384 0 T3
TOP 215 2.3420729 4.0773823 0 N 407 1 T4
TOP 216 2.3676634 4.0773823 0 N 303 1 T5
TOP 217 2.393254 4.0773823 0 N 307 1 T6
TOP 218 2.4188445 4.0773823 0 N 302 1 T7
TOP 219 2.4444351 4.0773823 0 N 424 379 T8
TOP 220 2.4700256 4.0773823 0 N 424 378 T9
TOP 221 2.4956162 4.0773823 0 N 424 377 T10
TOP 222 2.5212067 4.0773823 0 N 424 376 T11
TOP 223 2.5467973 4.0773823 0 N 113 0 T12
TOP 224 2.5723878 4.0773823 0 N 132 0 T13
TOP 225 2.5979784 4.0773823 0 N 403 1 T14
TOP 226 2.6235689 4.0773823 0 N 400 0 T15
TOP 227 2.6491595 4.0773823 0 N 399 0 T16
TOP 228 2.67475 4.0773823 0 N 396 2 T17
TOP 229 2.7003406 4.0773823 0 N 392 2 T18
TOP 230 2.2653012 4.1029728 0 N 424 375 U1
TOP 231 2.2908918 4.1029728 0 N 1 0 U2
TOP 232 2.3164823 4.1029728 0 N 22 0 U3
TOP 233 2.3420729 4.1029728 0 N 164 0 U4
TOP 234 2.3676634 4.1029728 0 N 165 0 U5
TOP 235 2.393254 4.1029728 0 N 304 1 U6
TOP 236 2.4188445 4.1029728 0 N 305 1 U7
TOP 237 2.4444351 4.1029728 0 N 306 1 U8
TOP 238 2.4700256 4.1029728 0 N 458 20 U9
TOP 239 2.4956162 4.1029728 0 N 457 19 U10
TOP 240 2.5212067 4.1029728 0 N 424 374 U11
TOP 241 2.5467973 4.1029728 0 N 455 11 U12
TOP 242 2.5723878 4.1029728 0 N 458 19 U13
TOP 243 2.5979784 4.1029728 0 N 404 0 U14
TOP 244 2.6235689 4.1029728 0 N 402 0 U15
TOP 245 2.6491595 4.1029728 0 N 401 0 U16
TOP 246 2.67475 4.1029728 0 N 397 0 U17
TOP 247 2.7003406 4.1029728 0 N 424 373 U18
#
# CMP 424
CMP 63 0.6887885 4.0754353 180 N Y1 NX3225SA-12.000M-STD-CRS-2 ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'Y'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ndk.com/images/products/catalog/c_NX3225SA-STD-CRS-2_e.pdf'
PRP CompType 'Crystal'
PRP Frequency_Stability '50 ppm'
PRP Frequency_Tolerance '15 ppm'
PRP Frequency_Fixed '12MHz'
PRP Frequency_Max ''
PRP Frequency_Min ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Load_Capacitance '8 pF'
PRP Manufacturer 'NDK'
PRP MountType 'SMT'
PRP PackageReference '3.2x0.55x2.5mm'
PRP PartNumber 'NX3225SA-12.000M-STD-CRS-2'
PRP REACh ''
PRP RoHS 'Y'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '644-1128-1-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-40°C'
TOP 0 0.6572925 4.0321282 0 N 240 2 1
TOP 1 0.6572925 4.1187424 0 N 424 352 2
TOP 2 0.7202846 4.1187424 0 N 239 2 3
TOP 3 0.7202846 4.0321282 0 N 424 353 4
#
# CMP 425
CMP 63 1.0687691 0.941556 180 N Y2 NX3225SA-16.000M-STD-CRS-2 ;0=1,1=0.0236
PRP AEC_Category 'Q200'
PRP AEC_Grade '1'
PRP AEC_Qualified 'N'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP ComponentLink1Description 'Datasheet Link'
PRP ComponentLink1URL 'http://www.ndk.com/images/products/catalog/c_NX3225SA-STD-CRS-2_e.pdf'
PRP CompType 'Crystal'
PRP Frequency_Stability '150 ppm'
PRP Frequency_Tolerance '10 ppm'
PRP Frequency_Fixed '16MHz'
PRP Frequency_Max ''
PRP Frequency_Min ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP Load_Capacitance '7.36 pF'
PRP Manufacturer 'NDK'
PRP MountType 'SMT'
PRP PackageReference '3.2x0.55x2.5mm'
PRP PartNumber 'NX3225SA-16.000M-STD-CRS-2'
PRP REACh ''
PRP RoHS 'Y'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm ''
PRP Supplier_1 'Digi-Key'
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 '644-1129-1-ND'
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C '125°C'
PRP TaMin_C '-40°C'
TOP 0 1.0372731 0.8982489 0 N 244 1 1
TOP 1 1.0372731 0.9848631 0 N 424 309 2
TOP 2 1.1002652 0.9848631 0 N 243 1 3
TOP 3 1.1002652 0.8982489 0 N 424 308 4
#
# CMP 426
CMP 55 1.9748878 3.6349354 180 N Y3 NX2016SA-50M-STD-CZS-3 ;0=1,1=0.0000
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://www.ndk.com/images/products/catalog/c_NX2016SA-2_e.pdf'
PRP Datasheet 'https://www.ndk.com/images/products/catalog/c_NX2016SA-2_e.pdf'
PRP Datasheet_Path 'datasheets/Crys-NX2016SA-50M-STD-CZS-3.pdf'
PRP Digikey_Description 'CRYSTAL 50.0000MHZ 8PF SMD'
PRP Digikey_Part_Number '644-1306-1-ND'
PRP ESR '50'
PRP Frequency_Stability '50ppm'
PRP Frequency_Tolerance '15ppm'
PRP Frequency_Fixed '50MHz'
PRP helpURL 'https://upverter.com/upn/revision/c2a1bfc0c5c5cdb9/'
PRP Lead_Free 'Yes'
PRP Load_Capacitance '8pF'
PRP Manufacturer 'NDK'
PRP Mouser_Description 'Parallel - Fundamental Quartz Crystal, 50MHz Nom'
PRP Mouser_Part_Number '344-NX2016SA50MSTZS3'
PRP Operating_Temperature_Range '-40°C to +125°C'
PRP PackageReference 'SMT4_2MM0_1MM6'
PRP Part_Number 'NX2016SA-50M-STD-CZS-3'
PRP PartNumber 'NX2016SA-50M-STD-CZS-3'
PRP RoHS 'TRUE'
PRP Series 'NX2016SA'
PRP SizeZ_mm '0.5mm'
PRP Supplier_1 'Digikey'
PRP Supplier_2 'Mouser'
PRP Supplier_Part_Number_1 '644-1306-1-ND'
PRP Supplier_Part_Number_2 '344-NX2016SA50MSTZS3'
PRP Tolerance__ '15ppm'
TOP 0 1.948313 3.6556047 0 N 32 2 1
TOP 1 2.0014626 3.6556047 0 N 424 341 2
TOP 2 2.0014626 3.6142661 0 N 17 2 3
TOP 3 1.948313 3.6142661 0 N 20 2 4
#
# CMP 427
CMP 5 0.7823621 4.1344904 270 N C83 GCM1555C1H8R0DA16D ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category ''
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case ''
PRP Cap_F '8pF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GCM1555C1H8R0DA16-01.pdf'
PRP CompType ''
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'Murata Electronics North America'
PRP MountType ''
PRP PackageReference '0402'
PRP PartNumber 'GCM1555C1H8R0DA16D'
PRP Polarized ''
PRP RoHS 'TRUE'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm '0.55mm'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C ''
PRP TaMin_C ''
PRP Technology ''
PRP TempCo '30ppm/°C'
PRP Tolerance__ ''
PRP U/M ''
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value ''
PRP Value1 ''
PRP Value2 ''
PRP ValueDisplayed ''
PRP VDC_V ''
TOP 0 0.7823621 4.1148054 0 N 239 0 1
TOP 1 0.7823621 4.1541755 0 N 424 310 2
#
# CMP 428
CMP 5 0.7823621 4.0262227 90 N C84 GCM1555C1H8R0DA16D ;0=1,1=0.0236
PRP AC_Safety ''
PRP AEC_Category ''
PRP AEC_Grade 'Grade 1'
PRP AEC_Qualified 'Yes'
PRP Alternate_Manufacturer ''
PRP Alternate_PartNumber ''
PRP Cap_Case ''
PRP Cap_F '8pF'
PRP ComponentLink1Description 'Datasheet'
PRP ComponentLink1URL 'https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GCM1555C1H8R0DA16-01.pdf'
PRP CompType ''
PRP ESR_ohm ''
PRP Green_EU_RoHS ''
PRP Green_EU_RoHS-2 ''
PRP Green_Lifecycle ''
PRP Green_REACh ''
PRP IRMS_A ''
PRP Manufacturer 'Murata Electronics North America'
PRP MountType ''
PRP PackageReference '0402'
PRP PartNumber 'GCM1555C1H8R0DA16D'
PRP Polarized ''
PRP RoHS 'TRUE'
PRP SizeArea_mm2 ''
PRP SizeAreaWB_mm2 ''
PRP SizeX_mm ''
PRP SizeY_mm ''
PRP SizeZ_mm '0.55mm'
PRP Supplier_1 ''
PRP Supplier_2 ''
PRP Supplier_3 ''
PRP Supplier_Part_Number_1 ''
PRP Supplier_Part_Number_2 ''
PRP Supplier_Part_Number_3 ''
PRP TaMax_C ''
PRP TaMin_C ''
PRP Technology ''
PRP TempCo '30ppm/°C'
PRP Tolerance__ ''
PRP U/M ''
PRP VAC ''
PRP VAC_X ''
PRP VAC_Y ''
PRP Value ''
PRP Value1 ''
PRP Value2 ''
PRP ValueDisplayed ''
PRP VDC_V ''
TOP 0 0.7823621 4.0459077 180 N 240 0 1
TOP 1 0.7823621 4.0065376 180 N 424 311 2
#
