
**Setup**







**Connections :-   
IC boost :- DC Jack , xds110\_usb  
DCA100- Ethernet cable, Radar\_FTDI  
Connect 60 pin connectors of IC boost and DCA1000 using samtec cable(As mentioned in the image).**


**Switch Settings  
6843AoP EVM**

**S3 -off**

****

**DCA1000  
Connections : Ethernet cable, Radar\_FTDI usb  
**

**IC BOOST  
Connections: DC Jack, XDS110\_USB  
Put it in sop2 (Bottom left corner Jumpers)**

****S1.1 -OFF  
S1.2 -ON  
S1.3 -ON  
S1.4 -ON   
S1.5 -ON   
S1.6 -OFF   
S1.7 -OFF   
S1.8 -OFF   
S1.9 -OFF   
S1.10 - ON   
S1.11 - ON  
S1.1 2- ON