After replacing power supply to 12 V , 2.5 Amper

Trying to flash default.cfg

***First Step***

C:\ti\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\mcu\_plus\_sdk\_awr2x44p\_10\_00\_00\_07\tools\boot\sbl\_prebuilt\awr2x44p-evm>setenv.bat

-----------------------------------------------

mmWave Build Environment Configured

-----------------------------------------------

Second step



Trying to falsh default\_sbl\_null.cfg

***First Step***

C:\ti\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\mcu\_plus\_sdk\_awr2x44p\_10\_00\_00\_07\tools\boot\sbl\_prebuilt\awr2x44p-evm>setenv.bat

'setenv.bat' is not recognized as an internal or external command,

operable program or batch file.

C:\ti\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\mcu\_plus\_sdk\_awr2x44p\_10\_00\_00\_07\tools\boot\sbl\_prebuilt\awr2x44p-evm>cd C:\ti\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\scripts\windows

C:\ti\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\scripts\windows>setenv.bat

C:\ti\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\scripts\windows>set MMWAVE\_SDK\_DEVICE=awr2x44P

C:\ti\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\scripts\windows>set DOWNLOAD\_FROM\_CCS=yes

C:\ti\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\scripts\windows>set MMWAVE\_SDK\_TOOLS\_INSTALL\_PATH=C:/ti/mmwave\_mcuplus\_sdk\_04\_07\_00\_01

C:\ti\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\scripts\windows>set MMWAVE\_SDK\_INSTALL\_PATH=C:/ti/mmwave\_mcuplus\_sdk\_04\_07\_00\_01/mmwave\_mcuplus\_sdk\_04\_07\_00\_01

C:\ti\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\scripts\windows>set CCS\_INSTALL\_PATH=C:/ti/ccs1281

C:\ti\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\scripts\windows>set R5F\_CLANG\_INSTALL\_PATH=C:/ti/ccs1281/ccs/tools/compiler/ti-cgt-armllvm\_3.2.2.LTS

C:\ti\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\scripts\windows>set XDC\_INSTALL\_PATH=C:/ti/ccs1281/xdctools\_3\_62\_01\_16\_core

C:\ti\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\scripts\windows>SET MCU\_PLUS\_AWR294X\_INSTALL\_PATH=C:/ti/mmwave\_mcuplus\_sdk\_04\_07\_00\_01/mcu\_plus\_sdk\_awr294x\_10\_00\_00\_07

C:\ti\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\scripts\windows>SET MCU\_PLUS\_AWR2X44P\_INSTALL\_PATH=C:/ti/mmwave\_mcuplus\_sdk\_04\_07\_00\_01/mcu\_plus\_sdk\_awr2x44p\_10\_00\_00\_07

C:\ti\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\scripts\windows>SET MCU\_PLUS\_AWR2544\_INSTALL\_PATH=C:/ti/mmwave\_mcuplus\_sdk\_04\_07\_00\_01/mcu\_plus\_sdk\_awr2544\_10\_00\_00\_07

C:\ti\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\scripts\windows>SET SYSCONFIG\_INSTALL\_PATH=C:/ti/sysconfig\_1.24.0

C:\ti\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\scripts\windows>set MMWAVE\_AWR294X\_DFP\_INSTALL\_PATH=C:/ti/mmwave\_mcuplus\_sdk\_04\_07\_00\_01/mmwave\_dfp\_02\_04\_17\_00

C:\ti\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\scripts\windows>set AWR294X\_RADARSS\_IMAGE\_BIN=C:/ti/mmwave\_mcuplus\_sdk\_04\_07\_00\_01/mmwave\_dfp\_02\_04\_17\_00/firmware/radarss/xwr29xx\_radarss\_metarprc.bin

C:\ti\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\scripts\windows>set AWR2544\_RADARSS\_IMAGE\_BIN=C:/ti/mmwave\_mcuplus\_sdk\_04\_07\_00\_01/mmwave\_dfp\_02\_04\_17\_00/firmware/radarss/xwr25xx\_radarss\_metarprc.bin

C:\ti\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\scripts\windows>set AWR2X44P\_RADARSS\_IMAGE\_BIN=C:/ti/mmwave\_mcuplus\_sdk\_04\_07\_00\_01/mmwave\_dfp\_02\_04\_17\_00/firmware/radarss/xwr2x4xp\_radarss\_metarprc.bin

C:\ti\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\scripts\windows>set C66X\_CODEGEN\_INSTALL\_PATH=C:/ti/ccs1281/ccs/tools/compiler/ti-cgt-c6000\_8.3.12

C:\ti\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\scripts\windows>set C66x\_DSPLIB\_INSTALL\_PATH=C:/ti/mmwave\_mcuplus\_sdk\_04\_07\_00\_01/dsplib\_c66x\_3\_4\_0\_0

C:\ti\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\scripts\windows>set C66x\_MATHLIB\_INSTALL\_PATH=C:/ti/mmwave\_mcuplus\_sdk\_04\_07\_00\_01/mathlib\_c66x\_3\_1\_2\_1

C:\ti\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\scripts\windows>call checkenv.bat

-----------------------------------------------

mmWave Build Environment Configured

-----------------------------------------------

C:\ti\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\mmwave\_mcuplus\_sdk\_04\_07\_00\_01\scripts\windows>

Second Step



