Minolta readings are 
x:0.2903 y:0.6079. 
u’: 0.1195 v’:0.5632
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opt4048 ti evm is u’:0.160 v’:0.562
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OPT4048 CIE Color Plotter

Connect your Microcontroller with OPT4048 sensor to visualize color measurements on a CIE diagram.
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