PHY to MAC interface (RX)

PHY: DP83620; MAC: Artix 7



Frequency: 125Mhz

Driver PHY DP83620 waveform:



Receiver FPGA Artix 7 waveform:



I can clearly see the non-monotonicity in the waveform even after providing 22 ohms series termination.

As per datasheet MAC-PHY interface can be routed upto 6 inches but it is degrading in 3 inches itself.

* Test case 1: Without any transmission line and load.



Driver waveforms:



Observation:

Overshoot and undershoot is more (290 mV approx.)

* Test case 2: With transmission line and cap load



Waveforms:



Observation: By adding termination line, non-monotonicity has been observed in the signal.

* Test case 3: With TL, cap load and series termination





Observation: After adding series termination still facing the same issue of non-monotonicity.

* Test case 4: With TL and 50 ohms resistive load.





Observation: Voltage level reduced to 2.5V. It is supposed to be 3.3V