|  |
| --- |
| **Pass/Fail Criteria (During Test):** For the test mode(s) given in Table 3 all DUT samples must continuously meet the acceptance criteria for each signal parameter defined in Table 4 at the “Level 2” requirement for all frequencies and modulations identified in Table 11 of GMW3097:2022.      -**Use wiring harness length of 1700 mm +300 mm/-0 mm.**  -**Dwell time: 2 s**  -**Position probe for DBCI: 1-30 MHz use only 150 mm and 450 mm**  **DBCI: 15-30 MHz use only 150 and 450 mm (level 2)**  **CBCI: 30-400 MHz use only 450 mm and 750 mm**  **Pass/Fail Criteria (Post Test):** No permanent DUT damage or performance deviations shall be observed after exposure. |