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111 Two Supply Configuration
‘The connection diagrams for the two-supply is shown below.
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For two supply configuration, both VDDA1PS pins must be left unconnected.
Place 1-4F and 0.1-4F decoupling capacitors as close as possible to component VDD pins.

VDDIO may be 33V or25Vor 18 V.
No Components should be connected to VDDATPS pins in Two-Supply Configuration.




