Board-1
· After power up of the PCBA
· Green LED is steady (LNK2/ACT2_N)  but no blink in Orange LED ( ACT2)
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Below is the waveform related to Power,Reset and MDC/MDIO
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· Later pinging by doing power recycle
· Orange LED in Ethernet port blinking and Green LED is steady[image: ]
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[C:\Users\SESA362849>ping 192.168.1.2 -t

Pinging 192.168.1.2 with 32 bytes of data:
Request timed out.
Request timed out.
Request timed out.
Request timed out.
Request timed out.
Request timed out.
Request timed out.
Request timed out.
Request timed out.
Request timed out.
Request timed out.
Request timed out.
Request timed out. 1
Request timed out.
Request timed out.
IRequest timed out.
Request timed out.
Request timed out.
IRequest timed out.
Request timed out.
Request timed out.
Request timed out.
Request timed out.
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