[bookmark: _GoBack]Dears，
  My product is TBOX, and I use TJA1043 as below. I want to change it to TCAN1043, but I have a trouble with it:
 When main controller is stand by,3.3V and 5V(STB、EN、VCC、VIO) will turn off. and 3.3V and 5V(STB、EN、VCC、VIO) also will turn on when main controller wake-up. So, after changing to TCAN1043, what software strategy can wake up it in this circuit?
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