* If using 954/960 CSI, set des reg 0x72
  + Machine generated alternative text: RX 0x72 CSI_VC_MAP 7:0 CSLVC_MAP RW OxE4 CSI-2 Virtual Channel Mapping Register This
    register provides a method for replacing the
    Virtual Channel Idenhiler WC-ID) of incoming
    CSI packets
    [7:6] : Map value for VC-ID of 3
    [5:4] Map value for VC-ID of 2
    [3:2] Map value for VC-lD of 1
    [1:0]: Map value for VC-ID 010
  + Supports four virtual channels, you can remap the input VC ID to a new ID
  + Example: imager input VC-ID is 1, you can change 0x72[3:2] = b'11
    - This remaps VC-ID 1 to VC-ID 3 on the des CSI output