###
GRL-USB-PD-C2 Compliance Test Report

# DUT Information

Manufacturer |
Model Number |
Serial Number | -1_CE

# Test Information

Test Lab |
Test Engineer |
Remarks |
Date and Time: | 20200116_145206

# Controller and Instrument Information

Parameter | Value
--- | ---
GRL USB-PD_C2 Serial No. | 218.316.218.081.251.
GRL USB-PD Software Version | 1.3.16.18
GRL USB-PD Firmware Version | 1.3.16.0.15
GRL USB-PD Eload Firmware Version | 9.7/9.7
Board Calibration | Calibration Success.
App Mode | COMMUNICATION_ENGINE_TESTS
Tx Mask | true
Rx Mask | false
RX mask Power selection | Neutral Power
Device Type | DRP
Cable IR drop Imp(R) | 0
Cable Type. | GRL-SPL-Cable
COMMUNICATION_ENGINE_TESTS CTS Version | 1.09
VIF File name |
Noise Pattern Generation: | Two-Tone Noise
VIF info | *Since VIF was not loaded below test results are information Only.
Test cases Execution Time: | 0h:0m:49s

# Product Capabilities

Parameter | VendorInfoFile | GetCapabilities
--- | --- | ---
VENDOR_NAME |  | Intel
VIF_PRODUCT_TYPE |  |
MODEL_PART_NUMBER |  |
PRODUCT_REVISION |  |
TID |  | 0
PORT_LABEL |  |
CONNECTOR_TYPE |  |
USB_PD_SUPPORT |  | YES
PD_PORT_TYPE |  |
MANUFACTURER_INFO_PID_PORT |  |
STRUCTURED_VDM_VERSION |  | Version 2.0
TYPE_C_STATE_MACHINE |  |
PORT_BATTERY_POWERED |  | NO
BC_1_2_SUPPORT |  |
BC_1_2_CHARGING_PORT_TYPE |  |
PD_SPECIFICATION_REVISION |  | Revision 3
SOP_CAPABLE |  | YES
SOP_P_CAPABLE |  | YES
SOP_PP_CAPABLE |  | NO
SOP_P_DEBUG_CAPABLE |  | NO
SOP_PP_DEBUG_CAPABLE |  | NO
SECURITY_MSGS_SUPPORTED |  | NO
MANUFACTURER_INFO_SUPPORTED |  | YES
MANUFACTURER_INFO_VID |  | 0x8087
MANUFACTURER_INFO_PID |  | 0x0
NUM_FIXED_BATTERIES |  | 0
NUM_SWAPPABLE_BATTERY_SLOTS |  | 0
USB_COMMS_CAPABLE |  | YES
DR_SWAP_TO_DFP_SUPPORTED |  | NO
DR_SWAP_TO_UFP_SUPPORTED |  | NO
UNCONSTRAINED_POWER |  | YES
VCONN_SWAP_TO_ON_SUPPORTED |  |
VCONN_SWAP_TO_OFF_SUPPORTED |  |
RESPONDS_TO_DISCOV_SOP_UFP |  |
RESPONDS_TO_DISCOV_SOP_DFP |  |
ATTEMPTS_DISCOV |  |
CHUNKING_IMPLEMENTED |  | NO
UNCHUNKED_EXTENDED_MESSAGES_SUPPORTED |  | YES
PRODUCT_TYPE_UFP |  |
PRODUCT_TYPE_DFP |  |
MODAL_OPERATION_SUPPORTED |  | YES
USB_VID |  | 0x8087
PID |  | 0x0
BCDDEVICE |  | 0x649
XID |  | 1105
DATA_CAPABLE_AS_USB_HOST |  | YES
DATA_CAPABLE_AS_USB_DEVICE |  | YES
PRODUCT_TYPE |  |
CABLE_HW_VERS |  |
CABLE_FW_VERS |  |
TYPE_C_TO_TYPE_A_B_C |  |
TYPE_C_TO_TYPE_C_CAPT_VDM_V2 |  |
TYPE_C_TO_PLUG_RECEPTACLE |  |
CABLE_LATENCY |  |
CABLE_TERMINATION_TYPE |  |
VBUS_THROUGH_CABLE |  |
CABLE_VBUS_CURRENT |  |
CABLE_SOP_PP_CONTROLLER |  |
CABLE_SUPERSPEED_SUPPORT |  |
MAX_VBUS_VOLTAGE_VDM_V2 |  |
ACCEPTS_PR_SWAP_AS_SRC |  |
ACCEPTS_PR_SWAP_AS_SNK |  |
REQUESTS_PR_SWAP_AS_SRC |  |
REQUESTS_PR_SWAP_AS_SNK |  |
FR_SWAP_SUPPORTED_AS_INITIAL_SINK |  |
AMA_FW_VERS |  |
AMA_HW_VERS |  |
AMA_SUPERSPEED_SUPPORT |  |
AMA_VBUS_REQD |  |
AMA_VCONN_POWER |  |
AMA_VCONN_REQD |  |
HOST_SPEED |  |
DEVICE_SPEED |  |
CABLE_NUM_SVIDS_MIN |  |
CABLE_NUM_SVIDS_MAX |  |
SVID_FIXED |  |
NUM_SVIDS_MIN |  | 1
NUM_SVIDS_MAX |  | 2
SVID1SOP | - | 8087
SVID1Modes Min | - | 1
SVID1Modes Max | - | 1
SVID1Modes Fixed | - | YES
SVID1Mode1 Enter Mode | - | NO
SVID2SOP | - | FF01
SVID2Modes Min | - | 1
SVID2Modes Max | - | 1
SVID2Modes Fixed | - | YES
SVID2Mode1 Enter Mode | - | YES
TYPE_C_IMPLEMENTS_TRY_SRC |  |
TYPE_C_IMPLEMENTS_TRY_SNK |  |
RP_VALUE |  |
TYPE_C_IS_VCONN_POWERED_ACCESSORY |  |
TYPE_C_IS_DEBUG_TARGET_SRC |  |
TYPE_C_IS_DEBUG_TARGET_SNK |  |
TYPE_C_CAN_ACT_AS_HOST |  |
TYPE_C_CAN_ACT_AS_DEVICE |  |
TYPE_C_IS_ALT_MODE_CONTROLLER |  |
TYPE_C_IS_ALT_MODE_ADAPTER |  |
TYPE_C_POWER_SOURCE |  |
TYPE_C_PORT_ON_HUB |  |
TYPE_C_SUPPORTS_AUDIO_ACCESSORY |  |
CAPTIVE_CABLE |  |
TYPE_C_SOURCES_VCONN |  |
HOST_SUSPEND_SUPPORTED |  |

# Power Capabilities

Parameter | VendorInfoFile | GetCapabilities
--- | --- | ---
PD_POWER_AS_SOURCE |  | 15000
USB_SUSPEND_MAY_BE_CLEARED |  | YES
SENDS_PINGS |  | NO
FR_SWAP_SUPPORTED_AS_SOURCE |  |
PD_OC_PROTECTION |  |
PD_OCP_METHOD |  |
NUM_SRC_PDOS |  | 1
Supply Type #1 | - | Fixed
Peak Current #1 | - | 0x0(A)
Voltage #1 | - | 0x64(5V)
Max Current #1 | - | 0x12C(3A)
PD_POWER_AS_SINK |  | 0
NO_USB_SUSPEND_MAY_BE_SET |  | NO
GIVEBACK_MAY_BE_SET |  | NO
HIGHER_CAPABILITY_SET |  | NO
FR_SWAP_REQD_TYPE_C_CURRENT_AS_INITIAL_SOURCE |  | 0
NUM_SNK_PDOS |  | 1
Supply Type #1 | - | Fixed
Voltage #1 | - | 0x64(5V)
OP Current #1 | - | 0x0(A)

# Test Result Summary

Sl No | Test ID | Test Name | Test Result
--- | --- | --- | ---
1 | TDA.2.1.1.1 | TDA.2.1.1.1 BMC PHY TX EYE | PASS
2 | TDA.2.1.1.2 | TDA.2.1.1.2 BMC PHY TX BIT | PASS
3 | TDA.2.1.2.2 | TDA.2.1.2.2 BMC PHY RX INT REJ | PASS
4 | TDA.2.1.2.1 | TDA.2.1.2.1 BMC PHY RX BUSIDL | FAIL
5 | TDA.2.1.3.1 | TDA.2.1.3.1 BMC PHY TERM | PASS
6 | TDA.2.1.3.2 | TDA.2.1.3.2 BMC PHY MSG | PASS
7 | TDA.2.2.1 | TDA.2.2.1 BMC PROT SEQ GETCAPS | PASS
8 | TDA.2.2.2.1 | TDA.2.2.2.1 BMC PROT SEQ CHKCAB P PC | PASS
9 | TDA.2.2.2.2 | TDA.2.2.2.2 BMC PROT SEQ CHKCAP NOMARK P PC | NA
10 | TDA.2.2.2.3 | TDA.2.2.2.3 BMC PROT SEQ CHKCAP CP ACC | PASS
11 | TDA.2.2.2.4 | TDA.2.2.2.4 BMC PROT SEQ CHKCAP NOMRK CP ACC | NA
12 | TDA.2.2.3 | TDA.2.2.3 BMC PROT SEQ DRSWAP | NA
13 | TDA.2.2.4 | TDA.2.2.4 BMC PROT SEQ VCSWAP DFP | NA
14 | TDA.2.2.5 | TDA.2.2.5 BMC PROT DISCOV | NA
15 | TDA.2.2.6 | TDA.2.2.6 BMC PROT SEQ PRSWAP | NA
16 | TDA.2.2.7 | TDA.2.2.7 BMC PROT BIST NOT 5V SRC | PASS
17 | TDA.2.2.8 | TDA.2.2.8 BMC PROT REV NUM | NA
18 | TDA.2.2.9 | TDA.2.2.9 BMC PROT GSC REC | PASS
19 | TDA.2.2.10 | TDA.2.2.10 BMC PROT IGN PPS | NA
20 | TDA.2.3.1.1 | TDA.2.3.1.1 POW SRC LOAD P PC | PASS
21 | TDA.2.3.1.2 | TDA.2.3.1.2 POW SRC LOAD CP ACC | PASS
22 | TDA.2.3.2.1 | TDA.2.3.2.1 POW SRC TRANS P PC | PASS
23 | TDA.2.3.2.2 | TDA.2.3.2.2 POW SRC TRANS CP ACC | NA
24 | TDA.2.3.3.1 | TDA.2.3.3.1 POW SNK TRANS C CP | FAIL
25 | TDA.2.3.3.2 | TDA.2.3.3.2 POW SNK TRANS PC | NA

# Detailed Test Result

Test Status | Test Description
--- | ---
PASS | 1. TDA.2.1.1.1 BMC PHY TX EYE (Click to View Protocol Trace)
PASS | TDA.2.1.1.1 BMC PHY TX EYE-1:
| Valid Protocol response for BIST Request
PASS | TDA.2.1.1.1 BMC PHY TX EYE-2:
| Valid BIST response pattern
PASS | TDA.2.1.1.1 BMC PHY TX EYE-3:
| Eye diagram plot
PASS | TDA.2.1.1.1 BMC PHY TX EYE-4:
| BIST pattern duration 45.6672013 mS (Limit <= 60ms)
PASS | BMC_PHY_TX_EYE_5:
| Rise time: Average value = 397.900435 nS Minimum value = 392.514188 nS Maximum value = 403.665854 nS Minimum Limit = 300 ns Fall time: Average value = 467.004366 nS Minimum value = 461.526877 nS Maximum value = 471.993242 nS Minimum Limit = 300 ns
PASS | 2. TDA.2.1.1.2 BMC PHY TX BIT (Click to View Protocol Trace)
PASS | TDA.2.1.1.2 BMC PHY TX BIT-1:
| Valid Protocol response for BIST Request
PASS | TDA.2.1.1.2 BMC PHY TX BIT-2:
| Valid BIST response pattern
PASS | TDA.2.1.1.2 BMC PHY TX BIT-3:
| Bit Rate is 296.075 Kbps. Test limit (270 ~ 330) Kbps
PASS | TDA.2.1.1.2 BMC PHY TX BIT-4:
| Bit Rate is 0.001 %. Test limit: X < 0.25%
PASS | TDA.2.1.1.2 BMC PHY TX BIT-5:
| BIST pattern duration 45.6672013 mS (Limit <= 60ms)
PASS | 3. TDA.2.1.2.2 BMC PHY RX INT REJ (Click to View Protocol Trace)
PASS | TDA.2.1.2.2 BMC PHY RX INT REJ_1_TstrSource:
PASS | TDA.2.1.2.2 BMC PHY RX INT REJ_2_TstrSourceNoiseGrp1:
| Total Sent BIST Test Data messages Count: 13362; Received GoodCRC: = 13362 )
PASS | TDA.2.1.2.2 BMC PHY RX INT REJ_3_TstrSourceNoiseGrp2:
| Total Sent BIST Test Data messages Count: 13362; Received GoodCRC: = 13362 )
PASS | TDA.2.1.2.2 BMC PHY RX INT REJ_4_TstrSink:
PASS | TDA.2.1.2.2 BMC PHY RX INT REJ_2_TstrSinkNoiseGrp1:
| Total Sent BIST Test Data messages Count: 13362; Received GoodCRC: = 13362 )
PASS | TDA.2.1.2.2 BMC PHY RX INT REJ_5_TstrSinkNoiseGrp3:
| Total Sent BIST Test Data messages Count: 13362; Received GoodCRC: = 13362 )
FAIL | 4. TDA.2.1.2.1 BMC PHY RX BUSIDL (Click to View Protocol Trace)
PASS | TDA.2.1.2.1 BMC PHY RX BUSIDL1_TstrSink:
FAIL | TDA.2.1.2.1 BMC PHY RX BUSIDL2_TstrSink:
| DUT sent GoodCRC when CCLine is not idle, Verify Protocol Capture and confirm Failure.
PASS | TDA.2.1.2.1 BMC PHY RX BUSIDL3_TstrSink:
PASS | 5. TDA.2.1.3.1 BMC PHY TERM (Click to View Protocol Trace)
PASS | TDA.2.1.3.1 BMC PHY TERM_1:
PASS | TDA.2.1.3.1 BMC PHY TERM_2:
| CC-line voltage = 1.767V
PASS | 6. TDA.2.1.3.2 BMC PHY MSG (Click to View Protocol Trace)
NA | TDA.2.1.3.2 BMC PHY MSG_SOPs_BIST_1:
| Vendor Info File was not Loaded.
PASS | TDA.2.1.3.2 BMC PHY MSG_PHY_ERR_2:
PASS | BMC_PHY_MSG_6:
PASS | BMC_PHY_MSG_7:
PASS | BMC_PHY_MSG_8:
PASS | BMC_PHY_MSG_9:
PASS | BMC_PHY_MSG_10:
PASS | BMC_PHY_MSG_11:
PASS | TDA.2.1.3.2 BMC PHY MSG_MsgID_init_3:
PASS | BMC_PHY_MSG_12:
PASS | BMC_PHY_MSG_13:
PASS | TDA.2.1.3.2 BMC PHY MSG_MsgID_Cable_Reset_4:
PASS | BMC_PHY_MSG_15:
PASS | TDA.2.1.3.2 BMC PHY MSG_MsgID_Rpt_5:
PASS | BMC_PHY_MSG_18:
PASS | TDA.2.1.3.2 BMC PHY MSG_MsgID_HardRst_6:
PASS | BMC_PHY_MSG_16:
PASS | TDA.2.1.3.2 BMC PHY MSG_MsgID_SoftRst_7:
PASS | BMC_PHY_MSG_14:
PASS | TDA.2.1.3.2 BMC PHY MSG_CRCCheck_8:
PASS | BMC_PHY_MSG_19:
PASS | PROT_PROC_GCRC_UUT_1:
PASS | 7. TDA.2.2.1 BMC PROT SEQ GETCAPS (Click to View Protocol Trace)
PASS | TDA.2.2.1 BMC PROT SEQ GETCAPS_GetSourceCap_UUT_Type-(Source):
PASS | TDA.2.2.1 BMC PROT SEQ GETCAPS_GetSourceCap_UUT_Type-(Source)_(1):
| Protocol Index # #36870
PASS | TDA.2.2.1 BMC PROT SEQ GETCAPS_GetSourceCap_UUT_Type-(Source)_(2):
PASS | TDA.2.2.1 BMC PROT SEQ GETCAPS_GetSinkCap_UUT-Type-(Source):
PASS | TDA.2.2.1 BMC PROT SEQ GETCAPS_GetSinkCap_UUT-Type-(Source)_(3):
PASS | TDA.2.2.1 BMC PROT SEQ GETCAPS_GetSinkCap_UUT-Type-(Source)_(4):
| DUT responded with sink capability message at protocol index # #36882
PASS | TDA.2.2.1 BMC PROT SEQ GETCAPS_GetSourceCap_UUT-Type-(Sink):
PASS | TDA.2.2.1 BMC PROT SEQ GETCAPS_GetSourceCap_UUT-Type-(Sink)_(1):
PASS | TDA.2.2.1 BMC PROT SEQ GETCAPS_GetSourceCap_UUT-Type-(Sink)_(2):
| DUT responded with source cap message at protocol index # #36906
PASS | TDA.2.2.1 BMC PROT SEQ GETCAPS_GetSinkCap_UUT-Type_(Sink):
PASS | TDA.2.2.1 BMC PROT SEQ GETCAPS_GetSinkCap_UUT-Type_(Sink)_(3):
| DUT responded with sink_cap message at protocol index # #36910
PASS | TDA.2.2.1 BMC PROT SEQ GETCAPS_GetSinkCap_UUT-Type_(Sink)_(4):
PASS | 8. TDA.2.2.2.1 BMC PROT SEQ CHKCAB P PC (Click to View Protocol Trace)
PASS | BMC_PROT_SEQ_CHKCAB_P_PC_1_DISC_SOP1:
PASS | BMC_PROT_SEQ_CHKCAB_ P_PC _2_(>3A):
NA | 9. TDA.2.2.2.2 BMC PROT SEQ CHKCAP NOMARK P PC (Click to View Protocol Trace)
| Test is not applicable for captive cable DUT's.
PASS | 10. TDA.2.2.2.3 BMC PROT SEQ CHKCAP CP ACC (Click to View Protocol Trace)
PASS | BMC_PROT_SEQ_CHKCAB_ CP_ACC _1(PRSwap):
PASS | BMC_PROT_SEQ_CHKCAB_CP_ACC_2_DISC(SOP1):
PASS | BMC_PROT_SEQ_CHKCAB_CP_ACC_3_(>3A):
NA | 11. TDA.2.2.2.4 BMC PROT SEQ CHKCAP NOMRK CP ACC (Click to View Protocol Trace)
| Test is not applicable for captive cable DUT's.
NA | 12. TDA.2.2.3 BMC PROT SEQ DRSWAP (Click to View Protocol Trace)
| Vendor Info is not imported
NA | 13. TDA.2.2.4 BMC PROT SEQ VCSWAP DFP (Click to View Protocol Trace)
| Vendor Info VCONN_SWAP_TO_OFF_SUPPORTED field is not updated
NA | 14. TDA.2.2.5 BMC PROT DISCOV (Click to View Protocol Trace)
| Vendor Info is not imported
NA | 15. TDA.2.2.6 BMC PROT SEQ PRSWAP (Click to View Protocol Trace)
| Vendor Info is not imported
PASS | 16. TDA.2.2.7 BMC PROT BIST NOT 5V SRC (Click to View Protocol Trace)
NA | 17. TDA.2.2.8 BMC PROT REV NUM (Click to View Protocol Trace)
| Vendor Info is not imported
PASS | 18. TDA.2.2.9 BMC PROT GSC REC (Click to View Protocol Trace)
PASS | TDA.2.2.9 BMC PROT GSC REC_Get_SrcCap:
NA | 19. TDA.2.2.10 BMC PROT IGN PPS (Click to View Protocol Trace)
| Test case is not applicable for Revision 3.0 DUT's
NA | TDA.2.2.10 BMC PROT IGN PPS_1:
NA | TDA.2.2.10 BMC PROT IGN PPS_2:
NA | TDA.2.2.10 BMC PROT IGN PPS_3:
PASS | 20. TDA.2.3.1.1 POW SRC LOAD P PC (Click to View Protocol Trace)
PASS | TDA.2.3.1.1 POW SRC LOAD P PC_PDO_1:
PASS | TDA.2.3.1.1 POW SRC LOAD P PC_PDO_1_2:
| Measured VBUS voltage value between start time 17.0410868S and stop time = 17.0425868S is = 5.30654762V limit[FS :4.75000000V~5.25000000V] after PS_RDY protocol index # #0
PASS | PROT_PROC_GCRC_UUT_1:
PASS | PROT_PROC_REQ_TSTR_4:
PASS | PROT_PROC_REQ_TSTR_5:
PASS | PROT_PROC_REQ_TSTR_6:
PASS | PROT_PROC_REQ_TSTR_9:
| Measured VBUS voltage value between start time 17.0410868S and stop time = 17.0425868S is = 5.30654762V limit[FS :4.75000000V~5.25000000V] after PS_RDY protocol index # #37293
PASS | DUT VBUS voltage before load of 0A is 5.30447V, voltage after Load: 5.3056V , Limit:[4.75-5.5V] at Protocol index #37299[ Measurement timeStamp24.4937653S]:
PASS | DUT VBUS voltage before load of 0.75A is 5.30556V, voltage after Load: 5.3041V , Limit:[4.75-5.5V] at Protocol index #37305 [Measurement timestamp :25.1347825S]:
PASS | DUT VBUS voltage before load of 1.5A is 5.22013V, voltage after Load: 5.1593V , Limit:[4.75-5.5V] at Protocol index #37311 [Measurement timestamp :25.7757677S]:
PASS | DUT VBUS voltage before load of 2.25A is 5.1316V, voltage after Load: 5.0782V , Limit:[4.75-5.5V] at Protocol index #37317 [Measurement timestamp :26.4167737S]:
PASS | DUT VBUS voltage before load of 3.0A is 5.04835V, voltage after Load: 4.9983V , Limit:[4.75-5.5V] at Protocol index #37323 [Measurement timestamp :27.0577314S]:
PASS | DUT VBUS voltage before load of 2.25A is 4.98259V, voltage after Load: 5.0483V , Limit:[4.75-5.5V] at Protocol index #37329 [Measurement timestamp :27.6987677S]:
PASS | DUT VBUS voltage before load of 1.5A is 5.07258V, voltage after Load: 5.132V , Limit:[4.75-5.5V] at Protocol index #37335 [Measurement timestamp :28.3397777S]:
PASS | DUT VBUS voltage before load of 0.75A is 5.15928V, voltage after Load: 5.2179V , Limit:[4.75-5.5V] at Protocol index #37341 [Measurement timestamp :28.9807651S]:
PASS | DUT VBUS voltage before load of 0A is 5.25692V, voltage after Load: 5.3057V , Limit:[4.75-5.5V] at Protocol index #37347[ Measurement timeStamp29.6217690S]:
PASS | PT_PROT_PROC_HR_TSTR_3:
PASS | PROT_PROC_HR_TSTR_1:
PASS | PROT_PROC_HR_TSTR_2:
PASS | PROT_PROC_HR_TSTR_3:
PASS | PROT_PROC_HR_TSTR_4:
| Vbus Voltage after 660ms is :0.02201V
PASS | PROT_PROC_HR_TSTR_5:
| Vbus voltage at >1s is:5.30228V
PASS | PROT_PROC_GCRC_UUT_1:
PASS | PT_TDA_2_3_1_1 POW SRC LOAD P PC_RequestHigherCurrent_PDO_1:
PASS | 21. TDA.2.3.1.2 POW SRC LOAD CP ACC (Click to View Protocol Trace)
PASS | TDA_2_3_1_2_POW_SRC_LOAD_CP_ACC_1:
PASS | TDA.2.3.1.2 POW SRC LOAD CP ACC_PDO_1:
PASS | TDA.2.3.1.2 POW SRC LOAD CP ACC_PDO_1(3):
| Measured VBUS voltage value between start time 22.0237208S and stop time = 22.0252208S is = 5.30441375V limit[FS :4.75000000V~5.25000000V] after PS_RDY protocol index # #0
PASS | PROT_PROC_GCRC_UUT_1:
PASS | PROT_PROC_REQ_TSTR_4:
PASS | PROT_PROC_REQ_TSTR_5:
PASS | PROT_PROC_REQ_TSTR_6:
PASS | PROT_PROC_REQ_TSTR_9:
| Measured VBUS voltage value between start time 22.0237208S and stop time = 22.0252208S is = 5.30441375V limit[FS :4.75000000V~5.25000000V] after PS_RDY protocol index # #37438
PASS | PT_TDA_2_3_1_2 POW SRC LOAD CP ACC_PROT_PROC_HR_TSTR:
PASS | PROT_PROC_HR_TSTR_1:
PASS | PROT_PROC_HR_TSTR_2:
PASS | PROT_PROC_HR_TSTR_3:
PASS | PROT_PROC_HR_TSTR_4:
| Vbus Voltage after 660ms is :0.02201V
PASS | PROT_PROC_HR_TSTR_5:
| Vbus voltage at >1s is:5.30228V
PASS | PROT_PROC_GCRC_UUT_1:
PASS | 22. TDA.2.3.2.1 POW SRC TRANS P PC (Click to View Protocol Trace)
| DUT advertised only PDO
NA | 23. TDA.2.3.2.2 POW SRC TRANS CP ACC (Click to View Protocol Trace)
| Vendor info file was not loaded, Please load it and re-run again
FAIL | 24. TDA.2.3.3.1 POW SNK TRANS C CP (Click to View Protocol Trace)
| VIF file was not loaded.
PASS | TDA.2.3.3.1 POW SNK TRANS C CP_1:
PASS | TDA.2.3.3.1 POW SNK TRANS C CP_3:
PASS | TDA.2.3.3.1 POW SNK TRANS C CP_2:
NA | 25. TDA.2.3.3.2 POW SNK TRANS PC (Click to View Protocol Trace)
| DUT not accepted PR_Swap message. Vendor info not loaded