###
GRL-USB-PD-C2 Compliance Test Report

# DUT Information

Manufacturer |
Model Number |
Serial Number | -1_CE

# Test Information

Test Lab |
Test Engineer |
Remarks |
Date and Time: | 20200116_145206

# Controller and Instrument Information

Parameter | Value
--- | ---
GRL USB-PD_C2 Serial No. | 218.316.218.081.251.
GRL USB-PD Software Version | 1.3.16.18
GRL USB-PD Firmware Version | 1.3.16.0.15
GRL USB-PD Eload Firmware Version | 9.7/9.7
Board Calibration | Calibration Success.
App Mode | COMMUNICATION_ENGINE_TESTS
Tx Mask | true
Rx Mask | false
RX mask Power selection | Neutral Power
Device Type | DRP
Cable IR drop Imp(R) | 0
Cable Type. | GRL-SPL-Cable
COMMUNICATION_ENGINE_TESTS CTS Version | 1.09
VIF File name |
Noise Pattern Generation: | Two-Tone Noise
VIF info | *Since VIF was not loaded below test results are information Only.
Test cases Execution Time: | 0h:0m:49s

# Product Capabilities

Parameter | VendorInfoFile | GetCapabilities
--- | --- | ---
VENDOR_NAME |  | Intel
VIF_PRODUCT_TYPE |  |
MODEL_PART_NUMBER |  |
PRODUCT_REVISION |  |
TID |  | 0
PORT_LABEL |  |
CONNECTOR_TYPE |  |
USB_PD_SUPPORT |  | YES
PD_PORT_TYPE |  |
MANUFACTURER_INFO_PID_PORT |  |
STRUCTURED_VDM_VERSION |  | Version 2.0
TYPE_C_STATE_MACHINE |  |
PORT_BATTERY_POWERED |  | NO
BC_1_2_SUPPORT |  |
BC_1_2_CHARGING_PORT_TYPE |  |
PD_SPECIFICATION_REVISION |  | Revision 3
SOP_CAPABLE |  | YES
SOP_P_CAPABLE |  | YES
SOP_PP_CAPABLE |  | NO
SOP_P_DEBUG_CAPABLE |  | NO
SOP_PP_DEBUG_CAPABLE |  | NO
SECURITY_MSGS_SUPPORTED |  | NO
MANUFACTURER_INFO_SUPPORTED |  | YES
MANUFACTURER_INFO_VID |  | 0x8087
MANUFACTURER_INFO_PID |  | 0x0
NUM_FIXED_BATTERIES |  | 0
NUM_SWAPPABLE_BATTERY_SLOTS |  | 0
USB_COMMS_CAPABLE |  | YES
DR_SWAP_TO_DFP_SUPPORTED |  | NO
DR_SWAP_TO_UFP_SUPPORTED |  | NO
UNCONSTRAINED_POWER |  | YES
VCONN_SWAP_TO_ON_SUPPORTED |  |
VCONN_SWAP_TO_OFF_SUPPORTED |  |
RESPONDS_TO_DISCOV_SOP_UFP |  |
RESPONDS_TO_DISCOV_SOP_DFP |  |
ATTEMPTS_DISCOV |  |
CHUNKING_IMPLEMENTED |  | NO
UNCHUNKED_EXTENDED_MESSAGES_SUPPORTED |  | YES
PRODUCT_TYPE_UFP |  |
PRODUCT_TYPE_DFP |  |
MODAL_OPERATION_SUPPORTED |  | YES
USB_VID |  | 0x8087
PID |  | 0x0
BCDDEVICE |  | 0x649
XID |  | 1105
DATA_CAPABLE_AS_USB_HOST |  | YES
DATA_CAPABLE_AS_USB_DEVICE |  | YES
PRODUCT_TYPE |  |
CABLE_HW_VERS |  |
CABLE_FW_VERS |  |
TYPE_C_TO_TYPE_A_B_C |  |
TYPE_C_TO_TYPE_C_CAPT_VDM_V2 |  |
TYPE_C_TO_PLUG_RECEPTACLE |  |
CABLE_LATENCY |  |
CABLE_TERMINATION_TYPE |  |
VBUS_THROUGH_CABLE |  |
CABLE_VBUS_CURRENT |  |
CABLE_SOP_PP_CONTROLLER |  |
CABLE_SUPERSPEED_SUPPORT |  |
MAX_VBUS_VOLTAGE_VDM_V2 |  |
ACCEPTS_PR_SWAP_AS_SRC |  |
ACCEPTS_PR_SWAP_AS_SNK |  |
REQUESTS_PR_SWAP_AS_SRC |  |
REQUESTS_PR_SWAP_AS_SNK |  |
FR_SWAP_SUPPORTED_AS_INITIAL_SINK |  |
AMA_FW_VERS |  |
AMA_HW_VERS |  |
AMA_SUPERSPEED_SUPPORT |  |
AMA_VBUS_REQD |  |
AMA_VCONN_POWER |  |
AMA_VCONN_REQD |  |
HOST_SPEED |  |
DEVICE_SPEED |  |
CABLE_NUM_SVIDS_MIN |  |
CABLE_NUM_SVIDS_MAX |  |
SVID_FIXED |  |
NUM_SVIDS_MIN |  | 1
NUM_SVIDS_MAX |  | 2
SVID1SOP | - | 8087
SVID1Modes Min | - | 1
SVID1Modes Max | - | 1
SVID1Modes Fixed | - | YES
SVID1Mode1 Enter Mode | - | NO
SVID2SOP | - | FF01
SVID2Modes Min | - | 1
SVID2Modes Max | - | 1
SVID2Modes Fixed | - | YES
SVID2Mode1 Enter Mode | - | YES
TYPE_C_IMPLEMENTS_TRY_SRC |  |
TYPE_C_IMPLEMENTS_TRY_SNK |  |
RP_VALUE |  |
TYPE_C_IS_VCONN_POWERED_ACCESSORY |  |
TYPE_C_IS_DEBUG_TARGET_SRC |  |
TYPE_C_IS_DEBUG_TARGET_SNK |  |
TYPE_C_CAN_ACT_AS_HOST |  |
TYPE_C_CAN_ACT_AS_DEVICE |  |
TYPE_C_IS_ALT_MODE_CONTROLLER |  |
TYPE_C_IS_ALT_MODE_ADAPTER |  |
TYPE_C_POWER_SOURCE |  |
TYPE_C_PORT_ON_HUB |  |
TYPE_C_SUPPORTS_AUDIO_ACCESSORY |  |
CAPTIVE_CABLE |  |
TYPE_C_SOURCES_VCONN |  |
HOST_SUSPEND_SUPPORTED |  |

# Power Capabilities

Parameter | VendorInfoFile | GetCapabilities
--- | --- | ---
PD_POWER_AS_SOURCE |  | 15000
USB_SUSPEND_MAY_BE_CLEARED |  | YES
SENDS_PINGS |  | NO
FR_SWAP_SUPPORTED_AS_SOURCE |  |
PD_OC_PROTECTION |  |
PD_OCP_METHOD |  |
NUM_SRC_PDOS |  | 1
Supply Type #1 | - | Fixed
Peak Current #1 | - | 0x0(A)
Voltage #1 | - | 0x64(5V)
Max Current #1 | - | 0x12C(3A)
PD_POWER_AS_SINK |  | 0
NO_USB_SUSPEND_MAY_BE_SET |  | NO
GIVEBACK_MAY_BE_SET |  | NO
HIGHER_CAPABILITY_SET |  | NO
FR_SWAP_REQD_TYPE_C_CURRENT_AS_INITIAL_SOURCE |  | 0
NUM_SNK_PDOS |  | 1
Supply Type #1 | - | Fixed
Voltage #1 | - | 0x64(5V)
OP Current #1 | - | 0x0(A)

# USB-IF High Level Mapping Summary

Sl No | Test Category | Test Group Description | Test Result
--- | --- | --- | ---
1 | PHY_PRIMARY_RX | BMC Physical Layer Receiver | FAIL
2 | POWER_PRIMARY | Power Source/Sink Primary | FAIL

# Result Summary

Sl No | Test ID | Test Name | Test Result
--- | --- | --- | ---
1 | TDA.2.1.2.1 | TDA.2.1.2.1 BMC PHY RX BUSIDL | FAIL
2 | TDA.2.3.3.1 | TDA.2.3.3.1 POW SNK TRANS C CP | FAIL

# Detailed Compliance Test Result

Test Status | Test Description
--- | ---
FAIL | 1. TDA.2.1.2.1 BMC PHY RX BUSIDL (Click to View Protocol Trace)
PASS | TDA.2.1.2.1 BMC PHY RX BUSIDL1_TstrSink:
FAIL | TDA.2.1.2.1 BMC PHY RX BUSIDL2_TstrSink:
| DUT sent GoodCRC when CCLine is not idle, Verify Protocol Capture and confirm Failure.
PASS | TDA.2.1.2.1 BMC PHY RX BUSIDL3_TstrSink:
FAIL | 2. TDA.2.3.3.1 POW SNK TRANS C CP (Click to View Protocol Trace)
| VIF file was not loaded.
PASS | TDA.2.3.3.1 POW SNK TRANS C CP_1:
PASS | TDA.2.3.3.1 POW SNK TRANS C CP_3:
PASS | TDA.2.3.3.1 POW SNK TRANS C CP_2:

# Packet List

Index | Start time(s.ms.μs.ns) | Stop time(s.ms.μs.ns) | Message Origin | Message | SOP | Port Type | Msg ID | PDO | Header(MSB to LSB) | Payload(LSB to MSB)
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
TDA.2.1.2.1 BMC PHY RX BUSIDL| Port A messages (Back)
1 | 3.099.684.001 | 3.099.684.001 | T-> | Ra_Asserted | NONE | NONE/NONE/R1 | 0 | CC2 | 0x0000 | 0x
2 | 5.600.132.020 | 5.600.132.020 | <-D | Attach | NONE | NONE/NONE/- | 0 | Rp_4_7k_3A_Detected | 0x0000 | 0x
3 | 5.815.091.095 | 5.815.091.095 | <-D | Attach | NONE | NONE/NONE/- | 0 | Rp_4_7k_3A_Detected | 0x0000 | 0x
4 | 5.939.942.036 | 5.940.583.056 | <-D | VendorDefined | SOP1 | NONE/DFP_UFP/R3/VDM_Ver1/ | 0 | Discover ID;Initiator; | 0x108F | 0x01-A0-00-FF-
5 | 5.940.631.076 | 5.941.096.096 | T-> | GoodCRC | SOP1 | NONE/CablePlug/R2 | 0 |  | 0x0141 | 0x
6 | 5.947.502.022 | 5.948.607.042 | T-> | VendorDefined | SOP1 | NONE/CablePlug/R2/VDM_Ver1/ | 0 | Discover ID;ACK; | 0x514F | 0x41-80-00-FF-00-00-00-58-00-00-00-00-00-00-03-00-42-2E-08-00-
7 | 5.948.792.083 | 5.949.299.003 | <-D | GoodCRC | SOP1 | NONE/DFP_UFP/R2 | 0 |  | 0x0041 | 0x
8 | 5.950.108.024 | 5.950.749.064 | <-D | SourceCap | SOP | DFP/Source/R3 | 0 | FS: 5V 3A; | 0x11A1 | 0x2C-91-01-2F-
9 | 5.951.901.005 | 5.952.542.026 | <-D | SourceCap | SOP | DFP/Source/R3 | 0 | FS: 5V 3A; | 0x11A1 | 0x2C-91-01-2F-
10 | 5.953.695.027 | 5.954.336.067 | <-D | SourceCap | SOP | DFP/Source/R3 | 0 | FS: 5V 3A; | 0x11A1 | 0x2C-91-01-2F-
11 | 6.043.753.001 | 6.043.753.001 | <-D | Rp_Change | NONE | NONE/NONE/R1 | 0 | Rp_To_4_7k_3A | 0x0000 | 0x
12 | 6.134.363.072 | 6.135.005.013 | <-D | SourceCap | SOP | DFP/Source/R3 | 0 | FS: 5V 3A; | 0x11A1 | 0x2C-91-01-2F-
13 | 6.135.052.053 | 6.135.517.073 | T-> | GoodCRC | SOP | UFP/Sink/R2 | 0 |  | 0x0041 | 0x
14 | 6.137.497.035 | 6.138.090.055 | T-> | Request | SOP | UFP/Sink/R2 | 0 | PDO#1; OpCurrent = 0.1A; MaxCurrent = 0.1A | 0x1042 | 0x0A-28-80-10-
15 | 6.138.273.075 | 6.138.779.096 | <-D | GoodCRC | SOP | DFP/Source/R2 | 0 |  | 0x0161 | 0x
16 | 6.142.355.079 | 6.142.861.099 | <-D | Accept | SOP | DFP/Source/R2 | 1 |  | 0x0363 | 0x
17 | 6.142.911.079 | 6.143.377.000 | T-> | GoodCRC | SOP | UFP/Sink/R2 | 1 |  | 0x0241 | 0x
18 | 6.177.964.068 | 6.178.470.088 | <-D | PS_RDY | SOP | DFP/Source/R2 | 2 |  | 0x0566 | 0x
19 | 6.178.518.048 | 6.178.983.069 | T-> | GoodCRC | SOP | UFP/Sink/R2 | 2 |  | 0x0441 | 0x
20 | 6.179.688.049 | 6.180.194.070 | <-D | DR_Swap | SOP | DFP/Source/R2 | 3 |  | 0x0769 | 0x
21 | 6.180.240.010 | 6.180.705.030 | T-> | GoodCRC | SOP | UFP/Sink/R2 | 3 |  | 0x0641 | 0x
22 | 6.182.496.012 | 6.182.961.032 | T-> | Reject | SOP | UFP/Sink/R2 | 1 |  | 0x0244 | 0x
23 | 6.183.144.092 | 6.183.651.012 | <-D | GoodCRC | SOP | DFP/Source/R2 | 1 |  | 0x0361 | 0x
24 | 6.194.435.081 | 6.195.077.002 | <-D | VendorDefined | SOP | DFP/Source/R2/VDM_Ver1/ | 4 | Discover ID;Initiator; | 0x196F | 0x01-80-00-FF-
25 | 6.195.123.042 | 6.195.588.062 | T-> | GoodCRC | SOP | UFP/Sink/R2 | 4 |  | 0x0841 | 0x
26 | 6.201.497.087 | 6.202.603.008 | T-> | VendorDefined | SOP | UFP/Sink/R2/VDM_Ver1/ | 2 | Discover ID;ACK; | 0x544F | 0x41-80-00-FF-B4-04-00-6C-00-00-00-00-00-20-31-3B-00-00-00-00-
27 | 6.202.780.028 | 6.203.286.048 | <-D | GoodCRC | SOP | DFP/Source/R2 | 2 |  | 0x0561 | 0x
28 | 6.206.862.051 | 6.207.503.092 | <-D | VendorDefined | SOP | DFP/Source/R2/VDM_Ver1/ | 5 | Discover SVID;Initiator; | 0x1B6F | 0x02-80-00-FF-
29 | 6.207.549.012 | 6.208.014.032 | T-> | GoodCRC | SOP | UFP/Sink/R2 | 5 |  | 0x0A41 | 0x
30 | 6.214.496.037 | 6.215.217.058 | T-> | VendorDefined | SOP | UFP/Sink/R2/VDM_Ver1/ | 3 | Discover SVID;ACK; | 0x264F | 0x42-80-00-FF-00-00-01-FF-
31 | 6.215.394.038 | 6.215.900.059 | <-D | GoodCRC | SOP | DFP/Source/R2 | 3 |  | 0x0761 | 0x
32 | 6.219.476.061 | 6.220.117.082 | <-D | VendorDefined | SOP | DFP/Source/R2/VDM_Ver1/ | 6 | Discover Mode;Initiator; | 0x1D6F | 0x03-80-01-FF-
33 | 6.220.163.062 | 6.220.628.082 | T-> | GoodCRC | SOP | UFP/Sink/R2 | 6 |  | 0x0C41 | 0x
34 | 6.226.496.047 | 6.227.217.067 | T-> | VendorDefined | SOP | UFP/Sink/R2/VDM_Ver1/ | 4 | Discover Mode;ACK; | 0x284F | 0x43-80-01-FF-05-04-00-00-
35 | 6.227.395.008 | 6.227.901.028 | <-D | GoodCRC | SOP | DFP/Source/R2 | 4 |  | 0x0961 | 0x
36 | 6.231.477.031 | 6.232.118.051 | <-D | VendorDefined | SOP | DFP/Source/R2/VDM_Ver1/ | 7 | Enter Mode;Initiator; | 0x1F6F | 0x04-81-01-FF-
37 | 6.232.166.091 | 6.232.632.012 | T-> | GoodCRC | SOP | UFP/Sink/R2 | 7 |  | 0x0E41 | 0x
38 | 6.238.499.076 | 6.239.092.097 | T-> | VendorDefined | SOP | UFP/Sink/R2/VDM_Ver1/ | 5 | Enter Mode;NAK; | 0x1A4F | 0x84-81-01-FF-
39 | 6.239.269.097 | 6.239.776.019 | <-D | GoodCRC | SOP | DFP/Source/R2 | 5 |  | 0x0B61 | 0x
40 | 12.721.774.008 | 12.723.136.001 | T-> | BIST | SOP | UFP/Sink/R2 | 6 | BIST_Test_Data | 0x7C43 | 0x00-00-00-80-DC-AB-C4-74-02-1E-94-21-A1-94-8E-14-38-4F-0B-07-B7-8A-6D-5E-45-85-2D-75-
41 | 12.723.313.005 | 12.723.819.007 | <-D | GoodCRC | SOP | DFP/Source/R2 | 6 |  | 0x0D61 | 0x
42 | 18.985.937.007 | 18.987.298.009 | T-> | BIST | SOP | UFP/Sink/R2 | 7 | BIST_Test_Data | 0x7E43 | 0x00-00-00-80-F2-04-C6-3C-F7-57-FD-47-88-25-35-30-C6-C8-E1-64-EE-30-DA-28-02-4C-F1-3D-
43 | 18.988.663.003 | 18.989.169.005 | <-D | GoodCRC | SOP | DFP/Source/R2 | 7 |  | 0x0F61 | 0x
44 | 27.531.447.000 | 27.532.808.002 | T-> | BIST | SOP | UFP/Sink/R2 | 0 | BIST_Test_Data | 0x7043 | 0x00-00-00-80-CC-AA-63-5D-0A-62-EE-5D-88-72-24-77-16-76-E4-55-A7-50-7F-16-E6-93-6E-7B-
45 | 36.301.698.000 | 36.301.698.000 | <-D | Detach | NONE | NONE/NONE/- | 0 |  | 0x0000 | 0x
46 | 36.301.769.007 | 36.301.769.007 | <-D | GroupCmdTimingPkt | NONE | NONE/NONE/- | 0 | 2 - 0A | 0x0000 | 0x