###
GRL-USB-PD-C2 Compliance Test Report

# DUT Information

Manufacturer |
Model Number |
Serial Number | -1_PD3

# Test Information

Test Lab |
Test Engineer |
Remarks | X
Date and Time: | 20200116_153900

# Controller and Instrument Information

Parameter | Value
--- | ---
GRL USB-PD_C2 Serial No. | 218.316.218.081.251.
GRL USB-PD Software Version | 1.3.16.18
GRL USB-PD Firmware Version | 1.3.16.0.15
GRL USB-PD Eload Firmware Version | 9.7/9.7
Board Calibration | Calibration Success.
App Mode | COMPLIANCE_TEST_PD3
Tx Mask | true
Rx Mask | false
RX mask Power selection | Neutral Power
Device Type | DRP
Cable IR drop Imp(R) | 0
Cable Type. | GRL-SPL-Cable
COMPLIANCE_TEST_PD3 CTS Version | 1.14
VIF File name |
Noise Pattern Generation: | Two-Tone Noise
VIF info | *Since VIF was not loaded below test results are information Only.
Test cases Execution Time: | 0h:32m:34s

# Product Capabilities

Parameter | VendorInfoFile | GetCapabilities
--- | --- | ---
VENDOR_NAME |  | Intel
VIF_PRODUCT_TYPE |  |
MODEL_PART_NUMBER |  |
PRODUCT_REVISION |  |
TID |  | 0
PORT_LABEL |  |
CONNECTOR_TYPE |  |
USB_PD_SUPPORT |  | YES
PD_PORT_TYPE |  |
MANUFACTURER_INFO_PID_PORT |  |
STRUCTURED_VDM_VERSION |  | Version 2.0
TYPE_C_STATE_MACHINE |  |
PORT_BATTERY_POWERED |  | NO
BC_1_2_SUPPORT |  |
BC_1_2_CHARGING_PORT_TYPE |  |
PD_SPECIFICATION_REVISION |  | Revision 3
SOP_CAPABLE |  | YES
SOP_P_CAPABLE |  | YES
SOP_PP_CAPABLE |  | NO
SOP_P_DEBUG_CAPABLE |  | NO
SOP_PP_DEBUG_CAPABLE |  | NO
SECURITY_MSGS_SUPPORTED |  | NO
MANUFACTURER_INFO_SUPPORTED |  | YES
MANUFACTURER_INFO_VID |  | 0x8087
MANUFACTURER_INFO_PID |  | 0x0
NUM_FIXED_BATTERIES |  | 0
NUM_SWAPPABLE_BATTERY_SLOTS |  | 0
USB_COMMS_CAPABLE |  | YES
DR_SWAP_TO_DFP_SUPPORTED |  | NO
DR_SWAP_TO_UFP_SUPPORTED |  | NO
UNCONSTRAINED_POWER |  | YES
VCONN_SWAP_TO_ON_SUPPORTED |  |
VCONN_SWAP_TO_OFF_SUPPORTED |  |
RESPONDS_TO_DISCOV_SOP_UFP |  |
RESPONDS_TO_DISCOV_SOP_DFP |  |
ATTEMPTS_DISCOV |  |
CHUNKING_IMPLEMENTED |  | NO
UNCHUNKED_EXTENDED_MESSAGES_SUPPORTED |  | YES
PRODUCT_TYPE_UFP |  |
PRODUCT_TYPE_DFP |  |
MODAL_OPERATION_SUPPORTED |  | YES
USB_VID |  | 0x8087
PID |  | 0x0
BCDDEVICE |  | 0x649
XID |  | 1105
DATA_CAPABLE_AS_USB_HOST |  | YES
DATA_CAPABLE_AS_USB_DEVICE |  | YES
PRODUCT_TYPE |  |
CABLE_HW_VERS |  |
CABLE_FW_VERS |  |
TYPE_C_TO_TYPE_A_B_C |  |
TYPE_C_TO_TYPE_C_CAPT_VDM_V2 |  |
TYPE_C_TO_PLUG_RECEPTACLE |  |
CABLE_LATENCY |  |
CABLE_TERMINATION_TYPE |  |
VBUS_THROUGH_CABLE |  |
CABLE_VBUS_CURRENT |  |
CABLE_SOP_PP_CONTROLLER |  |
CABLE_SUPERSPEED_SUPPORT |  |
MAX_VBUS_VOLTAGE_VDM_V2 |  |
ACCEPTS_PR_SWAP_AS_SRC |  |
ACCEPTS_PR_SWAP_AS_SNK |  |
REQUESTS_PR_SWAP_AS_SRC |  |
REQUESTS_PR_SWAP_AS_SNK |  |
FR_SWAP_SUPPORTED_AS_INITIAL_SINK |  |
AMA_FW_VERS |  |
AMA_HW_VERS |  |
AMA_SUPERSPEED_SUPPORT |  |
AMA_VBUS_REQD |  |
AMA_VCONN_POWER |  |
AMA_VCONN_REQD |  |
HOST_SPEED |  |
DEVICE_SPEED |  |
CABLE_NUM_SVIDS_MIN |  |
CABLE_NUM_SVIDS_MAX |  |
SVID_FIXED |  |
NUM_SVIDS_MIN |  | 1
NUM_SVIDS_MAX |  | 2
SVID1SOP | - | 8087
SVID1Modes Min | - | 1
SVID1Modes Max | - | 1
SVID1Modes Fixed | - | YES
SVID1Mode1 Enter Mode | - | NO
SVID2SOP | - | FF01
SVID2Modes Min | - | 1
SVID2Modes Max | - | 1
SVID2Modes Fixed | - | YES
SVID2Mode1 Enter Mode | - | YES
TYPE_C_IMPLEMENTS_TRY_SRC |  |
TYPE_C_IMPLEMENTS_TRY_SNK |  |
RP_VALUE |  |
TYPE_C_IS_VCONN_POWERED_ACCESSORY |  |
TYPE_C_IS_DEBUG_TARGET_SRC |  |
TYPE_C_IS_DEBUG_TARGET_SNK |  |
TYPE_C_CAN_ACT_AS_HOST |  |
TYPE_C_CAN_ACT_AS_DEVICE |  |
TYPE_C_IS_ALT_MODE_CONTROLLER |  |
TYPE_C_IS_ALT_MODE_ADAPTER |  |
TYPE_C_POWER_SOURCE |  |
TYPE_C_PORT_ON_HUB |  |
TYPE_C_SUPPORTS_AUDIO_ACCESSORY |  |
CAPTIVE_CABLE |  |
TYPE_C_SOURCES_VCONN |  |
HOST_SUSPEND_SUPPORTED |  |

# Power Capabilities

Parameter | VendorInfoFile | GetCapabilities
--- | --- | ---
PD_POWER_AS_SOURCE |  | 15000
USB_SUSPEND_MAY_BE_CLEARED |  | YES
SENDS_PINGS |  | NO
FR_SWAP_SUPPORTED_AS_SOURCE |  |
PD_OC_PROTECTION |  |
PD_OCP_METHOD |  |
NUM_SRC_PDOS |  | 1
Supply Type #1 | - | Fixed
Peak Current #1 | - | 0x0(A)
Voltage #1 | - | 0x64(5V)
Max Current #1 | - | 0x12C(3A)
PD_POWER_AS_SINK |  | 0
NO_USB_SUSPEND_MAY_BE_SET |  | NO
GIVEBACK_MAY_BE_SET |  | NO
HIGHER_CAPABILITY_SET |  | NO
FR_SWAP_REQD_TYPE_C_CURRENT_AS_INITIAL_SOURCE |  | 0
NUM_SNK_PDOS |  | 1
Supply Type #1 | - | Fixed
Voltage #1 | - | 0x64(5V)
OP Current #1 | - | 0x0(A)

# Test Result Summary

Sl No | Test ID | Test Name | Test Result
--- | --- | --- | ---
1 | TD.PD.LL3.E1 | TD.PD.LL3.E1 GoodCRC Specification Revision compatibility | PASS
2 | TD.PD.LL3.E2 | TD.PD.LL3.E2 Retransmission | PASS
3 | TD.PD.LL3.E3 | TD.PD.LL3.E3 GoodCRC Compatibility with PD2 | PASS
4 | TD.PD.SRC3.E1 | TD.PD.SRC3.E1 Source Capability Fields Checks | PASS
5 | TD.PD.SRC3.E2 | TD.PD.SRC3.E2 Accept Fields Checks | PASS
6 | TD.PD.SRC3.E3 | TD.PD.SRC3.E3 PSRDY Fields Checks | PASS
7 | TD.PD.SRC3.E4 | TD.PD.SRC3.E4 Specification Revision Check after Contract | PASS
8 | TD.PD.SRC3.E5 | TD.PD.SRC3.E5 Source Capabilities Extended sent timely | PASS
9 | TD.PD.SRC3.E6 | TD.PD.SRC3.E6 Source Capabilities Extended Fields Checks | PASS
10 | TD.PD.SRC3.E7 | TD.PD.SRC3.E7 Battery Status sent Timely | PASS
11 | TD.PD.SRC3.E8 | TD.PD.SRC3.E8 Battery Status Fields Checks | PASS
12 | TD.PD.SRC3.E9 | TD.PD.SRC3.E9 Battery Status Fields Checks Invalid Battery reference | PASS
13 | TD.PD.SRC3.E10 | TD.PD.SRC3.E10 Unrecognized Message Received in Ready State | PASS
14 | TD.PD.SRC3.E11 | TD.PD.SRC3.E11 Get Status Fields Checks | PASS
15 | TD.PD.SRC3.E12 | TD.PD.SRC3.E12 Get Battery Status Fields Checks | PASS
16 | TD.PD.SRC3.E13 | TD.PD.SRC3.E13 Status sent timely | PASS
17 | TD.PD.SRC3.E14 | TD.PD.SRC3.E14 Status Fields Checks | FAIL
18 | TD.PD.SRC3.E15 | TD.PD.SRC3.E15 Battery Capabilities sent timely | PASS
19 | TD.PD.SRC3.E16 | TD.PD.SRC3.E16 Battery Capabilities Fields Checks | PASS
20 | TD.PD.SRC3.E17 | TD.PD.SRC3.E17 Battery Capabilities Fields Checks Invalid Battery Reference | PASS
21 | TD.PD.SRC3.E18 | TD.PD.SRC3.E18 Manufacturer Info Sent Timely | PASS
22 | TD.PD.SRC3.E19 | TD.PD.SRC3.E19 Manufacturer Info Fields Checks | PASS
23 | TD.PD.SRC3.E20 | TD.PD.SRC3.E20 Manufacturer Info Fields Checks Invalid Manufacturer Info Target | FAIL
24 | TD.PD.SRC3.E21 | TD.PD.SRC3.E21 Manufacturer Info Fields Checks Invalid Manufacturer Info Ref | FAIL
25 | TD.PD.SRC3.E22 | TD.PD.SRC3.E22 Cable Type Detection | PASS
26 | TD.PD.SRC3.E23 | TD.PD.SRC3.E23 Vconn Swap | PASS
27 | TD.PD.SRC3.E24 | TD.PD.SRC3.E24 Unexpected Message Received in Ready State | PASS
28 | TD.PD.SRC3.E25 | TD.PD.SRC3.E25 Receiving chunked extended message | PASS
29 | TD.PD.SRC3.E26 | TD.PD.SRC3.E26 Soft Reset sent regardless of Rp value | PASS
30 | TD.PD.SRC3.E27 | TD.PD.SRC3.E27 PPS Status Sent Timely | NA
31 | TD.PD.SRC3.E28 | TD.PD.SRC3.E28 PPS Status Fields Check | NA
32 | TD.PD.SRC3.E29 | TD.PD.SRC3.E29 SourcePPSCommTimer Deadline | NA
33 | TD.PD.SRC3.E30 | TD.PD.SRC3.E30 SourcePPSCommTimer Timeout | NA
34 | TD.PD.SRC3.E31 | TD.PD.SRC3.E31 SourcePPSCommTimer Stopped | NA
35 | TD.PD.SRC3.E32 | TD.PD.SRC3.E32 ChunkSenderResponseTimer Timeout | FAIL
36 | TD.PD.SRC3.E33 | TD.PD.SRC3.E33 Country Codes Sent Timely | PASS
37 | TD.PD.SRC3.E34 | TD.PD.SRC3.E34 Country Codes Fields Checks | PASS
38 | TD.PD.SRC3.E35 | TD.PD.SRC3.E35 Country Info Sent Timely | PASS
39 | TD.PD.SRC3.E36 | TD.PD.SRC3.E36 Country Info Fields Checks | PASS
40 | TD.PD.SNK3.E1 | TD.PD.SNK3.E1 Request Fields Checks | PASS
41 | TD.PD.SNK3.E2 | TD.PD.SNK3.E2 Unrecognized Message Received in Ready State | PASS
42 | TD.PD.SNK3.E3 | TD.PD.SNK3.E3 Get Source Cap Extended Fields Checks | PASS
43 | TD.PD.SNK3.E4 | TD.PD.SNK3.E4 SenderResponseTimer Deadline Source Capabilities Extended | PASS
44 | TD.PD.SNK3.E5 | TD.PD.SNK3.E5 SenderResponseTimer Timeout Source Capabilities Extended | PASS
45 | TD.PD.SNK3.E6 | TD.PD.SNK3.E6 Get Status Fields Checks | PASS
46 | TD.PD.SNK3.E7 | TD.PD.SNK3.E7 Get Battery Status Fields Checks | PASS
47 | TD.PD.SNK3.E8 | TD.PD.SNK3.E8 Status sent timely | PASS
48 | TD.PD.SNK3.E9 | TD.PD.SNK3.E9 Manufacturer Info Sent Timely | PASS
49 | TD.PD.SNK3.E10 | TD.PD.SNK3.E10 Source Capabilities Extended sent timely | PASS
50 | TD.PD.SNK3.E11 | TD.PD.SNK3.E11 Receiving chunked extended message | PASS
51 | TD.PD.SNK3.E12 | TD.PD.SNK3.E12 Soft Reset sent regardless of Rp value | PASS
52 | TD.PD.SNK3.E13 | TD.PD.SNK3.E13 SinkPPSPeriodicTimer Timeout | NA
53 | TD.PD.SNK3.E14 | TD.PD.SNK3.E14 Request Fields Checks PPS | NA
54 | TD.PD.SNK3.E15 | TD.PD.SNK3.E15 Status Fields Checks | FAIL
55 | TD.PD.SNK3.E16 | TD.PD.SNK3.E16 Manufacturer Info Fields Checks | PASS
56 | TD.PD.SNK3.E17 | TD.PD.SNK3.E17 Manufacturer Info Fields Checks Invalid Manufacturer Info Target | FAIL
57 | TD.PD.SNK3.E18 | TD.PD.SNK3.E18 Manufacturer Info Fields Checks Invalid Manufacturer Info Ref | FAIL
58 | TD.PD.SNK3.E19 | TD.PD.SNK3.E19 ChunkSenderResponseTimer Timeout | PASS
59 | TD.PD.VDM3.E1 | TD.PD.VDM3.E1 Fields Checks Discover Identity | PASS
60 | TD.PD.VDM3.E2 | TD.PD.VDM3.E2 Unrecognized VID in Unstructured VDM | PASS
61 | TD.PD.PRSISNK3.E1 | TD.PD.PRSISNK3.E1 Collision Avoidance after PR-Swap | PASS

# Detailed Test Result

Test Status | Test Description
--- | ---
PASS | 1. TD.PD.LL3.E1 GoodCRC Specification Revision compatibility (Click to View Protocol Trace)
PASS | 2. TD.PD.LL3.E2 Retransmission (Click to View Protocol Trace)
PASS | 3. TD.PD.LL3.E3 GoodCRC Compatibility with PD2 (Click to View Protocol Trace)
PASS | 4. TD.PD.SRC3.E1 Source Capability Fields Checks (Click to View Protocol Trace)
PASS | 5. TD.PD.SRC3.E2 Accept Fields Checks (Click to View Protocol Trace)
PASS | 6. TD.PD.SRC3.E3 PSRDY Fields Checks (Click to View Protocol Trace)
PASS | 7. TD.PD.SRC3.E4 Specification Revision Check after Contract (Click to View Protocol Trace)
PASS | 8. TD.PD.SRC3.E5 Source Capabilities Extended sent timely (Click to View Protocol Trace)
PASS | 9. TD.PD.SRC3.E6 Source Capabilities Extended Fields Checks (Click to View Protocol Trace)
PASS | TD.PD.SRC3.E6 Source Capabilities Extended Fields Checks_Unchunked(True):
PASS | TD.PD.SRC3.E6 Source Capabilities Extended Fields Checks_Unchunked(False):
PASS | 10. TD.PD.SRC3.E7 Battery Status sent Timely (Click to View Protocol Trace)
| DUT sent (0) Batteries on Source capabilities Extended Message
PASS | 11. TD.PD.SRC3.E8 Battery Status Fields Checks (Click to View Protocol Trace)
PASS | 12. TD.PD.SRC3.E9 Battery Status Fields Checks Invalid Battery reference (Click to View Protocol Trace)
PASS | 13. TD.PD.SRC3.E10 Unrecognized Message Received in Ready State (Click to View Protocol Trace)
PASS | 14. TD.PD.SRC3.E11 Get Status Fields Checks (Click to View Protocol Trace)
PASS | 15. TD.PD.SRC3.E12 Get Battery Status Fields Checks (Click to View Protocol Trace)
PASS | TD.PD.SRC3.E12 Get Battery Status Fields Checks_Unchunked(True):
PASS | TD.PD.SRC3.E12 Get Battery Status Fields Checks_Unchunked(False):
PASS | 16. TD.PD.SRC3.E13 Status sent timely (Click to View Protocol Trace)
FAIL | 17. TD.PD.SRC3.E14 Status Fields Checks (Click to View Protocol Trace)
FAIL | TD.PD.SRC3.E14 Status Fields Checks_Unchunked(True):
| DataSize was 5 bytes but expected 6 bytes
FAIL | TD.PD.SRC3.E14 Status Fields Checks_Unchunked(False):
| DataSize was 5 bytes but expected 6 bytes
PASS | 18. TD.PD.SRC3.E15 Battery Capabilities sent timely (Click to View Protocol Trace)
| DUT sent (0) batteries in Source capabilities Extended message
PASS | 19. TD.PD.SRC3.E16 Battery Capabilities Fields Checks (Click to View Protocol Trace)
PASS | TD.PD.SRC3.E16 Battery Capabilities Fields Checks_Unchunked(True):
PASS | TD.PD.SRC3.E16 Battery Capabilities Fields Checks_Unchunked(False):
PASS | 20. TD.PD.SRC3.E17 Battery Capabilities Fields Checks Invalid Battery Reference (Click to View Protocol Trace)
PASS | TD.PD.SRC3.E17 Battery Capabilities Fields Checks Invalid Battery Reference_Unchunked(True):
PASS | TD.PD.SRC3.E17 Battery Capabilities Fields Checks Invalid Battery Reference_Unchunked(False):
PASS | 21. TD.PD.SRC3.E18 Manufacturer Info Sent Timely (Click to View Protocol Trace)
PASS | 22. TD.PD.SRC3.E19 Manufacturer Info Fields Checks (Click to View Protocol Trace)
PASS | TD.PD.SRC3.E19 Manufacturer Info Fields Checks_Unchunked(True):
PASS | TD.PD.SRC3.E19 Manufacturer Info Fields Checks_Unchunked(False):
FAIL | 23. TD.PD.SRC3.E20 Manufacturer Info Fields Checks Invalid Manufacturer Info Target (Click to View Protocol Trace)
FAIL | TD.PD.SRC3.E20 Manufacturer Info Fields Checks Invalid Manufacturer Info Target_Unchunked(True):
| DataSize was 4 bytes but expected 18 bytes DUT sent Invalid Byte List
FAIL | TD.PD.SRC3.E20 Manufacturer Info Fields Checks Invalid Manufacturer Info Target_Unchunked(False):
| No.of data objects was 2 but expected 5 DataSize was 4 bytes but expected 18 bytes DUT sent Invalid Byte List
FAIL | 24. TD.PD.SRC3.E21 Manufacturer Info Fields Checks Invalid Manufacturer Info Ref (Click to View Protocol Trace)
FAIL | TD.PD.SRC3.E21 Manufacturer Info Fields Checks Invalid Manufacturer Info Ref_Unchunked(True):
| DataSize was 4 bytes but expected 18 bytes DUT sent Invalid Byte List
FAIL | TD.PD.SRC3.E21 Manufacturer Info Fields Checks Invalid Manufacturer Info Ref_Unchunked(False):
| No.of data objects was 2 but expected 5 DataSize was 4 bytes but expected 18 bytes DUT sent Invalid Byte List
PASS | 25. TD.PD.SRC3.E22 Cable Type Detection (Click to View Protocol Trace)
PASS | TD.PD.SRC3.E22 Cable Type Detection_1:
| DUT incapable to offer current >3A or voltage >20V
PASS | 26. TD.PD.SRC3.E23 Vconn Swap (Click to View Protocol Trace)
PASS | 27. TD.PD.SRC3.E24 Unexpected Message Received in Ready State (Click to View Protocol Trace)
PASS | 28. TD.PD.SRC3.E25 Receiving chunked extended message (Click to View Protocol Trace)
PASS | 29. TD.PD.SRC3.E26 Soft Reset sent regardless of Rp value (Click to View Protocol Trace)
NA | 30. TD.PD.SRC3.E27 PPS Status Sent Timely (Click to View Protocol Trace)
| Tester could not find APDO's{0}
NA | 31. TD.PD.SRC3.E28 PPS Status Fields Check (Click to View Protocol Trace)
| Tester could not find APDO's{0}
NA | 32. TD.PD.SRC3.E29 SourcePPSCommTimer Deadline (Click to View Protocol Trace)
| Tester could not find APDO's{0}
NA | 33. TD.PD.SRC3.E30 SourcePPSCommTimer Timeout (Click to View Protocol Trace)
| DUT does not contains APDO's{0}
NA | 34. TD.PD.SRC3.E31 SourcePPSCommTimer Stopped (Click to View Protocol Trace)
| DUT does not contains APDO's{0}
FAIL | 35. TD.PD.SRC3.E32 ChunkSenderResponseTimer Timeout (Click to View Protocol Trace)
| DUT responded with Reserved message
PASS | 36. TD.PD.SRC3.E33 Country Codes Sent Timely (Click to View Protocol Trace)
| DUT responded with Not Supported message
PASS | 37. TD.PD.SRC3.E34 Country Codes Fields Checks (Click to View Protocol Trace)
PASS | TD.PD.SRC3.E34 Country Codes Fields Checks_Unchunked(True):
| DUT responded with Not Supported message
PASS | TD.PD.SRC3.E34 Country Codes Fields Checks_Unchunked(False):
| DUT responded with Not Supported message
PASS | 38. TD.PD.SRC3.E35 Country Info Sent Timely (Click to View Protocol Trace)
| DUT responded with Not Supported message
PASS | 39. TD.PD.SRC3.E36 Country Info Fields Checks (Click to View Protocol Trace)
PASS | TD.PD.SRC3.E36 Country Info Fields Checks_Unchunked(True):
| DUT responded with Not Supported message
PASS | TD.PD.SRC3.E36 Country Info Fields Checks_Unchunked(False):
| DUT responded with Not Supported message
PASS | 40. TD.PD.SNK3.E1 Request Fields Checks (Click to View Protocol Trace)
PASS | 41. TD.PD.SNK3.E2 Unrecognized Message Received in Ready State (Click to View Protocol Trace)
PASS | 42. TD.PD.SNK3.E3 Get Source Cap Extended Fields Checks (Click to View Protocol Trace)
PASS | 43. TD.PD.SNK3.E4 SenderResponseTimer Deadline Source Capabilities Extended (Click to View Protocol Trace)
PASS | 44. TD.PD.SNK3.E5 SenderResponseTimer Timeout Source Capabilities Extended (Click to View Protocol Trace)
| Dut not initiated Hardreset/softreset
PASS | 45. TD.PD.SNK3.E6 Get Status Fields Checks (Click to View Protocol Trace)
| DUT not responded for Alert message.
PASS | 46. TD.PD.SNK3.E7 Get Battery Status Fields Checks (Click to View Protocol Trace)
PASS | TD.PD.SNK3.E7 Get Battery Status Fields Checks_Unchunked(True):
| DUT not responded for Alert message.
PASS | TD.PD.SNK3.E7 Get Battery Status Fields Checks_Unchunked(False):
| DUT responded with Get status message.
PASS | 47. TD.PD.SNK3.E8 Status sent timely (Click to View Protocol Trace)
PASS | 48. TD.PD.SNK3.E9 Manufacturer Info Sent Timely (Click to View Protocol Trace)
PASS | 49. TD.PD.SNK3.E10 Source Capabilities Extended sent timely (Click to View Protocol Trace)
PASS | 50. TD.PD.SNK3.E11 Receiving chunked extended message (Click to View Protocol Trace)
PASS | 51. TD.PD.SNK3.E12 Soft Reset sent regardless of Rp value (Click to View Protocol Trace)
NA | 52. TD.PD.SNK3.E13 SinkPPSPeriodicTimer Timeout (Click to View Protocol Trace)
| DUT doesn't Requested APDO
NA | 53. TD.PD.SNK3.E14 Request Fields Checks PPS (Click to View Protocol Trace)
| DUT doesn't Requested APDO
FAIL | 54. TD.PD.SNK3.E15 Status Fields Checks (Click to View Protocol Trace)
FAIL | TD.PD.SNK3.E15 Status Fields Checks_Unchunked(True):
| DataSize was 5 bytes but expected 6 bytes
FAIL | TD.PD.SNK3.E15 Status Fields Checks_Unchunked(false):
| DataSize was 5 bytes but expected 6 bytes
PASS | 55. TD.PD.SNK3.E16 Manufacturer Info Fields Checks (Click to View Protocol Trace)
PASS | TD.PD.SNK3.E16 Manufacturer Info Fields Checks_Unchunked(True):
PASS | TD.PD.SNK3.E16 Manufacturer Info Fields Checks_Unchunked(false):
FAIL | 56. TD.PD.SNK3.E17 Manufacturer Info Fields Checks Invalid Manufacturer Info Target (Click to View Protocol Trace)
FAIL | TD.PD.SNK3.E17 Manufacturer Info Fields Checks Invalid Manufacturer Info Target_Unchunked(True):
| DataSize was 4 bytes but expected 18 bytes DUT sent Invalid Byte List
FAIL | TD.PD.SNK3.E17 Manufacturer Info Fields Checks Invalid Manufacturer Info Target_Unchunked(False):
| No.of data objects was 2 but expected 5 DataSize was 4 bytes but expected 18 bytes DUT sent Invalid Byte List
FAIL | 57. TD.PD.SNK3.E18 Manufacturer Info Fields Checks Invalid Manufacturer Info Ref (Click to View Protocol Trace)
FAIL | TD.PD.SNK3.E18 Manufacturer Info Fields Checks Invalid Manufacturer Info Ref_Unchunked(True):
| DataSize was 4 bytes but expected 18 bytes DUT sent Invalid Byte List
FAIL | TD.PD.SNK3.E18 Manufacturer Info Fields Checks Invalid Manufacturer Info Ref_Unchunked(False):
| No.of data objects was 2 but expected 5 DataSize was 4 bytes but expected 18 bytes DUT sent Invalid Byte List
PASS | 58. TD.PD.SNK3.E19 ChunkSenderResponseTimer Timeout (Click to View Protocol Trace)
PASS | 59. TD.PD.VDM3.E1 Fields Checks Discover Identity (Click to View Protocol Trace)
PASS | 60. TD.PD.VDM3.E2 Unrecognized VID in Unstructured VDM (Click to View Protocol Trace)
PASS | 61. TD.PD.PRSISNK3.E1 Collision Avoidance after PR-Swap (Click to View Protocol Trace)