# Results for C:\AutoMeas\AUTO_SIGTEST\Eden_Chang\P100IVA_R100\SATA\Internal_MPCIE\Gen2\Port1_1-1

Sigtest:

- Overall Sigtest Result: Pass!

- Mean Unit Interval (ps): 333.336407
  Mean Unit Interval Passes Sigtest Limits!

- Max Unit Interval (ps): 333.336407
  Max Unit Interval Passes Sigtest Limits!

- Min Unit Interval (ps): 333.336407
  Min Unit Interval Passes Sigtest Limits!

- Min Time Between Crossovers (ps): 315.123153
  Min Time Between Crossovers Passes Sigtest Limits!

- Data Rate (Gb/s): 2.999972

- Per Edge RMS Jitter (ps): 3.471503

- Mean Median to Peak Jitter: 9.397828 ps
  Mean Median to Peak Jitter Passes Sigtest Limits!

- Max Median to Peak Jitter: 14.312228 ps
  Max Median to Peak Jitter Passes Sigtest Limits!

- Min Median to Peak Jitter: 6.818719 ps
  Min Median to Peak Jitter Passes Sigtest Limits!

- Mean Peak to Peak Jitter: 17.064462 ps
  Mean Peak to Peak Jitter Passes Sigtest Limits!

- Max Peak to Peak Jitter: 24.234843 ps
  Max Peak to Peak Jitter Passes Sigtest Limits!

- Minimum eye width: 309.098457 ps

- Min Peak to Peak Jitter: 12.759478 ps
  Min Peak to Peak Jitter Passes Sigtest Limits!

- Minimum Transition Eye Voltage: -0.3276 volts
  Minimum Transition Eye Voltage Passes Sigtest Limits!

- Maximum Transition Eye Voltage: 0.3276 volts
  Maximum Transition Eye Voltage Passes Sigtest Limits!

- Minimum Non Transition Eye Voltage: -0.336 volts
  Minimum Non Transition Eye Voltage Passes Sigtest Limits!

- Maximum Non Transition Eye Voltage: 0.336 volts
  Maximum Non Transition Eye Voltage Passes Sigtest Limits!

- Composit Eye Height: 0.4187

- Composit Eye Location: 0.5

- Minimum Transition Eye Voltage Margin Above Eye: 0.005673 volts
  Minimum Transition Eye Voltage Margin Above Eye Passes Sigtest Limits!

- Minimum Transition Eye Voltage Margin Below Eye: -0.013027 volts
  Minimum Transition Eye Voltage Margin Below Eye Passes Sigtest Limits!

- Minimum Transition Eye Height: 0.4187 volts

- Minimum Non Transition Eye Voltage Margin Above Eye: 0.038605 volts
  Minimum Non Transition Eye Voltage Margin Above Eye Passes Sigtest Limits!

- Minimum Non Transition Eye Voltage Margin Below Eye: -0.058722 volts
  Minimum Non Transition Eye Voltage Margin Below Eye Passes Sigtest Limits!

- Minimum Non Transition Eye Height: 0.497326 volts

Worst Non Transition Signal Eye

Worst Transition Signal Eye

TEMPLATE FILE SETTINGS

- Template File: fbd_3_2gb_dimm_(beta) \ \satai_3_0gb\TX_CON_FBAUD_500

- Nominal Data Rate (bits/sec): 3000000000.0

- Target Unit Interval (s): 3.333333e-010

- Minimum Allowed Recovered Unit Interval (s): 3.332167e-010

- Maximum Allowed Recovered Unit Interval (s): 3.351167e-010

- Minimum Time Allowed Between Crossovers (s): 0.0

- Method For Normalizing Jitter: EYE_JITTER_NORM_HALF_PEAK_PEAK (2)

- Clock Recovery Method: EYE_CLOCK_MINIMIZE_DEVIATION (2)

- Clock Recovery Window Size (UI): 293

- Jitter Analysis Window Size (UI): 293

- Window Advance (UI): 50

- Minimum Data For Testing (UI): 5000

- Ambiguous UI Resolution Method: EYE_AMBIGUOUS_NONE (0)

- Peak to Peak Jitter Limit (s): 1.019e-010

  Sigtest Version: 3.2.0