# Results for C:\AutoMeas\AUTO_SIGTEST\Eden_Chang\P100IVA_R100\SATA\Internal_MPCIE\Gen1\Port1_2

Sigtest:

- Overall Sigtest Result: Fail!

- Mean Unit Interval (ps): 666.672755
  Mean Unit Interval Passes Sigtest Limits!

- Max Unit Interval (ps): 666.672755
  Max Unit Interval Passes Sigtest Limits!

- Min Unit Interval (ps): 666.672755
  Min Unit Interval Passes Sigtest Limits!

- Min Time Between Crossovers (ps): 645.366667
  Min Time Between Crossovers Passes Sigtest Limits!

- Data Rate (Gb/s): 1.499986

- Per Edge RMS Jitter (ps): 4.052981

- Mean Median to Peak Jitter: 10.302162 ps
  Mean Median to Peak Jitter Passes Sigtest Limits!

- Max Median to Peak Jitter: 15.047101 ps
  Max Median to Peak Jitter Passes Sigtest Limits!

- Min Median to Peak Jitter: 7.865899 ps
  Min Median to Peak Jitter Passes Sigtest Limits!

- Mean Peak to Peak Jitter: 19.264737 ps
  Mean Peak to Peak Jitter Passes Sigtest Limits!

- Max Peak to Peak Jitter: 27.267543 ps
  Max Peak to Peak Jitter Passes Sigtest Limits!

- Minimum eye width: 639.399157 ps

- Min Peak to Peak Jitter: 15.151172 ps
  Min Peak to Peak Jitter Passes Sigtest Limits!

- Minimum Transition Eye Voltage: -0.3388 volts
  Minimum Transition Eye Voltage Fails Sigtest Limits!

- Maximum Transition Eye Voltage: 0.3332 volts
  Maximum Transition Eye Voltage Fails Sigtest Limits!

- Minimum Non Transition Eye Voltage: -0.3444 volts
  Minimum Non Transition Eye Voltage Fails Sigtest Limits!

- Maximum Non Transition Eye Voltage: 0.336 volts
  Maximum Non Transition Eye Voltage Fails Sigtest Limits!

- Composit Eye Height: 0.496103

- Composit Eye Location: 0.5

- Minimum Transition Eye Voltage Margin Above Eye: 0.044082 volts
  Minimum Transition Eye Voltage Margin Above Eye Passes Sigtest Limits!

- Minimum Transition Eye Voltage Margin Below Eye: -0.052021 volts
  Minimum Transition Eye Voltage Margin Below Eye Passes Sigtest Limits!

- Minimum Transition Eye Height: 0.496103 volts

- Minimum Non Transition Eye Voltage Margin Above Eye: 0.069145 volts
  Minimum Non Transition Eye Voltage Margin Above Eye Passes Sigtest Limits!

- Minimum Non Transition Eye Voltage Margin Below Eye: -0.076947 volts
  Minimum Non Transition Eye Voltage Margin Below Eye Passes Sigtest Limits!

- Minimum Non Transition Eye Height: 0.546092 volts

Worst Non Transition Signal Eye

Worst Transition Signal Eye

TEMPLATE FILE SETTINGS

- Template File: fbd_3_2gb_dimm_(beta) \ \satai_1_5gb\TX_CON_250UI

- Nominal Data Rate (bits/sec): 1500000000.0

- Target Unit Interval (s): 6.666667e-010

- Minimum Allowed Recovered Unit Interval (s): 6.664333e-010

- Maximum Allowed Recovered Unit Interval (s): 6.702333e-010

- Minimum Time Allowed Between Crossovers (s): 0.0

- Method For Normalizing Jitter: EYE_JITTER_NORM_HALF_PEAK_PEAK (2)

- Clock Recovery Method: EYE_CLOCK_MINIMIZE_DEVIATION (2)

- Clock Recovery Window Size (UI): 250

- Jitter Analysis Window Size (UI): 250

- Window Advance (UI): 50

- Minimum Data For Testing (UI): 5000

- Ambiguous UI Resolution Method: EYE_AMBIGUOUS_NONE (0)

- Peak to Peak Jitter Limit (s): 2.5381e-010

  Sigtest Version: 3.2.0