ASUS . EA Report | SATA Test |

Project: P100IVM_R100 Tester: Eden_Chang
Result: FAIL
Configuration

Description | Comments
Motherboard Revision | R100
BIOS Revision | N/A
CPU | MIMX8MQ6CAVHZAB
Clock Generator | N/A
DIMM | On board
Power Supply | DELTA DPS-65VB
Expansion Cards | N/A
Software Utility | N/A
Oscilloscope | DPO73304DX
Start Date | 11/10/2022
Finish Date | 11/10/2022
Notes |

Revision History:

Revision | Date | Description
2.5 | 20220210 | Add Clock Jitter Tool version 5.0.2 "Noise Floor" PRAM. (by Dennis)
2.6 | 20220408 | Add PCI-E Gen5 Item,Merge the two Clock jitter test versions 1.6.7.6/5.0.5 (by Dennis)
2.7 |  | Add PDF

Measurement Signals Summary & Marginal EA Characterization:

Signal name | Result | Problem Description
Internal_MPCIE Signals
Gen1
| Port1 | FAIL | Minimum Transition Eye Voltage Fails Sigtest Limits! Maximum Transition Eye Voltage Fails Sigtest Limits! Minimum Non Transition Eye Voltage Fails Sigtest Limits! Maximum Non Transition Eye Voltage Fails Sigtest Limits!

Gen2
Port1 PASS

Auto Report Builder, Copyright © 2019 Dennis Wu, EA team, Motherboard RD, ASUSTek Computer Inc.