SafetyDSP 3.1.3 EtherCAT to Expansion 1.1.1

Without expansion :
1
Port
T2
MUX
Trancei
U14
DSP1
Main
Trancei
U12
Port
T1

2


3









1


2

3

P1_TD_N
[image: ]
P1_RD_N
[image: ]


SafetyDSP 3.1.3 EtherCAT to Expansion 1.1.1

With expansion :
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EX1_TD_N (goes to RX of Transceiver)
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EX1_RD_N (goes to TX of Transceiver)
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EX1_TD_N (goes to RX of Transceiver)
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EX1_RD_N (goes to TX of Transceiver)
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