We need to split output from serializer (DS99R105) to two different receivers. My question is regarding capacitive coupling. Do I need C72, C73 between DS99R105 and SY89876 and do I need capacitively couple outputs of U60 (DOUT0, DOUT1) connecting to DS99R106 on receiving end?

