传统收发Traditional sending and receiving



黄-TX，绿-DE/RE，红-A-B

Yellow-TX, green-DE/RE, red-A-B



自动收发Automatic sending and receiving in 115200 baud rate:



黄-TX，绿-DE/RE，红-A-B Yellow-TX, green-DE/RE, red-A-B

自动收发Automatic sending and receiving in 9600 baud rate

