1. **Change PHY to Reverse Loopback**


**Driver config：**

err = phy\_write(phydev, 0x16,0x0150);


Bit[5:2] Loopback Select: 0100 = Reverse Loopback

Bit[6] 1 = Transmit data to the MDI in xMII Loopback

**Wireshark info:**



**RXDV: OK**



**RCLK:25MHz OK**




**RX\_D0:**



**RX\_D1:**



**RX\_D2:**



**RX\_D3:**

