Hi,

I have question about cross point:

6A will send data to 7A and 7B

6B will send data to 6B and 6A

How to setup reg 0x96 bit 5?

Do 6A,6B,7A,&b all master?

Or

?





