Hi,

 I have question about cross point:

 6A will send data to 7A and 7B

 6B will send data to 6B and 6A

 How to setup reg 0x96 bit 5?

 Do 6A,6B,7A,&b all master?

 Or

 ?





