Receiver Return Loss

Application Version : 3.2.8.28

3ns to 5ns

<1.4ns

<500ps

<5%

<500ps(±250ps)

<1.4ns

<5%

<500ps

3ns to 5ns

3ns to 5ns

3ns to 5ns

0.98 to 1.02

-950mV to -1050mV

950mV to1050mV

Fit the template

Transmitter Return Loss

Distortion (Duty Cycle)

Transmit Jitter(-ve)

Transmit Jitter(+ve)

Overshoot(-ve)

Overshoot(+ve)

Rise/Fall Symmetry(-ve)

Rise/Fall Symmetry(+ve)

Fall Time(-ve)

Fall Time(+ve)

Rise Time(-ve)

Rise Time(+ve)

Amplitude Symmetry

Output Voltage (-Vout)

Output Voltage (+Vout)

AOI Template

Result

Measured Value

Spec. Range

Test

Time:

16:49:43

Test Report for 100Base-TX 

Device ID : 

Device Description : 

Port ID : 

Pass

Pass

 1002.4mV

-1004.5mV

0.998

Pass

 3.87ns

 3.78ns

 3.76ns

 3.67ns

Pass

Pass

Pass

Pass

 88.8ps

 88.8ps

Pass

Pass

0.00% 

0.00% 

Pass

Pass

  600ps

  480ps

  600ps

Not Available

Not Available

Pass

Fail

Pass

Pass

ANSI X3.263-1995: Annex J AOI Template

AOI Template Result : 
Pass

NOTE: Amplitude values are corrected for Baseline voltage

Spec Range : 950mV to 1050mV

Spec Range : -950mV to -1050mV

ANSI X.3.263-1995 : 9.1.2.2 Differential Output Voltage

Positive Amplitude(+Vout) :  1002.4mV

Negative Amplitude(-Vout) : -1004.5mV

Output Voltage(+Vout) Result : Pass

Output Voltage(-Vout) Result : Pass

Differential Output Voltage Result : Pass

Baseline(+ve) : -53.1mV

Baseline(-ve) : -63.1mV

Spec Range: 0.98 to 1.02

ANSI X3.263-1995: 9.1.4 Signal Amplitude Symmetry

Amplitude Symmetry : 0.998

Amplitude Symmetry Result : Pass

Spec Range: 3ns to 5ns

ANSI X3.263-1995: 9.1.6 Rise Time

Rise Time(+ve) :  3.87ns

Rise Time Test Result : Pass

Rise Time(+ve) Result : Pass

Spec Range: 3ns to 5ns

Rise Time(-ve) :  3.76ns

Rise Time(-ve) Result : Pass

Spec Range: 3ns to 5ns

Spec Range: 3ns to 5ns

ANSI X3.263-1995: 9.1.6 Fall Time

Fall Time(+ve) :  3.78ns

Fall Time(-ve) :  3.67ns

Fall Time Test Result : Pass

Fall Time(+ve) Result : Pass

Fall Time(-ve) Result : Pass

Spec Range: <500ps

Spec Range: <500ps

ANSI X3.263-1995: 9.1.6 Rise Fall Symmetry

Rise/Fall Symmetry Result : Pass

Rise/Fall Symmetry(+ve) :  88.8ps

Rise/Fall Symmetry(-ve) :  88.8ps

Rise/Fall Symmetry(+ve) Result : Pass

Rise/Fall Symmetry(-ve) Result : Pass

Rise/Fall Symmetry(Max-Min) :   194ps

Spec Range: <5%

Spec Range: <5%

ANSI X3.263-1995: 9.1.3 Waveform Overshoot

Overshoot(+ve) : 0.00% 

Overshoot(-ve) : 0.00% 

Waveform Overshoot Test Results : Pass

Overshoot(+ve) Result : Pass

Overshoot(-ve) Result : Pass

Spec Range: <1.4ns

Spec Range: <1.4ns

ANSI X3.263-1995: 9.1.9 Transmit Jitter

Transmit Jitter(-ve) :   480ps

Transmit Jitter(+ve) :   600ps

Transmit Jitter(-ve) Result : Pass

Transmit Jitter(+ve) Result : Pass

Spec Range: <500ps(+/-250ps)

ANSI X3.263-1995: 9.1.8 Distortion(Duty Cycle)

Distortion(Duty Cycle) :   600ps

Distortion(Duty Cycle) Result : 
Fail 
T1 =  40.0ps  T2 =   340ps
T3 =   600ps  T4 =   300ps
T5 =   260ps  T6 =   300ps

-10.00dB

-10.00dB

-9.97dB

-11.56dB

-13.50dB

-16.00dB

-16.00dB

-16.00dB

-16.00dB

60 MHz

70 MHz

80 MHz

50 MHz

40 MHz

30 MHz

20 MHz

10 MHz

1 MHz

Measured Value

Spec. Value

Frequency

ANSI X3.263-1995: 9.1.5 Transmitter Return Loss

Not Available

Not Available

Not Available

Not Available

Not Available

Not Available

Not Available

Not Available

Not Available

Not Available

Result

Transmitter Return Loss Result : Not Available

Not Available

-16.00dB

-16.00dB

-16.00dB

-16.00dB

-13.50dB

-11.56dB

-9.97dB

-10.00dB

-10.00dB

Not Available

Not Available

Not Available

Not Available

Not Available

Not Available

Not Available

Not Available

Not Available

60 MHz

70 MHz

80 MHz

50 MHz

40 MHz

30 MHz

20 MHz

10 MHz

1 MHz

Result

Measured Value

Spec. Value

Frequency

ANSI X3.263-1995: 9.1.5 Receiver Return Loss

Not Available

Receiver Return Loss Result : Not Available

Not Available