# Electrical Rule Check Report

Date: |  | 1/21/2025
Time: |  | 3:50:30 PM
Filename: |  | C:\Users\a0509466\AppData\Local\TempReleases\Snapshot\1\Validation\AMPS262A_ERC.html

Class | Document | Message
--- | --- | ---
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid C2 at 193mm,284.46mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid C3 at 206mm,284.46mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid C4 at 218mm,281.92mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid C5 at 239mm,281.92mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid C6 at 251mm,284.46mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid C7 at 264mm,284.46mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid C8 at 178mm,281.92mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid C9 at 277mm,281.92mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid C10 at 410mm,261.92mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid C11 at 198mm,254.08mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid C12 at 211mm,251.54mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid C13 at 406.4mm,233.68mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid C14 at 353.46mm,234mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid C15 at 208.54mm,231mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid C16 at 353.46mm,229mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid C17 at 213.54mm,224mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid C18 at 353.46mm,224mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid C19 at 220.92mm,221mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid C20 at 353.46mm,219mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid C22 at 116.84mm,81.28mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid H1 at 269.24mm,109.22mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid J1 at 373mm,281.62mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid J2 at 430.08mm,281mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid J3 at 185.16mm,259mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid J4 at 218mm,241.08mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid J5 at 226mm,241.08mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid J6 at 429.26mm,228.6mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid J7 at 373mm,228.62mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid J8 at 127mm,205.74mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid J9 at 198.12mm,154.94mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid J10 at 154.94mm,93.98mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid J11 at 215.9mm,93.98mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid L1 at 393.62mm,295mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid L2 at 393.62mm,269mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid L3 at 393.62mm,241mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid L4 at 393.62mm,216mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Net Label \PDN at 231.52mm,195.6mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Net Label ADR at 231.52mm,205.76mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Net Label AMP_SCL at 231.14mm,193.06mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Net Label AMP_SDA at 231.52mm,190.52mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Net Label BST_A+ at 335.54mm,231mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Net Label BST_A+ at 381mm,180.34mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Net Label BST_A- at 335.54mm,229mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Net Label BST_A- at 381mm,167.64mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Net Label BST_B+ at 335.28mm,224mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Net Label BST_B+ at 381mm,154.94mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Net Label BST_B- at 335.54mm,221mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Net Label BST_B- at 381mm,142.24mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Net Label GPIO0_F\A\U\L\T\ at 231.14mm,203.2mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Net Label GPIO1_Hybrid_Pro at 231.14mm,200.66mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Net Label GPIO2_W\A\R\N\ at 231.14mm,198.12mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Net Label Left- at 408.94mm,269mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Net Label LRCLK at 231.52mm,215.92mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Net Label OUT_A+ at 335.28mm,248.92mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Net Label OUT_A- at 335.28mm,246.38mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Net Label OUT_B+ at 335.06mm,241mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Net Label OUT_B- at 335.28mm,238.76mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Net Label Right+ at 409.3mm,241mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Net Label Right- at 409.3mm,216mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Net Label SCLK at 231.52mm,213.38mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Net Label SDIN at 231.52mm,210.84mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin C1-2 at 410mm,292.08mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin C2-1 at 193mm,279.38mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin C3-1 at 206mm,279.38mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin C5-2 at 239mm,279.38mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin C6-1 at 251mm,279.38mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin C7-1 at 264mm,279.38mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin C8-2 at 178mm,279.38mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin C9-2 at 277mm,279.38mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin C10-1 at 410mm,261.92mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin C11-2 at 198mm,256.62mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin C12-1 at 211mm,256.62mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin C13-1 at 406.4mm,233.68mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin C13-2 at 406.4mm,238.76mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin C14-1 at 348.38mm,234mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin C15-1 at 213.62mm,231mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin C16-1 at 348.38mm,229mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin C17-1 at 218.62mm,224mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin C18-1 at 348.38mm,224mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin C19-2 at 218.38mm,221mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin C20-1 at 348.38mm,219mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin C21-2 at 406mm,213.08mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin C22-1 at 116.84mm,86.36mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin C22-2 at 116.84mm,78.74mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin H1-1 at 271.78mm,109.22mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin H1-2 at 271.78mm,106.68mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin J1-2 at 373mm,289.24mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin J2-2 at 425mm,283.54mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin J3-2 at 195.32mm,259mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin J6-1 at 424.18mm,228.6mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin J6-2 at 424.18mm,226.06mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin J7-2 at 373mm,236.24mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin J8-1 at 119.38mm,208.28mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin J8-2 at 134.62mm,205.74mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin J8-3 at 119.38mm,203.2mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin J9-1 at 198.12mm,144.78mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin J9-2 at 198.12mm,165.1mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin J10-1 at 147.32mm,96.52mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin J10-2 at 162.56mm,93.98mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin J10-3 at 147.32mm,91.44mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin J11-1 at 208.28mm,96.52mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin J11-2 at 223.52mm,93.98mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin J11-3 at 208.28mm,91.44mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin L1-2 at 401.24mm,295mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin L2-2 at 401.24mm,269mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin L3-2 at 401.24mm,241mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin L4-2 at 401.24mm,216mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin R1-1 at 116.84mm,210.82mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin R1-2 at 116.84mm,220.98mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin R2-1 at 144.78mm,208.28mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin R2-2 at 144.78mm,218.44mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin R3-1 at 154.94mm,208.28mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin R3-2 at 154.94mm,218.44mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin R4-1 at 165.1mm,208.28mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin R4-2 at 165.1mm,218.44mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin R5-1 at 175.26mm,208.28mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin R5-2 at 175.26mm,218.44mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin R6-1 at 116.84mm,187.96mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin R6-2 at 116.84mm,198.12mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin R7-1 at 116.84mm,101.6mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin R7-2 at 116.84mm,111.76mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin R8-1 at 139.7mm,101.6mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin R8-2 at 139.7mm,111.76mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin R9-1 at 200.66mm,101.6mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin R9-2 at 200.66mm,111.76mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin R10-1 at 139.7mm,73.66mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin R10-2 at 139.7mm,83.82mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin R11-1 at 200.66mm,73.66mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin R11-2 at 200.66mm,83.82mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin S1-1 at 104.14mm,101.6mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin S1-3 at 83.82mm,101.6mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin S1-4 at 83.82mm,96.52mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin S1-5 at 104.14mm,93.98mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin S1-6 at 83.82mm,91.44mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin TP1-1 at 142.24mm,172.72mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin TP2-1 at 142.24mm,167.64mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin TP3-1 at 142.24mm,162.56mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin TP4-1 at 142.24mm,157.48mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin TP21-1 at 388.62mm,180.34mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin TP22-1 at 388.62mm,167.64mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin TP23-1 at 388.62mm,154.94mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin TP24-1 at 388.62mm,142.24mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin U1-1 at 317.88mm,203.22mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin U1-2 at 262mm,223.54mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin U1-4 at 262mm,195.6mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin U1-5 at 262mm,193.06mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin U1-6 at 262mm,190.52mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin U1-7 at 262mm,210.84mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin U1-8 at 262mm,213.38mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin U1-9 at 262mm,215.92mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin U1-10 at 262mm,198.14mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin U1-11 at 262mm,200.68mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin U1-12 at 262mm,203.22mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin U1-13 at 262mm,205.76mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin U1-14 at 262mm,228.62mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin U1-15 at 262mm,236.24mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin U1-16 at 317.88mm,200.68mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin U1-17 at 262mm,248.94mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin U1-18 at 262mm,246.4mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin U1-19 at 317.88mm,248.94mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin U1-20 at 317.88mm,223.54mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin U1-21 at 317.88mm,198.14mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin U1-22 at 317.88mm,195.6mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin U1-23 at 317.88mm,246.4mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin U1-24 at 317.88mm,221mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin U1-25 at 317.88mm,213.38mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin U1-26 at 317.88mm,233.7mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin U1-27 at 317.88mm,193.06mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin U1-28 at 317.88mm,190.52mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin U1-29 at 317.88mm,215.92mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin U1-30 at 317.88mm,236.24mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin U1-31 at 262mm,243.86mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Pin U1-32 at 262mm,241.32mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Port \PDN at 88.9mm,139.7mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Port AMP_SCL at 88.9mm,129.54mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Port AMP_SDA at 88.9mm,134.62mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Port GPIO0_F\A\U\L\T\ at 88.9mm,154.94mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Port GPIO1_Hybrid_Pro at 88.9mm,149.86mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Port GPIO2_W\A\R\N\ at 88.9mm,144.78mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Port LRCLK at 91.44mm,248.92mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Port SCLK at 91.44mm,246.38mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Port SDIN at 91.44mm,243.84mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Power Object DVDD1 at 116.84mm,114.3mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Power Object DVDD1 at 116.84mm,223.52mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Power Object DVDD1 at 139.7mm,114.3mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Power Object DVDD1 at 144.78mm,220.98mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Power Object DVDD1 at 154.94mm,220.98mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Power Object DVDD1 at 165.1mm,220.98mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Power Object DVDD1 at 175.26mm,220.98mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Power Object DVDD1 at 200.66mm,116.84mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Power Object GND at 78.74mm,88.9mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Power Object GND at 116.84mm,73.66mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Power Object GND at 116.84mm,185.42mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Power Object GND at 139.7mm,71.12mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Power Object GND at 198.12mm,228.6mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Power Object GND at 200.66mm,71.12mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Power Object GND at 259.08mm,99.06mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Power Object GND at 330.2mm,187.96mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Power Object GND at 406.4mm,231.14mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid Power Object GND at 410mm,284.48mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid R1 at 116.84mm,215.9mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid R2 at 144.78mm,213.36mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid R3 at 154.94mm,213.36mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid R4 at 165.1mm,213.36mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid R5 at 175.26mm,213.36mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid R6 at 116.84mm,193.04mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid R7 at 116.84mm,106.68mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid R8 at 139.7mm,106.68mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid R9 at 200.66mm,106.68mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid R10 at 139.7mm,78.74mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid R11 at 200.66mm,78.74mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid S1 at 93.98mm,96.52mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid TP1 at 139.7mm,172.72mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid TP2 at 139.7mm,167.64mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid TP3 at 139.7mm,162.56mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid TP4 at 139.7mm,157.48mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid TP21 at 391.16mm,180.34mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid TP22 at 391.16mm,167.64mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid TP23 at 391.16mm,154.94mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid TP24 at 391.16mm,142.24mm
Warning | AMPS262A_TAS5830_IO.SchDoc | Off grid U1 at 262mm,248.94mm

Back to top