LMP7721 LG sim

It looks like it might be more accurate to include the feedback network in the LG simulation – also, the parasitic input C then needs to be added separately – PDS says 11pF. This drops the PM to 50deg vs the 62deg for the older method shown pasted in.

