[bookmark: _GoBack]If one does not use the technique described by TI to measure the phase margin.
Ex editing below
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Is the phase margin =134 °? 
The bode plan never cuts the 0dB the gain = -12db
The method is to set the cursor A and B remote from -3dB and measure the phase margin
Cusor A -12db Cursor B -15db report on the phase curve = 134 °
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