
**** Build of configuration Debug for project TDC7200EVM_USB ****

"C:\\ti\\ccsv6\\utils\\bin\\gmake" -k all 
'Building file: C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/host_interface.c'
'Invoking: MSP430 Compiler'
"C:/ti/ccsv6/tools/compiler/ti-cgt-msp430_4.4.3/bin/cl430" -vmspx --abi=eabi --data_model=restricted --use_hw_mpy=F5 --include_path="C:/ti/ccsv6/ccs_base/msp430/include" --include_path="C:/ti/ccsv6/tools/compiler/ti-cgt-msp430_4.4.3/include" --include_path="C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/F5xx_F6xx_Core_Lib" --include_path="C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/include" --include_path="C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/driverlib/MSP430F5xx_6xx" --include_path="C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/driverlib/MSP430F5xx_6xx/deprecated" --include_path="C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/USB_API/USB_Common" --include_path="C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/USB_config" --include_path="C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/USB_app" --include_path="C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code" --include_path="C:/ti/ccsv6/tools/compiler/ti-cgt-msp430_4.4.3/include" --advice:power=all -g --define=__MSP430F5529__ --diag_warning=225 --display_error_number --diag_wrap=off --silicon_errata=CPU21 --silicon_errata=CPU22 --silicon_errata=CPU23 --silicon_errata=CPU40 --printf_support=minimal --preproc_with_compile --preproc_dependency="host_interface.pp"  "C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/host_interface.c"
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/host_interface.c", line 259: remark #1527-D: (ULP 2.1) Detected SW delay loop using __delay_cycles. Recommend using a timer module instead
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/host_interface.c", line 264: remark #1527-D: (ULP 2.1) Detected SW delay loop using __delay_cycles. Recommend using a timer module instead
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/host_interface.c", line 326: remark #2553-D: (ULP 14.1) Array index (involving "i") of type "int". Recommend using "unsigned int"
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/host_interface.c", line 344: remark #1544-D: (ULP 13.1) Detected loop counting up. Recommend loops count down as detecting zeros is easier
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/host_interface.c", line 345: remark #2553-D: (ULP 14.1) Array index (involving "i") of type "int". Recommend using "unsigned int"
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/host_interface.c", line 409: remark #1530-D: (ULP 5.1) Detected divide operation(s). Recommend moving them to RAM during run time or not using as these are processing/power intensive
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/host_interface.c", line 433: remark #1530-D: (ULP 5.1) Detected divide operation(s). Recommend moving them to RAM during run time or not using as these are processing/power intensive
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/host_interface.c", line 439: remark #1530-D: (ULP 5.1) Detected divide operation(s). Recommend moving them to RAM during run time or not using as these are processing/power intensive
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/host_interface.c", line 445: remark #1530-D: (ULP 5.1) Detected divide operation(s). Recommend moving them to RAM during run time or not using as these are processing/power intensive
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/host_interface.c", line 448: remark #1530-D: (ULP 5.1) Detected divide operation(s). Recommend moving them to RAM during run time or not using as these are processing/power intensive
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/host_interface.c", line 523: remark #1532-D: (ULP 5.3) Detected sprintf() operation(s). Recommend moving them to RAM during run time or not using as these are processing/power intensive
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/host_interface.c", line 326: remark #2553-D: (ULP 14.1) Array index (involving "i") of type "int". Recommend using "unsigned int"
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/host_interface.c", line 344: remark #1544-D: (ULP 13.1) Detected loop counting up. Recommend loops count down as detecting zeros is easier
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/host_interface.c", line 345: remark #2553-D: (ULP 14.1) Array index (involving "i") of type "int". Recommend using "unsigned int"
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/host_interface.c", line 409 (col. 12): remark #1531-D: (ULP 5.2) Detected floating point operation(s). Recommend moving them to RAM during run time or not using as these are processing/power intensive
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/host_interface.c", line 410 (col. 18): remark #1531-D: (ULP 5.2) Detected floating point operation(s). Recommend moving them to RAM during run time or not using as these are processing/power intensive
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/host_interface.c", line 411 (col. 12): remark #1531-D: (ULP 5.2) Detected floating point operation(s). Recommend moving them to RAM during run time or not using as these are processing/power intensive
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/host_interface.c", line 412 (col. 18): remark #1531-D: (ULP 5.2) Detected floating point operation(s). Recommend moving them to RAM during run time or not using as these are processing/power intensive
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/host_interface.c", line 413 (col. 12): remark #1531-D: (ULP 5.2) Detected floating point operation(s). Recommend moving them to RAM during run time or not using as these are processing/power intensive
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/host_interface.c", line 414 (col. 19): remark #1531-D: (ULP 5.2) Detected floating point operation(s). Recommend moving them to RAM during run time or not using as these are processing/power intensive
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/host_interface.c", line 415 (col. 12): remark #1531-D: (ULP 5.2) Detected floating point operation(s). Recommend moving them to RAM during run time or not using as these are processing/power intensive
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/host_interface.c", line 416 (col. 19): remark #1531-D: (ULP 5.2) Detected floating point operation(s). Recommend moving them to RAM during run time or not using as these are processing/power intensive
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/host_interface.c", line 427 (col. 15): remark #1531-D: (ULP 5.2) Detected floating point operation(s). Recommend moving them to RAM during run time or not using as these are processing/power intensive
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/host_interface.c", line 433 (col. 15): remark #1531-D: (ULP 5.2) Detected floating point operation(s). Recommend moving them to RAM during run time or not using as these are processing/power intensive
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/host_interface.c", line 439 (col. 15): remark #1531-D: (ULP 5.2) Detected floating point operation(s). Recommend moving them to RAM during run time or not using as these are processing/power intensive
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/host_interface.c", line 445 (col. 15): remark #1531-D: (ULP 5.2) Detected floating point operation(s). Recommend moving them to RAM during run time or not using as these are processing/power intensive
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/host_interface.c", line 448 (col. 22): remark #1531-D: (ULP 5.2) Detected floating point operation(s). Recommend moving them to RAM during run time or not using as these are processing/power intensive
'Finished building: C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/host_interface.c'
' '
'Building file: C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/main.c'
'Invoking: MSP430 Compiler'
"C:/ti/ccsv6/tools/compiler/ti-cgt-msp430_4.4.3/bin/cl430" -vmspx --abi=eabi --data_model=restricted --use_hw_mpy=F5 --include_path="C:/ti/ccsv6/ccs_base/msp430/include" --include_path="C:/ti/ccsv6/tools/compiler/ti-cgt-msp430_4.4.3/include" --include_path="C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/F5xx_F6xx_Core_Lib" --include_path="C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/include" --include_path="C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/driverlib/MSP430F5xx_6xx" --include_path="C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/driverlib/MSP430F5xx_6xx/deprecated" --include_path="C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/USB_API/USB_Common" --include_path="C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/USB_config" --include_path="C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/USB_app" --include_path="C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code" --include_path="C:/ti/ccsv6/tools/compiler/ti-cgt-msp430_4.4.3/include" --advice:power=all -g --define=__MSP430F5529__ --diag_warning=225 --display_error_number --diag_wrap=off --silicon_errata=CPU21 --silicon_errata=CPU22 --silicon_errata=CPU23 --silicon_errata=CPU40 --printf_support=minimal --preproc_with_compile --preproc_dependency="main.pp"  "C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/main.c"
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/main.c", line 117: remark #1527-D: (ULP 2.1) Detected SW delay loop using __delay_cycles. Recommend using a timer module instead
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/main.c", line 274: remark #1544-D: (ULP 13.1) Detected loop counting up. Recommend loops count down as detecting zeros is easier
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/main.c", line 245: remark #1535-D: (ULP 8.1) variable "receive_error" is used as a constant. Recommend declaring variable as either 'static const' or 'const'
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/main.c", line 363: remark #1527-D: (ULP 2.1) Detected SW delay loop using __delay_cycles. Recommend using a timer module instead
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/main.c", line 383: remark #1527-D: (ULP 2.1) Detected SW delay loop using __delay_cycles. Recommend using a timer module instead
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/main.c", line 392: remark #1527-D: (ULP 2.1) Detected SW delay loop using __delay_cycles. Recommend using a timer module instead
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/main.c", line 405: remark #1527-D: (ULP 2.1) Detected SW delay loop using __delay_cycles. Recommend using a timer module instead
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/main.c", line 436: remark #1538-D: (ULP 10.1) ISR UNMI_ISR calls function USB_disable. Recommend moving function call away from ISR, or inlining the function, or using pragmas
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/main.c", line 87: remark #1535-D: (ULP 8.1) variable "cmdResponseString" is used as a constant. Recommend declaring variable as either 'static const' or 'const'
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/main.c", line 89: remark #1535-D: (ULP 8.1) variable "tof_graph_state" is used as a constant. Recommend declaring variable as either 'static const' or 'const'
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/main.c", line 90: remark #1535-D: (ULP 8.1) variable "graph_delay_sweep_state" is used as a constant. Recommend declaring variable as either 'static const' or 'const'
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/main.c", line 91: remark #1535-D: (ULP 8.1) variable "double_resolution" is used as a constant. Recommend declaring variable as either 'static const' or 'const'
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/main.c", line 92: remark #1535-D: (ULP 8.1) variable "current_tdc" is used as a constant. Recommend declaring variable as either 'static const' or 'const'
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/main.c", line 93: remark #1535-D: (ULP 8.1) variable "TDC720xEVM_Device" is used as a constant. Recommend declaring variable as either 'static const' or 'const'
'Finished building: C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo2_tdc720x_usb/main.c'
' '
'Building target: TDC7200EVM_USB.out'
'Invoking: MSP430 Linker'
"C:/ti/ccsv6/tools/compiler/ti-cgt-msp430_4.4.3/bin/cl430" -vmspx --abi=eabi --data_model=restricted --use_hw_mpy=F5 --advice:power=all -g --define=__MSP430F5529__ --diag_warning=225 --display_error_number --diag_wrap=off --silicon_errata=CPU21 --silicon_errata=CPU22 --silicon_errata=CPU23 --silicon_errata=CPU40 --printf_support=minimal -z -m"TDC7200EVM_USB.map" --heap_size=160 --stack_size=160 --cinit_hold_wdt=on -i"C:/ti/ccsv6/ccs_base/msp430/include" -i"C:/ti/ccsv6/tools/compiler/ti-cgt-msp430_4.4.3/lib" -i"C:/ti/ccsv6/tools/compiler/ti-cgt-msp430_4.4.3/include" -i"C:/ti/ccsv6/ccs_base/msp430/lib/5xx_6xx_FRxx" --reread_libs --warn_sections --display_error_number --diag_wrap=off --xml_link_info="TDC7200EVM_USB_linkInfo.xml" --use_hw_mpy=F5 --rom_model -o "TDC7200EVM_USB.out" "./TI_MSP430_spi_USCIB0_5xx.obj" "./host_interface.obj" "./main.obj" "./tdc720x_calculation.obj" "./tdc720x_measurement_control.obj" "./tdc720x_mode1_lt12ns.obj" "./timer_queue.obj" "./uart_commn.obj" "./driverlib/MSP430F5xx_6xx/adc10_a.obj" "./driverlib/MSP430F5xx_6xx/adc12_a.obj" "./driverlib/MSP430F5xx_6xx/aes.obj" "./driverlib/MSP430F5xx_6xx/battbak.obj" "./driverlib/MSP430F5xx_6xx/comp_b.obj" "./driverlib/MSP430F5xx_6xx/crc.obj" "./driverlib/MSP430F5xx_6xx/dac12_a.obj" "./driverlib/MSP430F5xx_6xx/dma.obj" "./driverlib/MSP430F5xx_6xx/eusci_a_spi.obj" "./driverlib/MSP430F5xx_6xx/eusci_a_uart.obj" "./driverlib/MSP430F5xx_6xx/eusci_b_i2c.obj" "./driverlib/MSP430F5xx_6xx/eusci_b_spi.obj" "./driverlib/MSP430F5xx_6xx/flashctl.obj" "./driverlib/MSP430F5xx_6xx/gpio.obj" "./driverlib/MSP430F5xx_6xx/ldopwr.obj" "./driverlib/MSP430F5xx_6xx/mpy32.obj" "./driverlib/MSP430F5xx_6xx/pmap.obj" "./driverlib/MSP430F5xx_6xx/pmm.obj" "./driverlib/MSP430F5xx_6xx/ram.obj" "./driverlib/MSP430F5xx_6xx/ref.obj" "./driverlib/MSP430F5xx_6xx/rtc_a.obj" "./driverlib/MSP430F5xx_6xx/rtc_b.obj" "./driverlib/MSP430F5xx_6xx/rtc_c.obj" "./driverlib/MSP430F5xx_6xx/sd24_b.obj" "./driverlib/MSP430F5xx_6xx/sfr.obj" "./driverlib/MSP430F5xx_6xx/sysctl.obj" "./driverlib/MSP430F5xx_6xx/tec.obj" "./driverlib/MSP430F5xx_6xx/timer_a.obj" "./driverlib/MSP430F5xx_6xx/timer_b.obj" "./driverlib/MSP430F5xx_6xx/timer_d.obj" "./driverlib/MSP430F5xx_6xx/tlv.obj" "./driverlib/MSP430F5xx_6xx/ucs.obj" "./driverlib/MSP430F5xx_6xx/usci_a_spi.obj" "./driverlib/MSP430F5xx_6xx/usci_a_uart.obj" "./driverlib/MSP430F5xx_6xx/usci_b_i2c.obj" "./driverlib/MSP430F5xx_6xx/usci_b_spi.obj" "./driverlib/MSP430F5xx_6xx/wdt_a.obj" "./USB_config/UsbIsr.obj" "./USB_config/descriptors.obj" "./USB_app/usbConstructs.obj" "./USB_app/usbEventHandling.obj" "./USB_API/USB_PHDC_API/UsbPHDC.obj" "./USB_API/USB_MSC_API/UsbMscReq.obj" "./USB_API/USB_MSC_API/UsbMscScsi.obj" "./USB_API/USB_MSC_API/UsbMscStateMachine.obj" "./USB_API/USB_HID_API/UsbHid.obj" "./USB_API/USB_HID_API/UsbHidReq.obj" "./USB_API/USB_Common/usb.obj" "./USB_API/USB_Common/usbdma.obj" "./USB_API/USB_CDC_API/UsbCdc.obj" "./F5xx_F6xx_Core_Lib/HAL_FLASH.obj" "./F5xx_F6xx_Core_Lib/HAL_PMAP.obj" "./F5xx_F6xx_Core_Lib/HAL_PMM.obj" "./F5xx_F6xx_Core_Lib/HAL_TLV.obj" "./F5xx_F6xx_Core_Lib/HAL_UCS.obj" "../lnk_msp430f5529.cmd" "C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/USB_API/msp430USB.cmd"  -l"libmath.a" -l"libc.a" 
<Linking>
remark #10372-D: (ULP 4.1) Detected uninitialized Port D in this project. Recommend initializing all unused ports to eliminate wasted current consumption on unused pins.
'Finished building target: TDC7200EVM_USB.out'
' '
'Invoking: MSP430 Hex Utility'
"C:/ti/ccsv6/tools/compiler/ti-cgt-msp430_4.4.3/bin/hex430" --memwidth=8 --romwidth=8 --ti_txt -o "TDC7200EVM_USB.txt"  "TDC7200EVM_USB.out" 
Translating to TI-TXT format...
   "TDC7200EVM_USB.out" .text:_isr ==> .text:_isr
   "TDC7200EVM_USB.out" .const ==> .const
   "TDC7200EVM_USB.out" .cinit ==> .cinit
   "TDC7200EVM_USB.out" RTC ==> RTC
   "TDC7200EVM_USB.out" PORT2 ==> PORT2
   "TDC7200EVM_USB.out" TIMER2_A1 ==> TIMER2_A1
   "TDC7200EVM_USB.out" TIMER2_A0 ==> TIMER2_A0
   "TDC7200EVM_USB.out" USCI_B1 ==> USCI_B1
   "TDC7200EVM_USB.out" USCI_A1 ==> USCI_A1
   "TDC7200EVM_USB.out" PORT1 ==> PORT1
   "TDC7200EVM_USB.out" TIMER1_A1 ==> TIMER1_A1
   "TDC7200EVM_USB.out" TIMER1_A0 ==> TIMER1_A0
   "TDC7200EVM_USB.out" DMA ==> DMA
   "TDC7200EVM_USB.out" USB_UBM ==> USB_UBM
   "TDC7200EVM_USB.out" TIMER0_A1 ==> TIMER0_A1
   "TDC7200EVM_USB.out" TIMER0_A0 ==> TIMER0_A0
   "TDC7200EVM_USB.out" ADC12 ==> ADC12
   "TDC7200EVM_USB.out" USCI_B0 ==> USCI_B0
   "TDC7200EVM_USB.out" USCI_A0 ==> USCI_A0
   "TDC7200EVM_USB.out" WDT ==> WDT
   "TDC7200EVM_USB.out" TIMER0_B1 ==> TIMER0_B1
   "TDC7200EVM_USB.out" TIMER0_B0 ==> TIMER0_B0
   "TDC7200EVM_USB.out" COMP_B ==> COMP_B
   "TDC7200EVM_USB.out" UNMI ==> UNMI
   "TDC7200EVM_USB.out" SYSNMI ==> SYSNMI
   "TDC7200EVM_USB.out" .reset ==> .reset
   "TDC7200EVM_USB.out" .text ==> .text
'Finished building: TDC7200EVM_USB.txt'
' '

**** Build Finished ****
