[Stack]
FillEnabled=0
OverflowWarningsEnabled=1
WarningThreshold=90
SpWarningsEnabled=1
WarnLogOnly=1
UseTrigger=1
TriggerName=main
LimitSize=0
ByteLimit=50
[EEM State Storage]
Buffer=BAAAAAAAAAAAAAAAAAAAAAAA
[EEM Sequencer]
Buffer=AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA
[EEM Cycle Counter 0]
Counter0=AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA
[EEM Cycle Counter 1]
Counter1=AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA
[DebugChecksum]
Checksum=-691788216
[CallStack]
ShowArgs=0
[Disassembly]
MixedMode=1
[DataSample]
LogEnabled=0
GraphEnabled=0
ShowTimeLog=1
ShowTimeSum=1
[Log file]
LoggingEnabled=_ 0
LogFile=_ ""
Category=_ 0
[TermIOLog]
LoggingEnabled=_ 0
LogFile=_ ""
[Breakpoints]
Bp0=_ "STD_CODE" "{$PROJ_DIR$\code\demo_apps\demo2_tdc720x_usb\host_interface.c}.583.9" 0 0 0 0 "" 0 ""
Bp1=_ "STD_CODE" "{$PROJ_DIR$\code\demo_apps\demo2_tdc720x_usb\host_interface.c}.591.9" 0 0 0 0 "" 0 ""
Count=2
[FET]
Clock mode=46
Extended Clock mode=1
Secure Password=
Extended Clock Control Enable=1
Advanced Extended Clock Control=0
Emulation mode=0
Free running=0
Shutting Down=3
[Memory Dump]
Start address=
Lenghth=
Address info=0
Format=0
Dump registers=0
PC=0
SP=0
SR=0
all registers=0
File name=
[Aliases]
Count=0
SuppressDialog=0
