

|  |  |  |
| --- | --- | --- |
| Manufacturer P/N | Designator | Description |
| C0805C103K1RACTU | C1, C2, C8, C9 | CAPACITOR, CERAMIC X7R, 0.01uF, 100V, 10%, SMT 0805 (2012 METRIC) |
| 22201C106MAT2A | C3, C4, C6, C7 | CAPACITOR, CERAMIC X7R, 10uF, 100V, 20%, SMT 2220 (5750 METRIC) |
| C1608NP02A220J080AA | C5 | CAPACITOR, CERAMIC COG, 22pF, 100V, 5%, SMT 0603 (1608 METRIC) |
| ES3BB-13F | D1, D2 | DIODE, SCHOTTKY |
| 15-270-2-05 | P1, P2, P3, P4, P5, P6, P7 | TERMINAL, TURRET, BRASS (ASTM B16), TIN-LEAD OVER COPPER FINISH, 0.112" DIA MTG |
| ERJ-6ENF4991V | R1 | RESISTOR, CHIP, 4.99K, 1%, 125mW, 100ppm, SMT 0805 (2012 METRIC) |
| D55342E07B10B0R | R2, R3 | RESISTOR, CHIP, 10K, 0.1%, 250mW, 25ppm, 0.01% F.R., SMT 1206 |
| WSL2512R4000FEA | R4 | RESISTOR, 400 mohm, 1W, 5% |
| OPA541AP | U1 | IC, OP-AMP, POWER, GP 1.6MHZ, THRU-HOLE TO-220-11 |