
Input frequency 100 KHz, 0.8V peak to peak

No load



Load of 0.5 ohm

