**Updating boards already in customer hands follows this procedure**

1. Extract “TPLD1.0.0 BSL Batch File.zip”
2. Enter device Bootloader mode (Command b)
	1. Download puTTY
	2. Open the correct Serial/COM port
	3. Enter & ensure programmer communication
	4. Enter b
3. Unplug -> Plug in programmer
4. Indicate to click on the .bat file
5. Unplug -> Plug in programmer
6. Operation is 
	1. Open the correct Serial/COM port
	2. Enter # ensure programmer communication
	3. Observe correct version