





This is how the model gets instantiated into LTspice. The default values of the timing components are: C\_ext = 0.001uF & R\_ext = 1000 Ohms.







Cursors on the “V\_output” signal show a pulse width of about 87.3us (2V supply).



Cursors on the “V\_output” signal show a pulse width of about 86.8us (5V supply).