# README

### SysConfig Notice

All examples will soon be supported by SysConfig, a tool that will help you graphically configure your software components. A preview is available today in the examples/syscfg_preview directory. Starting in 3Q 2019, with SDK version 3.30, only SysConfig-enabled versions of examples will be provided. For more information, click here.

# empty

## Example Summary

This example is intended to be a starting point for new development where a fuller set of kernel features and debug capabilities are enabled.

## Peripherals Exercised

- `Board_GPIO_LED0` - LED0

## Resources & Jumper Settings

> If you’re using an IDE (such as CCS or IAR), please refer to Board.html in your project directory for resources used and board-specific jumper settings. Otherwise, you can find Board.html in the directory <SDK_INSTALL_DIR>/source/ti/boards/<BOARD>.

## Example Usage

- The example lights `Board_GPIO_LED0` as part of the initialization in the `mainThread()`. This thread then toggles the LED at a 1 second rate.

## Application Design Details

TI-RTOS:

- When building in Code Composer Studio, the kernel configuration project will be imported along with the example. The kernel configuration project is referenced by the example, so it will be built first. The “release” kernel configuration is the default project used. It has many debug features disabled. These feature include assert checking, logging and runtime stack checks. For a detailed difference between the “release” and “debug” kernel configurations and how to switch between them, please refer to the SimpleLink MCU SDK User’s Guide. The “release” and “debug” kernel configuration projects can be found under <SDK_INSTALL_DIR>/kernel/tirtos/builds/<BOARD>/(release|debug)/(ccs|gcc).

FreeRTOS:

- Please view the `FreeRTOSConfig.h` header file for example configuration information.