TI routine：[EasyLink Network Processor example](https://dev.ti.com/tirex/explore/content/simplelink_academy_cc13x0sdk_4_20_00_00/modules/prop_rf/prop_03_easylink_nwp/prop_03_easylink_nwp.html%22%20%5Ct%20%22_blank) Task5

Now, as long as the transmission and reception are set to less than 39 packets, the reception is OK. I don't know why?

The screenshot below shows that both transmit and receive are set to 35 packets.



