#

## Example Summary

This example is intended to be a starting point for new development.

## Peripherals & Pin Assignments

When this project is built, the SysConfig tool will generate the TI-Driver configurations into the ti_drivers_config.c and ti_drivers_config.h files. Information on pins and resources used is present in both generated files. Additionally, the System Configuration file (*.syscfg) present in the project may be opened with SysConfig’s graphical user interface to determine pins and resources used.

- `CONFIG_GPIO_LED_0`

## BoosterPacks, Board Resources & Jumper Settings

For board specific jumper settings, resources and BoosterPack modifications, refer to the Board.html file.

> If you’re using an IDE such as Code Composer Studio (CCS) or IAR, please refer to Board.html in your project directory for resources used and board-specific jumper settings.

The Board.html can also be found in your SDK installation:

    <SDK_INSTALL_DIR>/source/ti/boards/<BOARD>

## Example Usage

- The example lights `CONFIG_GPIO_LED_0` as part of the initialization in the `mainThread()`. This thread then toggles the LED at a 1 second rate.

## Application Design Details

FreeRTOS:

- Please view the `FreeRTOSConfig.h` header file for example configuration information.