#

# SimpleLink™ CC2652RSIP LaunchPad™ Settings & Resources

The [SimpleLink CC2652RSIP LaunchPad][launchpad] contains a [CC2652R1FSIP][device] device.

## Jumper Settings

- Close the `LEDs` jumper to enable the on-board LEDs.
- Close the `RXD<<` and `TXD>>` jumpers to enable UART via the XDS110 on-board USB debugger.

## SysConfig Board File

The LP_CC2652RSIP.syscfg.json is a handcrafted file used by SysConfig. It describes the physical pin-out and components on the LaunchPad.

## Driver Examples Resources

Examples utilize SysConfig to generate software configurations into the ti_drivers_config.c and ti_drivers_config.h files. The SysConfig user interface can be utilized to determine pins and resources used. Information on pins and resources used is also present in both generated files.

## TI BoosterPacks™

The following BoosterPack(s) are used with some driver examples.

#### BOOSTXL-SHARP128 LCD & SD Card BoosterPack

- No modifications are needed.

#### BP-BASSENSORSMKII BoosterPack

- No modifications are needed.

#### CC3200 Audio BoosterPack

- No modifications are needed.