# Static Call Graph for image .\Objects\Lab6.axf

#<CALLGRAPH># ARM Linker, 5060300: Last Updated: Fri Jan 13 19:34:25 2017

### Maximum Stack Usage = 32 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

__rt_entry_main ⇒ main ⇒ OutValue ⇒ UART0_OutUHex ⇒ UART0_OutUHex (Cycle)

### Functions with no stack information

- SysTick_Handler
- StartOS

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- SVC_Handler ⇒ SVC_Handler
- DebugMon_Handler ⇒ DebugMon_Handler
- PendSV_Handler ⇒ PendSV_Handler
- ADC14_IRQHandler ⇒ ADC14_IRQHandler
- UART0_OutUHex ⇒ UART0_OutUHex

  ### Function Pointers

  - ADC14_IRQHandler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - AES256_IRQHandler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - BusFault_Handler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - COMP_E0_IRQHandler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - COMP_E1_IRQHandler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - CS_IRQHandler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - DMA_ERR_IRQHandler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - DMA_INT0_IRQHandler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - DMA_INT1_IRQHandler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - DMA_INT2_IRQHandler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - DMA_INT3_IRQHandler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - DebugMon_Handler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - EUSCIA0_IRQHandler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - EUSCIA1_IRQHandler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - EUSCIA2_IRQHandler from uart1.o(i.EUSCIA2_IRQHandler) referenced from startup_msp432p401r_uvision.o(RESET)
  - EUSCIA3_IRQHandler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - EUSCIB0_IRQHandler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - EUSCIB1_IRQHandler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - EUSCIB2_IRQHandler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - EUSCIB3_IRQHandler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - FLCTL_IRQHandler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - FPU_IRQHandler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - HardFault_Handler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - MemManage_Handler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - NMI_Handler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - PCM_IRQHandler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - PORT1_IRQHandler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - PORT2_IRQHandler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - PORT3_IRQHandler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - PORT4_IRQHandler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - PORT5_IRQHandler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - PORT6_IRQHandler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - PSS_IRQHandler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - PendSV_Handler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - RTC_C_IRQHandler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - Reset_Handler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - SVC_Handler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - SysTick_Handler from osasm.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - SystemInit from system_msp432p401r.o(i.SystemInit) referenced from startup_msp432p401r_uvision.o(.text)
  - T32_INT1_IRQHandler from bsp.o(i.T32_INT1_IRQHandler) referenced from startup_msp432p401r_uvision.o(RESET)
  - T32_INT2_IRQHandler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - T32_INTC_IRQHandler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - TA0_0_IRQHandler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - TA0_N_IRQHandler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - TA1_0_IRQHandler from bsp.o(i.TA1_0_IRQHandler) referenced from startup_msp432p401r_uvision.o(RESET)
  - TA1_N_IRQHandler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - TA2_0_IRQHandler from bsp.o(i.TA2_0_IRQHandler) referenced from startup_msp432p401r_uvision.o(RESET)
  - TA2_N_IRQHandler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - TA3_0_IRQHandler from texas.o(i.TA3_0_IRQHandler) referenced from startup_msp432p401r_uvision.o(RESET)
  - TA3_N_IRQHandler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - UsageFault_Handler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - WDT_A_IRQHandler from startup_msp432p401r_uvision.o(.text) referenced from startup_msp432p401r_uvision.o(RESET)
  - __main from __main.o(!!!main) referenced from startup_msp432p401r_uvision.o(.text)

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __scatterload
  - >> __rt_entry

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 44 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_copy (Thumb, 26 bytes, Stack size unknown bytes, __scatter_copy.o(!!handler_copy), UNUSED)
  [Calls]

  - >> __scatterload_copy
  [Called By]
  - >> __scatterload_copy

  __scatterload_zeroinit (Thumb, 28 bytes, Stack size unknown bytes, __scatter_zi.o(!!handler_zi), UNUSED)

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Called By]

  - >> __rt_entry_li

  __rt_lib_init_fp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000001))
  [Calls]

  - >> _fp_init

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002C))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000032))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000030))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000023))

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000A))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000011))

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_preinit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000004))

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000E))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000033))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000025))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000C))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls

  __rt_lib_shutdown_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000002))

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000007))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000010))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000A))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000004))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000C))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, __rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __scatterload_rt2
  - >> __main

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, __rtentry4.o(.ARM.Collect$$rtentry$$00000004))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_sh ⇒ __user_setup_stackheap
  [Calls]
  - >> __user_setup_stackheap

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Calls]

  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Stack]

  - Max Depth = 32 + Unknown Stack Size
  - Call Chain = __rt_entry_main ⇒ main ⇒ OutValue ⇒ UART0_OutUHex ⇒ UART0_OutUHex (Cycle)
  [Calls]
  - >> main
  - >> exit

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000C))

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  DisableInterrupts (Thumb, 4 bytes, Stack size 0 bytes, cortexm.o(.emb_text))
  [Called By]

  - >> OS_Init

  EnableInterrupts (Thumb, 4 bytes, Stack size 0 bytes, cortexm.o(.emb_text), UNUSED)

  StartCritical (Thumb, 8 bytes, Stack size 0 bytes, cortexm.o(.emb_text), UNUSED)

  EndCritical (Thumb, 6 bytes, Stack size 0 bytes, cortexm.o(.emb_text), UNUSED)

  WaitForInterrupt (Thumb, 4 bytes, Stack size 0 bytes, cortexm.o(.emb_text), UNUSED)

  delay (Thumb, 6 bytes, Stack size 0 bytes, cortexm.o(.emb_text), UNUSED)
  [Calls]

  - >> delay
  [Called By]
  - >> delay

  SysTick_Handler (Thumb, 0 bytes, Stack size unknown bytes, osasm.o(.text))
  [Calls]

  - >> Scheduler
  [Address Reference Count : 1]
  - startup_msp432p401r_uvision.o(RESET)

  StartOS (Thumb, 0 bytes, Stack size unknown bytes, osasm.o(.text), UNUSED)

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - startup_msp432p401r_uvision.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_msp432p401r_uvision.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_msp432p401r_uvision.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_msp432p401r_uvision.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_msp432p401r_uvision.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - startup_msp432p401r_uvision.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Calls]

  - >> DebugMon_Handler
  [Called By]
  - >> DebugMon_Handler
  [Address Reference Count : 1]
  - startup_msp432p401r_uvision.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - startup_msp432p401r_uvision.o(RESET)

  ADC14_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Calls]

  - >> ADC14_IRQHandler
  [Called By]
  - >> ADC14_IRQHandler
  [Address Reference Count : 1]
  - startup_msp432p401r_uvision.o(RESET)

  AES256_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Address Reference Count : 1]

  - startup_msp432p401r_uvision.o(RESET)

  COMP_E0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Address Reference Count : 1]

  - startup_msp432p401r_uvision.o(RESET)

  COMP_E1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Address Reference Count : 1]

  - startup_msp432p401r_uvision.o(RESET)

  CS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Address Reference Count : 1]

  - startup_msp432p401r_uvision.o(RESET)

  DMA_ERR_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Address Reference Count : 1]

  - startup_msp432p401r_uvision.o(RESET)

  DMA_INT0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Address Reference Count : 1]

  - startup_msp432p401r_uvision.o(RESET)

  DMA_INT1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Address Reference Count : 1]

  - startup_msp432p401r_uvision.o(RESET)

  DMA_INT2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Address Reference Count : 1]

  - startup_msp432p401r_uvision.o(RESET)

  DMA_INT3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Address Reference Count : 1]

  - startup_msp432p401r_uvision.o(RESET)

  EUSCIA0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Address Reference Count : 1]

  - startup_msp432p401r_uvision.o(RESET)

  EUSCIA1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Address Reference Count : 1]

  - startup_msp432p401r_uvision.o(RESET)

  EUSCIA3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Address Reference Count : 1]

  - startup_msp432p401r_uvision.o(RESET)

  EUSCIB0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Address Reference Count : 1]

  - startup_msp432p401r_uvision.o(RESET)

  EUSCIB1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Address Reference Count : 1]

  - startup_msp432p401r_uvision.o(RESET)

  EUSCIB2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Address Reference Count : 1]

  - startup_msp432p401r_uvision.o(RESET)

  EUSCIB3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Address Reference Count : 1]

  - startup_msp432p401r_uvision.o(RESET)

  FLCTL_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Address Reference Count : 1]

  - startup_msp432p401r_uvision.o(RESET)

  FPU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Address Reference Count : 1]

  - startup_msp432p401r_uvision.o(RESET)

  PCM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Address Reference Count : 1]

  - startup_msp432p401r_uvision.o(RESET)

  PORT1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Address Reference Count : 1]

  - startup_msp432p401r_uvision.o(RESET)

  PORT2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Address Reference Count : 1]

  - startup_msp432p401r_uvision.o(RESET)

  PORT3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Address Reference Count : 1]

  - startup_msp432p401r_uvision.o(RESET)

  PORT4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Address Reference Count : 1]

  - startup_msp432p401r_uvision.o(RESET)

  PORT5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Address Reference Count : 1]

  - startup_msp432p401r_uvision.o(RESET)

  PORT6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Address Reference Count : 1]

  - startup_msp432p401r_uvision.o(RESET)

  PSS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Address Reference Count : 1]

  - startup_msp432p401r_uvision.o(RESET)

  RTC_C_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Address Reference Count : 1]

  - startup_msp432p401r_uvision.o(RESET)

  T32_INT2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Address Reference Count : 1]

  - startup_msp432p401r_uvision.o(RESET)

  T32_INTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Address Reference Count : 1]

  - startup_msp432p401r_uvision.o(RESET)

  TA0_0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Address Reference Count : 1]

  - startup_msp432p401r_uvision.o(RESET)

  TA0_N_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Address Reference Count : 1]

  - startup_msp432p401r_uvision.o(RESET)

  TA1_N_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Address Reference Count : 1]

  - startup_msp432p401r_uvision.o(RESET)

  TA2_N_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Address Reference Count : 1]

  - startup_msp432p401r_uvision.o(RESET)

  TA3_N_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Address Reference Count : 1]

  - startup_msp432p401r_uvision.o(RESET)

  WDT_A_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Address Reference Count : 1]

  - startup_msp432p401r_uvision.o(RESET)

  __user_initial_stackheap (Thumb, 10 bytes, Stack size 0 bytes, startup_msp432p401r_uvision.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_escrow$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_expand$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __user_setup_stackheap (Thumb, 74 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_perproc_libspace
  - >> __user_initial_stackheap
  [Called By]
  - >> __rt_entry_sh

  exit (Thumb, 18 bytes, Stack size 8 bytes, exit.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = exit
  [Calls]
  - >> __rt_exit
  [Called By]
  - >> __rt_entry_main

  __user_libspace (Thumb, 8 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __user_perthread_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  _sys_exit (Thumb, 8 bytes, Stack size 0 bytes, sys_exit.o(.text))
  [Called By]

  - >> __rt_exit_exit

  __I$use$semihosting (Thumb, 0 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __use_no_semihosting_swi (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __semihosting_library_function (Thumb, 0 bytes, Stack size unknown bytes, indicate_semi.o(.text), UNUSED)

  BSP_Clock_InitFastest (Thumb, 328 bytes, Stack size 0 bytes, bsp.o(i.BSP_Clock_InitFastest))
  [Called By]

  - >> OS_Init

  EUSCIA2_IRQHandler (Thumb, 26 bytes, Stack size 4 bytes, uart1.o(i.EUSCIA2_IRQHandler))
  [Stack]

  - Max Depth = 4
  - Call Chain = EUSCIA2_IRQHandler
  [Calls]
  - >> RxFifo_Put
  [Address Reference Count : 1]
  - startup_msp432p401r_uvision.o(RESET)

  OS_Init (Thumb, 12 bytes, Stack size 8 bytes, os.o(i.OS_Init))
  [Stack]

  - Max Depth = 8
  - Call Chain = OS_Init
  [Calls]
  - >> DisableInterrupts
  - >> BSP_Clock_InitFastest
  [Called By]
  - >> main

  OutValue (Thumb, 20 bytes, Stack size 16 bytes, lab6.o(i.OutValue))
  [Stack]

  - Max Depth = 24
  - Call Chain = OutValue ⇒ UART0_OutUHex ⇒ UART0_OutUHex (Cycle)
  [Calls]
  - >> UART0_OutUHex
  - >> UART0_OutString
  [Called By]
  - >> main

  RxFifo_Put (Thumb, 56 bytes, Stack size 0 bytes, uart1.o(i.RxFifo_Put))
  [Called By]

  - >> EUSCIA2_IRQHandler

  Scheduler (Thumb, 44 bytes, Stack size 0 bytes, os.o(i.Scheduler))
  [Called By]

  - >> SysTick_Handler

  SystemInit (Thumb, 74 bytes, Stack size 0 bytes, system_msp432p401r.o(i.SystemInit))
  [Address Reference Count : 1]

  - startup_msp432p401r_uvision.o(.text)

  T32_INT1_IRQHandler (Thumb, 16 bytes, Stack size 8 bytes, bsp.o(i.T32_INT1_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = T32_INT1_IRQHandler
  [Address Reference Count : 1]
  - startup_msp432p401r_uvision.o(RESET)

  TA1_0_IRQHandler (Thumb, 22 bytes, Stack size 8 bytes, bsp.o(i.TA1_0_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = TA1_0_IRQHandler
  [Address Reference Count : 1]
  - startup_msp432p401r_uvision.o(RESET)

  TA2_0_IRQHandler (Thumb, 22 bytes, Stack size 8 bytes, bsp.o(i.TA2_0_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = TA2_0_IRQHandler
  [Address Reference Count : 1]
  - startup_msp432p401r_uvision.o(RESET)

  TA3_0_IRQHandler (Thumb, 22 bytes, Stack size 8 bytes, texas.o(i.TA3_0_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = TA3_0_IRQHandler
  [Address Reference Count : 1]
  - startup_msp432p401r_uvision.o(RESET)

  UART0_Init (Thumb, 76 bytes, Stack size 0 bytes, uart0.o(i.UART0_Init))
  [Called By]

  - >> main

  UART0_OutChar (Thumb, 20 bytes, Stack size 0 bytes, uart0.o(i.UART0_OutChar))
  [Called By]

  - >> UART0_OutUHex
  - >> UART0_OutString

  UART0_OutString (Thumb, 24 bytes, Stack size 4 bytes, uart0.o(i.UART0_OutString))
  [Stack]

  - Max Depth = 4
  - Call Chain = UART0_OutString
  [Calls]
  - >> UART0_OutChar
  [Called By]
  - >> OutValue

  UART0_OutUHex (Thumb, 52 bytes, Stack size 8 bytes, uart0.o(i.UART0_OutUHex))
  [Stack]

  - Max Depth = 8 + In Cycle
  - Call Chain = UART0_OutUHex ⇒ UART0_OutUHex (Cycle)
  [Calls]
  - >> UART0_OutChar
  - >> UART0_OutUHex
  [Called By]
  - >> UART0_OutUHex
  - >> OutValue

  WDT_A_holdTimer (Thumb, 18 bytes, Stack size 0 bytes, wdt_a.o(i.WDT_A_holdTimer))
  [Called By]

  - >> main

  main (Thumb, 26 bytes, Stack size 8 bytes, lab6.o(i.main))
  [Stack]

  - Max Depth = 32
  - Call Chain = main ⇒ OutValue ⇒ UART0_OutUHex ⇒ UART0_OutUHex (Cycle)
  [Calls]
  - >> WDT_A_holdTimer
  - >> UART0_Init
  - >> OutValue
  - >> OS_Init
  [Called By]
  - >> __rt_entry_main

  _fp_init (Thumb, 10 bytes, Stack size 0 bytes, fpinit.o(x$fpl$fpinit))
  [Called By]

  - >> __rt_lib_init_fp_1

  __fplib_config_fpu_vfp (Thumb, 0 bytes, Stack size unknown bytes, fpinit.o(x$fpl$fpinit), UNUSED)

  __fplib_config_pureend_doubles (Thumb, 0 bytes, Stack size unknown bytes, fpinit.o(x$fpl$fpinit), UNUSED)

  ### Local Symbols

  ### Undefined Global Symbols