
- GPIOB:
	+ Standard Output: PB27
	+ Standard Output: PB26
	+ Standard Output: PB25
	+ Standard Output: PB19
- SYSCTL:
	+ HFXIN: PA5
	+ HFXOUT: PA6
- TIMA0
- ADC1:
	+ ADC12 Channel 0 Pin: PA15
	+ ADC12 Channel 1 Pin: PA16
	+ ADC12 Channel 2 Pin: PA17
	+ ADC12 Channel 4 Pin: PB17
	+ ADC12 Channel 5 Pin: PB18
- ADC0:
	+ ADC12 Channel 12 Pin: PA14
	+ ADC12 Channel 1 Pin: PA26
	+ ADC12 Channel 0 Pin: PA27
- EVENT
- SYSTICK
- WWDT0
- CANFD0:
	+ RX Pin: PA13
	+ TX Pin: PA12
- CANFD1:
	+ RX Pin: PB22
	+ TX Pin: PB21
- BOARD:
	+ Debug Clock: PA20
	+ Debug Data In Out: PA19
