MSP430™CapTIvateSoftwareLibraryAPIGuide 1_70_00_03

Data Fields
tParameterPacket Union Reference
CAPT_Protocol

`#include <CAPT_Protocol.h>`

## Data Fields
struct {
uint8_t ui8Sync
uint8_t ui8Blank
uint8_t ui8Length
uint8_t ui8Command
uint8_t ui8Write
uint8_t ui8SensorID
uint8_t ui8Param0
uint8_t ui8Param1
uint8_t ui8Param2
uint8_t ui8Param3
uint16_t ui16Checksum
}; |
uint8_t | ui8Packet [TL_PARAMETER_PACKET_LENGTH]

## Detailed Description

typedef tParameterPacket is a union structure that stores a CapTIvate™ parameter packet. The union allows the low-level serial driver to interface with a buffer, while higher-level applications can access specific portions of the packet.

## Field Documentation

## § ui8Sync

uint8_t tParameterPacket::ui8Sync

## § ui8Blank

uint8_t tParameterPacket::ui8Blank

## § ui8Length

uint8_t tParameterPacket::ui8Length

## § ui8Command

uint8_t tParameterPacket::ui8Command

## § ui8Write

uint8_t tParameterPacket::ui8Write

## § ui8SensorID

uint8_t tParameterPacket::ui8SensorID

## § ui8Param0

uint8_t tParameterPacket::ui8Param0

## § ui8Param1

uint8_t tParameterPacket::ui8Param1

## § ui8Param2

uint8_t tParameterPacket::ui8Param2

## § ui8Param3

uint8_t tParameterPacket::ui8Param3

## § ui16Checksum

uint16_t tParameterPacket::ui16Checksum

## § @13

struct { ... }

## § ui8Packet

uint8_t tParameterPacket::ui8Packet[TL_PARAMETER_PACKET_LENGTH]

The documentation for this union was generated from the following file:

- CAPT_Protocol.h

© Copyright 1995-2018, Texas Instruments Incorporated. All rights reserved.
Trademarks | Privacy policy | Terms of use | Terms of sale