MSP430™CapTIvateSoftwareLibraryAPIGuide 1_70_00_03

Data Fields
tTLProtocolProcessingVariables Struct Reference
CAPT_Protocol

`#include <CAPT_Protocol.h>`

## Data Fields
int8_t | i8currPacketIndex
bool | bStuffedByteDetected

## Detailed Description

typedef tTLProtocolProcessingVariables holds "static" variables that the protocol layer uses during packet framing. These variables are used by the CAPT_processReceivedData API.

## Field Documentation

## § i8currPacketIndex

int8_t tTLProtocolProcessingVariables::i8currPacketIndex

## § bStuffedByteDetected

bool tTLProtocolProcessingVariables::bStuffedByteDetected

The documentation for this struct was generated from the following file:

- CAPT_Protocol.h

© Copyright 1995-2018, Texas Instruments Incorporated. All rights reserved.
Trademarks | Privacy policy | Terms of use | Terms of sale